| MINI55_BSP V3.02.004 The Board Support Package for Mini55 Series MCU

Macros | Functions
gpio.h File Reference

MINI55 series GPIO driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | GPIO_PIN_MAX 8
#define | GPIO_MODE_INPUT 0x0UL
#define | GPIO_MODE_OUTPUT 0x1UL
#define | GPIO_MODE_OPEN_DRAIN 0x2UL
#define | GPIO_MODE_QUASI 0x3UL
#define | GPIO_INT_RISING 0x00010000UL
#define | GPIO_INT_FALLING 0x00000001UL
#define | GPIO_INT_BOTH_EDGE 0x00010001UL
#define | GPIO_INT_HIGH 0x01010000UL
#define | GPIO_INT_LOW 0x01000001UL
#define | GPIO_INTTYPE_EDGE 0UL
#define | GPIO_INTTYPE_LEVEL 1UL
#define | GPIO_DBCTL_ICLK_ON 0x00000020UL
#define | GPIO_DBCTL_ICLK_OFF 0x00000000UL
#define | GPIO_DBCTL_DBCLKSRC_IRC10K 0x00000010UL
#define | GPIO_DBCTL_DBCLKSRC_HCLK 0x00000000UL
#define | GPIO_DBCTL_DBCLKSEL_1 0x00000000UL
#define | GPIO_DBCTL_DBCLKSEL_2 0x00000001UL
#define | GPIO_DBCTL_DBCLKSEL_4 0x00000002UL
#define | GPIO_DBCTL_DBCLKSEL_8 0x00000003UL
#define | GPIO_DBCTL_DBCLKSEL_16 0x00000004UL
#define | GPIO_DBCTL_DBCLKSEL_32 0x00000005UL
#define | GPIO_DBCTL_DBCLKSEL_64 0x00000006UL
#define | GPIO_DBCTL_DBCLKSEL_128 0x00000007UL
#define | GPIO_DBCTL_DBCLKSEL_256 0x00000008UL
#define | GPIO_DBCTL_DBCLKSEL_512 0x00000009UL
#define | GPIO_DBCTL_DBCLKSEL_1024 0x0000000AUL
#define | GPIO_DBCTL_DBCLKSEL_2048 0x0000000BUL
#define | GPIO_DBCTL_DBCLKSEL_4096 0x0000000CUL
#define | GPIO_DBCTL_DBCLKSEL_8192 0x0000000DUL
#define | GPIO_DBCTL_DBCLKSEL_16384 0x0000000EUL
#define | GPIO_DBCTL_DBCLKSEL_32768 0x0000000FUL
#define | GPIO_PIN_ADDR(port, pin) (*((volatile uint32_t *)((GPIOBIT0_BASE+(0x20*(port))) + ((pin)<<2))))
#define | P00 GPIO_PIN_ADDR(0, 0)
#define | P01 GPIO_PIN_ADDR(0, 1)
#define | P02 GPIO_PIN_ADDR(0, 2)
#define | P03 GPIO_PIN_ADDR(0, 3)
#define | P04 GPIO_PIN_ADDR(0, 4)
#define | P05 GPIO_PIN_ADDR(0, 5)
#define | P06 GPIO_PIN_ADDR(0, 6)
#define | P07 GPIO_PIN_ADDR(0, 7)
#define | P10 GPIO_PIN_ADDR(1, 0)
#define | P11 GPIO_PIN_ADDR(1, 1)
#define | P12 GPIO_PIN_ADDR(1, 2)
#define | P13 GPIO_PIN_ADDR(1, 3)
#define | P14 GPIO_PIN_ADDR(1, 4)
#define | P15 GPIO_PIN_ADDR(1, 5)
#define | P16 GPIO_PIN_ADDR(1, 6)
#define | P17 GPIO_PIN_ADDR(1, 7)
#define | P20 GPIO_PIN_ADDR(2, 0)
#define | P21 GPIO_PIN_ADDR(2, 1)
#define | P22 GPIO_PIN_ADDR(2, 2)
#define | P23 GPIO_PIN_ADDR(2, 3)
#define | P24 GPIO_PIN_ADDR(2, 4)
#define | P25 GPIO_PIN_ADDR(2, 5)
#define | P26 GPIO_PIN_ADDR(2, 6)
#define | P27 GPIO_PIN_ADDR(2, 7)
#define | P30 GPIO_PIN_ADDR(3, 0)
#define | P31 GPIO_PIN_ADDR(3, 1)
#define | P32 GPIO_PIN_ADDR(3, 2)
#define | P33 GPIO_PIN_ADDR(3, 3)
#define | P34 GPIO_PIN_ADDR(3, 4)
#define | P35 GPIO_PIN_ADDR(3, 5)
#define | P36 GPIO_PIN_ADDR(3, 6)
#define | P37 GPIO_PIN_ADDR(3, 7)
#define | P40 GPIO_PIN_ADDR(4, 0)
#define | P41 GPIO_PIN_ADDR(4, 1)
#define | P42 GPIO_PIN_ADDR(4, 2)
#define | P43 GPIO_PIN_ADDR(4, 3)
#define | P44 GPIO_PIN_ADDR(4, 4)
#define | P45 GPIO_PIN_ADDR(4, 5)
#define | P46 GPIO_PIN_ADDR(4, 6)
#define | P47 GPIO_PIN_ADDR(4, 7)
#define | P50 GPIO_PIN_ADDR(5, 0)
#define | P51 GPIO_PIN_ADDR(5, 1)
#define | P52 GPIO_PIN_ADDR(5, 2)
#define | P53 GPIO_PIN_ADDR(5, 3)
#define | P54 GPIO_PIN_ADDR(5, 4)
#define | P55 GPIO_PIN_ADDR(5, 5)
#define | GPIO_CLR_INT_FLAG(gpio, u32PinMask) ((gpio)->INTSRC = u32PinMask)
| Clear GPIO Pin Interrupt Flag. More...
#define | GPIO_DISABLE_DEBOUNCE(gpio, u32PinMask) ((gpio)->DBEN &= ~u32PinMask)
| Disable Pin De-bounce Function. More...
#define | GPIO_ENABLE_DEBOUNCE(gpio, u32PinMask) ((gpio)->DBEN |= u32PinMask)
| Enable Pin De-bounce Function. More...
#define | GPIO_DISABLE_DIGITAL_PATH(gpio, u32PinMask) ((gpio)->DINOFF |= (u32PinMask << 16))
| Disable I/O Digital Input Path. More...
#define | GPIO_ENABLE_DIGITAL_PATH(gpio, u32PinMask) ((gpio)->DINOFF &= ~(u32PinMask << 16))
| Enable I/O Digital Input Path. More...
#define | GPIO_DISABLE_DOUT_MASK(gpio, u32PinMask) ((gpio)->DATMSK &= ~u32PinMask)
| Disable I/O DOUT mask. More...
#define | GPIO_ENABLE_DOUT_MASK(gpio, u32PinMask) ((gpio)->DATMSK |= u32PinMask)
| Enable I/O DOUT mask. More...
#define | GPIO_GET_INT_FLAG(gpio, u32PinMask) ((gpio)->INTSRC & u32PinMask)
| Get GPIO Pin Interrupt Flag. More...
#define | GPIO_SET_DEBOUNCE_TIME(clksrc, clksel) (GPIO->DBCTL = (GP_DBCTL_ICLKON_Msk | clksrc | clksel))
| Set De-bounce Sampling Cycle Time. More...
#define | GPIO_GET_IN_DATA(gpio) ((gpio)->PIN)
| Get GPIO Port IN Data. More...
#define | GPIO_SET_OUT_DATA(gpio, data) ((gpio)->DOUT = (data))
| Set GPIO Port OUT Data. More...
#define | GPIO_TOGGLE(u32Pin) ((u32Pin) ^= 1)
| Toggle Specified GPIO pin. More...
#define | GPIO_EnableEINT0 GPIO_EnableInt
| Enable External GPIO interrupt 0. More...
#define | GPIO_DisableEINT0 GPIO_DisableInt
| Disable External GPIO interrupt 0. More...
#define | GPIO_EnableEINT1 GPIO_EnableInt
| Enable External GPIO interrupt 1. More...
#define | GPIO_DisableEINT1 GPIO_DisableInt
| Disable External GPIO interrupt 1. More...

## Functions
void | GPIO_SetMode (GPIO_T *gpio, uint32_t u32PinMask, uint32_t u32Mode)
| Set GPIO operation mode. More...
void | GPIO_EnableInt (GPIO_T *gpio, uint32_t u32Pin, uint32_t u32IntAttribs)
| Enable GPIO interrupt. More...
void | GPIO_DisableInt (GPIO_T *gpio, uint32_t u32Pin)
| Disable GPIO interrupt. More...

## Detailed Description

MINI55 series GPIO driver header file.

Version
  V1.00

Revision
  11

Date
  15/07/09 9:40a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file gpio.h.