| MINI55_BSP V3.02.004 The Board Support Package for Mini55 Series MCU

Functions
uart.c File Reference

MINI55 series UART driver source file. More...

`#include <stdio.h>`
`#include "Mini55Series.h"`
Include dependency graph for uart.c:

Go to the source code of this file.

## Functions
void | UART_ClearIntFlag (UART_T *uart, uint32_t u32InterruptFlag)
| The function is used to clear UART specified interrupt flag. More...
void | UART_Close (UART_T *uart)
| The function is used to disable UART. More...
void | UART_DisableFlowCtrl (UART_T *uart)
| The function is used to disable UART auto flow control. More...
void | UART_DisableInt (UART_T *uart, uint32_t u32InterruptFlag)
| The function is used to disable UART specified interrupt and disable NVIC UART IRQ. More...
void | UART_EnableFlowCtrl (UART_T *uart)
| The function is used to Enable UART auto flow control. More...
void | UART_EnableInt (UART_T *uart, uint32_t u32InterruptFlag)
| The function is used to enable UART specified interrupt and disable NVIC UART IRQ. More...
void | UART_Open (UART_T *uart, uint32_t u32baudrate)
| This function use to enable UART function and set baud-rate. More...
uint32_t | UART_Read (UART_T *uart, uint8_t *pu8RxBuf, uint32_t u32ReadBytes)
| The function is used to read Rx data from RX FIFO and the data will be stored in pu8RxBuf. More...
void | UART_SetLine_Config (UART_T *uart, uint32_t u32baudrate, uint32_t u32data_width, uint32_t u32parity, uint32_t u32stop_bits)
| This function use to config UART line setting. More...
void | UART_SetTimeoutCnt (UART_T *uart, uint32_t u32TOC)
| This function use to set Rx timeout count. More...
void | UART_SelectIrDAMode (UART_T *uart, uint32_t u32Buadrate, uint32_t u32Direction)
| The function is used to configure IrDA relative settings. It consists of TX or RX mode and baudrate. More...
void | UART_SelectRS485Mode (UART_T *uart, uint32_t u32Mode, uint32_t u32Addr)
| The function is used to set RS485 relative setting. More...
uint32_t | UART_Write (UART_T *uart, uint8_t *pu8TxBuf, uint32_t u32WriteBytes)
| The function is to write data into TX buffer to transmit data by UART. More...

## Detailed Description

MINI55 series UART driver source file.

Version
  V1.00

Revision
  9

Date
  15/07/08 3:45p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file uart.c.