| MINI55_BSP V3.03.000 The Board Support Package for Mini55 Series MCU

Macros | Functions
ADC Exported Functions
MINI55 Device Driver » ADC Driver » ADC Exported Constants
Collaboration diagram for ADC Exported Functions:

## Macros
#define | ADC_CONFIG_CH7(adc, u32Source)
| Configure the analog input source of channel 7. More...
#define | ADC_GET_CONVERSION_DATA(adc, u32ChNum)
| Get the latest ADC conversion data. More...
#define | ADC_GET_INT_FLAG(adc, u32Mask)
| Return the user-specified interrupt flags. More...
#define | ADC_CLR_INT_FLAG(adc, u32Mask)
| This macro clear the selected interrupt status bits. More...
#define | ADC_IS_BUSY(adc)
| Get the busy state of ADC. More...
#define | ADC_IS_DATA_OVERRUN(adc, u32ChNum)
| Check if the ADC conversion data is over written or not. More...
#define | ADC_IS_DATA_VALID(adc, u32ChNum)
| Check if the ADC conversion data is valid or not. More...
#define | ADC_POWER_DOWN(adc)
| Power down ADC module. More...
#define | ADC_POWER_ON(adc)
| Power on ADC module. More...
#define | ADC_ENABLE_CMP0(adc, u32ChNum, u32Condition, u32Data, u32MatchCount)
| Configure the comparator 0 and enable it. More...
#define | ADC_DISABLE_CMP0(adc)
| Disable comparator 0. More...
#define | ADC_ENABLE_CMP1(adc, u32ChNum, u32Condition, u32Data, u32MatchCount)
| Configure the comparator 1 and enable it. More...
#define | ADC_DISABLE_CMP1(adc)
| Disable comparator 1. More...
#define | ADC_SET_INPUT_CHANNEL(adc, u32Mask)
| Set ADC input channel. Enabled channel will be converted while ADC starts. More...
#define | ADC_START_CONV(adc)
| Start the A/D conversion. More...
#define | ADC_STOP_CONV(adc)
| Stop the A/D conversion. More...

## Functions
void | ADC_Open (ADC_T *adc, uint32_t u32InputMode, uint32_t u32OpMode, uint32_t u32ChMask)
| This API configures ADC module to be ready for convert the input from selected channel. More...
void | ADC_Close (ADC_T *adc)
| Disable ADC module. More...
void | ADC_EnableHWTrigger (ADC_T *adc, uint32_t u32Source, uint32_t u32Param)
| Configure the hardware trigger condition and enable hardware trigger. More...
void | ADC_DisableHWTrigger (ADC_T *adc)
| Disable hardware trigger ADC function. More...
void | ADC_SetExtraSampleTime (ADC_T *adc, uint32_t u32ChNum, uint32_t u32SampleTime)
| Set ADC sample time for designated channel. More...
void | ADC_EnableInt (ADC_T *adc, uint32_t u32Mask)
| Enable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_DisableInt (ADC_T *adc, uint32_t u32Mask)
| Disable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_SeqModeEnable (ADC_T *adc, uint32_t u32SeqTYPE, uint32_t u32ModeSel)
| ADC PWM Sequential Mode Control. More...
void | ADC_SeqModeTriggerSrc (ADC_T *adc, uint32_t u32SeqModeTrgSrc1, uint32_t u32Trg1Type, uint32_t u32SeqModeTrgSrc2, uint32_t u32Trg2Type)
| ADC PWM Sequential Mode PWM Trigger Source and type. More...

## Detailed Description

## Macro Definition Documentation

## ◆ ADC_CLR_INT_FLAG

#define ADC_CLR_INT_FLAG | ( |  | adc,
|  |  | u32Mask
| ) |  |

This macro clear the selected interrupt status bits.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Mask | The combination of following interrupt status bits. Each bit corresponds to a interrupt status. ADC_ADIF_INT ADC_CMP0_INT ADC_CMP1_INT

Returns
  None

Definition at line 120 of file adc.h.

## ◆ ADC_CONFIG_CH7

#define ADC_CONFIG_CH7 | ( |  | adc,
|  |  | u32Source
| ) |  |

Configure the analog input source of channel 7.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Source | Decides the analog input source of channel 7, valid values are ADC_CH7_EXT ADC_CH7_BGP

Returns
  None

Note
  While using VBG as channel 7 source, ADC module clock must /b not exceed 300kHz

Definition at line 87 of file adc.h.

## ◆ ADC_DISABLE_CMP0

#define ADC_DISABLE_CMP0 | ( |  | adc | ) |

Disable comparator 0.

Parameters

  [in] | adc | Base address of ADC module

Definition at line 202 of file adc.h.

## ◆ ADC_DISABLE_CMP1

#define ADC_DISABLE_CMP1 | ( |  | adc | ) |

Disable comparator 1.

Parameters

  [in] | adc | Base address of ADC module

Definition at line 234 of file adc.h.

## ◆ ADC_ENABLE_CMP0

#define ADC_ENABLE_CMP0 | ( |  | adc,
|  |  | u32ChNum,
|  |  | u32Condition,
|  |  | u32Data,
|  |  | u32MatchCount
| ) |  |

Configure the comparator 0 and enable it.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32ChNum | Specifies the source channel, valid value are from 0 to 7
  [in] | u32Condition | Specifies the compare condition ADC_CMP_LESS_THAN ADC_CMP_GREATER_OR_EQUAL_TO
  [in] | u32Data | Specifies the compare value. Valid value are between 0 ~ 0x3FF
  [in] | u32MatchCount | Specifies the match count setting, valid values are between 1~16

Returns
  None

For example, ADC_ENABLE_CMP0(ADC, 5, ADC_CMP_GREATER_OR_EQUAL_TO, 0x800, 10); Means ADC will assert comparator 0 flag if channel 5 conversion result is greater or equal to 0x800 for 10 times continuously.

Definition at line 187 of file adc.h.

## ◆ ADC_ENABLE_CMP1

#define ADC_ENABLE_CMP1 | ( |  | adc,
|  |  | u32ChNum,
|  |  | u32Condition,
|  |  | u32Data,
|  |  | u32MatchCount
| ) |  |

Configure the comparator 1 and enable it.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32ChNum | Specifies the source channel, valid value are from 0 to 7
  [in] | u32Condition | Specifies the compare condition ADC_CMP_LESS_THAN ADC_CMP_GREATER_OR_EQUAL_TO
  [in] | u32Data | Specifies the compare value. Valid value are between 0 ~ 0x3FF
  [in] | u32MatchCount | Specifies the match count setting, valid values are between 1~16

Returns
  None

For example, ADC_ENABLE_CMP1(ADC, 5, ADC_CMP_GREATER_OR_EQUAL_TO, 0x800, 10); Means ADC will assert comparator 1 flag if channel 5 conversion result is greater or equal to 0x800 for 10 times continuously.

Definition at line 219 of file adc.h.

## ◆ ADC_GET_CONVERSION_DATA

#define ADC_GET_CONVERSION_DATA | ( |  | adc,
|  |  | u32ChNum
| ) |  |

Get the latest ADC conversion data.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32ChNum | Currently not used

Returns
  Latest ADC conversion data

Definition at line 96 of file adc.h.

## ◆ ADC_GET_INT_FLAG

#define ADC_GET_INT_FLAG | ( |  | adc,
|  |  | u32Mask
| ) |  |

Return the user-specified interrupt flags.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Mask | The combination of following interrupt status bits. Each bit corresponds to a interrupt status. ADC_ADIF_INT ADC_CMP0_INT ADC_CMP1_INT

Returns
  User specified interrupt flags

Definition at line 108 of file adc.h.

## ◆ ADC_IS_BUSY

#define ADC_IS_BUSY | ( |  | adc | ) |

Get the busy state of ADC.

Parameters

  [in] | adc | Base address of ADC module

Returns
  busy state of ADC

Return values

  0 | ADC is not busy
  1 | ADC is busy

Definition at line 132 of file adc.h.

## ◆ ADC_IS_DATA_OVERRUN

#define ADC_IS_DATA_OVERRUN | ( |  | adc,
|  |  | u32ChNum
| ) |  |

Check if the ADC conversion data is over written or not.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32ChNum | Currently not used

Returns
  Over run state of ADC data

Return values

  0 | ADC data is not overrun
  1 | ADC data us overrun

Definition at line 143 of file adc.h.

## ◆ ADC_IS_DATA_VALID

#define ADC_IS_DATA_VALID | ( |  | adc,
|  |  | u32ChNum
| ) |  |

Check if the ADC conversion data is valid or not.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32ChNum | Currently not used

Returns
  Valid state of ADC data

Return values

  0 | ADC data is not valid
  1 | ADC data us valid

Definition at line 154 of file adc.h.

## ◆ ADC_POWER_DOWN

#define ADC_POWER_DOWN | ( |  | adc | ) |

Power down ADC module.

Parameters

  [in] | adc | Base address of ADC module

Returns
  None

Definition at line 162 of file adc.h.

## ◆ ADC_POWER_ON

#define ADC_POWER_ON | ( |  | adc | ) |

Power on ADC module.

Parameters

  [in] | adc | Base address of ADC module

Returns
  None

Definition at line 170 of file adc.h.

## ◆ ADC_SET_INPUT_CHANNEL

#define ADC_SET_INPUT_CHANNEL | ( |  | adc,
|  |  | u32Mask
| ) |  |

Set ADC input channel. Enabled channel will be converted while ADC starts.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Mask | Channel enable bit. Each bit corresponds to a input channel. Bit 0 is channel 0, bit 1 is channel 1...

Returns
  None

Note
  MINI55 series MCU ADC can only convert 1 channel at a time. If more than 1 channels are enabled, only channel with smallest number will be convert.

Definition at line 245 of file adc.h.

## ◆ ADC_START_CONV

#define ADC_START_CONV | ( |  | adc | ) |

Start the A/D conversion.

Parameters

  [in] | adc | Base address of ADC module

Returns
  None

Definition at line 253 of file adc.h.

## ◆ ADC_STOP_CONV

#define ADC_STOP_CONV | ( |  | adc | ) |

Stop the A/D conversion.

Parameters

  [in] | adc | Base address of ADC module

Returns
  None

Definition at line 261 of file adc.h.

## Function Documentation

## ◆ ADC_Close()

void ADC_Close | ( | ADC_T * | adc | ) |

Disable ADC module.

Parameters

  [in] | adc | Base address of ADC module

Returns
  None

Definition at line 61 of file adc.c.

## ◆ ADC_DisableHWTrigger()

void ADC_DisableHWTrigger | ( | ADC_T * | adc | ) |

Disable hardware trigger ADC function.

Parameters

  [in] | adc | Base address of ADC module

Returns
  None

Definition at line 105 of file adc.c.

## ◆ ADC_DisableInt()

void ADC_DisableInt | ( | ADC_T * | adc,
|  | uint32_t | u32Mask
| ) |  |

Disable the interrupt(s) selected by u32Mask parameter.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Mask | The combination of interrupt status bits listed below. Each bit corresponds to a interrupt status. This parameter decides which interrupts will be disabled. ADC_ADIF_INT ADC_CMP0_INT ADC_CMP1_INT

Returns
  None

Definition at line 171 of file adc.c.

## ◆ ADC_EnableHWTrigger()

void ADC_EnableHWTrigger | ( | ADC_T * | adc,
|  | uint32_t | u32Source,
|  | uint32_t | u32Param
| ) |  |

Configure the hardware trigger condition and enable hardware trigger.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Source | Decides the hardware trigger source. Valid values are: ADC_TRIGGER_BY_EXT_PIN ADC_TRIGGER_BY_PWM
  [in] | u32Param | While ADC trigger by PWM, this parameter is used to set the delay between PWM trigger and ADC conversion. Valid values are from 0 ~ 0xFF, and actual delay time is (4 * u32Param * HCLK). While ADC trigger by external pin, this parameter is used to set trigger condition. Valid values are: ADC_FALLING_EDGE_TRIGGER ADC_RISING_EDGE_TRIGGER

Returns
  None

Definition at line 83 of file adc.c.

## ◆ ADC_EnableInt()

void ADC_EnableInt | ( | ADC_T * | adc,
|  | uint32_t | u32Mask
| ) |  |

Enable the interrupt(s) selected by u32Mask parameter.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32Mask | The combination of interrupt status bits listed below. Each bit corresponds to a interrupt status. This parameter decides which interrupts will be enabled. ADC_ADIF_INT ADC_CMP0_INT ADC_CMP1_INT

Returns
  None

Definition at line 148 of file adc.c.

## ◆ ADC_Open()

void ADC_Open | ( | ADC_T * | adc,
|  | uint32_t | u32InputMode,
|  | uint32_t | u32OpMode,
|  | uint32_t | u32ChMask
| ) |  |

This API configures ADC module to be ready for convert the input from selected channel.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32InputMode | This parameter is unused
  [in] | u32OpMode | This parameter is unused
  [in] | u32ChMask | Channel enable bit. Each bit corresponds to a input channel. Bit 0 is channel 0, bit 1 is channel 1...

Returns
  None

Note
  MINI55 series MCU ADC can only convert 1 channel at a time. If more than 1 channels are enabled, only channel with smallest number will be convert.
  This API does not turn on ADC power nor does trigger ADC conversion

Definition at line 38 of file adc.c.

## ◆ ADC_SeqModeEnable()

void ADC_SeqModeEnable | ( | ADC_T * | adc,
|  | uint32_t | u32SeqTYPE,
|  | uint32_t | u32ModeSel
| ) |  |

ADC PWM Sequential Mode Control.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32SeqTYPE | This parameter decides which type will be selected. ADC_SEQMODE_TYPE_23SHUNT ADC_SEQMODE_TYPE_1SHUNT
  [in] | u32ModeSel | This parameter decides which mode will be selected. ADC_SEQMODE_MODESELECT_CH01 ADC_SEQMODE_MODESELECT_CH12 ADC_SEQMODE_MODESELECT_CH02

Returns
  None

Definition at line 195 of file adc.c.

## ◆ ADC_SeqModeTriggerSrc()

void ADC_SeqModeTriggerSrc | ( | ADC_T * | adc,
|  | uint32_t | u32SeqModeTrgSrc1,
|  | uint32_t | u32Trg1Type,
|  | uint32_t | u32SeqModeTrgSrc2,
|  | uint32_t | u32Trg2Type
| ) |  |

ADC PWM Sequential Mode PWM Trigger Source and type.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32SeqModeTrgSrc1 | This parameter decides first PWM trigger source.
  [in] | u32Trg1Type | This parameter decides second PWM trigger type.
  [in] | u32SeqModeTrgSrc2 | This parameter decides first PWM trigger source.
  [in] | u32Trg2Type | This parameter decides second PWM trigger type.

Returns
  None

Definition at line 219 of file adc.c.

## ◆ ADC_SetExtraSampleTime()

void ADC_SetExtraSampleTime | ( | ADC_T * | adc,
|  | uint32_t | u32ChNum,
|  | uint32_t | u32SampleTime
| ) |  |

Set ADC sample time for designated channel.

Parameters

  [in] | adc | Base address of ADC module
  [in] | u32ChNum | This parameter is not used
  [in] | u32SampleTime | ADC sample ADC time, valid values are ADC_SAMPLE_CLOCK_0 ADC_SAMPLE_CLOCK_1 ADC_SAMPLE_CLOCK_2 ADC_SAMPLE_CLOCK_4 ADC_SAMPLE_CLOCK_8 ADC_SAMPLE_CLOCK_16 ADC_SAMPLE_CLOCK_32 ADC_SAMPLE_CLOCK_64 ADC_SAMPLE_CLOCK_128 ADC_SAMPLE_CLOCK_256 ADC_SAMPLE_CLOCK_512 ADC_SAMPLE_CLOCK_1024

Returns
  None

Definition at line 130 of file adc.c.