| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Data Fields
PWM_T Struct Reference
NUC029FAE Device CMSIS Definitions » NUC029FAE Control Register » Analog Comparator Controller(ACMP) » System Clock Controller(CLK) » Analog to Digital Converter(ADC) » Flash Memory Controller(FMC) » General Purpose Input/Output Controller(GPIO) » Inter-IC Bus Controller(I2C) » Interrupt Source Controller (INT) » Pulse Width Modulation Controller(PWM)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | PPR
__IO uint32_t | CSR
__IO uint32_t | PCR
__IO uint32_t | CNR [6]
__IO uint32_t | CMR [6]
uint32_t | RESERVED0 [6]
__IO uint32_t | PIER
__IO uint32_t | PIIR
__IO uint32_t | POE
__IO uint32_t | PFBCON
__IO uint32_t | PDZIR
__IO uint32_t | TRGCON0
__IO uint32_t | TRGCON1
__IO uint32_t | TRGSTS0
__IO uint32_t | TRGSTS1
__IO uint32_t | PHCHG
__IO uint32_t | PHCHGNXT
__IO uint32_t | PHCHGMASK
__IO uint32_t | INTACCUCTL

## Detailed Description

Definition at line 1171 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h