| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Modules | Macros
FMC Exported Constants
NUC029FAE Device Driver » FMC Driver
Collaboration diagram for FMC Exported Constants:

## Modules
| FMC Exported Functions

## Macros
#define | FMC_APROM_BASE 0x00000000UL
#define | FMC_LDROM_BASE 0x00100000UL
#define | FMC_LDROM_END 0x00100800UL
#define | FMC_CONFIG_BASE 0x00300000UL
#define | FMC_FLASH_PAGE_SIZE 0x200
#define | FMC_LDROM_SIZE 0x800
#define | FMC_TIMEOUT_READ
#define | FMC_TIMEOUT_WRITE
#define | FMC_TIMEOUT_ERASE
#define | FMC_TIMEOUT_CHKSUM
#define | FMC_ISPCMD_READ 0x00
#define | FMC_ISPCMD_PROGRAM 0x21
#define | FMC_ISPCMD_PAGE_ERASE 0x22
#define | FMC_ISPCMD_READ_CID 0x0B
#define | FMC_ISPCMD_READ_PID 0x0C
#define | FMC_ISPCMD_READ_UID 0x04
#define | FMC_ISPCMD_VECMAP 0x2E

## Detailed Description

## Macro Definition Documentation

## ◆ FMC_APROM_BASE

#define FMC_APROM_BASE 0x00000000UL

APROM Base Address

Definition at line 34 of file fmc.h.

## ◆ FMC_CONFIG_BASE

#define FMC_CONFIG_BASE 0x00300000UL

CONFIG Base Address

Definition at line 37 of file fmc.h.

## ◆ FMC_FLASH_PAGE_SIZE

#define FMC_FLASH_PAGE_SIZE 0x200

Flash Page Size (512 Bytes)

Definition at line 39 of file fmc.h.

## ◆ FMC_ISPCMD_PAGE_ERASE

#define FMC_ISPCMD_PAGE_ERASE 0x22

ISP Command: Page Erase Flash

Definition at line 52 of file fmc.h.

## ◆ FMC_ISPCMD_PROGRAM

#define FMC_ISPCMD_PROGRAM 0x21

ISP Command: Program Flash

Definition at line 51 of file fmc.h.

## ◆ FMC_ISPCMD_READ

#define FMC_ISPCMD_READ 0x00

ISP Command: Read Flash

Definition at line 50 of file fmc.h.

## ◆ FMC_ISPCMD_READ_CID

#define FMC_ISPCMD_READ_CID 0x0B

ISP Command: Read Company ID

Definition at line 53 of file fmc.h.

## ◆ FMC_ISPCMD_READ_PID

#define FMC_ISPCMD_READ_PID 0x0C

ISP Command: Read Product ID

Definition at line 54 of file fmc.h.

## ◆ FMC_ISPCMD_READ_UID

#define FMC_ISPCMD_READ_UID 0x04

ISP Command: Read Unique ID

Definition at line 55 of file fmc.h.

## ◆ FMC_ISPCMD_VECMAP

#define FMC_ISPCMD_VECMAP 0x2E

ISP Command: Vector Page Remap

Definition at line 56 of file fmc.h.

## ◆ FMC_LDROM_BASE

#define FMC_LDROM_BASE 0x00100000UL

LDROM Base Address

Definition at line 35 of file fmc.h.

## ◆ FMC_LDROM_END

#define FMC_LDROM_END 0x00100800UL

LDROM End Address

Definition at line 36 of file fmc.h.

## ◆ FMC_LDROM_SIZE

#define FMC_LDROM_SIZE 0x800

LDROM Size (2 Kbytes)

Definition at line 40 of file fmc.h.

## ◆ FMC_TIMEOUT_CHKSUM

#define FMC_TIMEOUT_CHKSUM

Get checksum command time-out 2 s

Definition at line 45 of file fmc.h.

## ◆ FMC_TIMEOUT_ERASE

#define FMC_TIMEOUT_ERASE

Erase command time-out 200 ms

Definition at line 44 of file fmc.h.

## ◆ FMC_TIMEOUT_READ

#define FMC_TIMEOUT_READ

Read command time-out 100 ms

Definition at line 42 of file fmc.h.

## ◆ FMC_TIMEOUT_WRITE

#define FMC_TIMEOUT_WRITE

Write command time-out 100 ms

Definition at line 43 of file fmc.h.