| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Data Fields
UART_T Struct Reference
NUC029FAE Device CMSIS Definitions » NUC029FAE Control Register » Analog Comparator Controller(ACMP) » System Clock Controller(CLK) » Analog to Digital Converter(ADC) » Flash Memory Controller(FMC) » General Purpose Input/Output Controller(GPIO) » Inter-IC Bus Controller(I2C) » Interrupt Source Controller (INT) » Pulse Width Modulation Controller(PWM) » Serial Peripheral Interface Controller(SPI) » System Manger Controller(SYS) » Timer Controller(TIMER) » Universal Asynchronous Receiver/Transmitter Controller(UART)

`#include <NUC029FAE.h>`

## Data Fields
union {
__I uint32_t UART_T::RBR
__O uint32_t UART_T::THR
}; |
__IO uint32_t | IER
__IO uint32_t | FCR
__IO uint32_t | LCR
__IO uint32_t | MCR
__IO uint32_t | MSR
__IO uint32_t | FSR
__IO uint32_t | ISR
__IO uint32_t | TOR
__IO uint32_t | BAUD
__IO uint32_t | IRCR
__IO uint32_t | ALT_CSR
__IO uint32_t | FUN_SEL

## Detailed Description

Definition at line 2867 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h