| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - g -

- g_FMC_i32ErrCode : fmc.c
- g_ICE_Conneced : retarget.c
- GET_BYTE0 : NUC029FAE.h
- GET_BYTE1 : NUC029FAE.h
- GET_BYTE2 : NUC029FAE.h
- GET_BYTE3 : NUC029FAE.h
- GetChar() : retarget.c
- GPIO : NUC029FAE.h
- GPIO01_IRQn : NUC029FAE.h
- GPIO234_IRQn : NUC029FAE.h
- GPIO5_IRQn : NUC029FAE.h
- GPIO_CLR_INT_FLAG : gpio.h
- GPIO_DBNCECON_BASE : NUC029FAE.h
- GPIO_DBNCECON_DBCLKSEL_1 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_1024 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_128 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_16 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_16384 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_2 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_2048 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_256 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_32 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_32768 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_4 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_4096 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_512 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_64 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_8 : gpio.h
- GPIO_DBNCECON_DBCLKSEL_8192 : gpio.h
- GPIO_DBNCECON_DBCLKSRC_HCLK : gpio.h
- GPIO_DBNCECON_DBCLKSRC_IRC10K : gpio.h
- GPIO_DBNCECON_ICLK_OFF : gpio.h
- GPIO_DBNCECON_ICLK_ON : gpio.h
- GPIO_DISABLE_DEBOUNCE : gpio.h
- GPIO_DISABLE_DIGITAL_PATH : gpio.h
- GPIO_DISABLE_DOUT_MASK : gpio.h
- GPIO_DisableEINT0 : gpio.h
- GPIO_DisableEINT1 : gpio.h
- GPIO_DisableInt() : gpio.h
- GPIO_ENABLE_DEBOUNCE : gpio.h
- GPIO_ENABLE_DIGITAL_PATH : gpio.h
- GPIO_ENABLE_DOUT_MASK : gpio.h
- GPIO_EnableEINT0 : gpio.h
- GPIO_EnableEINT1 : gpio.h
- GPIO_EnableInt() : gpio.h
- GPIO_GET_IN_DATA : gpio.h
- GPIO_GET_INT_FLAG : gpio.h
- GPIO_IMD_EDGE : gpio.h
- GPIO_IMD_LEVEL : gpio.h
- GPIO_INT_BOTH_EDGE : gpio.h
- GPIO_INT_FALLING : gpio.h
- GPIO_INT_HIGH : gpio.h
- GPIO_INT_LOW : gpio.h
- GPIO_INT_RISING : gpio.h
- GPIO_PIN_ADDR : gpio.h
- GPIO_PIN_DATA_BASE : NUC029FAE.h
- GPIO_PIN_MAX : gpio.h
- GPIO_PMD_INPUT : gpio.h
- GPIO_PMD_OPEN_DRAIN : gpio.h
- GPIO_PMD_OUTPUT : gpio.h
- GPIO_PMD_QUASI : gpio.h
- GPIO_RST : sys.h
- GPIO_SET_DEBOUNCE_TIME : gpio.h
- GPIO_SET_OUT_DATA : gpio.h
- GPIO_SetMode() : gpio.h
- GPIO_TOGGLE : gpio.h
- GPIOBIT0 : NUC029FAE.h
- GPIOBIT0_BASE : NUC029FAE.h
- GPIOBIT1 : NUC029FAE.h
- GPIOBIT1_BASE : NUC029FAE.h
- GPIOBIT2 : NUC029FAE.h
- GPIOBIT2_BASE : NUC029FAE.h
- GPIOBIT3 : NUC029FAE.h
- GPIOBIT3_BASE : NUC029FAE.h
- GPIOBIT4 : NUC029FAE.h
- GPIOBIT4_BASE : NUC029FAE.h
- GPIOBIT5 : NUC029FAE.h
- GPIOBIT5_BASE : NUC029FAE.h