| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Data Fields
SYS_T Struct Reference
NUC029FAE Device CMSIS Definitions » NUC029FAE Control Register » Analog Comparator Controller(ACMP) » System Clock Controller(CLK) » Analog to Digital Converter(ADC) » Flash Memory Controller(FMC) » General Purpose Input/Output Controller(GPIO) » Inter-IC Bus Controller(I2C) » Interrupt Source Controller (INT) » Pulse Width Modulation Controller(PWM) » Serial Peripheral Interface Controller(SPI) » System Manger Controller(SYS)

`#include <NUC029FAE.h>`

## Data Fields
__I uint32_t | PDID
__IO uint32_t | RSTSRC
__IO uint32_t | IPRSTC1
__IO uint32_t | IPRSTC2
uint32_t | RESERVED0 [2]
__IO uint32_t | BODCTL
uint32_t | RESERVED1 [5]
__IO uint32_t | P0_MFP
__IO uint32_t | P1_MFP
__IO uint32_t | P2_MFP
__IO uint32_t | P3_MFP
__IO uint32_t | P4_MFP
__IO uint32_t | P5_MFP
uint32_t | RESERVED3 [14]
__IO uint32_t | IRCTRIMCTL
__IO uint32_t | IRCTRIMIER
__IO uint32_t | IRCTRIMISR
uint32_t | RESERVED4 [29]
__IO uint32_t | RegLockAddr

## Detailed Description

Definition at line 1996 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h