| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Macros | Functions
SPI Exported Functions
NUC029FAE Device Driver » SPI Driver » SPI Exported Constants
Collaboration diagram for SPI Exported Functions:

## Macros
#define | SPI_ABORT_3WIRE_TRANSFER(spi) ( (spi)->CNTRL2 |= SPI_CNTRL2_SLV_ABORT_Msk )
| Abort the current transfer in slave 3-wire mode. More...
#define | SPI_CLR_3WIRE_START_INT_FLAG(spi) ( (spi)->STATUS = SPI_STATUS_SLV_START_INTSTS_Msk )
| Clear the slave 3-wire mode start interrupt flag. More...
#define | SPI_CLR_UNIT_TRANS_INT_FLAG(spi) ( (spi)->STATUS = SPI_STATUS_IF_Msk )
| Clear the unit transfer interrupt flag. More...
#define | SPI_DISABLE_3WIRE_MODE(spi) ( (spi)->CNTRL2 &= ~SPI_CNTRL2_NOSLVSEL_Msk )
| Disable slave 3-wire mode. More...
#define | SPI_ENABLE_3WIRE_MODE(spi) ( (spi)->CNTRL2 |= SPI_CNTRL2_NOSLVSEL_Msk )
| Enable slave 3-wire mode. More...
#define | SPI_GET_RX_FIFO_COUNT(spi) ( (((spi)->STATUS & SPI_STATUS_RX_FIFO_COUNT_Msk) >> SPI_STATUS_RX_FIFO_COUNT_Pos) & 0xf )
| Get the count of available data in RX FIFO. More...
#define | SPI_GET_RX_FIFO_EMPTY_FLAG(spi) ( ((spi)->STATUS & SPI_STATUS_RX_EMPTY_Msk) == SPI_STATUS_RX_EMPTY_Msk ? 1:0 )
| Get the Rx FIFO empty flag. More...
#define | SPI_GET_TX_FIFO_EMPTY_FLAG(spi) ( ((spi)->STATUS & SPI_STATUS_TX_EMPTY_Msk) == SPI_STATUS_TX_EMPTY_Msk ? 1:0 )
| Get the Tx FIFO empty flag. More...
#define | SPI_READ_RX(spi) ( (spi)->RX )
| Get the datum read from Rx FIFO. More...
#define | SPI_WRITE_TX(spi, u32TxData) ( (spi)->TX = u32TxData )
| Write datum to TX register. More...
#define | SPI_ENABLE_BYTE_REORDER(spi) ( (spi)->CNTRL |= SPI_CNTRL_REORDER_Msk )
| Enable byte reorder function. More...
#define | SPI_DISABLE_BYTE_REORDER(spi) ( (spi)->CNTRL &= ~SPI_CNTRL_REORDER_Msk )
| Disable byte reorder function. More...
#define | SPI_SET_SUSPEND_CYCLE(spi, u32SuspCycle) ( (spi)->CNTRL = ((spi)->CNTRL & ~SPI_CNTRL_SP_CYCLE_Msk) | (u32SuspCycle << SPI_CNTRL_SP_CYCLE_Pos) )
| Set the length of suspend interval. More...
#define | SPI_SET_LSB_FIRST(spi) ( (spi)->CNTRL |= SPI_CNTRL_LSB_Msk )
| Set the SPI transfer sequence with LSB first. More...
#define | SPI_SET_MSB_FIRST(spi) ( (spi)->CNTRL &= ~SPI_CNTRL_LSB_Msk )
| Set the SPI transfer sequence with MSB first. More...
#define | SPI_IS_BUSY(spi) ( ((spi)->CNTRL & SPI_CNTRL_GO_BUSY_Msk) == SPI_CNTRL_GO_BUSY_Msk ? 1:0 )
| Get the SPI busy state. More...
#define | SPI_TRIGGER(spi) ( (spi)->CNTRL |= SPI_CNTRL_GO_BUSY_Msk )
| Set the GO_BUSY bit to trigger SPI transfer. More...

## Functions
static __INLINE void | SPI_SET_SS_HIGH (SPI_T *spi)
| Disable automatic slave select function and set SPI_SS pin to high state. More...
static __INLINE void | SPI_SET_SS_LOW (SPI_T *spi)
| Disable automatic slave select function and set SPI_SS pin to low state. More...
static __INLINE void | SPI_SET_DATA_WIDTH (SPI_T *spi, uint32_t u32Width)
| Set the data width of a SPI transaction. More...
uint32_t | SPI_Open (SPI_T *spi, uint32_t u32MasterSlave, uint32_t u32SPIMode, uint32_t u32DataWidth, uint32_t u32BusClock)
| This function make SPI module be ready to transfer. By default, the SPI transfer sequence is MSB first and the automatic slave select function is disabled. In Slave mode, the u32BusClock must be NULL and the SPI clock divider setting will be 0. More...
void | SPI_Close (SPI_T *spi)
| Reset SPI module and disable SPI peripheral clock. More...
void | SPI_ClearRxFIFO (SPI_T *spi)
| Clear Rx FIFO buffer. More...
void | SPI_ClearTxFIFO (SPI_T *spi)
| Clear Tx FIFO buffer. More...
void | SPI_DisableAutoSS (SPI_T *spi)
| Disable the automatic slave select function. More...
void | SPI_EnableAutoSS (SPI_T *spi, uint32_t u32SSPinMask, uint32_t u32ActiveLevel)
| Enable the automatic slave select function. Only available in Master mode. More...
uint32_t | SPI_SetBusClock (SPI_T *spi, uint32_t u32BusClock)
| Set the SPI bus clock. Only available in Master mode. More...
void | SPI_EnableFIFO (SPI_T *spi, uint32_t u32TxThreshold, uint32_t u32RxThreshold)
| Enable FIFO mode with user-specified Tx FIFO threshold and Rx FIFO threshold configurations. More...
void | SPI_DisableFIFO (SPI_T *spi)
| Disable FIFO mode. More...
uint32_t | SPI_GetBusClock (SPI_T *spi)
| Get the actual frequency of SPI bus clock. Only available in Master mode. More...
void | SPI_EnableInt (SPI_T *spi, uint32_t u32Mask)
| Enable FIFO related interrupts specified by u32Mask parameter. More...
void | SPI_DisableInt (SPI_T *spi, uint32_t u32Mask)
| Disable FIFO related interrupts specified by u32Mask parameter. More...

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_ABORT_3WIRE_TRANSFER

#define SPI_ABORT_3WIRE_TRANSFER | ( |  | spi | ) | ( (spi)->CNTRL2 |= SPI_CNTRL2_SLV_ABORT_Msk )

Abort the current transfer in slave 3-wire mode.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 65 of file spi.h.

## ◆ SPI_CLR_3WIRE_START_INT_FLAG

#define SPI_CLR_3WIRE_START_INT_FLAG | ( |  | spi | ) | ( (spi)->STATUS = SPI_STATUS_SLV_START_INTSTS_Msk )

Clear the slave 3-wire mode start interrupt flag.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 72 of file spi.h.

## ◆ SPI_CLR_UNIT_TRANS_INT_FLAG

#define SPI_CLR_UNIT_TRANS_INT_FLAG | ( |  | spi | ) | ( (spi)->STATUS = SPI_STATUS_IF_Msk )

Clear the unit transfer interrupt flag.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 79 of file spi.h.

## ◆ SPI_DISABLE_3WIRE_MODE

#define SPI_DISABLE_3WIRE_MODE | ( |  | spi | ) | ( (spi)->CNTRL2 &= ~SPI_CNTRL2_NOSLVSEL_Msk )

Disable slave 3-wire mode.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 86 of file spi.h.

## ◆ SPI_DISABLE_BYTE_REORDER

#define SPI_DISABLE_BYTE_REORDER | ( |  | spi | ) | ( (spi)->CNTRL &= ~SPI_CNTRL_REORDER_Msk )

Disable byte reorder function.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 171 of file spi.h.

## ◆ SPI_ENABLE_3WIRE_MODE

#define SPI_ENABLE_3WIRE_MODE | ( |  | spi | ) | ( (spi)->CNTRL2 |= SPI_CNTRL2_NOSLVSEL_Msk )

Enable slave 3-wire mode.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 93 of file spi.h.

## ◆ SPI_ENABLE_BYTE_REORDER

#define SPI_ENABLE_BYTE_REORDER | ( |  | spi | ) | ( (spi)->CNTRL |= SPI_CNTRL_REORDER_Msk )

Enable byte reorder function.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 164 of file spi.h.

## ◆ SPI_GET_RX_FIFO_COUNT

#define SPI_GET_RX_FIFO_COUNT | ( |  | spi | ) | ( (((spi)->STATUS & SPI_STATUS_RX_FIFO_COUNT_Msk) >> SPI_STATUS_RX_FIFO_COUNT_Pos) & 0xf )

Get the count of available data in RX FIFO.

Parameters

  spi | is the base address of SPI module.

Returns
  The count of available data in RX FIFO.

Definition at line 100 of file spi.h.

## ◆ SPI_GET_RX_FIFO_EMPTY_FLAG

#define SPI_GET_RX_FIFO_EMPTY_FLAG | ( |  | spi | ) | ( ((spi)->STATUS & SPI_STATUS_RX_EMPTY_Msk) == SPI_STATUS_RX_EMPTY_Msk ? 1:0 )

Get the Rx FIFO empty flag.

Parameters

  spi | is the base address of SPI module.

Returns
  Rx FIFO flag

Return values

  0 | Rx FIFO is not empty
  1 | Rx FIFO is empty

Definition at line 109 of file spi.h.

## ◆ SPI_GET_TX_FIFO_EMPTY_FLAG

#define SPI_GET_TX_FIFO_EMPTY_FLAG | ( |  | spi | ) | ( ((spi)->STATUS & SPI_STATUS_TX_EMPTY_Msk) == SPI_STATUS_TX_EMPTY_Msk ? 1:0 )

Get the Tx FIFO empty flag.

Parameters

  spi | is the base address of SPI module.

Returns
  Tx FIFO flag

Return values

  0 | Tx FIFO is not empty
  1 | Tx FIFO is empty

Definition at line 118 of file spi.h.

## ◆ SPI_IS_BUSY

#define SPI_IS_BUSY | ( |  | spi | ) | ( ((spi)->CNTRL & SPI_CNTRL_GO_BUSY_Msk) == SPI_CNTRL_GO_BUSY_Msk ? 1:0 )

Get the SPI busy state.

Parameters

  spi | is the base address of SPI module.

Returns
  SPI busy status

Return values

  0 | SPI module is not busy
  1 | SPI module is busy

Definition at line 216 of file spi.h.

## ◆ SPI_READ_RX

#define SPI_READ_RX | ( |  | spi | ) | ( (spi)->RX )

Get the datum read from Rx FIFO.

Parameters

  spi | is the base address of SPI module.

Returns
  Data in Rx buffer

Definition at line 125 of file spi.h.

## ◆ SPI_SET_LSB_FIRST

#define SPI_SET_LSB_FIRST | ( |  | spi | ) | ( (spi)->CNTRL |= SPI_CNTRL_LSB_Msk )

Set the SPI transfer sequence with LSB first.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 186 of file spi.h.

## ◆ SPI_SET_MSB_FIRST

#define SPI_SET_MSB_FIRST | ( |  | spi | ) | ( (spi)->CNTRL &= ~SPI_CNTRL_LSB_Msk )

Set the SPI transfer sequence with MSB first.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 193 of file spi.h.

## ◆ SPI_SET_SUSPEND_CYCLE

#define SPI_SET_SUSPEND_CYCLE | ( |  | spi,
|  |  | u32SuspCycle
| ) |  | ( (spi)->CNTRL = ((spi)->CNTRL & ~SPI_CNTRL_SP_CYCLE_Msk) | (u32SuspCycle << SPI_CNTRL_SP_CYCLE_Pos) )

Set the length of suspend interval.

Parameters

  spi | is the base address of SPI module.
  u32SuspCycle | decides the length of suspend interval.

Returns
  none

Definition at line 179 of file spi.h.

## ◆ SPI_TRIGGER

#define SPI_TRIGGER | ( |  | spi | ) | ( (spi)->CNTRL |= SPI_CNTRL_GO_BUSY_Msk )

Set the GO_BUSY bit to trigger SPI transfer.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 223 of file spi.h.

## ◆ SPI_WRITE_TX

#define SPI_WRITE_TX | ( |  | spi,
|  |  | u32TxData
| ) |  | ( (spi)->TX = u32TxData )

Write datum to TX register.

Parameters

  spi | is the base address of SPI module.
  u32TxData | is the datum which user attempt to transfer through SPI bus.

Returns
  none

Definition at line 133 of file spi.h.

## Function Documentation

## ◆ SPI_ClearRxFIFO()

void SPI_ClearRxFIFO | ( | SPI_T * | spi | ) |

Clear Rx FIFO buffer.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 73 of file spi.c.

## ◆ SPI_ClearTxFIFO()

void SPI_ClearTxFIFO | ( | SPI_T * | spi | ) |

Clear Tx FIFO buffer.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 83 of file spi.c.

## ◆ SPI_Close()

void SPI_Close | ( | SPI_T * | spi | ) |

Reset SPI module and disable SPI peripheral clock.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 58 of file spi.c.

## ◆ SPI_DisableAutoSS()

void SPI_DisableAutoSS | ( | SPI_T * | spi | ) |

Disable the automatic slave select function.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 93 of file spi.c.

## ◆ SPI_DisableFIFO()

void SPI_DisableFIFO | ( | SPI_T * | spi | ) |

Disable FIFO mode.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 163 of file spi.c.

## ◆ SPI_DisableInt()

void SPI_DisableInt | ( | SPI_T * | spi,
|  | uint32_t | u32Mask
| ) |  |

Disable FIFO related interrupts specified by u32Mask parameter.

Parameters

  spi | is the base address of SPI module.
  u32Mask | is the combination of all related interrupt enable bits. Each bit corresponds to a interrupt bit. This parameter decides which interrupts will be disabled. (SPI_IE_MASK, SPI_SSTA_INTEN_MASK, SPI_FIFO_TX_INTEN_MASK, SPI_FIFO_RX_INTEN_MASK, SPI_FIFO_RXOV_INTEN_MASK, SPI_FIFO_TIMEOUT_INTEN_MASK)

Returns
  none

Definition at line 234 of file spi.c.

## ◆ SPI_EnableAutoSS()

void SPI_EnableAutoSS | ( | SPI_T * | spi,
|  | uint32_t | u32SSPinMask,
|  | uint32_t | u32ActiveLevel
| ) |  |

Enable the automatic slave select function. Only available in Master mode.

Parameters

  spi | is the base address of SPI module.
  u32SSPinMask | specifies slave select pins. (SPI_SS)
  u32ActiveLevel | specifies the active level of slave select signal. (SPI_SS_ACTIVE_HIGH, SPI_SS_ACTIVE_LOW)

Returns
  none

Definition at line 105 of file spi.c.

## ◆ SPI_EnableFIFO()

void SPI_EnableFIFO | ( | SPI_T * | spi,
|  | uint32_t | u32TxThreshold,
|  | uint32_t | u32RxThreshold
| ) |  |

Enable FIFO mode with user-specified Tx FIFO threshold and Rx FIFO threshold configurations.

Parameters

  spi | is the base address of SPI module.
  u32TxThreshold | decides the Tx FIFO threshold.
  u32RxThreshold | decides the Rx FIFO threshold.

Returns
  none

Definition at line 149 of file spi.c.

## ◆ SPI_EnableInt()

void SPI_EnableInt | ( | SPI_T * | spi,
|  | uint32_t | u32Mask
| ) |  |

Enable FIFO related interrupts specified by u32Mask parameter.

Parameters

  spi | is the base address of SPI module.
  u32Mask | is the combination of all related interrupt enable bits. Each bit corresponds to a interrupt bit. This parameter decides which interrupts will be enabled. (SPI_IE_MASK, SPI_SSTA_INTEN_MASK, SPI_FIFO_TX_INTEN_MASK, SPI_FIFO_RX_INTEN_MASK, SPI_FIFO_RXOV_INTEN_MASK, SPI_FIFO_TIMEOUT_INTEN_MASK)

Returns
  none

Definition at line 203 of file spi.c.

## ◆ SPI_GetBusClock()

uint32_t SPI_GetBusClock | ( | SPI_T * | spi | ) |

Get the actual frequency of SPI bus clock. Only available in Master mode.

Parameters

  spi | is the base address of SPI module.

Returns
  Actual SPI bus clock frequency.

Definition at line 173 of file spi.c.

Here is the call graph for this function:

## ◆ SPI_Open()

uint32_t SPI_Open | ( | SPI_T * | spi,
|  | uint32_t | u32MasterSlave,
|  | uint32_t | u32SPIMode,
|  | uint32_t | u32DataWidth,
|  | uint32_t | u32BusClock
| ) |  |

This function make SPI module be ready to transfer. By default, the SPI transfer sequence is MSB first and the automatic slave select function is disabled. In Slave mode, the u32BusClock must be NULL and the SPI clock divider setting will be 0.

Parameters

  spi | is the base address of SPI module.
  u32MasterSlave | decides the SPI module is operating in master mode or in slave mode. (SPI_SLAVE, SPI_MASTER)
  u32SPIMode | decides the transfer timing. (SPI_MODE_0, SPI_MODE_1, SPI_MODE_2, SPI_MODE_03)
  u32DataWidth | decides the data width of a SPI transaction.
  u32BusClock | is the expected frequency of SPI bus clock in Hz.

Returns
  Actual frequency of SPI peripheral clock.

Definition at line 39 of file spi.c.

Here is the call graph for this function:

## ◆ SPI_SET_DATA_WIDTH()

static __INLINE void SPI_SET_DATA_WIDTH | ( | SPI_T * | spi,
|  | uint32_t | u32Width
| ) |  |
| static

Set the data width of a SPI transaction.

Parameters

  spi | is the base address of SPI module.
  u32Width | is the bit width of transfer data.

Returns
  none

Definition at line 201 of file spi.h.

## ◆ SPI_SET_SS_HIGH()

static __INLINE void SPI_SET_SS_HIGH | ( | SPI_T * | spi | ) |
| static

Disable automatic slave select function and set SPI_SS pin to high state.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 140 of file spi.h.

## ◆ SPI_SET_SS_LOW()

static __INLINE void SPI_SET_SS_LOW | ( | SPI_T * | spi | ) |
| static

Disable automatic slave select function and set SPI_SS pin to low state.

Parameters

  spi | is the base address of SPI module.

Returns
  none

Definition at line 151 of file spi.h.

## ◆ SPI_SetBusClock()

uint32_t SPI_SetBusClock | ( | SPI_T * | spi,
|  | uint32_t | u32BusClock
| ) |  |

Set the SPI bus clock. Only available in Master mode.

Parameters

  spi | is the base address of SPI module.
  u32BusClock | is the expected frequency of SPI bus clock.

Returns
  Actual frequency of SPI peripheral clock.

Definition at line 116 of file spi.c.

Here is the call graph for this function:
Here is the caller graph for this function: