| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Data Fields
SPI_T Struct Reference
NUC029FAE Device CMSIS Definitions » NUC029FAE Control Register » Analog Comparator Controller(ACMP) » System Clock Controller(CLK) » Analog to Digital Converter(ADC) » Flash Memory Controller(FMC) » General Purpose Input/Output Controller(GPIO) » Inter-IC Bus Controller(I2C) » Interrupt Source Controller (INT) » Pulse Width Modulation Controller(PWM) » Serial Peripheral Interface Controller(SPI)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | CNTRL
__IO uint32_t | DIVIDER
__IO uint32_t | SSR
uint32_t | RESERVED0
__I uint32_t | RX
uint32_t | RESERVED1 [3]
__O uint32_t | TX
uint32_t | RESERVED2 [6]
__IO uint32_t | CNTRL2
__IO uint32_t | FIFO_CTL
__IO uint32_t | STATUS

## Detailed Description

Definition at line 1821 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h