| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Macros | Functions
timer.h File Reference

NUC029FAE TIMER driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | TIMER_ONESHOT_MODE (0UL)
#define | TIMER_PERIODIC_MODE (1UL << TIMER_TCSR_MODE_Pos)
#define | TIMER_TOGGLE_MODE (2UL << TIMER_TCSR_MODE_Pos)
#define | TIMER_CONTINUOUS_MODE (3UL << TIMER_TCSR_MODE_Pos)
#define | TIMER_CAPTURE_FREE_COUNTING_MODE (0UL)
#define | TIMER_CAPTURE_TRIGGER_COUNTING_MODE (TIMER_TEXCON_CAP_MODE_Msk)
#define | TIMER_CAPTURE_COUNTER_RESET_MODE (TIMER_TEXCON_RSTCAPSEL_Msk)
#define | TIMER_CAPTURE_FALLING_EDGE (0UL)
#define | TIMER_CAPTURE_RISING_EDGE (1UL << TIMER_TEXCON_TEX_EDGE_Pos)
#define | TIMER_CAPTURE_FALLING_THEN_RISING_EDGE (2UL << TIMER_TEXCON_TEX_EDGE_Pos)
#define | TIMER_CAPTURE_RISING_THEN_FALLING_EDGE (3UL << TIMER_TEXCON_TEX_EDGE_Pos)
#define | TIMER_COUNTER_RISING_EDGE (TIMER_TEXCON_TX_PHASE_Msk)
#define | TIMER_COUNTER_FALLING_EDGE (0UL)
#define | TIMER_TOGGLE_TX (0UL)
#define | TIMER_TOGGLE_TXEX (TIMER_TCSR_TOGGLE_PIN_Msk)
#define | TIMER_SET_CMP_VALUE(timer, u32Value)
| This macro is used to set new Timer compared value. More...
#define | TIMER_SET_PRESCALE_VALUE(timer, u32Value)
| This macro is used to set new Timer prescale value. More...
#define | TIMER_IS_ACTIVE(timer)
| This macro is used to check if specify Timer is inactive or active. More...
#define | TIMER_SELECT_TOUT_PIN(timer, u32ToutSel)
| This macro is used to select Timer toggle output pin. More...

## Functions
__STATIC_INLINE void | TIMER_Start (TIMER_T *timer)
| This function is used to start Timer counting. More...
__STATIC_INLINE void | TIMER_Stop (TIMER_T *timer)
| This function is used to stop Timer counting. More...
__STATIC_INLINE void | TIMER_EnableWakeup (TIMER_T *timer)
| This function is used to enable the Timer wake-up function. More...
__STATIC_INLINE void | TIMER_DisableWakeup (TIMER_T *timer)
| This function is used to disable the Timer wake-up function. More...
__STATIC_INLINE void | TIMER_EnableCaptureDebounce (TIMER_T *timer)
| This function is used to enable the capture pin detection de-bounce function. More...
__STATIC_INLINE void | TIMER_DisableCaptureDebounce (TIMER_T *timer)
| This function is used to disable the capture pin detection de-bounce function. More...
__STATIC_INLINE void | TIMER_EnableEventCounterDebounce (TIMER_T *timer)
| This function is used to enable the counter pin detection de-bounce function. More...
__STATIC_INLINE void | TIMER_DisableEventCounterDebounce (TIMER_T *timer)
| This function is used to disable the counter pin detection de-bounce function. More...
__STATIC_INLINE void | TIMER_EnableInt (TIMER_T *timer)
| This function is used to enable the Timer time-out interrupt function. More...
__STATIC_INLINE void | TIMER_DisableInt (TIMER_T *timer)
| This function is used to disable the Timer time-out interrupt function. More...
__STATIC_INLINE void | TIMER_EnableCaptureInt (TIMER_T *timer)
| This function is used to enable the Timer capture trigger interrupt function. More...
__STATIC_INLINE void | TIMER_DisableCaptureInt (TIMER_T *timer)
| This function is used to disable the Timer capture trigger interrupt function. More...
__STATIC_INLINE uint32_t | TIMER_GetIntFlag (TIMER_T *timer)
| This function indicates Timer time-out interrupt occurred or not. More...
__STATIC_INLINE void | TIMER_ClearIntFlag (TIMER_T *timer)
| This function clears the Timer time-out interrupt flag. More...
__STATIC_INLINE uint32_t | TIMER_GetCaptureIntFlag (TIMER_T *timer)
| This function indicates Timer capture interrupt occurred or not. More...
__STATIC_INLINE void | TIMER_ClearCaptureIntFlag (TIMER_T *timer)
| This function clears the Timer capture interrupt flag. More...
__STATIC_INLINE uint32_t | TIMER_GetWakeupFlag (TIMER_T *timer)
| This function indicates Timer has waked up system or not. More...
__STATIC_INLINE void | TIMER_ClearWakeupFlag (TIMER_T *timer)
| This function clears the Timer wakeup interrupt flag. More...
__STATIC_INLINE uint32_t | TIMER_GetCaptureData (TIMER_T *timer)
| This function gets the Timer capture data. More...
__STATIC_INLINE uint32_t | TIMER_GetCounter (TIMER_T *timer)
| This function reports the current timer counter value. More...
uint32_t | TIMER_Open (TIMER_T *timer, uint32_t u32Mode, uint32_t u32Freq)
| This API is used to configure timer to operate in specified mode and frequency. If timer cannot work in target frequency, a closest frequency will be chose and returned. More...
void | TIMER_Close (TIMER_T *timer)
| This API stops Timer counting and disable the Timer interrupt function. More...
void | TIMER_Delay (TIMER_T *timer, uint32_t u32Usec)
| This API is used to create a delay loop for u32usec micro seconds. More...
void | TIMER_EnableCapture (TIMER_T *timer, uint32_t u32CapMode, uint32_t u32Edge)
| This API is used to enable timer capture function with specified mode and capture edge. More...
void | TIMER_DisableCapture (TIMER_T *timer)
| This API is used to disable the Timer capture function. More...
void | TIMER_EnableEventCounter (TIMER_T *timer, uint32_t u32Edge)
| This function is used to enable the Timer counter function with specify detection edge. More...
void | TIMER_DisableEventCounter (TIMER_T *timer)
| This API is used to disable the Timer event counter function. More...
uint32_t | TIMER_GetModuleClock (TIMER_T *timer)
| This API is used to get the clock frequency of Timer. More...

## Detailed Description

NUC029FAE TIMER driver header file.

Version
  V1.00

Revision
  1

Date
  14/05/16 10:00a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file timer.h.