| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

SDCard.c
Go to the documentation of this file.
1/****************************************************************************/
12#include <stdio.h>
13#include "SDCard.h"
14#include "Nano100Series.h"
15
24int8_t Is_Initialized=0,SDtype=0;
25uint32_t LogicSector=0;
26
27// Command table for MMC. This table contains all commands available in SPI
28// mode; Format of command entries is described above in command structure
29// definition;
30 COMMAND __I command_list[] =
31{
32 { 0,NO,0x95,CMD,R1,NO }, // CMD0; GO_IDLE_STATE: reset card;
33 { 1,NO,0xFF,CMD,R1,NO }, // CMD1; SEND_OP_COND: initialize card;
34 { 8,YES,0xFF,CMD,R7,NO }, // CMD8; SEND_IF_COND
35 { 9,NO,0xFF,RD,R1,NO }, // CMD9; SEND_CSD: get card specific data;
36 {10,NO,0xFF,RD,R1,NO }, // CMD10; SEND_CID: get card identifier;
37 {12,NO,0xFF,CMD,R1b,NO }, // CMD12; STOP_TRANSMISSION: end read;
38 {13,NO,0xFF,CMD,R2,NO }, // CMD13; SEND_STATUS: read card status;
39 {16,YES,0xFF,CMD,R1,NO }, // CMD16; SET_BLOCKLEN: set block size;
40 {17,YES,0xFF,RDB,R1,NO }, // CMD17; READ_SINGLE_BLOCK: read 1 block;
41 {18,YES,0xFF,RD,R1,YES}, // CMD18; READ_MULTIPLE_BLOCK: read > 1;
42 {23,NO,0xFF,CMD,R1,NO }, // CMD23; SET_BLOCK_COUNT
43 {24,YES,0xFF,WR,R1,NO }, // CMD24; WRITE_BLOCK: write 1 block;
44 {25,YES,0xFF,WR,R1,YES}, // CMD25; WRITE_MULTIPLE_BLOCK: write > 1;
45 {27,NO,0xFF,CMD,R1,NO }, // CMD27; PROGRAM_CSD: program CSD;
46 {28,YES,0xFF,CMD,R1b,NO }, // CMD28; SET_WRITE_PROT: set wp for group;
47 {29,YES,0xFF,CMD,R1b,NO }, // CMD29; CLR_WRITE_PROT: clear group wp;
48 {30,YES,0xFF,CMD,R1,NO }, // CMD30; SEND_WRITE_PROT: check wp status;
49 {32,YES,0xFF,CMD,R1,NO }, // CMD32; TAG_SECTOR_START: tag 1st erase;
50 {33,YES,0xFF,CMD,R1,NO }, // CMD33; TAG_SECTOR_END: tag end(single);
51 {34,YES,0xFF,CMD,R1,NO }, // CMD34; UNTAG_SECTOR: deselect for erase;
52 {35,YES,0xFF,CMD,R1,NO }, // CMD35; TAG_ERASE_GROUP_START;
53 {36,YES,0xFF,CMD,R1,NO }, // CMD36; TAG_ERASE_GROUP_END;
54 {37,YES,0xFF,CMD,R1,NO }, // CMD37; UNTAG_ERASE_GROUP;
55 {38,YES,0xFF,CMD,R1b,NO }, // CMD38; ERASE: erase all tagged sectors;
56 {42,YES,0xFF,CMD,R1,NO }, // CMD42; LOCK_UNLOCK;
57 {55,NO,0xFF,CMD,R1,NO }, // CMD55; APP_CMD
58 {58,NO,0xFF,CMD,R3,NO }, // CMD58; READ_OCR: read OCR register;
59 {59,YES,0xFF,CMD,R1,NO }, // CMD59; CRC_ON_OFF: toggles CRC checking;
60 {0x80+13,NO,0xFF,CMD,R2,NO }, // ACMD13; SD_SEND_STATUS: read card status;
61 {0x80+23,YES,0xFF,CMD,R1,NO }, // ACMD23;SD_SET_WR_BLK_ERASE_COUNT
62 {0x80+41,YES,0xFF,CMD,R1,NO } // ACMD41; SD_SEND_OP_COND: initialize card;
63};
65
74 void SD_Delay(uint32_t count)
75{
76 uint32_t volatile loop;
77 for(loop=0; loop<count; loop++);
78}
79/*---------------------------------------------------------------------------------------------------------*/
80/* SD CARD Protocol */
81/*---------------------------------------------------------------------------------------------------------*/
82/*
83 Transfer Length:48bit
84 BIT POSITION WIDTH(BITS) VAULE
85 [47] 1 0:Start bit
86 [46] 1 1:Transmit 0:Receive
87 [45:40] 6 CMD8:001000
88 [39:8] 32 Reserved
89 [7:1] 7 Reserved
90 [0] 1 1:End bit
91
92*/
93
101 static uint32_t GenerateCRC(uint32_t u32Data, uint32_t u32GenPoly, uint32_t u32Accum)
102{
103 volatile uint8_t i;
104
105 u32Data <<= 8;
106 for (i=8; i>0; i--)
107 {
108 if ((u32Data ^ u32Accum) & 0x8000)
109 u32Accum = (u32Accum << 1) ^ u32GenPoly;
110 else
111 u32Accum <<= 1;
112 u32Data <<= 1;
113 }
114 return u32Accum;
115}
116
122 static uint32_t SingleWrite(uint32_t u32Data)
123{
124 SPI_WRITE_TX0(SPI1, u32Data);
125 SPI_TRIGGER(SPI1);
126 while(SPI_IS_BUSY(SPI1));
127
128 return SPI_READ_RX0(SPI1);
129}
130
140uint32_t MMC_Command_Exec (uint8_t nCmd, uint32_t nArg,uint8_t *pchar, uint32_t *response)
141{
142 uint8_t loopguard;
143 COMMAND current_command; // Local space for the command table
144 UINT32 long_arg; // Local space for argument
145 static uint32_t current_blklen = 512;
146 uint32_t old_blklen = 512;
147 int32_t counter = 0; // Byte counter for multi-byte fields;
148 UINT16 card_response; // Variable for storing card response;
149 uint8_t data_resp; // Variable for storing data response;
150 UINT16 dummy_CRC; // Dummy variable for storing CRC field;
151
152 card_response.i = 0;
153
154 current_command = command_list[nCmd];// Retrieve desired command table entry
155 // from code space;
156 if(current_command.command_byte & 0x80) // Detect ACMD
157 {
158 if(MMC_Command_Exec(APP_CMD,EMPTY,EMPTY,response)==FALSE)//Send APP_CMD
159 return FALSE;
160 }
161
162 SPI_SET_SS0_LOW(SPI1); // CS = 0
163
164 SingleWrite(0xFF);
165 SingleWrite((current_command.command_byte | 0x40)&0x7f);
166 DBG_PRINTF("CMD:%d,",current_command.command_byte&0x7f);
167
168 long_arg.l = nArg; // Make argument byte addressable;
169 // If current command changes block
170 // length, update block length variable
171 // to keep track;
172 // Command byte = 16 means that a set
173 // block length command is taking place
174 // and block length variable must be
175 // set;
176 if(current_command.command_byte == 16)
177 {
178 current_blklen = nArg;
179 }
180 // Command byte = 9 or 10 means that a
181 // 16-byte register value is being read
182 // from the card, block length must be
183 // set to 16 bytes, and restored at the
184 // end of the transfer;
185 if((current_command.command_byte == 9)||(current_command.command_byte == 10))
186 {
187 old_blklen = current_blklen; // Command is a GET_CSD or GET_CID,
188 current_blklen = 16; // set block length to 16-bytes;
189 }
190 // If an argument is required, transmit
191 // one, otherwise transmit 4 bytes of
192 // 0x00;
193 if(current_command.arg_required == YES)
194 {
195 dummy_CRC.i = GenerateCRC((current_command.command_byte | 0x40), 0x1200, 0);
196 for(counter=3; counter>=0; counter--)
197 {
198 SingleWrite(long_arg.b[counter]);
199 dummy_CRC.i = GenerateCRC(long_arg.b[counter], 0x1200, dummy_CRC.i);
200
201 }
202 dummy_CRC.i = (dummy_CRC.i >> 8)| 0x01;
203 SingleWrite(dummy_CRC.b[0]);
204 }
205 else
206 {
207 counter = 0;
208 while(counter <= 3)
209 {
210 SingleWrite(0x00);
211 counter++;
212 }
213 SingleWrite(current_command.CRC);
214 }
215
216 // The command table entry will indicate
217 // what type of response to expect for
218 // a given command; The following
219 // conditional handles the MMC response;
220 if(current_command.response == R1) // Read the R1 response from the card;
221 {
222 loopguard=0;
223 do
224 {
225 card_response.b[0] = SingleWrite(0xFF);
226 if(!++loopguard) break;
227 }
228 while((card_response.b[0] & BUSY_BIT));
229 DBG_PRINTF("R1:0x%x, counter:%d\n",card_response.b[0],loopguard);
230 if(!loopguard)
231 {
232 BACK_FROM_ERROR;
233 }
234 *response=card_response.b[0];
235 }
236 else if(current_command.response == R1b) // Read the R1b response;
237 {
238 loopguard = 0;
239 do
240 {
241 card_response.b[0] = SingleWrite(0xFF);
242 if(!++loopguard) break;
243 }
244 while((card_response.b[0] & BUSY_BIT));
245 while((SingleWrite(0xFF)&0xFF) == 0x00);
246 }
247 else if(current_command.response == R2)
248 {
249 loopguard=0;
250 do
251 {
252 card_response.b[0] = SingleWrite(0xFF);
253 if(!++loopguard) break;
254 }
255 while((card_response.b[0] & BUSY_BIT));
256 card_response.b[1] = SingleWrite(0xFF);
257 DBG_PRINTF("R2:0x%x, counter:%d\n",card_response.i,loopguard);
258 if(!loopguard)
259 {
260 BACK_FROM_ERROR;
261 }
262 *response=card_response.i;
263 }
264 else if(current_command.response == R3)
265 {
266 // Read R3 response;
267 loopguard=0;
268 do
269 {
270 card_response.b[0] = SingleWrite(0xFF);
271 if(!++loopguard) break;
272 }
273 while((card_response.b[0] & BUSY_BIT));
274 DBG_PRINTF("R3:0x%x, counter:%d\n",card_response.b[0],loopguard);
275 if(!loopguard)
276 {
277 BACK_FROM_ERROR;
278 }
279 counter = 0;
280 while(counter <= 3) // Read next three bytes and store them
281 {
282 // in local memory; These bytes make up
283 counter++; // the Operating Conditions Register
284 *pchar++ = SingleWrite(0xFF);
285 }
286 *response=card_response.b[0];
287 }
288 else
289 {
290 // Read R7 response;
291 loopguard=0;
292 do
293 {
294 card_response.b[0] = SingleWrite(0xFF);
295 if(!++loopguard) break;
296 }
297 while((card_response.b[0] & BUSY_BIT));
298 DBG_PRINTF("R7:0x%x, counter:%d\n",card_response.b[0],loopguard);
299 if(!loopguard)
300 {
301 BACK_FROM_ERROR;
302 }
303 counter = 0;
304 while(counter <= 3) // Read next three bytes and store them
305 {
306 // in local memory; These bytes make up
307 counter++; // the Operating Conditions Register
308 *pchar++ = SingleWrite(0xFF);
309 }
310 *response=card_response.b[0];
311 }
312
313
314 switch(current_command.trans_type) // This conditional handles all data
315 {
316 // operations; The command entry
317 // determines what type, if any, data
318 // operations need to occur;
319 case RDB: // Read data from the MMC;
320 loopguard = 0;
321
322 while((SingleWrite(0xFF)&0xFF)!=START_SBR)
323 {
324 if(!++loopguard)
325 {
326 BACK_FROM_ERROR;
327 }
328 SD_Delay(1);
329 }
330 counter = 0; // Reset byte counter;
331 // Read <current_blklen> bytes;
332
333 SPI_WRITE_TX0(SPI1, 0xFFFFFFFF);
334 if(pchar)
335 {
336 //SPI_SetBitLength(SPI1, 8);
337 //SPI_SetFIFOMode(SPI1, TRUE, 2);
338 //SPI_FIFOReadWrite8(SPI1, NULL, pchar, current_blklen);
339 //SPI_SetFIFOMode(SPI1, FALSE, 2);
340
341 for (counter=0; counter<current_blklen; counter++)
342 {
343 SPI_WRITE_TX0(SPI1, 0xFF);
344 SPI_TRIGGER(SPI1);
345 while(SPI_IS_BUSY(SPI1));
346 *(pchar+counter)=SPI_READ_RX0(SPI1);
347 }
348 }
349 else
350 {
351 for (; counter<current_blklen; counter++)
352 {
353 SPI_TRIGGER(SPI1);
354 while(SPI_IS_BUSY(SPI1));
355 }
356 }
357 dummy_CRC.b[1] = SingleWrite(0xFF); // After all data is read, read the two
358 dummy_CRC.b[0] = SingleWrite(0xFF); // CRC bytes; These bytes are not used
359 // in this mode, but the place holders
360 // must be read anyway;
361 break;
362 case RD: // Read data from the MMC;
363 loopguard = 0;
364
365 while((SingleWrite(0xFF)&0xFF)!=START_SBR)
366 {
367 if(!++loopguard)
368 {
369 BACK_FROM_ERROR;
370 }
371 }
372 counter = 0; // Reset byte counter;
373 // Read <current_blklen> bytes;
374 if(pchar)
375 {
376 for (counter=0; counter<current_blklen; counter++)
377 {
378 SPI_WRITE_TX0(SPI1, 0xFF);
379 SPI_TRIGGER(SPI1);
380 while(SPI_IS_BUSY(SPI1));
381 *(pchar+counter)=SPI_READ_RX0(SPI1);
382 }
383 }
384 else
385 {
386 for (counter=0; counter<current_blklen; counter++)
387 {
388 SPI_WRITE_TX0(SPI1, 0xFF);
389 SPI_TRIGGER(SPI1);
390 while(SPI_IS_BUSY(SPI1));
391 }
392 }
393 dummy_CRC.b[1] = SingleWrite(0xFF); // After all data is read, read the two
394 dummy_CRC.b[0] = SingleWrite(0xFF); // CRC bytes; These bytes are not used
395 // in this mode, but the place holders
396 // must be read anyway;
397 break;
398
399 case WR:
400 SingleWrite(0xFF);
401 SingleWrite(START_SBW);
402
403 for (counter=0; counter<current_blklen; counter++)
404 {
405 SPI_WRITE_TX0(SPI1, *(pchar+counter));
406 SPI_TRIGGER(SPI1);
407 dummy_CRC.i = GenerateCRC(*(pchar+counter), 0x1021, dummy_CRC.i);
408 while(SPI_IS_BUSY(SPI1));
409 }
410 SingleWrite(dummy_CRC.b[1]);
411 SingleWrite(dummy_CRC.b[0]);
412
413 loopguard = 0;
414 do // Read Data Response from card;
415 {
416 data_resp = SingleWrite(0xFF);
417 if(!++loopguard) break;
418 }
419 while((data_resp & DATA_RESP_MASK) != 0x01); // When bit 0 of the MMC response
420 // is clear, a valid data response
421 // has been received;
422
423 if(!loopguard)
424 {
425 BACK_FROM_ERROR;
426 }
427
428
429 while((SingleWrite(0xFF)&0xFF)!=0xFF);//Wait for Busy
430 SingleWrite(0xFF);
431 break;
432 default:
433 break;
434 }
435 SPI_SET_SS0_HIGH(SPI1); // CS = 1
436 if((current_command.command_byte == 9)||(current_command.command_byte == 10))
437 {
438 current_blklen = old_blklen;
439 }
440 return TRUE;
441}
442
447 void MMC_FLASH_Init(void)
448{
449 uint32_t response;
450 uint16_t loopguard;
451 uint32_t i;
452 uint8_t counter = 0;
453 uint8_t pchar[16]; // Data pointer for storing MMC
454 uint32_t c_size,bl_len;
455 uint8_t c_mult;
456
457
458 Is_Initialized = 0;
459
460re_init:
461 SPI_SET_SS0_HIGH(SPI1); // CS = 1
462 SD_Delay(1000);
463 //--------------------------------------------------------
464 // Send 74 SD clcok in SD mode for Toshiba SD Card
465 //--------------------------------------------------------
466 for(counter = 0; counter < 10; counter++)
467 {
468 SingleWrite(0xFF);
469 }
470 SD_Delay(1000);
471
472 SPI_SET_SS0_LOW(SPI1); // CS = 0
473 while(MMC_Command_Exec(GO_IDLE_STATE,EMPTY,EMPTY,&response)==FALSE)
474 SD_Delay(1000);
475 if(response!=0x01)
476 goto re_init;
477
478 if(MMC_Command_Exec(SEND_IF_COND,0x15A,pchar,&response) && response==1)
479 {
480 /* SDC ver 2.00 */
481 if (pchar[2] == 0x01 && pchar[3] == 0x5A)
482 {
483 /* The card can work at VDD range of 2.7-3.6V */
484 loopguard=0;
485 do
486 {
487 MMC_Command_Exec(SD_SEND_OP_COND,0x40000000,EMPTY,&response);//Enable HCS(OCR[30])
488 if(!++loopguard) break;
489 SD_Delay(0x100);
490 }
491 while(response!=0);
492 if(!loopguard)
493 return;
494
495 MMC_Command_Exec(READ_OCR,EMPTY,pchar,&response);
496 SDtype=(pchar[0]&0x40)?SDv2|SDBlock:SDv2;
497 }
498 }
499 else
500 {
501 /* SDv1 or MMCv3 */
502 MMC_Command_Exec(SD_SEND_OP_COND,0x00,EMPTY,&response);
503 if (response <= 1)
504 {
505 loopguard=0;
506 do
507 {
508 MMC_Command_Exec(SD_SEND_OP_COND,0x00,EMPTY,&response);
509 if(!++loopguard) break;
510 SD_Delay(50);
511 }
512 while(response!=0);
513 if(!loopguard)
514 return;
515 SDtype=SDv1; /* SDv1 */
516 }
517 else
518 {
519 loopguard=0;
520 do
521 {
522 MMC_Command_Exec(SEND_OP_COND,0x00,EMPTY,&response);
523 if(!++loopguard) break;
524 SD_Delay(50);
525 }
526 while(response!=0);
527 if(!loopguard)
528 return;
529 SDtype=MMCv3; /* MMCv3 */
530 }
531 MMC_Command_Exec(SET_BLOCKLEN,(uint32_t)PHYSICAL_BLOCK_SIZE,EMPTY,&response);
532 }
533 if(MMC_Command_Exec(SEND_CSD,EMPTY,pchar,&response)==FALSE)
534 return;
535
536 if(response==0)
537 {
538 DBG_PRINTF("Change speed:");
539 for(i=0; i<16; i++)
540 {
541 DBG_PRINTF("0x%X ",pchar[i]);
542 }
543
544 }
545 else
546 {
547 DBG_PRINTF("CARD STATUS 0x%X:\n",response);
548 for(i=0; i<16; i++)
549 {
550 DBG_PRINTF("0x%X ",pchar[i]);
551 }
552 LogicSector=0;
553 return;
554 }
555
556 if(SDtype&SDBlock) // Determine the number of MMC sectors;
557 {
558 bl_len = 1 << (pchar[5] & 0x0f) ;
559 c_size = ((pchar[7] & 0x3F) << 16) |(pchar[8] << 8) | (pchar[9]);
560 LogicSector=c_size*((512*1024)/bl_len);
561 }
562 else
563 {
564 bl_len = 1 << (pchar[5] & 0x0f) ;
565 c_size = ((pchar[6] & 0x03) << 10) |(pchar[7] << 2) | ((pchar[8] &0xc0) >> 6);
566 c_mult = (((pchar[9] & 0x03) << 1) | ((pchar[10] & 0x80) >> 7));
567 LogicSector=(c_size+1)*(1 << (c_mult+2))*(bl_len/512);
568 }
569 DBG_PRINTF("\nLogicSector:%d, PHYSICAL_SIZE:%dMB\n",LogicSector,(LogicSector/2/1024));
570
571 loopguard = 0;
572 while((MMC_Command_Exec(READ_SINGLE_BLOCK,0,0,&response)==FALSE))
573 {
574 if(!++loopguard) break;
575 }
576 Is_Initialized = 1;
577}
578
584uint32_t SDCARD_Open(void)
585{
586 /* Configure SPI1 as a master, 8-bit transaction*/
587 SPI_Open(SPI1, SPI_MASTER, SPI_MODE_0, 8, 300000);
588
589 SPI_DisableAutoSS(SPI1);
590 SPI_SET_MSB_FIRST(SPI1);
591
592 DBG_PRINTF("SPI is running at %d Hz\n", SPI_GetBusClock(SPI1));
593
594 MMC_FLASH_Init();
595 SD_Delay(3000);
596
597 if (Is_Initialized)
598 DBG_PRINTF("SDCARD INIT OK\n\n");
599 else
600 {
601 DBG_PRINTF("SDCARD INIT FAIL\n\n");
602 return SD_FAIL;
603 }
604
605 SPI_SetBusClock(SPI1, 5000000);
606 DBG_PRINTF("Now, SPI is running at %d Hz\n", SPI_GetBusClock(SPI1));
607
608 return SD_SUCCESS;
609}
610
615 void SDCARD_Close(void)
616{
617 SPI_Close(SPI1);
618}
619
626uint32_t SDCARD_GetCardSize(uint32_t *pu32TotSecCnt)
627{
628 if (LogicSector == 0)
629 return FALSE;
630 else
631 *pu32TotSecCnt = LogicSector;
632
633 return TRUE;
634}
635
640uint32_t GetLogicSector(void)
641{
642 return LogicSector;
643}
644
652 void SpiRead(uint32_t addr, uint32_t size, uint8_t* buffer)
653{
654 /* This is low level read function of USB Mass Storage */
655 uint32_t response;
656 if(SDtype&SDBlock)
657 {
658 while(size >= PHYSICAL_BLOCK_SIZE)
659 {
660 MMC_Command_Exec(READ_SINGLE_BLOCK,addr,buffer,&response);
661 addr ++;
662 buffer += PHYSICAL_BLOCK_SIZE;
663 size -= PHYSICAL_BLOCK_SIZE;
664 }
665
666 }
667 else
668 {
669 addr*=PHYSICAL_BLOCK_SIZE;
670 while(size >= PHYSICAL_BLOCK_SIZE)
671 {
672 MMC_Command_Exec(READ_SINGLE_BLOCK,addr,buffer,&response);
673 addr += PHYSICAL_BLOCK_SIZE;
674 buffer += PHYSICAL_BLOCK_SIZE;
675 size -= PHYSICAL_BLOCK_SIZE;
676 }
677 }
678}
679
687 void SpiWrite(uint32_t addr, uint32_t size, uint8_t* buffer)
688{
689 uint32_t response;
690 if(SDtype&SDBlock)
691 {
692 while(size >= PHYSICAL_BLOCK_SIZE)
693 {
694 MMC_Command_Exec(WRITE_BLOCK,addr,buffer,&response);
695 addr ++;
696 buffer += PHYSICAL_BLOCK_SIZE;
697 size -= PHYSICAL_BLOCK_SIZE;
698 }
699 }
700 else
701 {
702 addr*=PHYSICAL_BLOCK_SIZE;
703 while(size >= PHYSICAL_BLOCK_SIZE)
704 {
705 MMC_Command_Exec(WRITE_BLOCK,addr,buffer,&response);
706 addr += (PHYSICAL_BLOCK_SIZE);
707 buffer += PHYSICAL_BLOCK_SIZE;
708 size -= PHYSICAL_BLOCK_SIZE;
709 }
710 }
711} /* end of group NANO100_SDCARD_EXPORTED_FUNCTIONS */
713 /* end of group NANO100_SDCARD_Driver */
715 /* end of group NANO100_Library */
717
718/*** (C) COPYRIGHT 2014 Nuvoton Technology Corp. ***/
Nano100Series.h
Nano100 series peripheral access layer header file. This file contains all the peripheral register's ...
SDCard.h
Nano100 series SD Card driver header file.
SPI1
#define SPI1
Pointer to SPI1 register structure.
Definition: Nano100Series.h:11677
SEND_IF_COND
#define SEND_IF_COND
Definition: SDCard.h:97
PHYSICAL_BLOCK_SIZE
#define PHYSICAL_BLOCK_SIZE
Definition: SDCard.h:37
READ_SINGLE_BLOCK
#define READ_SINGLE_BLOCK
Definition: SDCard.h:103
CMD
#define CMD
Definition: SDCard.h:45
SDv1
#define SDv1
Definition: SDCard.h:90
SEND_OP_COND
#define SEND_OP_COND
Definition: SDCard.h:96
EMPTY
#define EMPTY
Definition: SDCard.h:42
SDBlock
#define SDBlock
Definition: SDCard.h:93
SD_SEND_OP_COND
#define SD_SEND_OP_COND
Definition: SDCard.h:125
BACK_FROM_ERROR
#define BACK_FROM_ERROR
Definition: SDCard.h:70
R7
#define R7
Definition: SDCard.h:54
START_SBW
#define START_SBW
Definition: SDCard.h:60
SD_FAIL
#define SD_FAIL
Definition: SDCard.h:84
R3
#define R3
Definition: SDCard.h:53
WRITE_BLOCK
#define WRITE_BLOCK
Definition: SDCard.h:106
R2
#define R2
Definition: SDCard.h:52
SDv2
#define SDv2
Definition: SDCard.h:91
BUSY_BIT
#define BUSY_BIT
Definition: SDCard.h:68
YES
#define YES
Definition: SDCard.h:43
SEND_CSD
#define SEND_CSD
Definition: SDCard.h:98
SD_SUCCESS
#define SD_SUCCESS
Definition: SDCard.h:83
R1
#define R1
Definition: SDCard.h:50
GO_IDLE_STATE
#define GO_IDLE_STATE
Definition: SDCard.h:95
R1b
#define R1b
Definition: SDCard.h:51
READ_OCR
#define READ_OCR
Definition: SDCard.h:121
NO
#define NO
Definition: SDCard.h:44
DATA_RESP_MASK
#define DATA_RESP_MASK
Definition: SDCard.h:65
DBG_PRINTF
#define DBG_PRINTF(...)
Definition: SDCard.h:34
RDB
#define RDB
Definition: SDCard.h:48
WR
#define WR
Definition: SDCard.h:47
APP_CMD
#define APP_CMD
Definition: SDCard.h:120
MMCv3
#define MMCv3
Definition: SDCard.h:92
START_SBR
#define START_SBR
Definition: SDCard.h:58
SET_BLOCKLEN
#define SET_BLOCKLEN
Definition: SDCard.h:102
RD
#define RD
Definition: SDCard.h:46
SDCARD_Open
uint32_t SDCARD_Open(void)
This function is used to Open GPIO function and initial SDCARD.
Definition: SDCard.c:584
SingleWrite
static uint32_t SingleWrite(uint32_t u32Data)
This function is used to send data though SPI to general clock for SDCARD operation.
Definition: SDCard.c:122
GetLogicSector
uint32_t GetLogicSector(void)
This function is used to get logic sector size.
Definition: SDCard.c:640
UINT32::b
uint8_t b[4]
Definition: SDCard.h:75
UINT16::b
uint8_t b[2]
Definition: SDCard.h:80
SpiWrite
void SpiWrite(uint32_t addr, uint32_t size, uint8_t *buffer)
This function is used to store data into SD card.
Definition: SDCard.c:687
COMMAND::trans_type
uint8_t trans_type
Definition: SDCard.h:137
SpiRead
void SpiRead(uint32_t addr, uint32_t size, uint8_t *buffer)
This function is used to Get data from SD card.
Definition: SDCard.c:652
SD_Delay
void SD_Delay(uint32_t count)
Delay function.
Definition: SDCard.c:74
MMC_FLASH_Init
void MMC_FLASH_Init(void)
This function is used to initialize the flash card.
Definition: SDCard.c:447
SDCARD_Close
void SDCARD_Close(void)
This function is used to close SDCARD.
Definition: SDCard.c:615
COMMAND::response
uint8_t response
Definition: SDCard.h:138
COMMAND::CRC
uint8_t CRC
Definition: SDCard.h:136
COMMAND::arg_required
uint8_t arg_required
Definition: SDCard.h:135
UINT32::l
uint32_t l
Definition: SDCard.h:74
GenerateCRC
static uint32_t GenerateCRC(uint32_t u32Data, uint32_t u32GenPoly, uint32_t u32Accum)
This function is used to generate CRC value.
Definition: SDCard.c:101
MMC_Command_Exec
uint32_t MMC_Command_Exec(uint8_t nCmd, uint32_t nArg, uint8_t *pchar, uint32_t *response)
This function is used to Send SDCARD CMD and Receive Response.
Definition: SDCard.c:140
UINT16::i
uint16_t i
Definition: SDCard.h:79
SDCARD_GetCardSize
uint32_t SDCARD_GetCardSize(uint32_t *pu32TotSecCnt)
This function is used to get card total sector after SDCARD is opened.
Definition: SDCard.c:626
COMMAND::command_byte
uint8_t command_byte
Definition: SDCard.h:134
SPI_MODE_0
#define SPI_MODE_0
Definition: spi.h:34
SPI_MASTER
#define SPI_MASTER
Definition: spi.h:40
SPI_WRITE_TX0
#define SPI_WRITE_TX0(spi, u32TxData)
Write datum to TX0 register.
Definition: spi.h:165
SPI_TRIGGER
#define SPI_TRIGGER(spi)
Set the GO_BUSY bit to trigger SPI transfer.
Definition: spi.h:295
SPI_READ_RX0
#define SPI_READ_RX0(spi)
Get the datum read from RX0 FIFO.
Definition: spi.h:149
SPI_DisableAutoSS
void SPI_DisableAutoSS(SPI_T *spi)
Disable the automatic slave select function.
Definition: spi.c:111
SPI_SET_MSB_FIRST
#define SPI_SET_MSB_FIRST(spi)
Set the SPI transfer sequence with MSB first.
Definition: spi.h:262
SPI_SET_SS0_LOW
#define SPI_SET_SS0_LOW(spi)
Set SPIn_SS0 pin to low state.
Definition: spi.h:192
SPI_SetBusClock
uint32_t SPI_SetBusClock(SPI_T *spi, uint32_t u32BusClock)
Set the SPI bus clock. Only available in Master mode.
Definition: spi.c:138
SPI_Close
void SPI_Close(SPI_T *spi)
Reset SPI module and disable SPI peripheral clock.
Definition: spi.c:66
SPI_IS_BUSY
#define SPI_IS_BUSY(spi)
Get the SPI busy state.
Definition: spi.h:287
SPI_SET_SS0_HIGH
#define SPI_SET_SS0_HIGH(spi)
Set SPIn_SS0 pin to high state.
Definition: spi.h:183
SPI_Open
uint32_t SPI_Open(SPI_T *spi, uint32_t u32MasterSlave, uint32_t u32SPIMode, uint32_t u32DataWidth, uint32_t u32BusClock)
This function make SPI module be ready to transfer. By default, the SPI transfer sequence is MSB firs...
Definition: spi.c:47
SPI_GetBusClock
uint32_t SPI_GetBusClock(SPI_T *spi)
Get the actual frequency of SPI bus clock. Only available in Master mode.
Definition: spi.c:212
TRUE
#define TRUE
Boolean true, define to use in API parameters or return value.
Definition: Nano100Series.h:11862
FALSE
#define FALSE
Boolean false, define to use in API parameters or return value.
Definition: Nano100Series.h:11863
COMMAND
Definition: SDCard.h:133
UINT16
Definition: SDCard.h:78
UINT32
Definition: SDCard.h:73