| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
scuart.c File Reference

Nano100 series Smartcard UART mode (SCUART) driver source file. More...

`#include "Nano100Series.h"`
Include dependency graph for scuart.c:

Go to the source code of this file.

## Functions
void | SCUART_Close (SC_T *sc)
| The function is used to disable smartcard interface UART mode. More...
uint32_t | SCUART_Open (SC_T *sc, uint32_t u32baudrate)
| This function use to enable smartcard module UART mode and set baudrate. More...
uint32_t | SCUART_Read (SC_T *sc, uint8_t *pu8RxBuf, uint32_t u32ReadBytes)
| The function is used to read Rx data from RX FIFO. More...
uint32_t | SCUART_SetLineConfig (SC_T *sc, uint32_t u32Baudrate, uint32_t u32DataWidth, uint32_t u32Parity, uint32_t u32StopBits)
| This function use to config smartcard UART mode line setting. More...
void | SCUART_SetTimeoutCnt (SC_T *sc, uint32_t u32TOC)
| This function use to set receive timeout count. More...
void | SCUART_Write (SC_T *sc, uint8_t *pu8TxBuf, uint32_t u32WriteBytes)
| This function is to write data into transmit FIFO to send data out. More...

## Detailed Description

Nano100 series Smartcard UART mode (SCUART) driver source file.

Version
  V1.00

Revision
  5

Date
  15/05/14 11:14a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file scuart.c.