| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Data Fields
RTC_T Struct Reference

`#include <Nano100Series.h>`

## Data Fields
__IO uint32_t | INIR
__IO uint32_t | AER
__IO uint32_t | FCR
__IO uint32_t | TLR
__IO uint32_t | CLR
__IO uint32_t | TSSR
__IO uint32_t | DWR
__IO uint32_t | TAR
__IO uint32_t | CAR
__I uint32_t | LIR
__IO uint32_t | RIER
__IO uint32_t | RIIR
__IO uint32_t | TTR
uint32_t | RESERVE0 [2]
__IO uint32_t | SPRCTL
__IO uint32_t | SPR [20]

## Detailed Description

    @addtogroup RTC Real Time Clock Controller(RTC)
    Memory Mapped Structure for RTC Controller

Definition at line 7772 of file Nano100Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano100Series/Include/Nano100Series.h