| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
sc.c File Reference

Nano100 series Smartcard(SC) driver source file. More...

`#include "Nano100Series.h"`
Include dependency graph for sc.c:

Go to the source code of this file.

## Functions
uint32_t | SC_IsCardInserted (SC_T *sc)
| This function indicates specified smartcard slot status. More...
void | SC_ClearFIFO (SC_T *sc)
| This function reset both transmit and receive FIFO of specified smartcard module. More...
void | SC_Close (SC_T *sc)
| This function disable specified smartcard module. More...
void | SC_Open (SC_T *sc, uint32_t u32CD, uint32_t u32PWR)
| This function initialized smartcard module. More...
void | SC_ResetReader (SC_T *sc)
| This function reset specified smartcard module to its default state for activate smartcard. More...
void | SC_SetBlockGuardTime (SC_T *sc, uint32_t u32BGT)
| This function block guard time (BGT) of specified smartcard module. More...
void | SC_SetCharGuardTime (SC_T *sc, uint32_t u32CGT)
| This function character guard time (CGT) of specified smartcard module. More...
void | SC_StopAllTimer (SC_T *sc)
| This function stop all smartcard timer of specified smartcard module. More...
void | SC_StartTimer (SC_T *sc, uint32_t u32TimerNum, uint32_t u32Mode, uint32_t u32ETUCount)
| This function configure and start a smartcard timer of specified smartcard module. More...
void | SC_StopTimer (SC_T *sc, uint32_t u32TimerNum)
| This function stop a smartcard timer of specified smartcard module. More...

## Detailed Description

Nano100 series Smartcard(SC) driver source file.

Version
  V1.00

Revision
  6

Date
  15/07/31 7:30p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Definition in file sc.c.