| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_System.c File Reference

NuEdu-Basic01 System driver source file for NuEdu-SDK-Nano130. More...

`#include <stdio.h>`
`#include "Nano100Series.h"`
`#include "NuEdu-Basic01_System.h"`
Include dependency graph for NuEdu-Basic01_System.c:

Go to the source code of this file.

## Functions
void | SYS_Init (void)
| This function enables HXT, LXT and LIRC clock and sets HCLK source from HXT to 42MHz. More...

## Detailed Description

NuEdu-Basic01 System driver source file for NuEdu-SDK-Nano130.

Version
  V1.00

Revision
  2

Date
  14/12/12 10:35a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_System.c.