| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Modules | Macros
Smartcard Library Exported Constants
NANO100 Library » Smartcard Library
Collaboration diagram for Smartcard Library Exported Constants:

## Modules
| Smartcard Library Exported Structs

## Macros
#define | SCLIB_MAX_ATR_LEN 32
| Max ATR length. ISO-7816 8.2.1. More...
#define | SCLIB_MIN_ATR_LEN 2
| Min ATR length, TS and T0. More...
#define | SCLIB_PROTOCOL_UNDEFINED 0x00000000
| There is no active protocol. More...
#define | SCLIB_PROTOCOL_T0 0x00000001
| T=0 is the active protocol. More...
#define | SCLIB_PROTOCOL_T1 0x00000002
| T=1 is the active protocol. More...
#define | SCLIB_SUCCESS 0x00000000
| Command successful without error. More...
#define | SCLIB_ERR_CARD_REMOVED 0x00000001
| Smartcard removed. More...
#define | SCLIB_ERR_OVER_RUN 0x00000002
| Rx FIFO over run. More...
#define | SCLIB_ERR_PARITY_ERROR 0x00000003
| Tx/Rx parity error. More...
#define | SCLIB_ERR_NO_STOP 0x00000004
| Stop bit not found. More...
#define | SCLIB_ERR_SILENT_BYTE 0x00000005
| I/O pin stay at low for longer than 1 character time. More...
#define | SCLIB_ERR_CMD 0x00000006
| Smartcard command error. More...
#define | SCLIB_ERR_UNSUPPORTEDCARD 0x00000007
| Unsupported smartcard error. More...
#define | SCLIB_ERR_READ 0x00000008
| Read error. More...
#define | SCLIB_ERR_WRITE 0x00000009
| Write error. More...
#define | SCLIB_ERR_TIME0OUT 0x0000000A
| Smartcard timer 0 timeout. More...
#define | SCLIB_ERR_TIME1OUT 0x0000000B
| Smartcard timer 1 timeout. More...
#define | SCLIB_ERR_TIME2OUT 0x0000000C
| Smartcard timer 2 timeout. More...
#define | SCLIB_ERR_AUTOCONVENTION 0x0000000D
| Smartcard is neither direct nor inverse convention. More...
#define | SCLIB_ERR_CLOCK 0x0000000E
| Smartcard clock frequency is not between 1MHz and 5 MHz. More...
#define | SCLIB_ERR_BGTIMEOUT 0x0000000E
| Block time out error occur. More...
#define | SCLIB_ERR_ATR_UNRECOGNIZED 0x00001001
| Unrecognised ATR. More...
#define | SCLIB_ERR_ATR_INVALID_PARAM 0x00001002
| ATR parsing interface bytes error. More...
#define | SCLIB_ERR_ATR_INVALID_TCK 0x00001003
| TCK check byte error. More...
#define | SCLIB_ERR_PPS 0x00001004
| Protocol Parameter Selection (PPS) exchange error. More...
#define | SCLIB_ERR_T1_PARITY 0x00002001
| T=1 Parity Error Notice. More...
#define | SCLIB_ERR_T1_ICC 0x00002002
| ICC communication error. More...
#define | SCLIB_ERR_T1_PROTOCOL 0x00002003
| T=1 Protocol Error. More...
#define | SCLIB_ERR_T1_ABORT_RECEIVED 0x00002004
| Received ABORT request. More...
#define | SCLIB_ERR_T1_RESYNCH_RECEIVED 0x00002005
| Received RESYNCH request. More...
#define | SCLIB_ERR_T1_VPP_ERROR_RECEIVED 0x00002006
| Received VPP error. More...
#define | SCLIB_ERR_T1_WTXRES_RECEIVED 0x00002007
| Received BWT extension request. More...
#define | SCLIB_ERR_T1_IFSRES_RECEIVED 0x00002008
| Received max IFS offer. More...
#define | SCLIB_ERR_T1_ABORTRES_RECEIVED 0x00002009
| Received ABORT response. More...
#define | SCLIB_ERR_T1_CHECKSUM 0x0000200A
| T=1 block check sum error. More...
#define | SCLIB_ERR_T0_PROTOCOL 0x00003003
| T=0 Protocol Error. More...
#define | SCLIB_ERR_DEACTIVE 0x0000F001
| Smartcard is de-active. More...
#define | SCLIB_ERR_CARDBUSY 0x0000F002
| Smartcard is busy, previous transmission is not complete yet. More...

## Detailed Description

## Macro Definition Documentation

## ◆ SCLIB_ERR_ATR_INVALID_PARAM

#define SCLIB_ERR_ATR_INVALID_PARAM 0x00001002

ATR parsing interface bytes error.

Definition at line 62 of file sclib.h.

## ◆ SCLIB_ERR_ATR_INVALID_TCK

#define SCLIB_ERR_ATR_INVALID_TCK 0x00001003

TCK check byte error.

Definition at line 63 of file sclib.h.

## ◆ SCLIB_ERR_ATR_UNRECOGNIZED

#define SCLIB_ERR_ATR_UNRECOGNIZED 0x00001001

Unrecognised ATR.

Definition at line 61 of file sclib.h.

## ◆ SCLIB_ERR_AUTOCONVENTION

#define SCLIB_ERR_AUTOCONVENTION 0x0000000D

Smartcard is neither direct nor inverse convention.

Definition at line 57 of file sclib.h.

## ◆ SCLIB_ERR_BGTIMEOUT

#define SCLIB_ERR_BGTIMEOUT 0x0000000E

Block time out error occur.

Definition at line 59 of file sclib.h.

## ◆ SCLIB_ERR_CARD_REMOVED

#define SCLIB_ERR_CARD_REMOVED 0x00000001

Smartcard removed.

Definition at line 45 of file sclib.h.

## ◆ SCLIB_ERR_CARDBUSY

#define SCLIB_ERR_CARDBUSY 0x0000F002

Smartcard is busy, previous transmission is not complete yet.

Definition at line 82 of file sclib.h.

## ◆ SCLIB_ERR_CLOCK

#define SCLIB_ERR_CLOCK 0x0000000E

Smartcard clock frequency is not between 1MHz and 5 MHz.

Definition at line 58 of file sclib.h.

## ◆ SCLIB_ERR_CMD

#define SCLIB_ERR_CMD 0x00000006

Smartcard command error.

Definition at line 50 of file sclib.h.

## ◆ SCLIB_ERR_DEACTIVE

#define SCLIB_ERR_DEACTIVE 0x0000F001

Smartcard is de-active.

Definition at line 81 of file sclib.h.

## ◆ SCLIB_ERR_NO_STOP

#define SCLIB_ERR_NO_STOP 0x00000004

Stop bit not found.

Definition at line 48 of file sclib.h.

## ◆ SCLIB_ERR_OVER_RUN

#define SCLIB_ERR_OVER_RUN 0x00000002

Rx FIFO over run.

Definition at line 46 of file sclib.h.

## ◆ SCLIB_ERR_PARITY_ERROR

#define SCLIB_ERR_PARITY_ERROR 0x00000003

Tx/Rx parity error.

Definition at line 47 of file sclib.h.

## ◆ SCLIB_ERR_PPS

#define SCLIB_ERR_PPS 0x00001004

Protocol Parameter Selection (PPS) exchange error.

Definition at line 64 of file sclib.h.

## ◆ SCLIB_ERR_READ

#define SCLIB_ERR_READ 0x00000008

Read error.

Definition at line 52 of file sclib.h.

## ◆ SCLIB_ERR_SILENT_BYTE

#define SCLIB_ERR_SILENT_BYTE 0x00000005

I/O pin stay at low for longer than 1 character time.

Definition at line 49 of file sclib.h.

## ◆ SCLIB_ERR_T0_PROTOCOL

#define SCLIB_ERR_T0_PROTOCOL 0x00003003

T=0 Protocol Error.

Definition at line 78 of file sclib.h.

## ◆ SCLIB_ERR_T1_ABORT_RECEIVED

#define SCLIB_ERR_T1_ABORT_RECEIVED 0x00002004

Received ABORT request.

Definition at line 69 of file sclib.h.

## ◆ SCLIB_ERR_T1_ABORTRES_RECEIVED

#define SCLIB_ERR_T1_ABORTRES_RECEIVED 0x00002009

Received ABORT response.

Definition at line 74 of file sclib.h.

## ◆ SCLIB_ERR_T1_CHECKSUM

#define SCLIB_ERR_T1_CHECKSUM 0x0000200A

T=1 block check sum error.

Definition at line 75 of file sclib.h.

## ◆ SCLIB_ERR_T1_ICC

#define SCLIB_ERR_T1_ICC 0x00002002

ICC communication error.

Definition at line 67 of file sclib.h.

## ◆ SCLIB_ERR_T1_IFSRES_RECEIVED

#define SCLIB_ERR_T1_IFSRES_RECEIVED 0x00002008

Received max IFS offer.

Definition at line 73 of file sclib.h.

## ◆ SCLIB_ERR_T1_PARITY

#define SCLIB_ERR_T1_PARITY 0x00002001

T=1 Parity Error Notice.

Definition at line 66 of file sclib.h.

## ◆ SCLIB_ERR_T1_PROTOCOL

#define SCLIB_ERR_T1_PROTOCOL 0x00002003

T=1 Protocol Error.

Definition at line 68 of file sclib.h.

## ◆ SCLIB_ERR_T1_RESYNCH_RECEIVED

#define SCLIB_ERR_T1_RESYNCH_RECEIVED 0x00002005

Received RESYNCH request.

Definition at line 70 of file sclib.h.

## ◆ SCLIB_ERR_T1_VPP_ERROR_RECEIVED

#define SCLIB_ERR_T1_VPP_ERROR_RECEIVED 0x00002006

Received VPP error.

Definition at line 71 of file sclib.h.

## ◆ SCLIB_ERR_T1_WTXRES_RECEIVED

#define SCLIB_ERR_T1_WTXRES_RECEIVED 0x00002007

Received BWT extension request.

Definition at line 72 of file sclib.h.

## ◆ SCLIB_ERR_TIME0OUT

#define SCLIB_ERR_TIME0OUT 0x0000000A

Smartcard timer 0 timeout.

Definition at line 54 of file sclib.h.

## ◆ SCLIB_ERR_TIME1OUT

#define SCLIB_ERR_TIME1OUT 0x0000000B

Smartcard timer 1 timeout.

Definition at line 55 of file sclib.h.

## ◆ SCLIB_ERR_TIME2OUT

#define SCLIB_ERR_TIME2OUT 0x0000000C

Smartcard timer 2 timeout.

Definition at line 56 of file sclib.h.

## ◆ SCLIB_ERR_UNSUPPORTEDCARD

#define SCLIB_ERR_UNSUPPORTEDCARD 0x00000007

Unsupported smartcard error.

Definition at line 51 of file sclib.h.

## ◆ SCLIB_ERR_WRITE

#define SCLIB_ERR_WRITE 0x00000009

Write error.

Definition at line 53 of file sclib.h.

## ◆ SCLIB_MAX_ATR_LEN

#define SCLIB_MAX_ATR_LEN 32

Max ATR length. ISO-7816 8.2.1.

Definition at line 35 of file sclib.h.

## ◆ SCLIB_MIN_ATR_LEN

#define SCLIB_MIN_ATR_LEN 2

Min ATR length, TS and T0.

Definition at line 36 of file sclib.h.

## ◆ SCLIB_PROTOCOL_T0

#define SCLIB_PROTOCOL_T0 0x00000001

T=0 is the active protocol.

Definition at line 40 of file sclib.h.

## ◆ SCLIB_PROTOCOL_T1

#define SCLIB_PROTOCOL_T1 0x00000002

T=1 is the active protocol.

Definition at line 41 of file sclib.h.

## ◆ SCLIB_PROTOCOL_UNDEFINED

#define SCLIB_PROTOCOL_UNDEFINED 0x00000000

There is no active protocol.

Definition at line 39 of file sclib.h.

## ◆ SCLIB_SUCCESS

#define SCLIB_SUCCESS 0x00000000

Command successful without error.

Definition at line 43 of file sclib.h.