| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Modules | Macros
SYS Exported Constants
NANO100 Device Driver » SYS Driver
Collaboration diagram for SYS Exported Constants:

## Modules
| SYS Exported Functions

## Macros
#define | CHIP_RST ((0x0<<24) | SYS_IPRST_CTL1_CHIP_RST_Pos )
#define | CPU_RST ((0x0<<24) | SYS_IPRST_CTL1_CPU_RST_Pos )
#define | DMA_RST ((0x0<<24) | SYS_IPRST_CTL1_DMA_RST_Pos )
#define | EBI_RST ((0x0<<24) | SYS_IPRST_CTL1_EBI_RST_Pos )
#define | SC1_RST ((0x4<<24) | SYS_IPRST_CTL2_SC1_RST_Pos )
#define | SC0_RST ((0x4<<24) | SYS_IPRST_CTL2_SC0_RST_Pos )
#define | I2S_RST ((0x4<<24) | SYS_IPRST_CTL2_I2S_RST_Pos )
#define | ADC_RST ((0x4<<24) | SYS_IPRST_CTL2_ADC_RST_Pos )
#define | USBD_RST ((0x4<<24) | SYS_IPRST_CTL2_USBD_RST_Pos )
#define | DAC_RST ((0x4<<24) | SYS_IPRST_CTL2_DAC_RST_Pos )
#define | PWM1_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM1_RST_Pos )
#define | PWM0_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM0_RST_Pos )
#define | UART1_RST ((0x4<<24) | SYS_IPRST_CTL2_UART1_RST_Pos )
#define | UART0_RST ((0x4<<24) | SYS_IPRST_CTL2_UART0_RST_Pos )
#define | SPI2_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI2_RST_Pos )
#define | SPI1_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI1_RST_Pos )
#define | SPI0_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI0_RST_Pos )
#define | I2C1_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C1_RST_Pos )
#define | I2C0_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C0_RST_Pos )
#define | TMR3_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR3_RST_Pos )
#define | TMR2_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR2_RST_Pos )
#define | TMR1_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR1_RST_Pos )
#define | TMR0_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR0_RST_Pos )
#define | GPIO_RST ((0x4<<24) | SYS_IPRST_CTL2_GPIO_RST_Pos )
#define | SYS_VREFCTL_BGP_EN SYS_VREFCTL_BGP_EN_Msk
#define | SYS_VREFCTL_REG_EN SYS_VREFCTL_REG_EN_Msk
#define | SYS_VREFCTL_SEL25 SYS_VREFCTL_SEL25_Msk
#define | SYS_VREFCTL_EXTMODE SYS_VREFCTL_EXT_MODE_Msk
#define | SYS_IRCTRIMCTL_TRIM_11_0592M (0x1UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)
#define | SYS_IRCTRIMCTL_TRIM_12M (0x2UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)
#define | SYS_IRCTRIMCTL_TRIM_12_288M (0x3UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)
#define | SYS_IRCTRIMCTL_LOOP_4CLK (0x0UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMCTL_LOOP_8CLK (0x1UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMCTL_LOOP_16CLK (0x2UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMCTL_LOOP_32CLK (0x3UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMCTL_RETRY_64 (0x0UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
#define | SYS_IRCTRIMCTL_RETRY_128 (0x1UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
#define | SYS_IRCTRIMCTL_RETRY_256 (0x2UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
#define | SYS_IRCTRIMCTL_RETRY_512 (0x3UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
#define | SYS_IRCTRIMIEN_DISABLE ((uint32_t)0x00000000)
#define | SYS_IRCTRIMIEN_FAIL_EN SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk
#define | SYS_IRCTRIMIEN_32KERR_EN SYS_IRCTRIMIEN_32K_ERR_IEN_Msk
#define | SYS_IRCTRIMINT_FREQLOCK SYS_IRCTRIMINT_FREQ_LOCK_Msk
#define | SYS_IRCTRIMINT_FAIL_INT SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk
#define | SYS_IRCTRIMINT_32KERR_INT SYS_IRCTRIMINT_32K_ERR_INT_Msk
#define | SYS_PA_L_MFP_PA7_MFP_GPA7 (0UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_ADC_CH7 (1UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_EBI_AD6 (2UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_TMR2_CAP (3UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_SC2_DAT (4UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_PWM0_CH2 (5UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_LCD_S36 (7UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_GPA6 (0UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_ADC_CH6 (1UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_EBI_AD7 (2UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_TMR3_CAP (3UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_SC2_CLK (4UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_PWM0_CH3 (5UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_LCD_S37 (7UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_LCD_S19 (7UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_GPA5 (0UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_ADC_CH5 (1UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_EBI_AD8 (2UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_SC2_RST (4UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_I2C0_SCL (5UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_LCD_S38 (7UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_LCD_S20 (7UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_GPA4 (0UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_ADC_CH4 (1UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_EBI_AD9 (2UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_SC2_PWR (4UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_I2C0_SDA (5UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_LCD_S39 (7UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_LCD_S21 (7UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_GPA3 (0UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_ADC_CH3 (1UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_EBI_AD10 (2UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_UART1_TX (5UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_LCD_S22 (7UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_GPA2 (0UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_ADC_CH2 (1UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_EBI_AD11 (2UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_UART1_RX (5UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_LCD_S23 (7UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_GPA1 (0UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_ADC_CH1 (1UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_EBI_AD12 (2UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA0_MFP_GPA0 (0UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
#define | SYS_PA_L_MFP_PA0_MFP_ADC_CH0 (1UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
#define | SYS_PA_L_MFP_PA0_MFP_SC2_CD (4UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_GPA15 (0UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_PWM0_CH3 (1UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_I2S_MCLK (2UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_TMR3_CAP (3UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_SC0_PWR (4UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_UART0_TX (6UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_LCD_S27 (7UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_GPA14 (0UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_PWM0_CH2 (1UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_EBI_AD15 (2UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_TMR2_CAP (3UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_UART0_RX (6UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_LCD_S26 (7UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_GPA13 (0UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_PWM0_CH1 (1UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_EBI_AD14 (2UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_TMR1_CAP (3UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_I2C0_SCL (5UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_LCD_S25 (7UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_GPA12 (0UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_PWM0_CH0 (1UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_EBI_AD13 (2UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_TMR0_CAP (3UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_I2C0_SDA (5UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_LCD_S24 (7UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_GPA11 (0UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_I2C1_SCL (1UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_EBI_NRE (2UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_SC0_RST (3UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_SPI2_MOSI0 (4UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_LCD_S23 (7UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_LCD_S9 (7UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_GPA10 (0UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_I2C1_SDA (1UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_EBI_NWE (2UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_SC0_PWR (3UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_SPI2_MISO0 (4UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_LCD_S22 (7UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_LCD_S8 (7UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_GPA9 (0UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_I2C0_SCL (1UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_SC0_DAT (3UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_SPI2_SCLK (4UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_LCD_S21 (7UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_LCD_S7 (7UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_GPA8 (0UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_I2C0_SDA (1UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_SC0_CLK (3UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_SPI2_SS0 (4UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_LCD_S20 (7UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_LCD_S6 (7UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_GPB7 (0UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_UART1_CTS (1UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_EBI_NCS (2UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_SPI2_MOSI0 (4UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_LCD_S10 (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_LCD_S2 (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_GPB6 (0UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_UART1_RTS (1UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_EBI_ALE (2UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_SPI2_MISO0 (4UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_LCD_S11 (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_LCD_S3 (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_GPB5 (0UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_UART1_TX (1UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_SC0_RST (3UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_SPI2_SCLK (4UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_LCD_S12 (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_LCD_S4 (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_GPB4 (0UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_UART1_RX (1UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_SC0_CD (3UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_SPI2_SS0 (4UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_LCD_S13 (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_LCD_S5 (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_GPB3 (0UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_UART0_CTS (1UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_EBI_NWRH (2UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_SPI1_SS0 (3UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_LCD_S4 (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_LCD_COM2 (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_GPB2 (0UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_UART0_RTS (1UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_EBI_NWRL (2UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_SPI1_SCLK (3UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_LCD_S5 (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_LCD_COM3 (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_GPB1 (0UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_UART0_TX (1UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_SPI1_MISO0 (3UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_LCD_S6 (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_LCD_S0 (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_GPB0 (0UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_UART0_RX (1UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_SPI1_MOSI0 (3UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_LCD_S7 (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_LCD_S1 (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_GPB15 (0UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_EXT_INT1 (1UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_SNOOPER (3UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_SC1_CD (4UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_LCD_S31 (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_LCD_S14 (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_GPB14 (0UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_EXT_INT0 (1UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_SC2_CD (3UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_SPI2_SS1 (4UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_LCD_S26 (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_LCD_S12 (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_GPB13 (0UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_EBI_AD1 (2UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_LCD_S25 (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_LCD_S11 (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_GPB12 (0UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_EBI_AD0 (2UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_CKO (4UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_LCD_S24 (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_LCD_S10 (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_GPB11 (0UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_PWM1_CH0 (1UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_TMR3_EXT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_TMR3_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_SC2_DAT (4UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_SPI0_MISO0 (5UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_LCD_V1 (7UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_GPB10 (0UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_SPI0_SS1 (1UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_TMR2_EXT (2UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_TMR2_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_SC2_CLK (4UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI0 (5UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_LCD_V2 (7UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_GPB9 (0UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_SPI1_SS1 (1UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_TMR1_EXT (2UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_TMR1_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_SC2_RST (4UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_EXT_INT0 (5UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_LCD_V3 (7UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_GPB8 (0UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_ADC_EXT (1UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_TMR0_EXT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_TMR0_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_EXT_INT0 (3UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_SC2_PWR (4UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_LCD_S30 (7UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_LCD_S13 (7UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_GPC7 (0UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_DA_OUT1 (1UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_EBI_AD5 (2UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_TMR1_CAP (3UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_PWM0_CH1 (5UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_LCD_S17 (7UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_GPC6 (0UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_DA_OUT0 (1UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_EBI_AD4 (2UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_TMR0_CAP (3UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_SC1_CD (4UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_PWM0_CH0 (5UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_GPC5 (0UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_SPI0_MOSI1 (1UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_LCD_COM3 (7UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_GPC4 (0UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_SPI0_MISO1 (1UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_LCD_COM2 (7UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_GPC3 (0UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_SPI0_MOSI0 (1UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_I2S_DOUT (2UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_SC1_RST (4UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_LCD_COM1 (7UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_GPC2 (0UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_SPI0_MISO0 (1UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_I2S_DIN (2UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_SC1_PWR (4UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_LCD_COM0 (7UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_GPC1 (0UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_SPI0_SCLK (1UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_I2S_BCLK (2UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_SC1_DAT (4UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_LCD_DH2 (7UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_GPC0 (0UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_SPI0_SS0 (1UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_I2S_WS (2UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_SC1_CLK (4UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_LCD_DH1 (7UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_GPC15 (0UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_EBI_AD3 (2UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_TMR0_CAP (3UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_PWM1_CH2 (4UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_LCD_S33 (7UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_LCD_S16 (7UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_GPC14 (0UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_EBI_AD2 (2UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_PWM1_CH3 (4UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_LCD_S32 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_LCD_S15 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_GPC13 (0UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_SPI1_MOSI1 (1UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_PWM1_CH1 (2UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_SNOOPER (4UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_EXT_INT1 (5UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_I2C0_SCL (6UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_GPC12 (0UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_SPI1_MISO1 (1UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_PWM1_CH0 (2UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_EXT_INT0 (5UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_I2C0_SDA (6UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_GPC11 (0UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_SPI1_MOSI0 (1UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_UART1_TX (5UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_LCD_S31 (7UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_GPC10 (0UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_SPI1_MISO0 (1UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_UART1_RX (5UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_LCD_S30 (7UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_GPC9 (0UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_SPI1_SCLK (1UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_I2C1_SCL (5UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_LCD_S29 (7UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_GPC8 (0UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_SPI1_SS0 (1UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_EBI_XCLK (2UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_I2C1_SDA (5UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_LCD_S28 (7UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PD_L_MFP_PD7_MFP_GPD7 (0UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
#define | SYS_PD_L_MFP_PD7_MFP_LCD_S2 (7UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
#define | SYS_PD_L_MFP_PD6_MFP_GPD6 (0UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
#define | SYS_PD_L_MFP_PD6_MFP_LCD_S3 (7UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_GPD5 (0UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_I2S_DOUT (2UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_SPI2_MOSI1 (3UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_LCD_S34 (7UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_GPD4 (0UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_I2S_DIN (2UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_SPI2_MISO1 (3UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_SC1_CD (4UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_LCD_S35 (7UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_GPD3 (0UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_UART1_CTS (1UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_I2S_BCLK (2UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_SPI2_MOSI0 (3UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_SC1_RST (4UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_ADC_CH11 (5UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_GPD2 (0UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_UART1_RTS (1UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_I2S_WS (2UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_SPI2_MISO0 (3UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_SC1_PWR (4UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_ADC_CH10 (5UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_GPD1 (0UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_UART1_TX (1UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_SPI2_SCLK (3UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_SC1_DAT (4UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_ADC_CH9 (5UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_GPD0 (0UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_UART1_RX (1UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_SPI2_SS0 (3UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_SC1_CLK (4UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_ADC_CH8 (5UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_H_MFP_PD15_MFP_GPD15 (0UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
#define | SYS_PD_H_MFP_PD15_MFP_LCD_S0 (7UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
#define | SYS_PD_H_MFP_PD14_MFP_GPD14 (0UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
#define | SYS_PD_H_MFP_PD14_MFP_LCD_S1 (7UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
#define | SYS_PD_H_MFP_PD13_MFP_GPD13 (0UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
#define | SYS_PD_H_MFP_PD13_MFP_LCD_S14 (7UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_GPD12 (0UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_LCD_S15 (7UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_GPD11 (0UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_LCD_S16 (7uL<<SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_GPD10 (0UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_LCD_S17 (7UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_GPD9 (0UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_LCD_S18 (7UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD8_MFP_GPD8 (0UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
#define | SYS_PD_H_MFP_PD8_MFP_LCD_S19 (7UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
#define | SYS_PE_L_MFP_PE7_MFP_GPE7 (0UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
#define | SYS_PE_L_MFP_PE7_MFP_LCD_S8 (7UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
#define | SYS_PE_L_MFP_PE6_MFP_GPE6 (0UL<<SYS_PE_L_MFP_PE6_MFP_Pos)
#define | SYS_PE_L_MFP_PE5_MFP_GPE5 (0UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
#define | SYS_PE_L_MFP_PE5_MFP_PWM1_CH1 (1UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
#define | SYS_PE_L_MFP_PE4_MFP_GPE4 (0UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
#define | SYS_PE_L_MFP_PE4_MFP_SPI0_MOSI0 (6UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
#define | SYS_PE_L_MFP_PE3_MFP_GPE3 (0UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
#define | SYS_PE_L_MFP_PE3_MFP_SPI0_MISO0 (6UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
#define | SYS_PE_L_MFP_PE2_MFP_GPE2 (0UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
#define | SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK (6UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
#define | SYS_PE_L_MFP_PE1_MFP_GPE1 (0UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
#define | SYS_PE_L_MFP_PE1_MFP_PWM1_CH3 (1UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
#define | SYS_PE_L_MFP_PE1_MFP_SPI0_SS0 (6UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
#define | SYS_PE_L_MFP_PE0_MFP_GPE0 (0UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
#define | SYS_PE_L_MFP_PE0_MFP_PWM1_CH2 (1UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
#define | SYS_PE_L_MFP_PE0_MFP_I2S_MCLK (2UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
#define | SYS_PE_H_MFP_PE15_MFP_GPE15 (0UL<<SYS_PE_H_MFP_PE15_MFP_Pos)
#define | SYS_PE_H_MFP_PE15_MFP_LCD_S29 (7UL<<SYS_PE_H_MFP_PE15_MFP_Pos)
#define | SYS_PE_H_MFP_PE14_MFP_GPE14 (0UL<<SYS_PE_H_MFP_PE14_MFP_Pos)
#define | SYS_PE_H_MFP_PE14_MFP_LCD_S28 (7UL<<SYS_PE_H_MFP_PE14_MFP_Pos)
#define | SYS_PE_H_MFP_PE13_MFP_GPE13 (0UL<<SYS_PE_H_MFP_PE13_MFP_Pos)
#define | SYS_PE_H_MFP_PE13_MFP_LCD_S27 (7UL<<SYS_PE_H_MFP_PE13_MFP_Pos)
#define | SYS_PE_H_MFP_PE12_MFP_GPE12 (0UL<<SYS_PE_H_MFP_PE12_MFP_Pos)
#define | SYS_PE_H_MFP_PE12_MFP_UART1_CTS (7UL<<SYS_PE_H_MFP_PE12_MFP_Pos)
#define | SYS_PE_H_MFP_PE11_MFP_GPE11 (0UL<<SYS_PE_H_MFP_PE11_MFP_Pos)
#define | SYS_PE_H_MFP_PE11_MFP_UART1_RTS (7UL<<SYS_PE_H_MFP_PE11_MFP_Pos)
#define | SYS_PE_H_MFP_PE10_MFP_GPE10 (0UL<<SYS_PE_H_MFP_PE10_MFP_Pos)
#define | SYS_PE_H_MFP_PE10_MFP_UART1_TX (7UL<<SYS_PE_H_MFP_PE10_MFP_Pos)
#define | SYS_PE_H_MFP_PE9_MFP_GPE9 (0UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
#define | SYS_PE_H_MFP_PE9_MFP_UART1_RX (7UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
#define | SYS_PE_H_MFP_PE8_MFP_GPE8 (0UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
#define | SYS_PE_H_MFP_PE8_MFP_LCD_S9 (7UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_GPF5 (0UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_I2C0_SCL (1UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_GPF4 (0UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_I2C0_SDA (1UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_GPF3 (0UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_HXT_IN (7UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_GPF2 (0UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_HXT_OUT (7UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_GPF1 (0UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_CKO (4UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_EXT_INT1 (5UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_ICE_CLK (7UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_GPF0 (0UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_EXT_INT0 (5UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_ICE_DAT (7UL<<SYS_PF_L_MFP_PF0_MFP_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ ADC_RST

#define ADC_RST ((0x4<<24) | SYS_IPRST_CTL2_ADC_RST_Pos )

ADC reset is one of the SYS_ResetModule parameter

Definition at line 42 of file sys.h.

## ◆ CHIP_RST

#define CHIP_RST ((0x0<<24) | SYS_IPRST_CTL1_CHIP_RST_Pos )

CHIP reset is one of the SYS_ResetModule parameter

Definition at line 35 of file sys.h.

## ◆ CPU_RST

#define CPU_RST ((0x0<<24) | SYS_IPRST_CTL1_CPU_RST_Pos )

CPU reset is one of the SYS_ResetModule parameter

Definition at line 36 of file sys.h.

## ◆ DAC_RST

#define DAC_RST ((0x4<<24) | SYS_IPRST_CTL2_DAC_RST_Pos )

DAC reset is one of the SYS_ResetModule parameter

Definition at line 44 of file sys.h.

## ◆ DMA_RST

#define DMA_RST ((0x0<<24) | SYS_IPRST_CTL1_DMA_RST_Pos )

DMA reset is one of the SYS_ResetModule parameter

Definition at line 37 of file sys.h.

## ◆ EBI_RST

#define EBI_RST ((0x0<<24) | SYS_IPRST_CTL1_EBI_RST_Pos )

EBI reset is one of the SYS_ResetModule parameter

Definition at line 38 of file sys.h.

## ◆ GPIO_RST

#define GPIO_RST ((0x4<<24) | SYS_IPRST_CTL2_GPIO_RST_Pos )

GPIO reset is one of the SYS_ResetModule parameter

Definition at line 58 of file sys.h.

## ◆ I2C0_RST

#define I2C0_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C0_RST_Pos )

I2C0 reset is one of the SYS_ResetModule parameter

Definition at line 53 of file sys.h.

## ◆ I2C1_RST

#define I2C1_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C1_RST_Pos )

I2C1 reset is one of the SYS_ResetModule parameter

Definition at line 52 of file sys.h.

## ◆ I2S_RST

#define I2S_RST ((0x4<<24) | SYS_IPRST_CTL2_I2S_RST_Pos )

I2S reset is one of the SYS_ResetModule parameter

Definition at line 41 of file sys.h.

## ◆ PWM0_RST

#define PWM0_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM0_RST_Pos )

PWM0 reset is one of the SYS_ResetModule parameter

Definition at line 46 of file sys.h.

## ◆ PWM1_RST

#define PWM1_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM1_RST_Pos )

PWM1 reset is one of the SYS_ResetModule parameter

Definition at line 45 of file sys.h.

## ◆ SC0_RST

#define SC0_RST ((0x4<<24) | SYS_IPRST_CTL2_SC0_RST_Pos )

SmartCard0 reset is one of the SYS_ResetModule parameter

Definition at line 40 of file sys.h.

## ◆ SC1_RST

#define SC1_RST ((0x4<<24) | SYS_IPRST_CTL2_SC1_RST_Pos )

SmartCard1 reset is one of the SYS_ResetModule parameter

Definition at line 39 of file sys.h.

## ◆ SPI0_RST

#define SPI0_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI0_RST_Pos )

SPI0 reset is one of the SYS_ResetModule parameter

Definition at line 51 of file sys.h.

## ◆ SPI1_RST

#define SPI1_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI1_RST_Pos )

SPI1 reset is one of the SYS_ResetModule parameter

Definition at line 50 of file sys.h.

## ◆ SPI2_RST

#define SPI2_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI2_RST_Pos )

SPI2 reset is one of the SYS_ResetModule parameter

Definition at line 49 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_16CLK

#define SYS_IRCTRIMCTL_LOOP_16CLK (0x2UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

Based on average difference in 16 x 32.768 kHz clock

Definition at line 77 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_32CLK

#define SYS_IRCTRIMCTL_LOOP_32CLK (0x3UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

Based on average difference in 32 x 32.768 kHz clock

Definition at line 78 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_4CLK

#define SYS_IRCTRIMCTL_LOOP_4CLK (0x0UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

Based on average difference in 4 x 32.768 kHz clock

Definition at line 75 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_8CLK

#define SYS_IRCTRIMCTL_LOOP_8CLK (0x1UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

Based on average difference in 8 x 32.768 kHz clock

Definition at line 76 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_128

#define SYS_IRCTRIMCTL_RETRY_128 (0x1UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)

Trim retry count limitation is 128

Definition at line 81 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_256

#define SYS_IRCTRIMCTL_RETRY_256 (0x2UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)

Trim retry count limitation is 256

Definition at line 82 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_512

#define SYS_IRCTRIMCTL_RETRY_512 (0x3UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)

Trim retry count limitation is 512

Definition at line 83 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_64

#define SYS_IRCTRIMCTL_RETRY_64 (0x0UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)

Trim retry count limitation is 64

Definition at line 80 of file sys.h.

## ◆ SYS_IRCTRIMCTL_TRIM_11_0592M

#define SYS_IRCTRIMCTL_TRIM_11_0592M (0x1UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)

Trim HIRC to 11.0592 MHz

Definition at line 71 of file sys.h.

## ◆ SYS_IRCTRIMCTL_TRIM_12_288M

#define SYS_IRCTRIMCTL_TRIM_12_288M (0x3UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)

Trim HIRC to 12.288 MHz

Definition at line 73 of file sys.h.

## ◆ SYS_IRCTRIMCTL_TRIM_12M

#define SYS_IRCTRIMCTL_TRIM_12M (0x2UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)

Trim HIRC to 12 MHz

Definition at line 72 of file sys.h.

## ◆ SYS_IRCTRIMIEN_32KERR_EN

#define SYS_IRCTRIMIEN_32KERR_EN SYS_IRCTRIMIEN_32K_ERR_IEN_Msk

32.768 kHz Clock Error Interrupt Enable

Definition at line 88 of file sys.h.

## ◆ SYS_IRCTRIMIEN_DISABLE

#define SYS_IRCTRIMIEN_DISABLE ((uint32_t)0x00000000)

Trim failure interrupt disable

Definition at line 86 of file sys.h.

## ◆ SYS_IRCTRIMIEN_FAIL_EN

#define SYS_IRCTRIMIEN_FAIL_EN SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk

Trim failure interrupt enable

Definition at line 87 of file sys.h.

## ◆ SYS_IRCTRIMINT_32KERR_INT

#define SYS_IRCTRIMINT_32KERR_INT SYS_IRCTRIMINT_32K_ERR_INT_Msk

32.768 kHz Clock Error Interrupt Status

Definition at line 93 of file sys.h.

## ◆ SYS_IRCTRIMINT_FAIL_INT

#define SYS_IRCTRIMINT_FAIL_INT SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk

Trim failure interrupt status

Definition at line 92 of file sys.h.

## ◆ SYS_IRCTRIMINT_FREQLOCK

#define SYS_IRCTRIMINT_FREQLOCK SYS_IRCTRIMINT_FREQ_LOCK_Msk

HIRC frequency lock status

Definition at line 91 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_EBI_NWE

#define SYS_PA_H_MFP_PA10_MFP_EBI_NWE (2UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - EBI nWE

Definition at line 190 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_GPA10

#define SYS_PA_H_MFP_PA10_MFP_GPA10 (0UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - GPIOA[10]

Definition at line 188 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_I2C1_SDA

#define SYS_PA_H_MFP_PA10_MFP_I2C1_SDA (1UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - I2C1 DATA

Definition at line 189 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_LCD_S22

#define SYS_PA_H_MFP_PA10_MFP_LCD_S22 (7UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - LCD SEG 22

Definition at line 193 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_LCD_S8

#define SYS_PA_H_MFP_PA10_MFP_LCD_S8 (7UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - LCD SEG 8

Definition at line 194 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_SC0_PWR

#define SYS_PA_H_MFP_PA10_MFP_SC0_PWR (3UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - SmartCard0 Power

Definition at line 191 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_SPI2_MISO0

#define SYS_PA_H_MFP_PA10_MFP_SPI2_MISO0 (4UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - SPI2 MISO[0]

Definition at line 192 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_EBI_NRE

#define SYS_PA_H_MFP_PA11_MFP_EBI_NRE (2UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - EBI nRE

Definition at line 182 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_GPA11

#define SYS_PA_H_MFP_PA11_MFP_GPA11 (0UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - GPIOA[11]

Definition at line 180 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_I2C1_SCL

#define SYS_PA_H_MFP_PA11_MFP_I2C1_SCL (1UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - I2C1 clock

Definition at line 181 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_LCD_S23

#define SYS_PA_H_MFP_PA11_MFP_LCD_S23 (7UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - LCD SEG 23

Definition at line 185 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_LCD_S9

#define SYS_PA_H_MFP_PA11_MFP_LCD_S9 (7UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - LCD SEG 9

Definition at line 186 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_SC0_RST

#define SYS_PA_H_MFP_PA11_MFP_SC0_RST (3UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - SmartCard0 RST

Definition at line 183 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_SPI2_MOSI0

#define SYS_PA_H_MFP_PA11_MFP_SPI2_MOSI0 (4UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - SPI2 MOSI[0]

Definition at line 184 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_EBI_AD13

#define SYS_PA_H_MFP_PA12_MFP_EBI_AD13 (2UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - EBI AD[13]

Definition at line 175 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_GPA12

#define SYS_PA_H_MFP_PA12_MFP_GPA12 (0UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - GPIOA[12]

Definition at line 173 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_I2C0_SDA

#define SYS_PA_H_MFP_PA12_MFP_I2C0_SDA (5UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - I2C0 DATA

Definition at line 177 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_LCD_S24

#define SYS_PA_H_MFP_PA12_MFP_LCD_S24 (7UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - LCD SEG 24

Definition at line 178 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_PWM0_CH0

#define SYS_PA_H_MFP_PA12_MFP_PWM0_CH0 (1UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - PWM0 Channel 0

Definition at line 174 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_TMR0_CAP

#define SYS_PA_H_MFP_PA12_MFP_TMR0_CAP (3UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - Timer0 capture event

Definition at line 176 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_EBI_AD14

#define SYS_PA_H_MFP_PA13_MFP_EBI_AD14 (2UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - EBI AD[14]

Definition at line 168 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_GPA13

#define SYS_PA_H_MFP_PA13_MFP_GPA13 (0UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - GPIOA[13]

Definition at line 166 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_I2C0_SCL

#define SYS_PA_H_MFP_PA13_MFP_I2C0_SCL (5UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - I2C0 clock

Definition at line 170 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_LCD_S25

#define SYS_PA_H_MFP_PA13_MFP_LCD_S25 (7UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - LCD SEG 25

Definition at line 171 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_PWM0_CH1

#define SYS_PA_H_MFP_PA13_MFP_PWM0_CH1 (1UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - PWM0 Channel 1

Definition at line 167 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_TMR1_CAP

#define SYS_PA_H_MFP_PA13_MFP_TMR1_CAP (3UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - Timer1 capture event

Definition at line 169 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_EBI_AD15

#define SYS_PA_H_MFP_PA14_MFP_EBI_AD15 (2UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - EBI AD[15]

Definition at line 161 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_GPA14

#define SYS_PA_H_MFP_PA14_MFP_GPA14 (0UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - GPIOA[14]

Definition at line 159 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_LCD_S26

#define SYS_PA_H_MFP_PA14_MFP_LCD_S26 (7UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - LCD SEG 26

Definition at line 164 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_PWM0_CH2

#define SYS_PA_H_MFP_PA14_MFP_PWM0_CH2 (1UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - PWM0 Channel 2

Definition at line 160 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_TMR2_CAP

#define SYS_PA_H_MFP_PA14_MFP_TMR2_CAP (3UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - Timer2 capture event

Definition at line 162 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_UART0_RX

#define SYS_PA_H_MFP_PA14_MFP_UART0_RX (6UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - UART0 RX

Definition at line 163 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_GPA15

#define SYS_PA_H_MFP_PA15_MFP_GPA15 (0UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - GPIOA[15]

Definition at line 151 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_I2S_MCLK

#define SYS_PA_H_MFP_PA15_MFP_I2S_MCLK (2UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - I2S MCLK

Definition at line 153 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_LCD_S27

#define SYS_PA_H_MFP_PA15_MFP_LCD_S27 (7UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - LCD SEG 27

Definition at line 157 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_PWM0_CH3

#define SYS_PA_H_MFP_PA15_MFP_PWM0_CH3 (1UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - PWM0 Channel 3

Definition at line 152 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_SC0_PWR

#define SYS_PA_H_MFP_PA15_MFP_SC0_PWR (4UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - SmartCard 0 power

Definition at line 155 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_TMR3_CAP

#define SYS_PA_H_MFP_PA15_MFP_TMR3_CAP (3UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - Timer3 capture event

Definition at line 154 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_UART0_TX

#define SYS_PA_H_MFP_PA15_MFP_UART0_TX (6UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - UART0 TX

Definition at line 156 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_GPA8

#define SYS_PA_H_MFP_PA8_MFP_GPA8 (0UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - GPIOA[8]

Definition at line 203 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_I2C0_SDA

#define SYS_PA_H_MFP_PA8_MFP_I2C0_SDA (1UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - I2C0 DATA

Definition at line 204 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_LCD_S20

#define SYS_PA_H_MFP_PA8_MFP_LCD_S20 (7UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - LCD SEG 20

Definition at line 207 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_LCD_S6

#define SYS_PA_H_MFP_PA8_MFP_LCD_S6 (7UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - LCD SEG 6

Definition at line 208 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_SC0_CLK

#define SYS_PA_H_MFP_PA8_MFP_SC0_CLK (3UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - SmartCard0 clock

Definition at line 205 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_SPI2_SS0

#define SYS_PA_H_MFP_PA8_MFP_SPI2_SS0 (4UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - SPI2 1st chip selection

Definition at line 206 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_GPA9

#define SYS_PA_H_MFP_PA9_MFP_GPA9 (0UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - GPIOA[9]

Definition at line 196 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_I2C0_SCL

#define SYS_PA_H_MFP_PA9_MFP_I2C0_SCL (1UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - I2C0 clock

Definition at line 197 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_LCD_S21

#define SYS_PA_H_MFP_PA9_MFP_LCD_S21 (7UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - LCD SEG 21

Definition at line 200 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_LCD_S7

#define SYS_PA_H_MFP_PA9_MFP_LCD_S7 (7UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - LCD SEG 7

Definition at line 201 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_SC0_DAT

#define SYS_PA_H_MFP_PA9_MFP_SC0_DAT (3UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - SmartCard0 DATA

Definition at line 198 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_SPI2_SCLK

#define SYS_PA_H_MFP_PA9_MFP_SPI2_SCLK (4UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - SPI2 SCLK

Definition at line 199 of file sys.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_ADC_CH0

#define SYS_PA_L_MFP_PA0_MFP_ADC_CH0 (1UL<<SYS_PA_L_MFP_PA0_MFP_Pos)

PA0 Pin Function - ADC input channel 0

Definition at line 147 of file sys.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_GPA0

#define SYS_PA_L_MFP_PA0_MFP_GPA0 (0UL<<SYS_PA_L_MFP_PA0_MFP_Pos)

PA0 Pin Function - GPIOA[0]

Definition at line 146 of file sys.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_SC2_CD

#define SYS_PA_L_MFP_PA0_MFP_SC2_CD (4UL<<SYS_PA_L_MFP_PA0_MFP_Pos)

PA0 Pin Function - SmartCard 2 card detect

Definition at line 148 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_ADC_CH1

#define SYS_PA_L_MFP_PA1_MFP_ADC_CH1 (1UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - ADC input channel 1

Definition at line 143 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_EBI_AD12

#define SYS_PA_L_MFP_PA1_MFP_EBI_AD12 (2UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - EBI AD[12]

Definition at line 144 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_GPA1

#define SYS_PA_L_MFP_PA1_MFP_GPA1 (0UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - GPIOA[1]

Definition at line 142 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_ADC_CH2

#define SYS_PA_L_MFP_PA2_MFP_ADC_CH2 (1UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - ADC input channel 2

Definition at line 137 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_EBI_AD11

#define SYS_PA_L_MFP_PA2_MFP_EBI_AD11 (2UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - EBI AD[11]

Definition at line 138 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_GPA2

#define SYS_PA_L_MFP_PA2_MFP_GPA2 (0UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - GPIOA[2]

Definition at line 136 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_LCD_S23

#define SYS_PA_L_MFP_PA2_MFP_LCD_S23 (7UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - LCD SEG 23

Definition at line 140 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_UART1_RX

#define SYS_PA_L_MFP_PA2_MFP_UART1_RX (5UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - UART1 TX

Definition at line 139 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_ADC_CH3

#define SYS_PA_L_MFP_PA3_MFP_ADC_CH3 (1UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - ADC input channel 3

Definition at line 131 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_EBI_AD10

#define SYS_PA_L_MFP_PA3_MFP_EBI_AD10 (2UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - EBI AD[10]

Definition at line 132 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_GPA3

#define SYS_PA_L_MFP_PA3_MFP_GPA3 (0UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - GPIOA[3]

Definition at line 130 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_LCD_S22

#define SYS_PA_L_MFP_PA3_MFP_LCD_S22 (7UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - LCD SEG 22

Definition at line 134 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_UART1_TX

#define SYS_PA_L_MFP_PA3_MFP_UART1_TX (5UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - UART 1 RX

Definition at line 133 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_ADC_CH4

#define SYS_PA_L_MFP_PA4_MFP_ADC_CH4 (1UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - ADC input channel 4

Definition at line 123 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_EBI_AD9

#define SYS_PA_L_MFP_PA4_MFP_EBI_AD9 (2UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - EBI AD[9]

Definition at line 124 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_GPA4

#define SYS_PA_L_MFP_PA4_MFP_GPA4 (0UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - GPIOA[4]

Definition at line 122 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_I2C0_SDA

#define SYS_PA_L_MFP_PA4_MFP_I2C0_SDA (5UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - I2C0 DATA

Definition at line 126 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_LCD_S21

#define SYS_PA_L_MFP_PA4_MFP_LCD_S21 (7UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - LCD SEG 21

Definition at line 128 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_LCD_S39

#define SYS_PA_L_MFP_PA4_MFP_LCD_S39 (7UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - LCD SEG 39

Definition at line 127 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_SC2_PWR

#define SYS_PA_L_MFP_PA4_MFP_SC2_PWR (4UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - SmartCard 2 power

Definition at line 125 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_ADC_CH5

#define SYS_PA_L_MFP_PA5_MFP_ADC_CH5 (1UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - ADC input channel 5

Definition at line 115 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_EBI_AD8

#define SYS_PA_L_MFP_PA5_MFP_EBI_AD8 (2UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - EBI AD[8]

Definition at line 116 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_GPA5

#define SYS_PA_L_MFP_PA5_MFP_GPA5 (0UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - GPIOA[5]

Definition at line 114 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_I2C0_SCL

#define SYS_PA_L_MFP_PA5_MFP_I2C0_SCL (5UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - I2C0 clock

Definition at line 118 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_LCD_S20

#define SYS_PA_L_MFP_PA5_MFP_LCD_S20 (7UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - LCD SEG 20

Definition at line 120 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_LCD_S38

#define SYS_PA_L_MFP_PA5_MFP_LCD_S38 (7UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - LCD SEG 38

Definition at line 119 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_SC2_RST

#define SYS_PA_L_MFP_PA5_MFP_SC2_RST (4UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - SmartCard2 RST

Definition at line 117 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_ADC_CH6

#define SYS_PA_L_MFP_PA6_MFP_ADC_CH6 (1UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - ADC input channel 6

Definition at line 106 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_EBI_AD7

#define SYS_PA_L_MFP_PA6_MFP_EBI_AD7 (2UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - EBI AD[7]

Definition at line 107 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_GPA6

#define SYS_PA_L_MFP_PA6_MFP_GPA6 (0UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - GPIOA[6]

Definition at line 105 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_LCD_S19

#define SYS_PA_L_MFP_PA6_MFP_LCD_S19 (7UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - LCD SEG 19

Definition at line 112 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_LCD_S37

#define SYS_PA_L_MFP_PA6_MFP_LCD_S37 (7UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - LCD SEG 37

Definition at line 111 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_PWM0_CH3

#define SYS_PA_L_MFP_PA6_MFP_PWM0_CH3 (5UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - PWM0 Channel 3

Definition at line 110 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_SC2_CLK

#define SYS_PA_L_MFP_PA6_MFP_SC2_CLK (4UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - SmartCard 2 clock

Definition at line 109 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_TMR3_CAP

#define SYS_PA_L_MFP_PA6_MFP_TMR3_CAP (3UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - Timer 3 Capture event

Definition at line 108 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_ADC_CH7

#define SYS_PA_L_MFP_PA7_MFP_ADC_CH7 (1UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - ADC input channel 7

Definition at line 98 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_EBI_AD6

#define SYS_PA_L_MFP_PA7_MFP_EBI_AD6 (2UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - EBI AD[6]

Definition at line 99 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_GPA7

#define SYS_PA_L_MFP_PA7_MFP_GPA7 (0UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - GPIOA[7]

Definition at line 97 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_LCD_S36

#define SYS_PA_L_MFP_PA7_MFP_LCD_S36 (7UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - LCD SEG 36

Definition at line 103 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_PWM0_CH2

#define SYS_PA_L_MFP_PA7_MFP_PWM0_CH2 (5UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - PWM0 Channel 2

Definition at line 102 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_SC2_DAT

#define SYS_PA_L_MFP_PA7_MFP_SC2_DAT (4UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - SmartCard 2 data pin

Definition at line 101 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_TMR2_CAP

#define SYS_PA_L_MFP_PA7_MFP_TMR2_CAP (3UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - Timer 2 capture event

Definition at line 100 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_GPB10

#define SYS_PB_H_MFP_PB10_MFP_GPB10 (0UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - GPIOB[10]

Definition at line 299 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_LCD_V2

#define SYS_PB_H_MFP_PB10_MFP_LCD_V2 (7UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - LCD V2

Definition at line 305 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_SC2_CLK

#define SYS_PB_H_MFP_PB10_MFP_SC2_CLK (4UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - SmartCard2 clock

Definition at line 303 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI0

#define SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI0 (5UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - SPI0 MOSI[0]

Definition at line 304 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_SPI0_SS1

#define SYS_PB_H_MFP_PB10_MFP_SPI0_SS1 (1UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - SPI0 chip selection 1

Definition at line 300 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_TMR2_EXT

#define SYS_PB_H_MFP_PB10_MFP_TMR2_EXT (2UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - Timer2 external event input

Definition at line 301 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_TMR2_TOGGLE_OUT

#define SYS_PB_H_MFP_PB10_MFP_TMR2_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - Timer2 toggle output

Definition at line 302 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_GPB11

#define SYS_PB_H_MFP_PB11_MFP_GPB11 (0UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - GPIOB[11]

Definition at line 291 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_LCD_V1

#define SYS_PB_H_MFP_PB11_MFP_LCD_V1 (7UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - LCD V1

Definition at line 297 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_PWM1_CH0

#define SYS_PB_H_MFP_PB11_MFP_PWM1_CH0 (1UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - PWM1 Channel 0

Definition at line 292 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_SC2_DAT

#define SYS_PB_H_MFP_PB11_MFP_SC2_DAT (4UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - SmartCard2 DATA

Definition at line 295 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_SPI0_MISO0

#define SYS_PB_H_MFP_PB11_MFP_SPI0_MISO0 (5UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - SPI 0 MISO[0]

Definition at line 296 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_TMR3_EXT

#define SYS_PB_H_MFP_PB11_MFP_TMR3_EXT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - Timer3 external event input

Definition at line 293 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_TMR3_TOGGLE_OUT

#define SYS_PB_H_MFP_PB11_MFP_TMR3_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - Timer3 toggle output

Definition at line 294 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_CKO

#define SYS_PB_H_MFP_PB12_MFP_CKO (4UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - CKO

Definition at line 287 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_EBI_AD0

#define SYS_PB_H_MFP_PB12_MFP_EBI_AD0 (2UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - EBI AD[0]

Definition at line 286 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_GPB12

#define SYS_PB_H_MFP_PB12_MFP_GPB12 (0UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - GPIOB[12]

Definition at line 285 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_LCD_S10

#define SYS_PB_H_MFP_PB12_MFP_LCD_S10 (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - LCD SEG 10

Definition at line 289 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_LCD_S24

#define SYS_PB_H_MFP_PB12_MFP_LCD_S24 (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - LCD SEG 24

Definition at line 288 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_EBI_AD1

#define SYS_PB_H_MFP_PB13_MFP_EBI_AD1 (2UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - EBI AD[1]

Definition at line 281 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_GPB13

#define SYS_PB_H_MFP_PB13_MFP_GPB13 (0UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - GPIOB[13]

Definition at line 280 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_LCD_S11

#define SYS_PB_H_MFP_PB13_MFP_LCD_S11 (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - LCD SEG 11

Definition at line 283 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_LCD_S25

#define SYS_PB_H_MFP_PB13_MFP_LCD_S25 (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - LCD SEG 25

Definition at line 282 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_EXT_INT0

#define SYS_PB_H_MFP_PB14_MFP_EXT_INT0 (1UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - External interrupt 0

Definition at line 274 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_GPB14

#define SYS_PB_H_MFP_PB14_MFP_GPB14 (0UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - GPIOB[14]

Definition at line 273 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_LCD_S12

#define SYS_PB_H_MFP_PB14_MFP_LCD_S12 (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - LCD SEG 12

Definition at line 278 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_LCD_S26

#define SYS_PB_H_MFP_PB14_MFP_LCD_S26 (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - LCD SEG 26

Definition at line 277 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_SC2_CD

#define SYS_PB_H_MFP_PB14_MFP_SC2_CD (3UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - SmartCard 2 card detect

Definition at line 275 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_SPI2_SS1

#define SYS_PB_H_MFP_PB14_MFP_SPI2_SS1 (4UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - SPI2 2nd chip selection

Definition at line 276 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_EXT_INT1

#define SYS_PB_H_MFP_PB15_MFP_EXT_INT1 (1UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - External interrupt 1

Definition at line 267 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_GPB15

#define SYS_PB_H_MFP_PB15_MFP_GPB15 (0UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - GPIOB[15]

Definition at line 266 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_LCD_S14

#define SYS_PB_H_MFP_PB15_MFP_LCD_S14 (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - LCD SEG 14

Definition at line 271 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_LCD_S31

#define SYS_PB_H_MFP_PB15_MFP_LCD_S31 (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - LCD SEG 31

Definition at line 270 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_SC1_CD

#define SYS_PB_H_MFP_PB15_MFP_SC1_CD (4UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - SmartCard1 card detect

Definition at line 269 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_SNOOPER

#define SYS_PB_H_MFP_PB15_MFP_SNOOPER (3UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - Snooper pin

Definition at line 268 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_ADC_EXT

#define SYS_PB_H_MFP_PB8_MFP_ADC_EXT (1UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - ADC external trigger

Definition at line 316 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_EXT_INT0

#define SYS_PB_H_MFP_PB8_MFP_EXT_INT0 (3UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - External interrupt 0

Definition at line 319 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_GPB8

#define SYS_PB_H_MFP_PB8_MFP_GPB8 (0UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - GPIOB[8]

Definition at line 315 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_LCD_S13

#define SYS_PB_H_MFP_PB8_MFP_LCD_S13 (7UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - LCD SEG 13

Definition at line 322 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_LCD_S30

#define SYS_PB_H_MFP_PB8_MFP_LCD_S30 (7UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - LCD SEG 30

Definition at line 321 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_SC2_PWR

#define SYS_PB_H_MFP_PB8_MFP_SC2_PWR (4UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - SmartCard 2 power

Definition at line 320 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_TMR0_EXT

#define SYS_PB_H_MFP_PB8_MFP_TMR0_EXT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - Timer0 external event input

Definition at line 317 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_TMR0_TOGGLE_OUT

#define SYS_PB_H_MFP_PB8_MFP_TMR0_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - Timer0 toggle output

Definition at line 318 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_EXT_INT0

#define SYS_PB_H_MFP_PB9_MFP_EXT_INT0 (5UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - External interrupt 0

Definition at line 312 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_GPB9

#define SYS_PB_H_MFP_PB9_MFP_GPB9 (0UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - GPIOB[9]

Definition at line 307 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_LCD_V3

#define SYS_PB_H_MFP_PB9_MFP_LCD_V3 (7UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - LCD V3

Definition at line 313 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_SC2_RST

#define SYS_PB_H_MFP_PB9_MFP_SC2_RST (4UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - SmartCard2 RST

Definition at line 311 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_SPI1_SS1

#define SYS_PB_H_MFP_PB9_MFP_SPI1_SS1 (1UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - SPI1 chip selection 1

Definition at line 308 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_TMR1_EXT

#define SYS_PB_H_MFP_PB9_MFP_TMR1_EXT (2UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - Timer1 external event input

Definition at line 309 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_TMR1_TOGGLE_OUT

#define SYS_PB_H_MFP_PB9_MFP_TMR1_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - Timer1 toggle output

Definition at line 310 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_GPB0

#define SYS_PB_L_MFP_PB0_MFP_GPB0 (0UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - GPIOB[0]

Definition at line 259 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_LCD_S1

#define SYS_PB_L_MFP_PB0_MFP_LCD_S1 (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - LCD SEG 1

Definition at line 263 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_LCD_S7

#define SYS_PB_L_MFP_PB0_MFP_LCD_S7 (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - LCD SEG 7

Definition at line 262 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_SPI1_MOSI0

#define SYS_PB_L_MFP_PB0_MFP_SPI1_MOSI0 (3UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - SPI1 MOSI[0]

Definition at line 261 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_UART0_RX

#define SYS_PB_L_MFP_PB0_MFP_UART0_RX (1UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - UART0 RX

Definition at line 260 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_GPB1

#define SYS_PB_L_MFP_PB1_MFP_GPB1 (0UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - GPIOB[1]

Definition at line 253 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_LCD_S0

#define SYS_PB_L_MFP_PB1_MFP_LCD_S0 (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - LCD SEG 0

Definition at line 257 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_LCD_S6

#define SYS_PB_L_MFP_PB1_MFP_LCD_S6 (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - LCD SEG 6

Definition at line 256 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_SPI1_MISO0

#define SYS_PB_L_MFP_PB1_MFP_SPI1_MISO0 (3UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - SPI1 MISO[0]

Definition at line 255 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_UART0_TX

#define SYS_PB_L_MFP_PB1_MFP_UART0_TX (1UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - UART0 TX

Definition at line 254 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_EBI_NWRL

#define SYS_PB_L_MFP_PB2_MFP_EBI_NWRL (2UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - EBI nWRL

Definition at line 248 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_GPB2

#define SYS_PB_L_MFP_PB2_MFP_GPB2 (0UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - GPIOB[2]

Definition at line 246 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_LCD_COM3

#define SYS_PB_L_MFP_PB2_MFP_LCD_COM3 (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - LCD COM 3

Definition at line 251 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_LCD_S5

#define SYS_PB_L_MFP_PB2_MFP_LCD_S5 (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - LCD SEG 5

Definition at line 250 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_SPI1_SCLK

#define SYS_PB_L_MFP_PB2_MFP_SPI1_SCLK (3UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - SPI1 SCLK

Definition at line 249 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_UART0_RTS

#define SYS_PB_L_MFP_PB2_MFP_UART0_RTS (1UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - UART0 RTSn

Definition at line 247 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_EBI_NWRH

#define SYS_PB_L_MFP_PB3_MFP_EBI_NWRH (2UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - EBI nWRH

Definition at line 241 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_GPB3

#define SYS_PB_L_MFP_PB3_MFP_GPB3 (0UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - GPIOB[3]

Definition at line 239 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_LCD_COM2

#define SYS_PB_L_MFP_PB3_MFP_LCD_COM2 (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - LCD COM 2

Definition at line 244 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_LCD_S4

#define SYS_PB_L_MFP_PB3_MFP_LCD_S4 (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - LCD SEG 4

Definition at line 243 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_SPI1_SS0

#define SYS_PB_L_MFP_PB3_MFP_SPI1_SS0 (3UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - SPI1 chip selection 0

Definition at line 242 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_UART0_CTS

#define SYS_PB_L_MFP_PB3_MFP_UART0_CTS (1UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - UART0 CTSn

Definition at line 240 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_GPB4

#define SYS_PB_L_MFP_PB4_MFP_GPB4 (0UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - GPIOB[4]

Definition at line 232 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_LCD_S13

#define SYS_PB_L_MFP_PB4_MFP_LCD_S13 (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - LCD SEG 13

Definition at line 236 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_LCD_S5

#define SYS_PB_L_MFP_PB4_MFP_LCD_S5 (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - LCD SEG 5

Definition at line 237 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_SC0_CD

#define SYS_PB_L_MFP_PB4_MFP_SC0_CD (3UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - SmartCard0 card detection

Definition at line 234 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_SPI2_SS0

#define SYS_PB_L_MFP_PB4_MFP_SPI2_SS0 (4UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - SPI2 chip selection 0

Definition at line 235 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_UART1_RX

#define SYS_PB_L_MFP_PB4_MFP_UART1_RX (1UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - UART1 RX

Definition at line 233 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_GPB5

#define SYS_PB_L_MFP_PB5_MFP_GPB5 (0UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - GPIOB[5]

Definition at line 225 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_LCD_S12

#define SYS_PB_L_MFP_PB5_MFP_LCD_S12 (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - LCD SEG 12

Definition at line 229 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_LCD_S4

#define SYS_PB_L_MFP_PB5_MFP_LCD_S4 (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - LCD SEG 4

Definition at line 230 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_SC0_RST

#define SYS_PB_L_MFP_PB5_MFP_SC0_RST (3UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - SmartCard0 RST

Definition at line 227 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_SPI2_SCLK

#define SYS_PB_L_MFP_PB5_MFP_SPI2_SCLK (4UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - SPI2 SCLK

Definition at line 228 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_UART1_TX

#define SYS_PB_L_MFP_PB5_MFP_UART1_TX (1UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - UART1 TX

Definition at line 226 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_EBI_ALE

#define SYS_PB_L_MFP_PB6_MFP_EBI_ALE (2UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - EBI ALE

Definition at line 220 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_GPB6

#define SYS_PB_L_MFP_PB6_MFP_GPB6 (0UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - GPIOB[6]

Definition at line 218 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_LCD_S11

#define SYS_PB_L_MFP_PB6_MFP_LCD_S11 (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - LCD SEG 11

Definition at line 222 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_LCD_S3

#define SYS_PB_L_MFP_PB6_MFP_LCD_S3 (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - LCD SEG 3

Definition at line 223 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_SPI2_MISO0

#define SYS_PB_L_MFP_PB6_MFP_SPI2_MISO0 (4UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - SPI2 MISO[0]

Definition at line 221 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_UART1_RTS

#define SYS_PB_L_MFP_PB6_MFP_UART1_RTS (1UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - UART1 RTSn

Definition at line 219 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_EBI_NCS

#define SYS_PB_L_MFP_PB7_MFP_EBI_NCS (2UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - EBI nCS

Definition at line 213 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_GPB7

#define SYS_PB_L_MFP_PB7_MFP_GPB7 (0UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - GPIOB[7]

Definition at line 211 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_LCD_S10

#define SYS_PB_L_MFP_PB7_MFP_LCD_S10 (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - LCD SEG 10

Definition at line 215 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_LCD_S2

#define SYS_PB_L_MFP_PB7_MFP_LCD_S2 (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - LCD SEG 2

Definition at line 216 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_SPI2_MOSI0

#define SYS_PB_L_MFP_PB7_MFP_SPI2_MOSI0 (4UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - SPI2 MOSI[0]

Definition at line 214 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_UART1_CTS

#define SYS_PB_L_MFP_PB7_MFP_UART1_CTS (1UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - UART1 CTSn

Definition at line 212 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_GPC10

#define SYS_PC_H_MFP_PC10_MFP_GPC10 (0UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - GPIOC[10]

Definition at line 403 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_LCD_S30

#define SYS_PC_H_MFP_PC10_MFP_LCD_S30 (7UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - LCD SEG 30

Definition at line 406 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_SPI1_MISO0

#define SYS_PC_H_MFP_PC10_MFP_SPI1_MISO0 (1UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - SPI1 MISO[0]

Definition at line 404 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_UART1_RX

#define SYS_PC_H_MFP_PC10_MFP_UART1_RX (5UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - UART1 RX

Definition at line 405 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_GPC11

#define SYS_PC_H_MFP_PC11_MFP_GPC11 (0UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - GPIOC[11]

Definition at line 398 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_LCD_S31

#define SYS_PC_H_MFP_PC11_MFP_LCD_S31 (7UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - LCD SEG 31

Definition at line 401 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_SPI1_MOSI0

#define SYS_PC_H_MFP_PC11_MFP_SPI1_MOSI0 (1UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - SPI1 MOSI[0]

Definition at line 399 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_UART1_TX

#define SYS_PC_H_MFP_PC11_MFP_UART1_TX (5UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - UART1 TX

Definition at line 400 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_EXT_INT0

#define SYS_PC_H_MFP_PC12_MFP_EXT_INT0 (5UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - External interrupt 0

Definition at line 395 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_GPC12

#define SYS_PC_H_MFP_PC12_MFP_GPC12 (0UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - GPIOC[12]

Definition at line 392 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_I2C0_SDA

#define SYS_PC_H_MFP_PC12_MFP_I2C0_SDA (6UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - I2C0 DATA

Definition at line 396 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_PWM1_CH0

#define SYS_PC_H_MFP_PC12_MFP_PWM1_CH0 (2UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - PWM1 Channel 0

Definition at line 394 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_SPI1_MISO1

#define SYS_PC_H_MFP_PC12_MFP_SPI1_MISO1 (1UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - SPI1 MISO[1]

Definition at line 393 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_EXT_INT1

#define SYS_PC_H_MFP_PC13_MFP_EXT_INT1 (5UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - External interrupt 1

Definition at line 389 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_GPC13

#define SYS_PC_H_MFP_PC13_MFP_GPC13 (0UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - GPIOC[13]

Definition at line 385 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_I2C0_SCL

#define SYS_PC_H_MFP_PC13_MFP_I2C0_SCL (6UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - I2C0 clock

Definition at line 390 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_PWM1_CH1

#define SYS_PC_H_MFP_PC13_MFP_PWM1_CH1 (2UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - PWM1 Channel 1

Definition at line 387 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_SNOOPER

#define SYS_PC_H_MFP_PC13_MFP_SNOOPER (4UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - Snooper pin

Definition at line 388 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_SPI1_MOSI1

#define SYS_PC_H_MFP_PC13_MFP_SPI1_MOSI1 (1UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - SPI1 MOSI[1]

Definition at line 386 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_EBI_AD2

#define SYS_PC_H_MFP_PC14_MFP_EBI_AD2 (2UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - EBI AD[2]

Definition at line 380 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_GPC14

#define SYS_PC_H_MFP_PC14_MFP_GPC14 (0UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - GPIOC[14]

Definition at line 379 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_LCD_S15

#define SYS_PC_H_MFP_PC14_MFP_LCD_S15 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - LCD SEG 15

Definition at line 383 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_LCD_S32

#define SYS_PC_H_MFP_PC14_MFP_LCD_S32 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - LCD SEG 32

Definition at line 382 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_PWM1_CH3

#define SYS_PC_H_MFP_PC14_MFP_PWM1_CH3 (4UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - PWM1 Channel 3

Definition at line 381 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_EBI_AD3

#define SYS_PC_H_MFP_PC15_MFP_EBI_AD3 (2UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - EBI AD[3]

Definition at line 373 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_GPC15

#define SYS_PC_H_MFP_PC15_MFP_GPC15 (0UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - GPIOC[15]

Definition at line 372 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_LCD_S16

#define SYS_PC_H_MFP_PC15_MFP_LCD_S16 (7UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - LCD SEG 16

Definition at line 377 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_LCD_S33

#define SYS_PC_H_MFP_PC15_MFP_LCD_S33 (7UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - LCD SEG 33

Definition at line 376 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_PWM1_CH2

#define SYS_PC_H_MFP_PC15_MFP_PWM1_CH2 (4UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - PWM1 Channel 2

Definition at line 375 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_TMR0_CAP

#define SYS_PC_H_MFP_PC15_MFP_TMR0_CAP (3UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - Timer0 capture event

Definition at line 374 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_EBI_XCLK

#define SYS_PC_H_MFP_PC8_MFP_EBI_XCLK (2UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - EBI XCLK

Definition at line 415 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_GPC8

#define SYS_PC_H_MFP_PC8_MFP_GPC8 (0UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - GPIOC[8]

Definition at line 413 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_I2C1_SDA

#define SYS_PC_H_MFP_PC8_MFP_I2C1_SDA (5UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - I2C1 DATA

Definition at line 416 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_LCD_S28

#define SYS_PC_H_MFP_PC8_MFP_LCD_S28 (7UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - LCD SEG 28

Definition at line 417 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_SPI1_SS0

#define SYS_PC_H_MFP_PC8_MFP_SPI1_SS0 (1UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - SPI1 SS[0]

Definition at line 414 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_GPC9

#define SYS_PC_H_MFP_PC9_MFP_GPC9 (0UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - GPIOC[9]

Definition at line 408 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_I2C1_SCL

#define SYS_PC_H_MFP_PC9_MFP_I2C1_SCL (5UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - I2C1 clock

Definition at line 410 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_LCD_S29

#define SYS_PC_H_MFP_PC9_MFP_LCD_S29 (7UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - LCD SEG 29

Definition at line 411 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_SPI1_SCLK

#define SYS_PC_H_MFP_PC9_MFP_SPI1_SCLK (1UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - SPI1 SCLK

Definition at line 409 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_GPC0

#define SYS_PC_L_MFP_PC0_MFP_GPC0 (0UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - GPIOC[0]

Definition at line 365 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_I2S_WS

#define SYS_PC_L_MFP_PC0_MFP_I2S_WS (2UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - I2S WS

Definition at line 367 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_LCD_DH1

#define SYS_PC_L_MFP_PC0_MFP_LCD_DH1 (7UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - LCD DH1

Definition at line 369 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_SC1_CLK

#define SYS_PC_L_MFP_PC0_MFP_SC1_CLK (4UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - SmartCard1 clock

Definition at line 368 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_SPI0_SS0

#define SYS_PC_L_MFP_PC0_MFP_SPI0_SS0 (1UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - SPI0 chip selection 0

Definition at line 366 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_GPC1

#define SYS_PC_L_MFP_PC1_MFP_GPC1 (0UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - GPIOC[1]

Definition at line 359 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_I2S_BCLK

#define SYS_PC_L_MFP_PC1_MFP_I2S_BCLK (2UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - I2S BCLK

Definition at line 361 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_LCD_DH2

#define SYS_PC_L_MFP_PC1_MFP_LCD_DH2 (7UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - LCD DH2

Definition at line 363 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_SC1_DAT

#define SYS_PC_L_MFP_PC1_MFP_SC1_DAT (4UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - SmartCard1 DATA

Definition at line 362 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_SPI0_SCLK

#define SYS_PC_L_MFP_PC1_MFP_SPI0_SCLK (1UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - SPI0 SCLK

Definition at line 360 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_GPC2

#define SYS_PC_L_MFP_PC2_MFP_GPC2 (0UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - GPIOC[2]

Definition at line 353 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_I2S_DIN

#define SYS_PC_L_MFP_PC2_MFP_I2S_DIN (2UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - I2S Din

Definition at line 355 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_LCD_COM0

#define SYS_PC_L_MFP_PC2_MFP_LCD_COM0 (7UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - LCD COM 0

Definition at line 357 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_SC1_PWR

#define SYS_PC_L_MFP_PC2_MFP_SC1_PWR (4UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - SmartCard1 Power

Definition at line 356 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_SPI0_MISO0

#define SYS_PC_L_MFP_PC2_MFP_SPI0_MISO0 (1UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - SPI0 MISO[0]

Definition at line 354 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_GPC3

#define SYS_PC_L_MFP_PC3_MFP_GPC3 (0UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - GPIOC[3]

Definition at line 347 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_I2S_DOUT

#define SYS_PC_L_MFP_PC3_MFP_I2S_DOUT (2UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - I2S Dout

Definition at line 349 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_LCD_COM1

#define SYS_PC_L_MFP_PC3_MFP_LCD_COM1 (7UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - LCD COM 1

Definition at line 351 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_SC1_RST

#define SYS_PC_L_MFP_PC3_MFP_SC1_RST (4UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - SmartCard1 RST

Definition at line 350 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_SPI0_MOSI0

#define SYS_PC_L_MFP_PC3_MFP_SPI0_MOSI0 (1UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - SPI0 MOSI[0]

Definition at line 348 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_GPC4

#define SYS_PC_L_MFP_PC4_MFP_GPC4 (0UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - GPIOC[4]

Definition at line 343 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_LCD_COM2

#define SYS_PC_L_MFP_PC4_MFP_LCD_COM2 (7UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - LCD COM 2

Definition at line 345 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_SPI0_MISO1

#define SYS_PC_L_MFP_PC4_MFP_SPI0_MISO1 (1UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - SPI0 MISO[1]

Definition at line 344 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_GPC5

#define SYS_PC_L_MFP_PC5_MFP_GPC5 (0UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - GPIOC[5]

Definition at line 339 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_LCD_COM3

#define SYS_PC_L_MFP_PC5_MFP_LCD_COM3 (7UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - LCD COM 3

Definition at line 341 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_SPI0_MOSI1

#define SYS_PC_L_MFP_PC5_MFP_SPI0_MOSI1 (1UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - SPI0 MOSI[1]

Definition at line 340 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_DA_OUT0

#define SYS_PC_L_MFP_PC6_MFP_DA_OUT0 (1UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - DA out0

Definition at line 333 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_EBI_AD4

#define SYS_PC_L_MFP_PC6_MFP_EBI_AD4 (2UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - EBI AD[4]

Definition at line 334 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_GPC6

#define SYS_PC_L_MFP_PC6_MFP_GPC6 (0UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - GPIOC[6]

Definition at line 332 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_PWM0_CH0

#define SYS_PC_L_MFP_PC6_MFP_PWM0_CH0 (5UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - PWM0 Channel 0

Definition at line 337 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_SC1_CD

#define SYS_PC_L_MFP_PC6_MFP_SC1_CD (4UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - SmartCard1 card detection

Definition at line 336 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_TMR0_CAP

#define SYS_PC_L_MFP_PC6_MFP_TMR0_CAP (3UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - Timer0 Capture event

Definition at line 335 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_DA_OUT1

#define SYS_PC_L_MFP_PC7_MFP_DA_OUT1 (1UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - DA out1

Definition at line 326 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_EBI_AD5

#define SYS_PC_L_MFP_PC7_MFP_EBI_AD5 (2UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - EBI AD[5]

Definition at line 327 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_GPC7

#define SYS_PC_L_MFP_PC7_MFP_GPC7 (0UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - GPIOC[7]

Definition at line 325 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_LCD_S17

#define SYS_PC_L_MFP_PC7_MFP_LCD_S17 (7UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - LCD SEG 17

Definition at line 330 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_PWM0_CH1

#define SYS_PC_L_MFP_PC7_MFP_PWM0_CH1 (5UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - PWM0 Channel 1

Definition at line 329 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_TMR1_CAP

#define SYS_PC_L_MFP_PC7_MFP_TMR1_CAP (3UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - Timer1 capture event

Definition at line 328 of file sys.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_GPD10

#define SYS_PD_H_MFP_PD10_MFP_GPD10 (0UL<<SYS_PD_H_MFP_PD10_MFP_Pos)

PD10 Pin Function - GPIOD[10]

Definition at line 479 of file sys.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_LCD_S17

#define SYS_PD_H_MFP_PD10_MFP_LCD_S17 (7UL<<SYS_PD_H_MFP_PD10_MFP_Pos)

PD10 Pin Function - LCD SEG 17

Definition at line 480 of file sys.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_GPD11

#define SYS_PD_H_MFP_PD11_MFP_GPD11 (0UL<<SYS_PD_H_MFP_PD11_MFP_Pos)

PD11 Pin Function - GPIOD[11]

Definition at line 476 of file sys.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_LCD_S16

#define SYS_PD_H_MFP_PD11_MFP_LCD_S16 (7uL<<SYS_PD_H_MFP_PD11_MFP_Pos)

PD11 Pin Function - LCD SEG 16

Definition at line 477 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_GPD12

#define SYS_PD_H_MFP_PD12_MFP_GPD12 (0UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - GPIOD[12]

Definition at line 473 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_LCD_S15

#define SYS_PD_H_MFP_PD12_MFP_LCD_S15 (7UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - LCD SEG 15

Definition at line 474 of file sys.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_GPD13

#define SYS_PD_H_MFP_PD13_MFP_GPD13 (0UL<<SYS_PD_H_MFP_PD13_MFP_Pos)

PD13 Pin Function - GPIOD[13]

Definition at line 470 of file sys.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_LCD_S14

#define SYS_PD_H_MFP_PD13_MFP_LCD_S14 (7UL<<SYS_PD_H_MFP_PD13_MFP_Pos)

PD13 Pin Function - LCD SEG 14

Definition at line 471 of file sys.h.

## ◆ SYS_PD_H_MFP_PD14_MFP_GPD14

#define SYS_PD_H_MFP_PD14_MFP_GPD14 (0UL<<SYS_PD_H_MFP_PD14_MFP_Pos)

PD14 Pin Function - GPIOD[14]

Definition at line 467 of file sys.h.

## ◆ SYS_PD_H_MFP_PD14_MFP_LCD_S1

#define SYS_PD_H_MFP_PD14_MFP_LCD_S1 (7UL<<SYS_PD_H_MFP_PD14_MFP_Pos)

PD14 Pin Function - LCD SEG 1

Definition at line 468 of file sys.h.

## ◆ SYS_PD_H_MFP_PD15_MFP_GPD15

#define SYS_PD_H_MFP_PD15_MFP_GPD15 (0UL<<SYS_PD_H_MFP_PD15_MFP_Pos)

PD15 Pin Function - GPIOD[15]

Definition at line 464 of file sys.h.

## ◆ SYS_PD_H_MFP_PD15_MFP_LCD_S0

#define SYS_PD_H_MFP_PD15_MFP_LCD_S0 (7UL<<SYS_PD_H_MFP_PD15_MFP_Pos)

PD15 Pin Function - LCD SEG 0

Definition at line 465 of file sys.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_GPD8

#define SYS_PD_H_MFP_PD8_MFP_GPD8 (0UL<<SYS_PD_H_MFP_PD8_MFP_Pos)

PD8 Pin Function - GPIOD[8]

Definition at line 485 of file sys.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_LCD_S19

#define SYS_PD_H_MFP_PD8_MFP_LCD_S19 (7UL<<SYS_PD_H_MFP_PD8_MFP_Pos)

PD8 Pin Function - LCD SEG 19

Definition at line 486 of file sys.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_GPD9

#define SYS_PD_H_MFP_PD9_MFP_GPD9 (0UL<<SYS_PD_H_MFP_PD9_MFP_Pos)

PD9 Pin Function - GPIOD[9]

Definition at line 482 of file sys.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_LCD_S18

#define SYS_PD_H_MFP_PD9_MFP_LCD_S18 (7UL<<SYS_PD_H_MFP_PD9_MFP_Pos)

PD9 Pin Function - LCD SEG 18

Definition at line 483 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_ADC_CH8

#define SYS_PD_L_MFP_PD0_MFP_ADC_CH8 (5UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - ADC input channel 8

Definition at line 461 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_GPD0

#define SYS_PD_L_MFP_PD0_MFP_GPD0 (0UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - GPIOD[0]

Definition at line 457 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_SC1_CLK

#define SYS_PD_L_MFP_PD0_MFP_SC1_CLK (4UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - SmartCard1 clock

Definition at line 460 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_SPI2_SS0

#define SYS_PD_L_MFP_PD0_MFP_SPI2_SS0 (3UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - SPI2 chip selection 0

Definition at line 459 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_UART1_RX

#define SYS_PD_L_MFP_PD0_MFP_UART1_RX (1UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - UART1 RX

Definition at line 458 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_ADC_CH9

#define SYS_PD_L_MFP_PD1_MFP_ADC_CH9 (5UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - ADC input channel 9

Definition at line 455 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_GPD1

#define SYS_PD_L_MFP_PD1_MFP_GPD1 (0UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - GPIOD[1]

Definition at line 451 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_SC1_DAT

#define SYS_PD_L_MFP_PD1_MFP_SC1_DAT (4UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - SmartCard1 DATA

Definition at line 454 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_SPI2_SCLK

#define SYS_PD_L_MFP_PD1_MFP_SPI2_SCLK (3UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - SPI2 SCLK

Definition at line 453 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_UART1_TX

#define SYS_PD_L_MFP_PD1_MFP_UART1_TX (1UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - UART1 TX

Definition at line 452 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_ADC_CH10

#define SYS_PD_L_MFP_PD2_MFP_ADC_CH10 (5UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - ADC input channel 10

Definition at line 449 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_GPD2

#define SYS_PD_L_MFP_PD2_MFP_GPD2 (0UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - GPIOD[2]

Definition at line 444 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_I2S_WS

#define SYS_PD_L_MFP_PD2_MFP_I2S_WS (2UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - I2S WS

Definition at line 446 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_SC1_PWR

#define SYS_PD_L_MFP_PD2_MFP_SC1_PWR (4UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - SmartCard1 power

Definition at line 448 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_SPI2_MISO0

#define SYS_PD_L_MFP_PD2_MFP_SPI2_MISO0 (3UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - SPI2 MISO[0]

Definition at line 447 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_UART1_RTS

#define SYS_PD_L_MFP_PD2_MFP_UART1_RTS (1UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - UART1 RTSn

Definition at line 445 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_ADC_CH11

#define SYS_PD_L_MFP_PD3_MFP_ADC_CH11 (5UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - ADC input channel 11

Definition at line 442 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_GPD3

#define SYS_PD_L_MFP_PD3_MFP_GPD3 (0UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - GPIOD[3]

Definition at line 437 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_I2S_BCLK

#define SYS_PD_L_MFP_PD3_MFP_I2S_BCLK (2UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - I2S BCLK

Definition at line 439 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_SC1_RST

#define SYS_PD_L_MFP_PD3_MFP_SC1_RST (4UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - SmartCard1 reset

Definition at line 441 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_SPI2_MOSI0

#define SYS_PD_L_MFP_PD3_MFP_SPI2_MOSI0 (3UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - SPI2 MOSI[0]

Definition at line 440 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_UART1_CTS

#define SYS_PD_L_MFP_PD3_MFP_UART1_CTS (1UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - UART1 CTSn

Definition at line 438 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_GPD4

#define SYS_PD_L_MFP_PD4_MFP_GPD4 (0UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - GPIOD[4]

Definition at line 431 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_I2S_DIN

#define SYS_PD_L_MFP_PD4_MFP_I2S_DIN (2UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - I2S Din

Definition at line 432 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_LCD_S35

#define SYS_PD_L_MFP_PD4_MFP_LCD_S35 (7UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - LCD SEG 35

Definition at line 435 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_SC1_CD

#define SYS_PD_L_MFP_PD4_MFP_SC1_CD (4UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - SmartCard1 card detection

Definition at line 434 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_SPI2_MISO1

#define SYS_PD_L_MFP_PD4_MFP_SPI2_MISO1 (3UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - SPI2 MISO[1]

Definition at line 433 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_GPD5

#define SYS_PD_L_MFP_PD5_MFP_GPD5 (0UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - GPIOD[5]

Definition at line 426 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_I2S_DOUT

#define SYS_PD_L_MFP_PD5_MFP_I2S_DOUT (2UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - I2S Dout

Definition at line 427 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_LCD_S34

#define SYS_PD_L_MFP_PD5_MFP_LCD_S34 (7UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - LCD SEG 34

Definition at line 429 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_SPI2_MOSI1

#define SYS_PD_L_MFP_PD5_MFP_SPI2_MOSI1 (3UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - SPI2 MOSI[1]

Definition at line 428 of file sys.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_GPD6

#define SYS_PD_L_MFP_PD6_MFP_GPD6 (0UL<<SYS_PD_L_MFP_PD6_MFP_Pos)

PD6 Pin Function - GPIOD[6]

Definition at line 423 of file sys.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_LCD_S3

#define SYS_PD_L_MFP_PD6_MFP_LCD_S3 (7UL<<SYS_PD_L_MFP_PD6_MFP_Pos)

PD6 Pin Function - LCD SEG 3

Definition at line 424 of file sys.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_GPD7

#define SYS_PD_L_MFP_PD7_MFP_GPD7 (0UL<<SYS_PD_L_MFP_PD7_MFP_Pos)

PD7 Pin Function - GPIOD[7]

Definition at line 420 of file sys.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_LCD_S2

#define SYS_PD_L_MFP_PD7_MFP_LCD_S2 (7UL<<SYS_PD_L_MFP_PD7_MFP_Pos)

PD7 Pin Function - LCD SEG 2

Definition at line 421 of file sys.h.

## ◆ SYS_PE_H_MFP_PE10_MFP_GPE10

#define SYS_PE_H_MFP_PE10_MFP_GPE10 (0UL<<SYS_PE_H_MFP_PE10_MFP_Pos)

PE10 Pin Function - GPIOE[10]

Definition at line 530 of file sys.h.

## ◆ SYS_PE_H_MFP_PE10_MFP_UART1_TX

#define SYS_PE_H_MFP_PE10_MFP_UART1_TX (7UL<<SYS_PE_H_MFP_PE10_MFP_Pos)

PE10 Pin Function - UART1 TX

Definition at line 531 of file sys.h.

## ◆ SYS_PE_H_MFP_PE11_MFP_GPE11

#define SYS_PE_H_MFP_PE11_MFP_GPE11 (0UL<<SYS_PE_H_MFP_PE11_MFP_Pos)

PE11 Pin Function - GPIOE[11]

Definition at line 527 of file sys.h.

## ◆ SYS_PE_H_MFP_PE11_MFP_UART1_RTS

#define SYS_PE_H_MFP_PE11_MFP_UART1_RTS (7UL<<SYS_PE_H_MFP_PE11_MFP_Pos)

PE11 Pin Function - UART1 RTSn

Definition at line 528 of file sys.h.

## ◆ SYS_PE_H_MFP_PE12_MFP_GPE12

#define SYS_PE_H_MFP_PE12_MFP_GPE12 (0UL<<SYS_PE_H_MFP_PE12_MFP_Pos)

PE12 Pin Function - GPIOE[12]

Definition at line 524 of file sys.h.

## ◆ SYS_PE_H_MFP_PE12_MFP_UART1_CTS

#define SYS_PE_H_MFP_PE12_MFP_UART1_CTS (7UL<<SYS_PE_H_MFP_PE12_MFP_Pos)

PE12 Pin Function - UART1 CTSn

Definition at line 525 of file sys.h.

## ◆ SYS_PE_H_MFP_PE13_MFP_GPE13

#define SYS_PE_H_MFP_PE13_MFP_GPE13 (0UL<<SYS_PE_H_MFP_PE13_MFP_Pos)

PE13 Pin Function - GPIOE[13]

Definition at line 521 of file sys.h.

## ◆ SYS_PE_H_MFP_PE13_MFP_LCD_S27

#define SYS_PE_H_MFP_PE13_MFP_LCD_S27 (7UL<<SYS_PE_H_MFP_PE13_MFP_Pos)

PE13 Pin Function - LCD SEG 27

Definition at line 522 of file sys.h.

## ◆ SYS_PE_H_MFP_PE14_MFP_GPE14

#define SYS_PE_H_MFP_PE14_MFP_GPE14 (0UL<<SYS_PE_H_MFP_PE14_MFP_Pos)

PE14 Pin Function - GPIOE[14]

Definition at line 518 of file sys.h.

## ◆ SYS_PE_H_MFP_PE14_MFP_LCD_S28

#define SYS_PE_H_MFP_PE14_MFP_LCD_S28 (7UL<<SYS_PE_H_MFP_PE14_MFP_Pos)

PE14 Pin Function - LCD SEG 28

Definition at line 519 of file sys.h.

## ◆ SYS_PE_H_MFP_PE15_MFP_GPE15

#define SYS_PE_H_MFP_PE15_MFP_GPE15 (0UL<<SYS_PE_H_MFP_PE15_MFP_Pos)

PE15 Pin Function - GPIOE[15]

Definition at line 515 of file sys.h.

## ◆ SYS_PE_H_MFP_PE15_MFP_LCD_S29

#define SYS_PE_H_MFP_PE15_MFP_LCD_S29 (7UL<<SYS_PE_H_MFP_PE15_MFP_Pos)

PE15 Pin Function - LCD SEG 29

Definition at line 516 of file sys.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_GPE8

#define SYS_PE_H_MFP_PE8_MFP_GPE8 (0UL<<SYS_PE_H_MFP_PE8_MFP_Pos)

PE8 Pin Function - GPIOA[8]

Definition at line 536 of file sys.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_LCD_S9

#define SYS_PE_H_MFP_PE8_MFP_LCD_S9 (7UL<<SYS_PE_H_MFP_PE8_MFP_Pos)

PE8 Pin Function - LCD SEG 9

Definition at line 537 of file sys.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_GPE9

#define SYS_PE_H_MFP_PE9_MFP_GPE9 (0UL<<SYS_PE_H_MFP_PE9_MFP_Pos)

PE9 Pin Function - GPIOE[9]

Definition at line 533 of file sys.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_UART1_RX

#define SYS_PE_H_MFP_PE9_MFP_UART1_RX (7UL<<SYS_PE_H_MFP_PE9_MFP_Pos)

PE9 Pin Function - UART1 RX

Definition at line 534 of file sys.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_GPE0

#define SYS_PE_L_MFP_PE0_MFP_GPE0 (0UL<<SYS_PE_L_MFP_PE0_MFP_Pos)

PE0 Pin Function - GPIOE[0]

Definition at line 510 of file sys.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_I2S_MCLK

#define SYS_PE_L_MFP_PE0_MFP_I2S_MCLK (2UL<<SYS_PE_L_MFP_PE0_MFP_Pos)

PE0 Pin Function - I2S MCLK

Definition at line 512 of file sys.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_PWM1_CH2

#define SYS_PE_L_MFP_PE0_MFP_PWM1_CH2 (1UL<<SYS_PE_L_MFP_PE0_MFP_Pos)

PE0 Pin Function - PWM1 Channel 2

Definition at line 511 of file sys.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_GPE1

#define SYS_PE_L_MFP_PE1_MFP_GPE1 (0UL<<SYS_PE_L_MFP_PE1_MFP_Pos)

PE1 Pin Function - GPIOE[1]

Definition at line 506 of file sys.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_PWM1_CH3

#define SYS_PE_L_MFP_PE1_MFP_PWM1_CH3 (1UL<<SYS_PE_L_MFP_PE1_MFP_Pos)

PE1 Pin Function - PWM1 Channel 3

Definition at line 507 of file sys.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_SPI0_SS0

#define SYS_PE_L_MFP_PE1_MFP_SPI0_SS0 (6UL<<SYS_PE_L_MFP_PE1_MFP_Pos)

PE1 Pin Function - SPI0 chip selection 0

Definition at line 508 of file sys.h.

## ◆ SYS_PE_L_MFP_PE2_MFP_GPE2

#define SYS_PE_L_MFP_PE2_MFP_GPE2 (0UL<<SYS_PE_L_MFP_PE2_MFP_Pos)

PE2 Pin Function - GPIOE[2]

Definition at line 503 of file sys.h.

## ◆ SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK

#define SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK (6UL<<SYS_PE_L_MFP_PE2_MFP_Pos)

PE2 Pin Function - SPI0 SCLK

Definition at line 504 of file sys.h.

## ◆ SYS_PE_L_MFP_PE3_MFP_GPE3

#define SYS_PE_L_MFP_PE3_MFP_GPE3 (0UL<<SYS_PE_L_MFP_PE3_MFP_Pos)

PE3 Pin Function - GPIOE[3]

Definition at line 500 of file sys.h.

## ◆ SYS_PE_L_MFP_PE3_MFP_SPI0_MISO0

#define SYS_PE_L_MFP_PE3_MFP_SPI0_MISO0 (6UL<<SYS_PE_L_MFP_PE3_MFP_Pos)

PE3 Pin Function - SPI0 MISO[0]

Definition at line 501 of file sys.h.

## ◆ SYS_PE_L_MFP_PE4_MFP_GPE4

#define SYS_PE_L_MFP_PE4_MFP_GPE4 (0UL<<SYS_PE_L_MFP_PE4_MFP_Pos)

PE4 Pin Function - GPIOE[4]

Definition at line 497 of file sys.h.

## ◆ SYS_PE_L_MFP_PE4_MFP_SPI0_MOSI0

#define SYS_PE_L_MFP_PE4_MFP_SPI0_MOSI0 (6UL<<SYS_PE_L_MFP_PE4_MFP_Pos)

PE4 Pin Function - SPI0 MOSI[0]

Definition at line 498 of file sys.h.

## ◆ SYS_PE_L_MFP_PE5_MFP_GPE5

#define SYS_PE_L_MFP_PE5_MFP_GPE5 (0UL<<SYS_PE_L_MFP_PE5_MFP_Pos)

PE5 Pin Function - GPIOE[5]

Definition at line 494 of file sys.h.

## ◆ SYS_PE_L_MFP_PE5_MFP_PWM1_CH1

#define SYS_PE_L_MFP_PE5_MFP_PWM1_CH1 (1UL<<SYS_PE_L_MFP_PE5_MFP_Pos)

PE5 Pin Function - PWM1 Channel 1

Definition at line 495 of file sys.h.

## ◆ SYS_PE_L_MFP_PE6_MFP_GPE6

#define SYS_PE_L_MFP_PE6_MFP_GPE6 (0UL<<SYS_PE_L_MFP_PE6_MFP_Pos)

PE6 Pin Function - GPIOE[6]

Definition at line 492 of file sys.h.

## ◆ SYS_PE_L_MFP_PE7_MFP_GPE7

#define SYS_PE_L_MFP_PE7_MFP_GPE7 (0UL<<SYS_PE_L_MFP_PE7_MFP_Pos)

PE7 Pin Function - GPIOE[7]

Definition at line 489 of file sys.h.

## ◆ SYS_PE_L_MFP_PE7_MFP_LCD_S8

#define SYS_PE_L_MFP_PE7_MFP_LCD_S8 (7UL<<SYS_PE_L_MFP_PE7_MFP_Pos)

PE7 Pin Function - LCD SEG 8

Definition at line 490 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_EXT_INT0

#define SYS_PF_L_MFP_PF0_MFP_EXT_INT0 (5UL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - External interrupt 0

Definition at line 558 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_GPF0

#define SYS_PF_L_MFP_PF0_MFP_GPF0 (0UL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - GPIOF[0]

Definition at line 557 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_ICE_DAT

#define SYS_PF_L_MFP_PF0_MFP_ICE_DAT (7UL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - ICE DATA

Definition at line 559 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_CKO

#define SYS_PF_L_MFP_PF1_MFP_CKO (4UL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - CKO

Definition at line 553 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_EXT_INT1

#define SYS_PF_L_MFP_PF1_MFP_EXT_INT1 (5UL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - External interrupt 1

Definition at line 554 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_GPF1

#define SYS_PF_L_MFP_PF1_MFP_GPF1 (0UL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - GPIOF[1]

Definition at line 552 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_ICE_CLK

#define SYS_PF_L_MFP_PF1_MFP_ICE_CLK (7UL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - ICE CLOCK

Definition at line 555 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_GPF2

#define SYS_PF_L_MFP_PF2_MFP_GPF2 (0UL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - GPIOF[2]

Definition at line 549 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_HXT_OUT

#define SYS_PF_L_MFP_PF2_MFP_HXT_OUT (7UL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - HXT OUT

Definition at line 550 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_GPF3

#define SYS_PF_L_MFP_PF3_MFP_GPF3 (0UL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - GPIOF[3]

Definition at line 546 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_HXT_IN

#define SYS_PF_L_MFP_PF3_MFP_HXT_IN (7UL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - HXT IN

Definition at line 547 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_GPF4

#define SYS_PF_L_MFP_PF4_MFP_GPF4 (0UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - GPIOF[4]

Definition at line 543 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_I2C0_SDA

#define SYS_PF_L_MFP_PF4_MFP_I2C0_SDA (1UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - I2C0 DATA

Definition at line 544 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_GPF5

#define SYS_PF_L_MFP_PF5_MFP_GPF5 (0UL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - GPIOF[5]

Definition at line 540 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_I2C0_SCL

#define SYS_PF_L_MFP_PF5_MFP_I2C0_SCL (1UL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - I2C0 clock

Definition at line 541 of file sys.h.

## ◆ SYS_VREFCTL_BGP_EN

#define SYS_VREFCTL_BGP_EN SYS_VREFCTL_BGP_EN_Msk

Band-gap Enable

Definition at line 65 of file sys.h.

## ◆ SYS_VREFCTL_EXTMODE

#define SYS_VREFCTL_EXTMODE SYS_VREFCTL_EXT_MODE_Msk

Regulator External Mode

Definition at line 68 of file sys.h.

## ◆ SYS_VREFCTL_REG_EN

#define SYS_VREFCTL_REG_EN SYS_VREFCTL_REG_EN_Msk

Regulator Enable

Definition at line 66 of file sys.h.

## ◆ SYS_VREFCTL_SEL25

#define SYS_VREFCTL_SEL25 SYS_VREFCTL_SEL25_Msk

Regulator Output Voltage 2.5V

Definition at line 67 of file sys.h.

## ◆ TMR0_RST

#define TMR0_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR0_RST_Pos )

Timer0 reset is one of the SYS_ResetModule parameter

Definition at line 57 of file sys.h.

## ◆ TMR1_RST

#define TMR1_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR1_RST_Pos )

Timer1 reset is one of the SYS_ResetModule parameter

Definition at line 56 of file sys.h.

## ◆ TMR2_RST

#define TMR2_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR2_RST_Pos )

Timer2 reset is one of the SYS_ResetModule parameter

Definition at line 55 of file sys.h.

## ◆ TMR3_RST

#define TMR3_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR3_RST_Pos )

Timer3 reset is one of the SYS_ResetModule parameter

Definition at line 54 of file sys.h.

## ◆ UART0_RST

#define UART0_RST ((0x4<<24) | SYS_IPRST_CTL2_UART0_RST_Pos )

UART0 reset is one of the SYS_ResetModule parameter

Definition at line 48 of file sys.h.

## ◆ UART1_RST

#define UART1_RST ((0x4<<24) | SYS_IPRST_CTL2_UART1_RST_Pos )

UART1 reset is one of the SYS_ResetModule parameter

Definition at line 47 of file sys.h.

## ◆ USBD_RST

#define USBD_RST ((0x4<<24) | SYS_IPRST_CTL2_USBD_RST_Pos )

USBD reset is one of the SYS_ResetModule parameter

Definition at line 43 of file sys.h.