| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Data Fields
CLK_T Struct Reference
NANO100 Definitions » Device CMSIS Definitions

`#include <Nano100Series.h>`

## Data Fields
__IO uint32_t | PWRCTL
__IO uint32_t | AHBCLK
__IO uint32_t | APBCLK
__I uint32_t | CLKSTATUS
__IO uint32_t | CLKSEL0
__IO uint32_t | CLKSEL1
__IO uint32_t | CLKSEL2
__IO uint32_t | CLKDIV0
__IO uint32_t | CLKDIV1
__IO uint32_t | PLLCTL
__IO uint32_t | FRQDIV
__IO uint32_t | MCLKO
__IO uint32_t | WK_INTSTS

## Detailed Description

    @addtogroup CLK System Clock Controller(CLK)
    Memory Mapped Structure for CLK Controller

Definition at line 714 of file Nano100Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano100Series/Include/Nano100Series.h