| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_Interrupt.c File Reference

NuEdu-Basic01_Interrupt.c interrupt driver source file for NuEdu-SDK-Nano130. More...

`#include <stdio.h>`
`#include "NUC200Series.h"`
`#include "NuEdu-Basic01_Interrupt.h"`
Include dependency graph for NuEdu-Basic01_Interrupt.c:

Go to the source code of this file.

## Functions
void | Initial_EINT1_GPIO (void)
| This function initializes PB.15 multi-function for EINT1 to detect external interrupt. More...
void | Open_EINT1 (void)
| This function enables EINT1 interrupt and IRQ handler, and configs trigger condition for falling edge. More...

## Detailed Description

NuEdu-Basic01_Interrupt.c interrupt driver source file for NuEdu-SDK-Nano130.

Version
  V1.00

Revision
  2

Date
  14/12/12 10:35a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_Interrupt.c.