| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Modules | Macros
NANO100 Peripheral Memory Map
Collaboration diagram for NANO100 Peripheral Memory Map:

## Modules
| NANO100 Peripheral Declaration

## Macros
#define | FLASH_BASE ((uint32_t)0x00000000)
| Flash base address. More...
#define | SRAM_BASE ((uint32_t)0x20000000)
| SRAM base address. More...
#define | APB1PERIPH_BASE ((uint32_t)0x40000000)
| APB1 base address. More...
#define | APB2PERIPH_BASE ((uint32_t)0x40100000)
| APB2 base address. More...
#define | AHBPERIPH_BASE ((uint32_t)0x50000000)
| AHB base address. More...
#define | WDT_BASE (APB1PERIPH_BASE + 0x04000)
| WDT register base address. More...
#define | WWDT_BASE (APB1PERIPH_BASE + 0x04100)
| WWDT register base address. More...
#define | RTC_BASE (APB1PERIPH_BASE + 0x08000)
| RTC register base address. More...
#define | TIMER0_BASE (APB1PERIPH_BASE + 0x10000)
| TIMER0 register base address. More...
#define | TIMER1_BASE (APB1PERIPH_BASE + 0x10100)
| TIMER1 register base address. More...
#define | I2C0_BASE (APB1PERIPH_BASE + 0x20000)
| I2C0 register base address. More...
#define | SPI0_BASE (APB1PERIPH_BASE + 0x30000)
| SPI0 register base address. More...
#define | PWM0_BASE (APB1PERIPH_BASE + 0x40000)
| PWM0 register base address. More...
#define | UART0_BASE (APB1PERIPH_BASE + 0x50000)
| UART0 register base address. More...
#define | DAC_BASE (APB1PERIPH_BASE + 0xA0000)
| DAC register base address. More...
#define | LCD_BASE (APB1PERIPH_BASE + 0xB0000)
| LCD register base address. More...
#define | SPI2_BASE (APB1PERIPH_BASE + 0xD0000)
| SPI2 register base address. More...
#define | ADC_BASE (APB1PERIPH_BASE + 0xE0000)
| ADC register base address. More...
#define | TIMER2_BASE (APB2PERIPH_BASE + 0x10000)
| TIMER2 register base address. More...
#define | TIMER3_BASE (APB2PERIPH_BASE + 0x10100)
| TIMER3 register base address. More...
#define | SHADOW_BASE (APB1PERIPH_BASE + 0x10200)
| GPIO shadow register base address. More...
#define | I2C1_BASE (APB2PERIPH_BASE + 0x20000)
| I2C1 register base address. More...
#define | SPI1_BASE (APB2PERIPH_BASE + 0x30000)
| SPI1 register base address. More...
#define | PWM1_BASE (APB2PERIPH_BASE + 0x40000)
| PWM1 register base address. More...
#define | UART1_BASE (APB2PERIPH_BASE + 0x50000)
| UART1 register base address. More...
#define | USBD_BASE (APB1PERIPH_BASE + 0x60000)
| USBD register base address. More...
#define | SC0_BASE (APB2PERIPH_BASE + 0x90000)
| SC0 register base address. More...
#define | I2S_BASE (APB2PERIPH_BASE + 0xA0000)
| I2S register base address. More...
#define | SC1_BASE (APB2PERIPH_BASE + 0xB0000)
| SC1 register base address. More...
#define | SC2_BASE (APB2PERIPH_BASE + 0xC0000)
| SC2 register base address. More...
#define | SYS_BASE (AHBPERIPH_BASE + 0x00000)
| SYS register base address. More...
#define | CLK_BASE (AHBPERIPH_BASE + 0x00200)
| CLK register base address. More...
#define | INT_BASE (AHBPERIPH_BASE + 0x00300)
| INT register base address. More...
#define | GPIOA_BASE (AHBPERIPH_BASE + 0x04000)
| GPIO port A register base address. More...
#define | GPIOB_BASE (AHBPERIPH_BASE + 0x04040)
| GPIO port B register base address. More...
#define | GPIOC_BASE (AHBPERIPH_BASE + 0x04080)
| GPIO port C register base address. More...
#define | GPIOD_BASE (AHBPERIPH_BASE + 0x040C0)
| GPIO port D register base address. More...
#define | GPIOE_BASE (AHBPERIPH_BASE + 0x04100)
| GPIO port E register base address. More...
#define | GPIOF_BASE (AHBPERIPH_BASE + 0x04140)
| GPIO port F register base address. More...
#define | GPIODBNCE_BASE (AHBPERIPH_BASE + 0x04180)
| GPIO debounce register base address. More...
#define | GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO bit access register base address. More...
#define | VDMA_BASE (AHBPERIPH_BASE + 0x08000)
| VDMA register base address. More...
#define | PDMA1_BASE (AHBPERIPH_BASE + 0x08100)
| PDMA1 register base address. More...
#define | PDMA2_BASE (AHBPERIPH_BASE + 0x08200)
| PDMA2 register base address. More...
#define | PDMA3_BASE (AHBPERIPH_BASE + 0x08300)
| PDMA3 register base address. More...
#define | PDMA4_BASE (AHBPERIPH_BASE + 0x08400)
| PDMA4 register base address. More...
#define | PDMA5_BASE (AHBPERIPH_BASE + 0x08500)
| PDMA5 register base address. More...
#define | PDMA6_BASE (AHBPERIPH_BASE + 0x08600)
| PDMA6 register base address. More...
#define | PDMACRC_BASE (AHBPERIPH_BASE + 0x08E00)
| PDMA global control register base address. More...
#define | PDMAGCR_BASE (AHBPERIPH_BASE + 0x08F00)
| PDMA CRC register base address. More...
#define | FMC_BASE (AHBPERIPH_BASE + 0x0C000)
| FMC register base address. More...
#define | EBI_BASE (AHBPERIPH_BASE + 0x10000)
| EBI register base address. More...

## Detailed Description

Memory Mapped Structure for NANO100 Series Peripheral

## Macro Definition Documentation

## ◆ ADC_BASE

#define ADC_BASE (APB1PERIPH_BASE + 0xE0000)

ADC register base address.

Definition at line 11621 of file Nano100Series.h.

## ◆ AHBPERIPH_BASE

#define AHBPERIPH_BASE ((uint32_t)0x50000000)

AHB base address.

Peripheral memory map

Definition at line 11607 of file Nano100Series.h.

## ◆ APB1PERIPH_BASE

#define APB1PERIPH_BASE ((uint32_t)0x40000000)

APB1 base address.

Definition at line 11603 of file Nano100Series.h.

## ◆ APB2PERIPH_BASE

#define APB2PERIPH_BASE ((uint32_t)0x40100000)

APB2 base address.

Definition at line 11604 of file Nano100Series.h.

## ◆ CLK_BASE

#define CLK_BASE (AHBPERIPH_BASE + 0x00200)

CLK register base address.

Definition at line 11637 of file Nano100Series.h.

## ◆ DAC_BASE

#define DAC_BASE (APB1PERIPH_BASE + 0xA0000)

DAC register base address.

Definition at line 11618 of file Nano100Series.h.

## ◆ EBI_BASE

#define EBI_BASE (AHBPERIPH_BASE + 0x10000)

EBI register base address.

Definition at line 11657 of file Nano100Series.h.

## ◆ FLASH_BASE

#define FLASH_BASE ((uint32_t)0x00000000)

Flash base address.

<Peripheral and SRAM base address

Definition at line 11601 of file Nano100Series.h.

## ◆ FMC_BASE

#define FMC_BASE (AHBPERIPH_BASE + 0x0C000)

FMC register base address.

Definition at line 11656 of file Nano100Series.h.

## ◆ GPIO_PIN_DATA_BASE

#define GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)

GPIO bit access register base address.

Definition at line 11646 of file Nano100Series.h.

## ◆ GPIOA_BASE

#define GPIOA_BASE (AHBPERIPH_BASE + 0x04000)

GPIO port A register base address.

Definition at line 11639 of file Nano100Series.h.

## ◆ GPIOB_BASE

#define GPIOB_BASE (AHBPERIPH_BASE + 0x04040)

GPIO port B register base address.

Definition at line 11640 of file Nano100Series.h.

## ◆ GPIOC_BASE

#define GPIOC_BASE (AHBPERIPH_BASE + 0x04080)

GPIO port C register base address.

Definition at line 11641 of file Nano100Series.h.

## ◆ GPIOD_BASE

#define GPIOD_BASE (AHBPERIPH_BASE + 0x040C0)

GPIO port D register base address.

Definition at line 11642 of file Nano100Series.h.

## ◆ GPIODBNCE_BASE

#define GPIODBNCE_BASE (AHBPERIPH_BASE + 0x04180)

GPIO debounce register base address.

Definition at line 11645 of file Nano100Series.h.

## ◆ GPIOE_BASE

#define GPIOE_BASE (AHBPERIPH_BASE + 0x04100)

GPIO port E register base address.

Definition at line 11643 of file Nano100Series.h.

## ◆ GPIOF_BASE

#define GPIOF_BASE (AHBPERIPH_BASE + 0x04140)

GPIO port F register base address.

Definition at line 11644 of file Nano100Series.h.

## ◆ I2C0_BASE

#define I2C0_BASE (APB1PERIPH_BASE + 0x20000)

I2C0 register base address.

Definition at line 11614 of file Nano100Series.h.

## ◆ I2C1_BASE

#define I2C1_BASE (APB2PERIPH_BASE + 0x20000)

I2C1 register base address.

Definition at line 11626 of file Nano100Series.h.

## ◆ I2S_BASE

#define I2S_BASE (APB2PERIPH_BASE + 0xA0000)

I2S register base address.

Definition at line 11632 of file Nano100Series.h.

## ◆ INT_BASE

#define INT_BASE (AHBPERIPH_BASE + 0x00300)

INT register base address.

Definition at line 11638 of file Nano100Series.h.

## ◆ LCD_BASE

#define LCD_BASE (APB1PERIPH_BASE + 0xB0000)

LCD register base address.

Definition at line 11619 of file Nano100Series.h.

## ◆ PDMA1_BASE

#define PDMA1_BASE (AHBPERIPH_BASE + 0x08100)

PDMA1 register base address.

Definition at line 11648 of file Nano100Series.h.

## ◆ PDMA2_BASE

#define PDMA2_BASE (AHBPERIPH_BASE + 0x08200)

PDMA2 register base address.

Definition at line 11649 of file Nano100Series.h.

## ◆ PDMA3_BASE

#define PDMA3_BASE (AHBPERIPH_BASE + 0x08300)

PDMA3 register base address.

Definition at line 11650 of file Nano100Series.h.

## ◆ PDMA4_BASE

#define PDMA4_BASE (AHBPERIPH_BASE + 0x08400)

PDMA4 register base address.

Definition at line 11651 of file Nano100Series.h.

## ◆ PDMA5_BASE

#define PDMA5_BASE (AHBPERIPH_BASE + 0x08500)

PDMA5 register base address.

Definition at line 11652 of file Nano100Series.h.

## ◆ PDMA6_BASE

#define PDMA6_BASE (AHBPERIPH_BASE + 0x08600)

PDMA6 register base address.

Definition at line 11653 of file Nano100Series.h.

## ◆ PDMACRC_BASE

#define PDMACRC_BASE (AHBPERIPH_BASE + 0x08E00)

PDMA global control register base address.

Definition at line 11654 of file Nano100Series.h.

## ◆ PDMAGCR_BASE

#define PDMAGCR_BASE (AHBPERIPH_BASE + 0x08F00)

PDMA CRC register base address.

Definition at line 11655 of file Nano100Series.h.

## ◆ PWM0_BASE

#define PWM0_BASE (APB1PERIPH_BASE + 0x40000)

PWM0 register base address.

Definition at line 11616 of file Nano100Series.h.

## ◆ PWM1_BASE

#define PWM1_BASE (APB2PERIPH_BASE + 0x40000)

PWM1 register base address.

Definition at line 11628 of file Nano100Series.h.

## ◆ RTC_BASE

#define RTC_BASE (APB1PERIPH_BASE + 0x08000)

RTC register base address.

Definition at line 11611 of file Nano100Series.h.

## ◆ SC0_BASE

#define SC0_BASE (APB2PERIPH_BASE + 0x90000)

SC0 register base address.

Definition at line 11631 of file Nano100Series.h.

## ◆ SC1_BASE

#define SC1_BASE (APB2PERIPH_BASE + 0xB0000)

SC1 register base address.

Definition at line 11633 of file Nano100Series.h.

## ◆ SC2_BASE

#define SC2_BASE (APB2PERIPH_BASE + 0xC0000)

SC2 register base address.

Definition at line 11634 of file Nano100Series.h.

## ◆ SHADOW_BASE

#define SHADOW_BASE (APB1PERIPH_BASE + 0x10200)

GPIO shadow register base address.

Definition at line 11625 of file Nano100Series.h.

## ◆ SPI0_BASE

#define SPI0_BASE (APB1PERIPH_BASE + 0x30000)

SPI0 register base address.

Definition at line 11615 of file Nano100Series.h.

## ◆ SPI1_BASE

#define SPI1_BASE (APB2PERIPH_BASE + 0x30000)

SPI1 register base address.

Definition at line 11627 of file Nano100Series.h.

## ◆ SPI2_BASE

#define SPI2_BASE (APB1PERIPH_BASE + 0xD0000)

SPI2 register base address.

Definition at line 11620 of file Nano100Series.h.

## ◆ SRAM_BASE

#define SRAM_BASE ((uint32_t)0x20000000)

SRAM base address.

Definition at line 11602 of file Nano100Series.h.

## ◆ SYS_BASE

#define SYS_BASE (AHBPERIPH_BASE + 0x00000)

SYS register base address.

Definition at line 11636 of file Nano100Series.h.

## ◆ TIMER0_BASE

#define TIMER0_BASE (APB1PERIPH_BASE + 0x10000)

TIMER0 register base address.

Definition at line 11612 of file Nano100Series.h.

## ◆ TIMER1_BASE

#define TIMER1_BASE (APB1PERIPH_BASE + 0x10100)

TIMER1 register base address.

Definition at line 11613 of file Nano100Series.h.

## ◆ TIMER2_BASE

#define TIMER2_BASE (APB2PERIPH_BASE + 0x10000)

TIMER2 register base address.

Definition at line 11623 of file Nano100Series.h.

## ◆ TIMER3_BASE

#define TIMER3_BASE (APB2PERIPH_BASE + 0x10100)

TIMER3 register base address.

Definition at line 11624 of file Nano100Series.h.

## ◆ UART0_BASE

#define UART0_BASE (APB1PERIPH_BASE + 0x50000)

UART0 register base address.

Definition at line 11617 of file Nano100Series.h.

## ◆ UART1_BASE

#define UART1_BASE (APB2PERIPH_BASE + 0x50000)

UART1 register base address.

Definition at line 11629 of file Nano100Series.h.

## ◆ USBD_BASE

#define USBD_BASE (APB1PERIPH_BASE + 0x60000)

USBD register base address.

Definition at line 11630 of file Nano100Series.h.

## ◆ VDMA_BASE

#define VDMA_BASE (AHBPERIPH_BASE + 0x08000)

VDMA register base address.

Definition at line 11647 of file Nano100Series.h.

## ◆ WDT_BASE

#define WDT_BASE (APB1PERIPH_BASE + 0x04000)

WDT register base address.

Definition at line 11609 of file Nano100Series.h.

## ◆ WWDT_BASE

#define WWDT_BASE (APB1PERIPH_BASE + 0x04100)

WWDT register base address.

Definition at line 11610 of file Nano100Series.h.