| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

sys.h
Go to the documentation of this file.
1/**************************************************************************/
12#ifndef __SYS_H__
13#define __SYS_H__
14
15#ifdef __cplusplus
16 extern "C"
17{
18#endif
19
32/*---------------------------------------------------------------------------------------------------------*/
33/* Module Reset Control Resister constant definitions. */
34/*---------------------------------------------------------------------------------------------------------*/
35#define CHIP_RST ((0x0<<24) | SYS_IPRST_CTL1_CHIP_RST_Pos )
36#define CPU_RST ((0x0<<24) | SYS_IPRST_CTL1_CPU_RST_Pos )
37#define DMA_RST ((0x0<<24) | SYS_IPRST_CTL1_DMA_RST_Pos )
38#define EBI_RST ((0x0<<24) | SYS_IPRST_CTL1_EBI_RST_Pos )
39#define SC1_RST ((0x4<<24) | SYS_IPRST_CTL2_SC1_RST_Pos )
40#define SC0_RST ((0x4<<24) | SYS_IPRST_CTL2_SC0_RST_Pos )
41#define I2S_RST ((0x4<<24) | SYS_IPRST_CTL2_I2S_RST_Pos )
42#define ADC_RST ((0x4<<24) | SYS_IPRST_CTL2_ADC_RST_Pos )
43#define USBD_RST ((0x4<<24) | SYS_IPRST_CTL2_USBD_RST_Pos )
44#define DAC_RST ((0x4<<24) | SYS_IPRST_CTL2_DAC_RST_Pos )
45#define PWM1_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM1_RST_Pos )
46#define PWM0_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM0_RST_Pos )
47#define UART1_RST ((0x4<<24) | SYS_IPRST_CTL2_UART1_RST_Pos )
48#define UART0_RST ((0x4<<24) | SYS_IPRST_CTL2_UART0_RST_Pos )
49#define SPI2_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI2_RST_Pos )
50#define SPI1_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI1_RST_Pos )
51#define SPI0_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI0_RST_Pos )
52#define I2C1_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C1_RST_Pos )
53#define I2C0_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C0_RST_Pos )
54#define TMR3_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR3_RST_Pos )
55#define TMR2_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR2_RST_Pos )
56#define TMR1_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR1_RST_Pos )
57#define TMR0_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR0_RST_Pos )
58#define GPIO_RST ((0x4<<24) | SYS_IPRST_CTL2_GPIO_RST_Pos )
60/*---------------------------------------------------------------------------------------------------------*/
61/* Multi-Function constant definitions. */
62/*---------------------------------------------------------------------------------------------------------*/
63
64/********************* Bit definition of VREFCTL register **********************/
65#define SYS_VREFCTL_BGP_EN SYS_VREFCTL_BGP_EN_Msk
66#define SYS_VREFCTL_REG_EN SYS_VREFCTL_REG_EN_Msk
67#define SYS_VREFCTL_SEL25 SYS_VREFCTL_SEL25_Msk
68#define SYS_VREFCTL_EXTMODE SYS_VREFCTL_EXT_MODE_Msk
70/********************* Bit definition of IRCTRIMCTL register **********************/
71#define SYS_IRCTRIMCTL_TRIM_11_0592M (0x1UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)
72#define SYS_IRCTRIMCTL_TRIM_12M (0x2UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)
73#define SYS_IRCTRIMCTL_TRIM_12_288M (0x3UL<<SYS_IRCTRIMCTL_TRIM_SEL_Pos)
75#define SYS_IRCTRIMCTL_LOOP_4CLK (0x0UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
76#define SYS_IRCTRIMCTL_LOOP_8CLK (0x1UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
77#define SYS_IRCTRIMCTL_LOOP_16CLK (0x2UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
78#define SYS_IRCTRIMCTL_LOOP_32CLK (0x3UL<<SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
80#define SYS_IRCTRIMCTL_RETRY_64 (0x0UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
81#define SYS_IRCTRIMCTL_RETRY_128 (0x1UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
82#define SYS_IRCTRIMCTL_RETRY_256 (0x2UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
83#define SYS_IRCTRIMCTL_RETRY_512 (0x3UL<<SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
85/********************* Bit definition of IRCTRIMIEN register **********************/
86#define SYS_IRCTRIMIEN_DISABLE ((uint32_t)0x00000000)
87#define SYS_IRCTRIMIEN_FAIL_EN SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk
88#define SYS_IRCTRIMIEN_32KERR_EN SYS_IRCTRIMIEN_32K_ERR_IEN_Msk
90/********************* Bit definition of IRCTRIMINT register **********************/
91#define SYS_IRCTRIMINT_FREQLOCK SYS_IRCTRIMINT_FREQ_LOCK_Msk
92#define SYS_IRCTRIMINT_FAIL_INT SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk
93#define SYS_IRCTRIMINT_32KERR_INT SYS_IRCTRIMINT_32K_ERR_INT_Msk
95/********************* Bit definition of PA_L_MFP register **********************/
96
97#define SYS_PA_L_MFP_PA7_MFP_GPA7 (0UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
98#define SYS_PA_L_MFP_PA7_MFP_ADC_CH7 (1UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
99#define SYS_PA_L_MFP_PA7_MFP_EBI_AD6 (2UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
100#define SYS_PA_L_MFP_PA7_MFP_TMR2_CAP (3UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
101#define SYS_PA_L_MFP_PA7_MFP_SC2_DAT (4UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
102#define SYS_PA_L_MFP_PA7_MFP_PWM0_CH2 (5UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
103#define SYS_PA_L_MFP_PA7_MFP_LCD_S36 (7UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
105#define SYS_PA_L_MFP_PA6_MFP_GPA6 (0UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
106#define SYS_PA_L_MFP_PA6_MFP_ADC_CH6 (1UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
107#define SYS_PA_L_MFP_PA6_MFP_EBI_AD7 (2UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
108#define SYS_PA_L_MFP_PA6_MFP_TMR3_CAP (3UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
109#define SYS_PA_L_MFP_PA6_MFP_SC2_CLK (4UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
110#define SYS_PA_L_MFP_PA6_MFP_PWM0_CH3 (5UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
111#define SYS_PA_L_MFP_PA6_MFP_LCD_S37 (7UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
112#define SYS_PA_L_MFP_PA6_MFP_LCD_S19 (7UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
114#define SYS_PA_L_MFP_PA5_MFP_GPA5 (0UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
115#define SYS_PA_L_MFP_PA5_MFP_ADC_CH5 (1UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
116#define SYS_PA_L_MFP_PA5_MFP_EBI_AD8 (2UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
117#define SYS_PA_L_MFP_PA5_MFP_SC2_RST (4UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
118#define SYS_PA_L_MFP_PA5_MFP_I2C0_SCL (5UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
119#define SYS_PA_L_MFP_PA5_MFP_LCD_S38 (7UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
120#define SYS_PA_L_MFP_PA5_MFP_LCD_S20 (7UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
122#define SYS_PA_L_MFP_PA4_MFP_GPA4 (0UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
123#define SYS_PA_L_MFP_PA4_MFP_ADC_CH4 (1UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
124#define SYS_PA_L_MFP_PA4_MFP_EBI_AD9 (2UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
125#define SYS_PA_L_MFP_PA4_MFP_SC2_PWR (4UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
126#define SYS_PA_L_MFP_PA4_MFP_I2C0_SDA (5UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
127#define SYS_PA_L_MFP_PA4_MFP_LCD_S39 (7UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
128#define SYS_PA_L_MFP_PA4_MFP_LCD_S21 (7UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
130#define SYS_PA_L_MFP_PA3_MFP_GPA3 (0UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
131#define SYS_PA_L_MFP_PA3_MFP_ADC_CH3 (1UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
132#define SYS_PA_L_MFP_PA3_MFP_EBI_AD10 (2UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
133#define SYS_PA_L_MFP_PA3_MFP_UART1_TX (5UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
134#define SYS_PA_L_MFP_PA3_MFP_LCD_S22 (7UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
136#define SYS_PA_L_MFP_PA2_MFP_GPA2 (0UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
137#define SYS_PA_L_MFP_PA2_MFP_ADC_CH2 (1UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
138#define SYS_PA_L_MFP_PA2_MFP_EBI_AD11 (2UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
139#define SYS_PA_L_MFP_PA2_MFP_UART1_RX (5UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
140#define SYS_PA_L_MFP_PA2_MFP_LCD_S23 (7UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
142#define SYS_PA_L_MFP_PA1_MFP_GPA1 (0UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
143#define SYS_PA_L_MFP_PA1_MFP_ADC_CH1 (1UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
144#define SYS_PA_L_MFP_PA1_MFP_EBI_AD12 (2UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
146#define SYS_PA_L_MFP_PA0_MFP_GPA0 (0UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
147#define SYS_PA_L_MFP_PA0_MFP_ADC_CH0 (1UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
148#define SYS_PA_L_MFP_PA0_MFP_SC2_CD (4UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
150/********************* Bit definition of PA_H_MFP register **********************/
151#define SYS_PA_H_MFP_PA15_MFP_GPA15 (0UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
152#define SYS_PA_H_MFP_PA15_MFP_PWM0_CH3 (1UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
153#define SYS_PA_H_MFP_PA15_MFP_I2S_MCLK (2UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
154#define SYS_PA_H_MFP_PA15_MFP_TMR3_CAP (3UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
155#define SYS_PA_H_MFP_PA15_MFP_SC0_PWR (4UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
156#define SYS_PA_H_MFP_PA15_MFP_UART0_TX (6UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
157#define SYS_PA_H_MFP_PA15_MFP_LCD_S27 (7UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
159#define SYS_PA_H_MFP_PA14_MFP_GPA14 (0UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
160#define SYS_PA_H_MFP_PA14_MFP_PWM0_CH2 (1UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
161#define SYS_PA_H_MFP_PA14_MFP_EBI_AD15 (2UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
162#define SYS_PA_H_MFP_PA14_MFP_TMR2_CAP (3UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
163#define SYS_PA_H_MFP_PA14_MFP_UART0_RX (6UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
164#define SYS_PA_H_MFP_PA14_MFP_LCD_S26 (7UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
166#define SYS_PA_H_MFP_PA13_MFP_GPA13 (0UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
167#define SYS_PA_H_MFP_PA13_MFP_PWM0_CH1 (1UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
168#define SYS_PA_H_MFP_PA13_MFP_EBI_AD14 (2UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
169#define SYS_PA_H_MFP_PA13_MFP_TMR1_CAP (3UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
170#define SYS_PA_H_MFP_PA13_MFP_I2C0_SCL (5UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
171#define SYS_PA_H_MFP_PA13_MFP_LCD_S25 (7UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
173#define SYS_PA_H_MFP_PA12_MFP_GPA12 (0UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
174#define SYS_PA_H_MFP_PA12_MFP_PWM0_CH0 (1UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
175#define SYS_PA_H_MFP_PA12_MFP_EBI_AD13 (2UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
176#define SYS_PA_H_MFP_PA12_MFP_TMR0_CAP (3UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
177#define SYS_PA_H_MFP_PA12_MFP_I2C0_SDA (5UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
178#define SYS_PA_H_MFP_PA12_MFP_LCD_S24 (7UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
180#define SYS_PA_H_MFP_PA11_MFP_GPA11 (0UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
181#define SYS_PA_H_MFP_PA11_MFP_I2C1_SCL (1UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
182#define SYS_PA_H_MFP_PA11_MFP_EBI_NRE (2UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
183#define SYS_PA_H_MFP_PA11_MFP_SC0_RST (3UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
184#define SYS_PA_H_MFP_PA11_MFP_SPI2_MOSI0 (4UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
185#define SYS_PA_H_MFP_PA11_MFP_LCD_S23 (7UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
186#define SYS_PA_H_MFP_PA11_MFP_LCD_S9 (7UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
188#define SYS_PA_H_MFP_PA10_MFP_GPA10 (0UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
189#define SYS_PA_H_MFP_PA10_MFP_I2C1_SDA (1UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
190#define SYS_PA_H_MFP_PA10_MFP_EBI_NWE (2UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
191#define SYS_PA_H_MFP_PA10_MFP_SC0_PWR (3UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
192#define SYS_PA_H_MFP_PA10_MFP_SPI2_MISO0 (4UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
193#define SYS_PA_H_MFP_PA10_MFP_LCD_S22 (7UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
194#define SYS_PA_H_MFP_PA10_MFP_LCD_S8 (7UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
196#define SYS_PA_H_MFP_PA9_MFP_GPA9 (0UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
197#define SYS_PA_H_MFP_PA9_MFP_I2C0_SCL (1UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
198#define SYS_PA_H_MFP_PA9_MFP_SC0_DAT (3UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
199#define SYS_PA_H_MFP_PA9_MFP_SPI2_SCLK (4UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
200#define SYS_PA_H_MFP_PA9_MFP_LCD_S21 (7UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
201#define SYS_PA_H_MFP_PA9_MFP_LCD_S7 (7UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
203#define SYS_PA_H_MFP_PA8_MFP_GPA8 (0UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
204#define SYS_PA_H_MFP_PA8_MFP_I2C0_SDA (1UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
205#define SYS_PA_H_MFP_PA8_MFP_SC0_CLK (3UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
206#define SYS_PA_H_MFP_PA8_MFP_SPI2_SS0 (4UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
207#define SYS_PA_H_MFP_PA8_MFP_LCD_S20 (7UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
208#define SYS_PA_H_MFP_PA8_MFP_LCD_S6 (7UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
210/********************* Bit definition of PB_L_MFP register **********************/
211#define SYS_PB_L_MFP_PB7_MFP_GPB7 (0UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
212#define SYS_PB_L_MFP_PB7_MFP_UART1_CTS (1UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
213#define SYS_PB_L_MFP_PB7_MFP_EBI_NCS (2UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
214#define SYS_PB_L_MFP_PB7_MFP_SPI2_MOSI0 (4UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
215#define SYS_PB_L_MFP_PB7_MFP_LCD_S10 (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
216#define SYS_PB_L_MFP_PB7_MFP_LCD_S2 (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
218#define SYS_PB_L_MFP_PB6_MFP_GPB6 (0UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
219#define SYS_PB_L_MFP_PB6_MFP_UART1_RTS (1UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
220#define SYS_PB_L_MFP_PB6_MFP_EBI_ALE (2UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
221#define SYS_PB_L_MFP_PB6_MFP_SPI2_MISO0 (4UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
222#define SYS_PB_L_MFP_PB6_MFP_LCD_S11 (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
223#define SYS_PB_L_MFP_PB6_MFP_LCD_S3 (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
225#define SYS_PB_L_MFP_PB5_MFP_GPB5 (0UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
226#define SYS_PB_L_MFP_PB5_MFP_UART1_TX (1UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
227#define SYS_PB_L_MFP_PB5_MFP_SC0_RST (3UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
228#define SYS_PB_L_MFP_PB5_MFP_SPI2_SCLK (4UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
229#define SYS_PB_L_MFP_PB5_MFP_LCD_S12 (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
230#define SYS_PB_L_MFP_PB5_MFP_LCD_S4 (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
232#define SYS_PB_L_MFP_PB4_MFP_GPB4 (0UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
233#define SYS_PB_L_MFP_PB4_MFP_UART1_RX (1UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
234#define SYS_PB_L_MFP_PB4_MFP_SC0_CD (3UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
235#define SYS_PB_L_MFP_PB4_MFP_SPI2_SS0 (4UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
236#define SYS_PB_L_MFP_PB4_MFP_LCD_S13 (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
237#define SYS_PB_L_MFP_PB4_MFP_LCD_S5 (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
239#define SYS_PB_L_MFP_PB3_MFP_GPB3 (0UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
240#define SYS_PB_L_MFP_PB3_MFP_UART0_CTS (1UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
241#define SYS_PB_L_MFP_PB3_MFP_EBI_NWRH (2UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
242#define SYS_PB_L_MFP_PB3_MFP_SPI1_SS0 (3UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
243#define SYS_PB_L_MFP_PB3_MFP_LCD_S4 (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
244#define SYS_PB_L_MFP_PB3_MFP_LCD_COM2 (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
246#define SYS_PB_L_MFP_PB2_MFP_GPB2 (0UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
247#define SYS_PB_L_MFP_PB2_MFP_UART0_RTS (1UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
248#define SYS_PB_L_MFP_PB2_MFP_EBI_NWRL (2UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
249#define SYS_PB_L_MFP_PB2_MFP_SPI1_SCLK (3UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
250#define SYS_PB_L_MFP_PB2_MFP_LCD_S5 (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
251#define SYS_PB_L_MFP_PB2_MFP_LCD_COM3 (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
253#define SYS_PB_L_MFP_PB1_MFP_GPB1 (0UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
254#define SYS_PB_L_MFP_PB1_MFP_UART0_TX (1UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
255#define SYS_PB_L_MFP_PB1_MFP_SPI1_MISO0 (3UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
256#define SYS_PB_L_MFP_PB1_MFP_LCD_S6 (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
257#define SYS_PB_L_MFP_PB1_MFP_LCD_S0 (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
259#define SYS_PB_L_MFP_PB0_MFP_GPB0 (0UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
260#define SYS_PB_L_MFP_PB0_MFP_UART0_RX (1UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
261#define SYS_PB_L_MFP_PB0_MFP_SPI1_MOSI0 (3UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
262#define SYS_PB_L_MFP_PB0_MFP_LCD_S7 (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
263#define SYS_PB_L_MFP_PB0_MFP_LCD_S1 (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
265/********************* Bit definition of PB_H_MFP register **********************/
266#define SYS_PB_H_MFP_PB15_MFP_GPB15 (0UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
267#define SYS_PB_H_MFP_PB15_MFP_EXT_INT1 (1UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
268#define SYS_PB_H_MFP_PB15_MFP_SNOOPER (3UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
269#define SYS_PB_H_MFP_PB15_MFP_SC1_CD (4UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
270#define SYS_PB_H_MFP_PB15_MFP_LCD_S31 (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
271#define SYS_PB_H_MFP_PB15_MFP_LCD_S14 (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
273#define SYS_PB_H_MFP_PB14_MFP_GPB14 (0UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
274#define SYS_PB_H_MFP_PB14_MFP_EXT_INT0 (1UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
275#define SYS_PB_H_MFP_PB14_MFP_SC2_CD (3UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
276#define SYS_PB_H_MFP_PB14_MFP_SPI2_SS1 (4UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
277#define SYS_PB_H_MFP_PB14_MFP_LCD_S26 (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
278#define SYS_PB_H_MFP_PB14_MFP_LCD_S12 (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
280#define SYS_PB_H_MFP_PB13_MFP_GPB13 (0UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
281#define SYS_PB_H_MFP_PB13_MFP_EBI_AD1 (2UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
282#define SYS_PB_H_MFP_PB13_MFP_LCD_S25 (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
283#define SYS_PB_H_MFP_PB13_MFP_LCD_S11 (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
285#define SYS_PB_H_MFP_PB12_MFP_GPB12 (0UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
286#define SYS_PB_H_MFP_PB12_MFP_EBI_AD0 (2UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
287#define SYS_PB_H_MFP_PB12_MFP_CKO (4UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
288#define SYS_PB_H_MFP_PB12_MFP_LCD_S24 (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
289#define SYS_PB_H_MFP_PB12_MFP_LCD_S10 (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
291#define SYS_PB_H_MFP_PB11_MFP_GPB11 (0UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
292#define SYS_PB_H_MFP_PB11_MFP_PWM1_CH0 (1UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
293#define SYS_PB_H_MFP_PB11_MFP_TMR3_EXT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
294#define SYS_PB_H_MFP_PB11_MFP_TMR3_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
295#define SYS_PB_H_MFP_PB11_MFP_SC2_DAT (4UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
296#define SYS_PB_H_MFP_PB11_MFP_SPI0_MISO0 (5UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
297#define SYS_PB_H_MFP_PB11_MFP_LCD_V1 (7UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
299#define SYS_PB_H_MFP_PB10_MFP_GPB10 (0UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
300#define SYS_PB_H_MFP_PB10_MFP_SPI0_SS1 (1UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
301#define SYS_PB_H_MFP_PB10_MFP_TMR2_EXT (2UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
302#define SYS_PB_H_MFP_PB10_MFP_TMR2_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
303#define SYS_PB_H_MFP_PB10_MFP_SC2_CLK (4UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
304#define SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI0 (5UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
305#define SYS_PB_H_MFP_PB10_MFP_LCD_V2 (7UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
307#define SYS_PB_H_MFP_PB9_MFP_GPB9 (0UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
308#define SYS_PB_H_MFP_PB9_MFP_SPI1_SS1 (1UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
309#define SYS_PB_H_MFP_PB9_MFP_TMR1_EXT (2UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
310#define SYS_PB_H_MFP_PB9_MFP_TMR1_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
311#define SYS_PB_H_MFP_PB9_MFP_SC2_RST (4UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
312#define SYS_PB_H_MFP_PB9_MFP_EXT_INT0 (5UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
313#define SYS_PB_H_MFP_PB9_MFP_LCD_V3 (7UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
315#define SYS_PB_H_MFP_PB8_MFP_GPB8 (0UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
316#define SYS_PB_H_MFP_PB8_MFP_ADC_EXT (1UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
317#define SYS_PB_H_MFP_PB8_MFP_TMR0_EXT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
318#define SYS_PB_H_MFP_PB8_MFP_TMR0_TOGGLE_OUT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
319#define SYS_PB_H_MFP_PB8_MFP_EXT_INT0 (3UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
320#define SYS_PB_H_MFP_PB8_MFP_SC2_PWR (4UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
321#define SYS_PB_H_MFP_PB8_MFP_LCD_S30 (7UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
322#define SYS_PB_H_MFP_PB8_MFP_LCD_S13 (7UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
324/********************* Bit definition of PC_L_MFP register **********************/
325#define SYS_PC_L_MFP_PC7_MFP_GPC7 (0UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
326#define SYS_PC_L_MFP_PC7_MFP_DA_OUT1 (1UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
327#define SYS_PC_L_MFP_PC7_MFP_EBI_AD5 (2UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
328#define SYS_PC_L_MFP_PC7_MFP_TMR1_CAP (3UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
329#define SYS_PC_L_MFP_PC7_MFP_PWM0_CH1 (5UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
330#define SYS_PC_L_MFP_PC7_MFP_LCD_S17 (7UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
332#define SYS_PC_L_MFP_PC6_MFP_GPC6 (0UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
333#define SYS_PC_L_MFP_PC6_MFP_DA_OUT0 (1UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
334#define SYS_PC_L_MFP_PC6_MFP_EBI_AD4 (2UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
335#define SYS_PC_L_MFP_PC6_MFP_TMR0_CAP (3UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
336#define SYS_PC_L_MFP_PC6_MFP_SC1_CD (4UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
337#define SYS_PC_L_MFP_PC6_MFP_PWM0_CH0 (5UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
339#define SYS_PC_L_MFP_PC5_MFP_GPC5 (0UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
340#define SYS_PC_L_MFP_PC5_MFP_SPI0_MOSI1 (1UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
341#define SYS_PC_L_MFP_PC5_MFP_LCD_COM3 (7UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
343#define SYS_PC_L_MFP_PC4_MFP_GPC4 (0UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
344#define SYS_PC_L_MFP_PC4_MFP_SPI0_MISO1 (1UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
345#define SYS_PC_L_MFP_PC4_MFP_LCD_COM2 (7UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
347#define SYS_PC_L_MFP_PC3_MFP_GPC3 (0UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
348#define SYS_PC_L_MFP_PC3_MFP_SPI0_MOSI0 (1UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
349#define SYS_PC_L_MFP_PC3_MFP_I2S_DOUT (2UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
350#define SYS_PC_L_MFP_PC3_MFP_SC1_RST (4UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
351#define SYS_PC_L_MFP_PC3_MFP_LCD_COM1 (7UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
353#define SYS_PC_L_MFP_PC2_MFP_GPC2 (0UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
354#define SYS_PC_L_MFP_PC2_MFP_SPI0_MISO0 (1UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
355#define SYS_PC_L_MFP_PC2_MFP_I2S_DIN (2UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
356#define SYS_PC_L_MFP_PC2_MFP_SC1_PWR (4UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
357#define SYS_PC_L_MFP_PC2_MFP_LCD_COM0 (7UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
359#define SYS_PC_L_MFP_PC1_MFP_GPC1 (0UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
360#define SYS_PC_L_MFP_PC1_MFP_SPI0_SCLK (1UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
361#define SYS_PC_L_MFP_PC1_MFP_I2S_BCLK (2UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
362#define SYS_PC_L_MFP_PC1_MFP_SC1_DAT (4UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
363#define SYS_PC_L_MFP_PC1_MFP_LCD_DH2 (7UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
365#define SYS_PC_L_MFP_PC0_MFP_GPC0 (0UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
366#define SYS_PC_L_MFP_PC0_MFP_SPI0_SS0 (1UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
367#define SYS_PC_L_MFP_PC0_MFP_I2S_WS (2UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
368#define SYS_PC_L_MFP_PC0_MFP_SC1_CLK (4UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
369#define SYS_PC_L_MFP_PC0_MFP_LCD_DH1 (7UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
371/********************* Bit definition of PC_H_MFP register **********************/
372#define SYS_PC_H_MFP_PC15_MFP_GPC15 (0UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
373#define SYS_PC_H_MFP_PC15_MFP_EBI_AD3 (2UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
374#define SYS_PC_H_MFP_PC15_MFP_TMR0_CAP (3UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
375#define SYS_PC_H_MFP_PC15_MFP_PWM1_CH2 (4UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
376#define SYS_PC_H_MFP_PC15_MFP_LCD_S33 (7UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
377#define SYS_PC_H_MFP_PC15_MFP_LCD_S16 (7UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
379#define SYS_PC_H_MFP_PC14_MFP_GPC14 (0UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
380#define SYS_PC_H_MFP_PC14_MFP_EBI_AD2 (2UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
381#define SYS_PC_H_MFP_PC14_MFP_PWM1_CH3 (4UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
382#define SYS_PC_H_MFP_PC14_MFP_LCD_S32 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
383#define SYS_PC_H_MFP_PC14_MFP_LCD_S15 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
385#define SYS_PC_H_MFP_PC13_MFP_GPC13 (0UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
386#define SYS_PC_H_MFP_PC13_MFP_SPI1_MOSI1 (1UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
387#define SYS_PC_H_MFP_PC13_MFP_PWM1_CH1 (2UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
388#define SYS_PC_H_MFP_PC13_MFP_SNOOPER (4UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
389#define SYS_PC_H_MFP_PC13_MFP_EXT_INT1 (5UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
390#define SYS_PC_H_MFP_PC13_MFP_I2C0_SCL (6UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
392#define SYS_PC_H_MFP_PC12_MFP_GPC12 (0UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
393#define SYS_PC_H_MFP_PC12_MFP_SPI1_MISO1 (1UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
394#define SYS_PC_H_MFP_PC12_MFP_PWM1_CH0 (2UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
395#define SYS_PC_H_MFP_PC12_MFP_EXT_INT0 (5UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
396#define SYS_PC_H_MFP_PC12_MFP_I2C0_SDA (6UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
398#define SYS_PC_H_MFP_PC11_MFP_GPC11 (0UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
399#define SYS_PC_H_MFP_PC11_MFP_SPI1_MOSI0 (1UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
400#define SYS_PC_H_MFP_PC11_MFP_UART1_TX (5UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
401#define SYS_PC_H_MFP_PC11_MFP_LCD_S31 (7UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
403#define SYS_PC_H_MFP_PC10_MFP_GPC10 (0UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
404#define SYS_PC_H_MFP_PC10_MFP_SPI1_MISO0 (1UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
405#define SYS_PC_H_MFP_PC10_MFP_UART1_RX (5UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
406#define SYS_PC_H_MFP_PC10_MFP_LCD_S30 (7UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
408#define SYS_PC_H_MFP_PC9_MFP_GPC9 (0UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
409#define SYS_PC_H_MFP_PC9_MFP_SPI1_SCLK (1UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
410#define SYS_PC_H_MFP_PC9_MFP_I2C1_SCL (5UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
411#define SYS_PC_H_MFP_PC9_MFP_LCD_S29 (7UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
413#define SYS_PC_H_MFP_PC8_MFP_GPC8 (0UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
414#define SYS_PC_H_MFP_PC8_MFP_SPI1_SS0 (1UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
415#define SYS_PC_H_MFP_PC8_MFP_EBI_XCLK (2UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
416#define SYS_PC_H_MFP_PC8_MFP_I2C1_SDA (5UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
417#define SYS_PC_H_MFP_PC8_MFP_LCD_S28 (7UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
419/********************* Bit definition of PD_L_MFP register **********************/
420#define SYS_PD_L_MFP_PD7_MFP_GPD7 (0UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
421#define SYS_PD_L_MFP_PD7_MFP_LCD_S2 (7UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
423#define SYS_PD_L_MFP_PD6_MFP_GPD6 (0UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
424#define SYS_PD_L_MFP_PD6_MFP_LCD_S3 (7UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
426#define SYS_PD_L_MFP_PD5_MFP_GPD5 (0UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
427#define SYS_PD_L_MFP_PD5_MFP_I2S_DOUT (2UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
428#define SYS_PD_L_MFP_PD5_MFP_SPI2_MOSI1 (3UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
429#define SYS_PD_L_MFP_PD5_MFP_LCD_S34 (7UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
431#define SYS_PD_L_MFP_PD4_MFP_GPD4 (0UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
432#define SYS_PD_L_MFP_PD4_MFP_I2S_DIN (2UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
433#define SYS_PD_L_MFP_PD4_MFP_SPI2_MISO1 (3UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
434#define SYS_PD_L_MFP_PD4_MFP_SC1_CD (4UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
435#define SYS_PD_L_MFP_PD4_MFP_LCD_S35 (7UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
437#define SYS_PD_L_MFP_PD3_MFP_GPD3 (0UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
438#define SYS_PD_L_MFP_PD3_MFP_UART1_CTS (1UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
439#define SYS_PD_L_MFP_PD3_MFP_I2S_BCLK (2UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
440#define SYS_PD_L_MFP_PD3_MFP_SPI2_MOSI0 (3UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
441#define SYS_PD_L_MFP_PD3_MFP_SC1_RST (4UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
442#define SYS_PD_L_MFP_PD3_MFP_ADC_CH11 (5UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
444#define SYS_PD_L_MFP_PD2_MFP_GPD2 (0UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
445#define SYS_PD_L_MFP_PD2_MFP_UART1_RTS (1UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
446#define SYS_PD_L_MFP_PD2_MFP_I2S_WS (2UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
447#define SYS_PD_L_MFP_PD2_MFP_SPI2_MISO0 (3UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
448#define SYS_PD_L_MFP_PD2_MFP_SC1_PWR (4UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
449#define SYS_PD_L_MFP_PD2_MFP_ADC_CH10 (5UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
451#define SYS_PD_L_MFP_PD1_MFP_GPD1 (0UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
452#define SYS_PD_L_MFP_PD1_MFP_UART1_TX (1UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
453#define SYS_PD_L_MFP_PD1_MFP_SPI2_SCLK (3UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
454#define SYS_PD_L_MFP_PD1_MFP_SC1_DAT (4UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
455#define SYS_PD_L_MFP_PD1_MFP_ADC_CH9 (5UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
457#define SYS_PD_L_MFP_PD0_MFP_GPD0 (0UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
458#define SYS_PD_L_MFP_PD0_MFP_UART1_RX (1UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
459#define SYS_PD_L_MFP_PD0_MFP_SPI2_SS0 (3UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
460#define SYS_PD_L_MFP_PD0_MFP_SC1_CLK (4UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
461#define SYS_PD_L_MFP_PD0_MFP_ADC_CH8 (5UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
463/********************* Bit definition of PD_H_MFP register **********************/
464#define SYS_PD_H_MFP_PD15_MFP_GPD15 (0UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
465#define SYS_PD_H_MFP_PD15_MFP_LCD_S0 (7UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
467#define SYS_PD_H_MFP_PD14_MFP_GPD14 (0UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
468#define SYS_PD_H_MFP_PD14_MFP_LCD_S1 (7UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
470#define SYS_PD_H_MFP_PD13_MFP_GPD13 (0UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
471#define SYS_PD_H_MFP_PD13_MFP_LCD_S14 (7UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
473#define SYS_PD_H_MFP_PD12_MFP_GPD12 (0UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
474#define SYS_PD_H_MFP_PD12_MFP_LCD_S15 (7UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
476#define SYS_PD_H_MFP_PD11_MFP_GPD11 (0UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
477#define SYS_PD_H_MFP_PD11_MFP_LCD_S16 (7uL<<SYS_PD_H_MFP_PD11_MFP_Pos)
479#define SYS_PD_H_MFP_PD10_MFP_GPD10 (0UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
480#define SYS_PD_H_MFP_PD10_MFP_LCD_S17 (7UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
482#define SYS_PD_H_MFP_PD9_MFP_GPD9 (0UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
483#define SYS_PD_H_MFP_PD9_MFP_LCD_S18 (7UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
485#define SYS_PD_H_MFP_PD8_MFP_GPD8 (0UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
486#define SYS_PD_H_MFP_PD8_MFP_LCD_S19 (7UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
488/********************* Bit definition of PE_L_MFP register **********************/
489#define SYS_PE_L_MFP_PE7_MFP_GPE7 (0UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
490#define SYS_PE_L_MFP_PE7_MFP_LCD_S8 (7UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
492#define SYS_PE_L_MFP_PE6_MFP_GPE6 (0UL<<SYS_PE_L_MFP_PE6_MFP_Pos)
494#define SYS_PE_L_MFP_PE5_MFP_GPE5 (0UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
495#define SYS_PE_L_MFP_PE5_MFP_PWM1_CH1 (1UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
497#define SYS_PE_L_MFP_PE4_MFP_GPE4 (0UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
498#define SYS_PE_L_MFP_PE4_MFP_SPI0_MOSI0 (6UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
500#define SYS_PE_L_MFP_PE3_MFP_GPE3 (0UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
501#define SYS_PE_L_MFP_PE3_MFP_SPI0_MISO0 (6UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
503#define SYS_PE_L_MFP_PE2_MFP_GPE2 (0UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
504#define SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK (6UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
506#define SYS_PE_L_MFP_PE1_MFP_GPE1 (0UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
507#define SYS_PE_L_MFP_PE1_MFP_PWM1_CH3 (1UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
508#define SYS_PE_L_MFP_PE1_MFP_SPI0_SS0 (6UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
510#define SYS_PE_L_MFP_PE0_MFP_GPE0 (0UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
511#define SYS_PE_L_MFP_PE0_MFP_PWM1_CH2 (1UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
512#define SYS_PE_L_MFP_PE0_MFP_I2S_MCLK (2UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
514/********************* Bit definition of PE_H_MFP register **********************/
515#define SYS_PE_H_MFP_PE15_MFP_GPE15 (0UL<<SYS_PE_H_MFP_PE15_MFP_Pos)
516#define SYS_PE_H_MFP_PE15_MFP_LCD_S29 (7UL<<SYS_PE_H_MFP_PE15_MFP_Pos)
518#define SYS_PE_H_MFP_PE14_MFP_GPE14 (0UL<<SYS_PE_H_MFP_PE14_MFP_Pos)
519#define SYS_PE_H_MFP_PE14_MFP_LCD_S28 (7UL<<SYS_PE_H_MFP_PE14_MFP_Pos)
521#define SYS_PE_H_MFP_PE13_MFP_GPE13 (0UL<<SYS_PE_H_MFP_PE13_MFP_Pos)
522#define SYS_PE_H_MFP_PE13_MFP_LCD_S27 (7UL<<SYS_PE_H_MFP_PE13_MFP_Pos)
524#define SYS_PE_H_MFP_PE12_MFP_GPE12 (0UL<<SYS_PE_H_MFP_PE12_MFP_Pos)
525#define SYS_PE_H_MFP_PE12_MFP_UART1_CTS (7UL<<SYS_PE_H_MFP_PE12_MFP_Pos)
527#define SYS_PE_H_MFP_PE11_MFP_GPE11 (0UL<<SYS_PE_H_MFP_PE11_MFP_Pos)
528#define SYS_PE_H_MFP_PE11_MFP_UART1_RTS (7UL<<SYS_PE_H_MFP_PE11_MFP_Pos)
530#define SYS_PE_H_MFP_PE10_MFP_GPE10 (0UL<<SYS_PE_H_MFP_PE10_MFP_Pos)
531#define SYS_PE_H_MFP_PE10_MFP_UART1_TX (7UL<<SYS_PE_H_MFP_PE10_MFP_Pos)
533#define SYS_PE_H_MFP_PE9_MFP_GPE9 (0UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
534#define SYS_PE_H_MFP_PE9_MFP_UART1_RX (7UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
536#define SYS_PE_H_MFP_PE8_MFP_GPE8 (0UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
537#define SYS_PE_H_MFP_PE8_MFP_LCD_S9 (7UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
539/********************* Bit definition of PF_L_MFP register **********************/
540#define SYS_PF_L_MFP_PF5_MFP_GPF5 (0UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
541#define SYS_PF_L_MFP_PF5_MFP_I2C0_SCL (1UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
543#define SYS_PF_L_MFP_PF4_MFP_GPF4 (0UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
544#define SYS_PF_L_MFP_PF4_MFP_I2C0_SDA (1UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
546#define SYS_PF_L_MFP_PF3_MFP_GPF3 (0UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
547#define SYS_PF_L_MFP_PF3_MFP_HXT_IN (7UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
549#define SYS_PF_L_MFP_PF2_MFP_GPF2 (0UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
550#define SYS_PF_L_MFP_PF2_MFP_HXT_OUT (7UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
552#define SYS_PF_L_MFP_PF1_MFP_GPF1 (0UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
553#define SYS_PF_L_MFP_PF1_MFP_CKO (4UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
554#define SYS_PF_L_MFP_PF1_MFP_EXT_INT1 (5UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
555#define SYS_PF_L_MFP_PF1_MFP_ICE_CLK (7UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
557#define SYS_PF_L_MFP_PF0_MFP_GPF0 (0UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
558#define SYS_PF_L_MFP_PF0_MFP_EXT_INT0 (5UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
559#define SYS_PF_L_MFP_PF0_MFP_ICE_DAT (7UL<<SYS_PF_L_MFP_PF0_MFP_Pos) /* end of group NANO100_SYS_EXPORTED_CONSTANTS */
562
573#define SYS_CLEAR_BOD_INT_FLAG() (SYS->BODSTS |= SYS_BODSTS_BOD_INT_Msk)
574
581#define SYS_DISABLE_BOD25() (SYS->BODCTL &= ~SYS_BODCTL_BOD25_EN_Msk)
582
589#define SYS_ENABLE_BOD25() (SYS->BODCTL |= SYS_BODCTL_BOD25_EN_Msk)
590
597#define SYS_DISABLE_BOD20() (SYS->BODCTL &= ~SYS_BODCTL_BOD20_EN_Msk)
598
605#define SYS_ENABLE_BOD20() (SYS->BODCTL |= SYS_BODCTL_BOD20_EN_Msk)
606
613#define SYS_DISABLE_BOD17() (SYS->BODCTL &= ~SYS_BODCTL_BOD17_EN_Msk)
614
621#define SYS_ENABLE_BOD17() (SYS->BODCTL |= SYS_BODCTL_BOD17_EN_Msk)
622
630#define SYS_GET_BOD_INT_FLAG() (SYS->BODSTS & SYS_BODSTS_BOD_INT_Msk)
631
640#define SYS_GET_BOD25_OUTPUT() (SYS->BODSTS & SYS_BODSTS_BOD25_drop_Msk)
641
650#define SYS_GET_BOD20_OUTPUT() (SYS->BODSTS & SYS_BODSTS_BOD20_drop_Msk)
651
660#define SYS_GET_BOD17_OUTPUT() (SYS->BODSTS & SYS_BODSTS_BOD17_drop_Msk)
661
668#define SYS_DISABLE_BOD25_RST() (SYS->BODCTL &= ~SYS_BODCTL_BOD25_RST_EN_Msk)
669
676#define SYS_ENABLE_BOD25_RST() (SYS->BODCTL |= SYS_BODCTL_BOD25_RST_EN_Msk)
677
684#define SYS_DISABLE_BOD20_RST() (SYS->BODCTL &= ~SYS_BODCTL_BOD20_RST_EN_Msk)
685
692#define SYS_ENABLE_BOD20_RST() (SYS->BODCTL |= SYS_BODCTL_BOD20_RST_EN_Msk)
693
700#define SYS_DISABLE_BOD17_RST() (SYS->BODCTL &= ~SYS_BODCTL_BOD17_RST_EN_Msk)
701
708#define SYS_ENABLE_BOD17_RST() (SYS->BODCTL |= SYS_BODCTL_BOD17_RST_EN_Msk)
709
717#define SYS_IS_BOD_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_BOD_Msk)
718
719
727#define SYS_IS_CPU_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_CPU_Msk)
728
736#define SYS_IS_POR_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_POR_Msk)
737
745#define SYS_IS_RSTPIN_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_PAD_Msk)
746
747
755#define SYS_IS_SYSTEM_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_SYS_Msk)
756
757
765#define SYS_IS_WDT_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_WDT_Msk)
766
773#define SYS_DISABLE_POR() (SYS->PORCTL = 0x5AA5)
774
781#define SYS_ENABLE_POR() (SYS->PORCTL = 0)
782
783
796#define SYS_CLEAR_RST_SOURCE(u32RstSrc) (SYS->RST_SRC = u32RstSrc )
797
806#define SYS_GET_IRCTRIM_INT_FLAG() (SYS->IRCTRIMINT)
807
816#define SYS_CLEAR_IRCTRIM_INT_FLAG(u32IRCTrimFlg) (SYS->IRCTRIMINT = u32IRCTrimFlg )
817
818
826__STATIC_INLINE void SYS_UnlockReg(void)
827{
828 while(SYS->RegLockAddr != SYS_RegLockAddr_RegUnLock_Msk)
829 {
830 SYS->RegLockAddr = 0x59;
831 SYS->RegLockAddr = 0x16;
832 SYS->RegLockAddr = 0x88;
833 }
834}
835
843__STATIC_INLINE void SYS_LockReg(void)
844{
845 SYS->RegLockAddr = 0;
846}
847
848 void SYS_ClearResetSrc(uint32_t u32Src);
849uint32_t SYS_GetBODStatus(void);
850uint32_t SYS_GetResetSrc(void);
851uint32_t SYS_IsRegLocked(void);
852uint32_t SYS_ReadPDID(void);
853 void SYS_ResetChip(void);
854 void SYS_ResetCPU(void);
855 void SYS_ResetModule(uint32_t u32ModuleIndex);
856 void SYS_EnableBOD(int32_t i32Mode, uint32_t u32BODLevel);
857 void SYS_DisableBOD(void);
858 void SYS_EnableIRCTrim(uint32_t u32TrimSel,uint32_t u32TrimEnInt);
859 void SYS_DisableIRCTrim(void); /* end of group NANO100_SYS_EXPORTED_FUNCTIONS */
861 /* end of group NANO100_SYS_Driver */
863 /* end of group NANO100_Device_Driver */
865
866#ifdef __cplusplus
867}
868#endif
869
870#endif //__SYS_H__
871
872/*** (C) COPYRIGHT 2013 Nuvoton Technology Corp. ***/
873
874
SYS_RegLockAddr_RegUnLock_Msk
#define SYS_RegLockAddr_RegUnLock_Msk
Definition: Nano100Series.h:3401
SYS
#define SYS
Pointer to SYS register structure.
Definition: Nano100Series.h:11692
SYS_ResetCPU
void SYS_ResetCPU(void)
This function reset CPU.
Definition: sys.c:95
SYS_LockReg
__STATIC_INLINE void SYS_LockReg(void)
Enable register write-protection function.
Definition: sys.h:843
SYS_GetResetSrc
uint32_t SYS_GetResetSrc(void)
This function get the system reset source register value.
Definition: sys.c:54
SYS_EnableBOD
void SYS_EnableBOD(int32_t i32Mode, uint32_t u32BODLevel)
This function configure BOD function. Configure BOD reset or interrupt mode and set Brown-out voltage...
Definition: sys.c:150
SYS_ResetModule
void SYS_ResetModule(uint32_t u32ModuleIndex)
This function reset selected modules.
Definition: sys.c:129
SYS_EnableIRCTrim
void SYS_EnableIRCTrim(uint32_t u32TrimSel, uint32_t u32TrimEnInt)
This function enable HIRC trim function.
Definition: sys.c:177
SYS_ReadPDID
uint32_t SYS_ReadPDID(void)
This function get product ID.
Definition: sys.c:75
SYS_GetBODStatus
uint32_t SYS_GetBODStatus(void)
This function get Brown-out detector output status.
Definition: sys.c:44
SYS_DisableIRCTrim
void SYS_DisableIRCTrim(void)
This function disable HIRC trim function.
Definition: sys.c:188
SYS_DisableBOD
void SYS_DisableBOD(void)
This function disable BOD function.
Definition: sys.c:160
SYS_IsRegLocked
uint32_t SYS_IsRegLocked(void)
This function check register write-protection bit setting.
Definition: sys.c:65
SYS_UnlockReg
__STATIC_INLINE void SYS_UnlockReg(void)
Disable register write-protection function.
Definition: sys.h:826
SYS_ClearResetSrc
void SYS_ClearResetSrc(uint32_t u32Src)
This function clear the selected system reset source.
Definition: sys.c:32
SYS_ResetChip
void SYS_ResetChip(void)
This function reset chip.
Definition: sys.c:85