| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Data Fields
UART_T Struct Reference

`#include <Nano100Series.h>`

## Data Fields
union {
__I uint32_t UART_T::RBR
__O uint32_t UART_T::THR
}; |
__IO uint32_t | CTL
__IO uint32_t | TLCTL
__IO uint32_t | IER
__IO uint32_t | ISR
__IO uint32_t | TRSR
__IO uint32_t | FSR
__IO uint32_t | MCSR
__IO uint32_t | TMCTL
__IO uint32_t | BAUD
uint32_t | RESERVE0 [2]
__IO uint32_t | IRCR
__IO uint32_t | ALT_CTL
__IO uint32_t | FUN_SEL

## Detailed Description

    @addtogroup UART Universal Asynchronous Receiver/Transmitter Controller(UART)
    Memory Mapped Structure for UART Controller

Definition at line 10098 of file Nano100Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano100Series/Include/Nano100Series.h