| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
ebi.c File Reference

NANO100 series EBI driver source file. More...

`#include "Nano100Series.h"`
`#include "ebi.h"`
Include dependency graph for ebi.c:

Go to the source code of this file.

## Functions
void | EBI_Open (uint32_t u32Bank, uint32_t u32DataWidth, uint32_t u32TimingClass, uint32_t u32BusMode, uint32_t u32CSActiveLevel)
| Initialize and enable EBI. More...
void | EBI_Close (uint8_t u32Bank)
| Disable EBI. More...
void | EBI_SetBusTiming (uint32_t u32Bank, uint32_t u32TimingConfig, uint32_t u32MclkDiv)
| Set EBI bus timings. More...

## Detailed Description

NANO100 series EBI driver source file.

Version
  V0.10

Revision
  3

Date
  14/02/05 10:36a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file ebi.c.