| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_Timer_Ouput_Capture.c File Reference

Nano100 series ACMP Threashold driver source file. More...

`#include <stdio.h>`
`#include "NuEdu-Basic01_Timer_Ouput_Capture.h"`
Include dependency graph for NuEdu-Basic01_Timer_Ouput_Capture.c:

Go to the source code of this file.

## Functions
void | Initial_Timer_port (void)
| This function is used to TM2 output and TMR3 capture function. More...
void | initial_Timer_Toggle (void)
| This function is enable TM2 toggle. More...
void | initial_Timer_count (void)
| This function is enable TM2 count. More...
void | initial_Timer_capture (void)
| This function is enable TM3 Capture. More...

## Detailed Description

Nano100 series ACMP Threashold driver source file.

Version
  V1.00

Revision
  2

Date
  14/09/18 11:58a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_Timer_Ouput_Capture.c.