| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Data Fields
LCD_T Struct Reference

`#include <Nano100Series.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | DISPCTL
__IO uint32_t | MEM_0
__IO uint32_t | MEM_1
__IO uint32_t | MEM_2
__IO uint32_t | MEM_3
__IO uint32_t | MEM_4
__IO uint32_t | MEM_5
__IO uint32_t | MEM_6
__IO uint32_t | MEM_7
__IO uint32_t | MEM_8
__IO uint32_t | MEM_9
__IO uint32_t | FCR
__IO uint32_t | FCSTS

## Detailed Description

    @addtogroup LCD LCD Controller(LCD)
    Memory Mapped Structure for LCD Controller

Definition at line 5056 of file Nano100Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano100Series/Include/Nano100Series.h