| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
i2s.c File Reference

Nano100 series I2S driver header file. More...

`#include <stdio.h>`
`#include "Nano100Series.h"`
Include dependency graph for i2s.c:

Go to the source code of this file.

## Functions
uint32_t | I2S_Open (I2S_T *i2s, uint32_t u32MasterSlave, uint32_t u32SampleRate, uint32_t u32WordWidth, uint32_t u32Channels, uint32_t u32DataFormat, uint32_t u32AudioInterface)
| This function configures some parameters of I2S interface for general purpose use. The sample rate may not be used from the parameter, it depends on system's clock settings, but real sample rate used by system will be returned for reference. More...
void | I2S_Close (I2S_T *i2s)
| Disable I2S function and I2S clock. More...
void | I2S_EnableInt (I2S_T *i2s, uint32_t u32Mask)
| This function enables the interrupt according to the mask parameter. More...
void | I2S_DisableInt (I2S_T *i2s, uint32_t u32Mask)
| This function disables the interrupt according to the mask parameter. More...
uint32_t | I2S_EnableMCLK (I2S_T *i2s, uint32_t u32BusClock)
| Enable MCLK . More...
void | I2S_DisableMCLK (I2S_T *i2s)
| Disable MCLK . More...
void | I2S_SetFIFO (I2S_T *i2s, uint32_t u32TxThreshold, uint32_t u32RxThreshold)
| Configure FIFO threshold setting. More...

## Detailed Description

Nano100 series I2S driver header file.

Version
  V1.00

Revision
  4

Date
  15/06/08 4:58p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file i2s.c.