| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_RGBLED.c File Reference
`#include <stdio.h>`
`#include "Nano100Series.h"`
`#include "NuEdu-Basic01_RGBLED.h"`
Include dependency graph for NuEdu-Basic01_RGBLED.c:

Go to the source code of this file.

## Functions
void | Initial_PWM_LED (void)
| Set multi-function pins for PWM0 channel 0,1,2. More...
void | PWM_LED (void)
| Set PWM clock enable and HCLK as PWM clock source, PWM frequency is 100Hz, duty 30% and enable output of all PWM channels. More...