| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Data Structures | Macros | Typedefs | Enumerations
Nano100Series.h File Reference

Nano100 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Nano100 series MCU. More...

`#include "core_cm0.h"`
`#include "system_Nano100Series.h"`
`#include <stdint.h>`
`#include "sys.h"`
`#include "clk.h"`
`#include "adc.h"`
`#include "dac.h"`
`#include "fmc.h"`
`#include "ebi.h"`
`#include "gpio.h"`
`#include "i2c.h"`
`#include "crc.h"`
`#include "pdma.h"`
`#include "pwm.h"`
`#include "rtc.h"`
`#include "sc.h"`
`#include "scuart.h"`
`#include "spi.h"`
`#include "timer.h"`
`#include "uart.h"`
`#include "usbd.h"`
`#include "wdt.h"`
`#include "wwdt.h"`
`#include "i2s.h"`
`#include "lcd.h"`
Include dependency graph for Nano100Series.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | ADC_T
struct | CLK_T
struct | DAC_T
struct | EBI_T
struct | FMC_T
struct | SYS_T
struct | GPIO_T
struct | GP_DB_T
struct | I2C_T
struct | I2S_T
struct | INTR_T
struct | LCD_T
struct | DMA_CRC_T
struct | DMA_GCR_T
struct | PDMA_T
struct | VDMA_T
struct | PWM_T
struct | RTC_T
struct | SC_T
struct | SPI_T
struct | TIMER_T
struct | UART_T
struct | USBD_EP_T
| USBD endpoints register. More...
struct | USBD_T
struct | WDT_T
struct | WWDT_T

## Macros
#define | __CM0_REV 0x0201
#define | __NVIC_PRIO_BITS 2
#define | __Vendor_SysTickConfig 0
#define | __MPU_PRESENT 0
#define | __FPU_PRESENT 0
#define | FLASH_BASE ((uint32_t)0x00000000)
| Flash base address. More...
#define | SRAM_BASE ((uint32_t)0x20000000)
| SRAM base address. More...
#define | APB1PERIPH_BASE ((uint32_t)0x40000000)
| APB1 base address. More...
#define | APB2PERIPH_BASE ((uint32_t)0x40100000)
| APB2 base address. More...
#define | AHBPERIPH_BASE ((uint32_t)0x50000000)
| AHB base address. More...
#define | WDT_BASE (APB1PERIPH_BASE + 0x04000)
| WDT register base address. More...
#define | WWDT_BASE (APB1PERIPH_BASE + 0x04100)
| WWDT register base address. More...
#define | RTC_BASE (APB1PERIPH_BASE + 0x08000)
| RTC register base address. More...
#define | TIMER0_BASE (APB1PERIPH_BASE + 0x10000)
| TIMER0 register base address. More...
#define | TIMER1_BASE (APB1PERIPH_BASE + 0x10100)
| TIMER1 register base address. More...
#define | I2C0_BASE (APB1PERIPH_BASE + 0x20000)
| I2C0 register base address. More...
#define | SPI0_BASE (APB1PERIPH_BASE + 0x30000)
| SPI0 register base address. More...
#define | PWM0_BASE (APB1PERIPH_BASE + 0x40000)
| PWM0 register base address. More...
#define | UART0_BASE (APB1PERIPH_BASE + 0x50000)
| UART0 register base address. More...
#define | DAC_BASE (APB1PERIPH_BASE + 0xA0000)
| DAC register base address. More...
#define | LCD_BASE (APB1PERIPH_BASE + 0xB0000)
| LCD register base address. More...
#define | SPI2_BASE (APB1PERIPH_BASE + 0xD0000)
| SPI2 register base address. More...
#define | ADC_BASE (APB1PERIPH_BASE + 0xE0000)
| ADC register base address. More...
#define | TIMER2_BASE (APB2PERIPH_BASE + 0x10000)
| TIMER2 register base address. More...
#define | TIMER3_BASE (APB2PERIPH_BASE + 0x10100)
| TIMER3 register base address. More...
#define | SHADOW_BASE (APB1PERIPH_BASE + 0x10200)
| GPIO shadow register base address. More...
#define | I2C1_BASE (APB2PERIPH_BASE + 0x20000)
| I2C1 register base address. More...
#define | SPI1_BASE (APB2PERIPH_BASE + 0x30000)
| SPI1 register base address. More...
#define | PWM1_BASE (APB2PERIPH_BASE + 0x40000)
| PWM1 register base address. More...
#define | UART1_BASE (APB2PERIPH_BASE + 0x50000)
| UART1 register base address. More...
#define | USBD_BASE (APB1PERIPH_BASE + 0x60000)
| USBD register base address. More...
#define | SC0_BASE (APB2PERIPH_BASE + 0x90000)
| SC0 register base address. More...
#define | I2S_BASE (APB2PERIPH_BASE + 0xA0000)
| I2S register base address. More...
#define | SC1_BASE (APB2PERIPH_BASE + 0xB0000)
| SC1 register base address. More...
#define | SC2_BASE (APB2PERIPH_BASE + 0xC0000)
| SC2 register base address. More...
#define | SYS_BASE (AHBPERIPH_BASE + 0x00000)
| SYS register base address. More...
#define | CLK_BASE (AHBPERIPH_BASE + 0x00200)
| CLK register base address. More...
#define | INT_BASE (AHBPERIPH_BASE + 0x00300)
| INT register base address. More...
#define | GPIOA_BASE (AHBPERIPH_BASE + 0x04000)
| GPIO port A register base address. More...
#define | GPIOB_BASE (AHBPERIPH_BASE + 0x04040)
| GPIO port B register base address. More...
#define | GPIOC_BASE (AHBPERIPH_BASE + 0x04080)
| GPIO port C register base address. More...
#define | GPIOD_BASE (AHBPERIPH_BASE + 0x040C0)
| GPIO port D register base address. More...
#define | GPIOE_BASE (AHBPERIPH_BASE + 0x04100)
| GPIO port E register base address. More...
#define | GPIOF_BASE (AHBPERIPH_BASE + 0x04140)
| GPIO port F register base address. More...
#define | GPIODBNCE_BASE (AHBPERIPH_BASE + 0x04180)
| GPIO debounce register base address. More...
#define | GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO bit access register base address. More...
#define | VDMA_BASE (AHBPERIPH_BASE + 0x08000)
| VDMA register base address. More...
#define | PDMA1_BASE (AHBPERIPH_BASE + 0x08100)
| PDMA1 register base address. More...
#define | PDMA2_BASE (AHBPERIPH_BASE + 0x08200)
| PDMA2 register base address. More...
#define | PDMA3_BASE (AHBPERIPH_BASE + 0x08300)
| PDMA3 register base address. More...
#define | PDMA4_BASE (AHBPERIPH_BASE + 0x08400)
| PDMA4 register base address. More...
#define | PDMA5_BASE (AHBPERIPH_BASE + 0x08500)
| PDMA5 register base address. More...
#define | PDMA6_BASE (AHBPERIPH_BASE + 0x08600)
| PDMA6 register base address. More...
#define | PDMACRC_BASE (AHBPERIPH_BASE + 0x08E00)
| PDMA global control register base address. More...
#define | PDMAGCR_BASE (AHBPERIPH_BASE + 0x08F00)
| PDMA CRC register base address. More...
#define | FMC_BASE (AHBPERIPH_BASE + 0x0C000)
| FMC register base address. More...
#define | EBI_BASE (AHBPERIPH_BASE + 0x10000)
| EBI register base address. More...
#define | WDT ((WDT_T *) WDT_BASE)
| Pointer to WDT register structure. More...
#define | WWDT ((WWDT_T *) WWDT_BASE)
| Pointer to WWDT register structure. More...
#define | RTC ((RTC_T *) RTC_BASE)
| Pointer to RTC register structure. More...
#define | TIMER0 ((TIMER_T *) TIMER0_BASE)
| Pointer to TIMER0 register structure. More...
#define | TIMER1 ((TIMER_T *) TIMER1_BASE)
| Pointer to TIMER1 register structure. More...
#define | TIMER2 ((TIMER_T *) TIMER2_BASE)
| Pointer to TIMER2 register structure. More...
#define | TIMER3 ((TIMER_T *) TIMER3_BASE)
| Pointer to TIMER3 register structure. More...
#define | SHADOW ((SHADOW_T *) SHADOW_BASE)
| Pointer to GPIO shadow register structure. More...
#define | I2C0 ((I2C_T *) I2C0_BASE)
| Pointer to I2C0 register structure. More...
#define | I2C1 ((I2C_T *) I2C1_BASE)
| Pointer to I2C1 register structure. More...
#define | SPI0 ((SPI_T *) SPI0_BASE)
| Pointer to SPI0 register structure. More...
#define | SPI1 ((SPI_T *) SPI1_BASE)
| Pointer to SPI1 register structure. More...
#define | SPI2 ((SPI_T *) SPI2_BASE)
| Pointer to SPI2 register structure. More...
#define | PWM0 ((PWM_T *) PWM0_BASE)
| Pointer to PWM0 register structure. More...
#define | PWM1 ((PWM_T *) PWM1_BASE)
| Pointer to PWM1 register structure. More...
#define | UART0 ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure. More...
#define | UART1 ((UART_T *) UART1_BASE)
| Pointer to UART1 register structure. More...
#define | LCD ((LCD_T *) LCD_BASE)
| Pointer to LCD register structure. More...
#define | ADC ((ADC_T *) ADC_BASE)
| Pointer to ADC register structure. More...
#define | SC0 ((SC_T *) SC0_BASE)
| Pointer to SC0 register structure. More...
#define | SC1 ((SC_T *) SC1_BASE)
| Pointer to SC1 register structure. More...
#define | SC2 ((SC_T *) SC2_BASE)
| Pointer to SC2 register structure. More...
#define | USBD ((USBD_T *) USBD_BASE)
| Pointer to USBD register structure. More...
#define | I2S ((I2S_T *) I2S_BASE)
| Pointer to I2S register structure. More...
#define | DAC ((DAC_T *) DAC_BASE)
| Pointer to DAC register structure. More...
#define | SYS ((SYS_T *) SYS_BASE)
| Pointer to SYS register structure. More...
#define | CLK ((CLK_T *) CLK_BASE)
| Pointer to CLK register structure. More...
#define | INTR ((INTR_T *) INT_BASE)
| Pointer to INTR register structure. More...
#define | PA ((GPIO_T *) GPIOA_BASE)
| Pointer to GPIO port A register structure. More...
#define | PB ((GPIO_T *) GPIOB_BASE)
| Pointer to GPIO port B register structure. More...
#define | PC ((GPIO_T *) GPIOC_BASE)
| Pointer to GPIO port C register structure. More...
#define | PD ((GPIO_T *) GPIOD_BASE)
| Pointer to GPIO port D register structure. More...
#define | PE ((GPIO_T *) GPIOE_BASE)
| Pointer to GPIO port E register structure. More...
#define | PF ((GPIO_T *) GPIOF_BASE)
| Pointer to GPIO port F register structure. More...
#define | GPIO ((GP_DB_T *) GPIODBNCE_BASE)
| Pointer to GPIO debounce register structure. More...
#define | VDMA ((VDMA_T *) VDMA_BASE)
| Pointer to VDMA register structure. More...
#define | PDMA1 ((PDMA_T *) PDMA1_BASE)
| Pointer to PDMA1 register structure. More...
#define | PDMA2 ((PDMA_T *) PDMA2_BASE)
| Pointer to PDMA2 register structure. More...
#define | PDMA3 ((PDMA_T *) PDMA3_BASE)
| Pointer to PDMA3 register structure. More...
#define | PDMA4 ((PDMA_T *) PDMA4_BASE)
| Pointer to PDMA4 register structure. More...
#define | PDMA5 ((PDMA_T *) PDMA5_BASE)
| Pointer to PDMA5 register structure. More...
#define | PDMA6 ((PDMA_T *) PDMA6_BASE)
| Pointer to PDMA6 register structure. More...
#define | PDMACRC ((DMA_CRC_T *) PDMACRC_BASE)
| Pointer to PDMA CRC register structure. More...
#define | PDMAGCR ((DMA_GCR_T *) PDMAGCR_BASE)
| Pointer to PDMA global control register structure. More...
#define | FMC ((FMC_T *) FMC_BASE)
| Pointer to FMC register structure. More...
#define | EBI ((EBI_T *) EBI_BASE)
| Pointer to EBI register structure. More...
#define | M8(addr) (*((vu8 *) (addr)))
| Get a 8-bit unsigned value from specified address. More...
#define | M16(addr) (*((vu16 *) (addr)))
| Get a 16-bit unsigned value from specified address. More...
#define | M32(addr) (*((vu32 *) (addr)))
| Get a 32-bit unsigned value from specified address. More...
#define | outpw(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inpw(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outps(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inps(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outpb(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inpb(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | outp32(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inp32(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outp16(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inp16(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outp8(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inp8(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | NULL (0)
| NULL pointer. More...
#define | TRUE (1)
| Boolean true, define to use in API parameters or return value. More...
#define | FALSE (0)
| Boolean false, define to use in API parameters or return value. More...
#define | ENABLE (1)
| Enable, define to use in API parameters. More...
#define | DISABLE (0)
| Disable, define to use in API parameters. More...
#define | BIT0 (0x00000001)
| Bit 0 mask of an 32 bit integer. More...
#define | BIT1 (0x00000002)
| Bit 1 mask of an 32 bit integer. More...
#define | BIT2 (0x00000004)
| Bit 2 mask of an 32 bit integer. More...
#define | BIT3 (0x00000008)
| Bit 3 mask of an 32 bit integer. More...
#define | BIT4 (0x00000010)
| Bit 4 mask of an 32 bit integer. More...
#define | BIT5 (0x00000020)
| Bit 5 mask of an 32 bit integer. More...
#define | BIT6 (0x00000040)
| Bit 6 mask of an 32 bit integer. More...
#define | BIT7 (0x00000080)
| Bit 7 mask of an 32 bit integer. More...
#define | BIT8 (0x00000100)
| Bit 8 mask of an 32 bit integer. More...
#define | BIT9 (0x00000200)
| Bit 9 mask of an 32 bit integer. More...
#define | BIT10 (0x00000400)
| Bit 10 mask of an 32 bit integer. More...
#define | BIT11 (0x00000800)
| Bit 11 mask of an 32 bit integer. More...
#define | BIT12 (0x00001000)
| Bit 12 mask of an 32 bit integer. More...
#define | BIT13 (0x00002000)
| Bit 13 mask of an 32 bit integer. More...
#define | BIT14 (0x00004000)
| Bit 14 mask of an 32 bit integer. More...
#define | BIT15 (0x00008000)
| Bit 15 mask of an 32 bit integer. More...
#define | BIT16 (0x00010000)
| Bit 16 mask of an 32 bit integer. More...
#define | BIT17 (0x00020000)
| Bit 17 mask of an 32 bit integer. More...
#define | BIT18 (0x00040000)
| Bit 18 mask of an 32 bit integer. More...
#define | BIT19 (0x00080000)
| Bit 19 mask of an 32 bit integer. More...
#define | BIT20 (0x00100000)
| Bit 20 mask of an 32 bit integer. More...
#define | BIT21 (0x00200000)
| Bit 21 mask of an 32 bit integer. More...
#define | BIT22 (0x00400000)
| Bit 22 mask of an 32 bit integer. More...
#define | BIT23 (0x00800000)
| Bit 23 mask of an 32 bit integer. More...
#define | BIT24 (0x01000000)
| Bit 24 mask of an 32 bit integer. More...
#define | BIT25 (0x02000000)
| Bit 25 mask of an 32 bit integer. More...
#define | BIT26 (0x04000000)
| Bit 26 mask of an 32 bit integer. More...
#define | BIT27 (0x08000000)
| Bit 27 mask of an 32 bit integer. More...
#define | BIT28 (0x10000000)
| Bit 28 mask of an 32 bit integer. More...
#define | BIT29 (0x20000000)
| Bit 29 mask of an 32 bit integer. More...
#define | BIT30 (0x40000000)
| Bit 30 mask of an 32 bit integer. More...
#define | BIT31 (0x80000000)
| Bit 31 mask of an 32 bit integer. More...
#define | BYTE0_Msk (0x000000FF)
| Mask to get bit0~bit7 from a 32 bit integer. More...
#define | BYTE1_Msk (0x0000FF00)
| Mask to get bit8~bit15 from a 32 bit integer. More...
#define | BYTE2_Msk (0x00FF0000)
| Mask to get bit16~bit23 from a 32 bit integer. More...
#define | BYTE3_Msk (0xFF000000)
| Mask to get bit24~bit31 from a 32 bit integer. More...
#define | GET_BYTE0(u32Param) ((u32Param & BYTE0_Msk) )
#define | GET_BYTE1(u32Param) ((u32Param & BYTE1_Msk) >> 8)
#define | GET_BYTE2(u32Param) ((u32Param & BYTE2_Msk) >> 16)
#define | GET_BYTE3(u32Param) ((u32Param & BYTE3_Msk) >> 24)
#define | ADC_RESULT_RSLT_Pos (0)
#define | ADC_RESULT_RSLT_Msk (0xffful << ADC_RESULT_RSLT_Pos)
#define | ADC_RESULT_VALID_Pos (16)
#define | ADC_RESULT_VALID_Msk (0x1ul << ADC_RESULT_VALID_Pos)
#define | ADC_RESULT_OVERRUN_Pos (17)
#define | ADC_RESULT_OVERRUN_Msk (0x1ul << ADC_RESULT_OVERRUN_Pos)
#define | ADC_CR_ADEN_Pos (0)
#define | ADC_CR_ADEN_Msk (0x1ul << ADC_CR_ADEN_Pos)
#define | ADC_CR_ADIE_Pos (1)
#define | ADC_CR_ADIE_Msk (0x1ul << ADC_CR_ADIE_Pos)
#define | ADC_CR_ADMD_Pos (2)
#define | ADC_CR_ADMD_Msk (0x3ul << ADC_CR_ADMD_Pos)
#define | ADC_CR_TRGS_Pos (4)
#define | ADC_CR_TRGS_Msk (0x3ul << ADC_CR_TRGS_Pos)
#define | ADC_CR_TRGCOND_Pos (6)
#define | ADC_CR_TRGCOND_Msk (0x3ul << ADC_CR_TRGCOND_Pos)
#define | ADC_CR_TRGE_Pos (8)
#define | ADC_CR_TRGE_Msk (0x1ul << ADC_CR_TRGE_Pos)
#define | ADC_CR_PTEN_Pos (9)
#define | ADC_CR_PTEN_Msk (0x1ul << ADC_CR_PTEN_Pos)
#define | ADC_CR_DIFF_Pos (10)
#define | ADC_CR_DIFF_Msk (0x1ul << ADC_CR_DIFF_Pos)
#define | ADC_CR_ADST_Pos (11)
#define | ADC_CR_ADST_Msk (0x1ul << ADC_CR_ADST_Pos)
#define | ADC_CR_TMSEL_Pos (12)
#define | ADC_CR_TMSEL_Msk (0x3ul << ADC_CR_TMSEL_Pos)
#define | ADC_CR_TMTRGMOD_Pos (15)
#define | ADC_CR_TMTRGMOD_Msk (0x1ul << ADC_CR_TMTRGMOD_Pos)
#define | ADC_CR_REFSEL_Pos (16)
#define | ADC_CR_REFSEL_Msk (0x3ul << ADC_CR_REFSEL_Pos)
#define | ADC_CR_RESSEL_Pos (18)
#define | ADC_CR_RESSEL_Msk (0x3ul << ADC_CR_RESSEL_Pos)
#define | ADC_CR_TMPDMACNT_Pos (24)
#define | ADC_CR_TMPDMACNT_Msk (0xfful << ADC_CR_TMPDMACNT_Pos)
#define | ADC_CHEN_CHEN0_Pos (0)
#define | ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)
#define | ADC_CMPR_CMPEN_Pos (0)
#define | ADC_CMPR_CMPEN_Msk (0x1ul << ADC_CMPR_CMPEN_Pos)
#define | ADC_CMPR_CMPIE_Pos (1)
#define | ADC_CMPR_CMPIE_Msk (0x1ul << ADC_CMPR_CMPIE_Pos)
#define | ADC_CMPR_CMPCOND_Pos (2)
#define | ADC_CMPR_CMPCOND_Msk (0x1ul << ADC_CMPR_CMPCOND_Pos)
#define | ADC_CMPR_CMPCH_Pos (3)
#define | ADC_CMPR_CMPCH_Msk (0x1ful << ADC_CMPR_CMPCH_Pos)
#define | ADC_CMPR_CMPMATCNT_Pos (8)
#define | ADC_CMPR_CMPMATCNT_Msk (0xful << ADC_CMPR_CMPMATCNT_Pos)
#define | ADC_CMPR_CMPD_Pos (16)
#define | ADC_CMPR_CMPD_Msk (0xffful << ADC_CMPR_CMPD_Pos)
#define | ADC_SR_ADF_Pos (0)
#define | ADC_SR_ADF_Msk (0x1ul << ADC_SR_ADF_Pos)
#define | ADC_SR_CMPF0_Pos (1)
#define | ADC_SR_CMPF0_Msk (0x1ul << ADC_SR_CMPF0_Pos)
#define | ADC_SR_CMPF1_Pos (2)
#define | ADC_SR_CMPF1_Msk (0x1ul << ADC_SR_CMPF1_Pos)
#define | ADC_SR_BUSY_Pos (3)
#define | ADC_SR_BUSY_Msk (0x1ul << ADC_SR_BUSY_Pos)
#define | ADC_SR_CHANNEL_Pos (4)
#define | ADC_SR_CHANNEL_Msk (0x1ful << ADC_SR_CHANNEL_Pos)
#define | ADC_SR_INITRDY_Pos (16)
#define | ADC_SR_INITRDY_Msk (0x1ul << ADC_SR_INITRDY_Pos)
#define | ADC_PDMA_AD_PDMA_Pos (0)
#define | ADC_PDMA_AD_PDMA_Msk (0xffful << ADC_PDMA_AD_PDMA_Pos)
#define | ADC_PWRCTL_PWUPRDY_Pos (0)
#define | ADC_PWRCTL_PWUPRDY_Msk (0x1ul << ADC_PWRCTL_PWUPRDY_Pos)
#define | ADC_PWRCTL_PWDCALEN_Pos (1)
#define | ADC_PWRCTL_PWDCALEN_Msk (0x1ul << ADC_PWRCTL_PWDCALEN_Pos)
#define | ADC_PWRCTL_PWDMOD_Pos (2)
#define | ADC_PWRCTL_PWDMOD_Msk (0x3ul << ADC_PWRCTL_PWDMOD_Pos)
#define | ADC_CALCTL_CALEN_Pos (0)
#define | ADC_CALCTL_CALEN_Msk (0x1ul << ADC_CALCTL_CALEN_Pos)
#define | ADC_CALCTL_CALSTART_Pos (1)
#define | ADC_CALCTL_CALSTART_Msk (0x1ul << ADC_CALCTL_CALSTART_Pos)
#define | ADC_CALCTL_CALDONE_Pos (2)
#define | ADC_CALCTL_CALDONE_Msk (0x1ul << ADC_CALCTL_CALDONE_Pos)
#define | ADC_CALCTL_CALSEL_Pos (3)
#define | ADC_CALCTL_CALSEL_Msk (0x1ul << ADC_CALCTL_CALSEL_Pos)
#define | ADC_CALWORD_CALWORD_Pos (0)
#define | ADC_CALWORD_CALWORD_Msk (0x7ful << ADC_CALWORD_CALWORD_Pos)
#define | ADC_SMPLCNT0_CH0SAMPCNT_Pos (0)
#define | ADC_SMPLCNT0_CH0SAMPCNT_Msk (0xful << ADC_SMPLCNT0_CH0SAMPCNT_Pos)
#define | ADC_SMPLCNT1_CH8SAMPCNT_Pos (0)
#define | ADC_SMPLCNT1_CH8SAMPCNT_Msk (0xful << ADC_SMPLCNT1_CH8SAMPCNT_Pos)
#define | ADC_SMPLCNT1_INTCHSAMPCNT_Pos (16)
#define | ADC_SMPLCNT1_INTCHSAMPCNT_Msk (0xful << ADC_SMPLCNT1_INTCHSAMPCNT_Pos)
#define | CLK_PWRCTL_HXT_EN_Pos (0)
#define | CLK_PWRCTL_HXT_EN_Msk (0x1ul << CLK_PWRCTL_HXT_EN_Pos)
#define | CLK_PWRCTL_LXT_EN_Pos (1)
#define | CLK_PWRCTL_LXT_EN_Msk (0x1ul << CLK_PWRCTL_LXT_EN_Pos)
#define | CLK_PWRCTL_HIRC_EN_Pos (2)
#define | CLK_PWRCTL_HIRC_EN_Msk (0x1ul << CLK_PWRCTL_HIRC_EN_Pos)
#define | CLK_PWRCTL_LIRC_EN_Pos (3)
#define | CLK_PWRCTL_LIRC_EN_Msk (0x1ul << CLK_PWRCTL_LIRC_EN_Pos)
#define | CLK_PWRCTL_WK_DLY_Pos (4)
#define | CLK_PWRCTL_WK_DLY_Msk (0x1ul << CLK_PWRCTL_WK_DLY_Pos)
#define | CLK_PWRCTL_PD_WK_IE_Pos (5)
#define | CLK_PWRCTL_PD_WK_IE_Msk (0x1ul << CLK_PWRCTL_PD_WK_IE_Pos)
#define | CLK_PWRCTL_PD_EN_Pos (6)
#define | CLK_PWRCTL_PD_EN_Msk (0x1ul << CLK_PWRCTL_PD_EN_Pos)
#define | CLK_PWRCTL_HXT_SELXT_Pos (8)
#define | CLK_PWRCTL_HXT_SELXT_Msk (0x1ul << CLK_PWRCTL_HXT_SELXT_Pos)
#define | CLK_PWRCTL_HXT_GAIN_Pos (9)
#define | CLK_PWRCTL_HXT_GAIN_Msk (0x1ul << CLK_PWRCTL_HXT_GAIN_Pos)
#define | CLK_PWRCTL_LXT_SCNT_Pos (10)
#define | CLK_PWRCTL_LXT_SCNT_Msk (0x1ul << CLK_PWRCTL_LXT_SCNT_Pos)
#define | CLK_PWRCTL_HXT_HF_ST_Pos (11)
#define | CLK_PWRCTL_HXT_HF_ST_Msk (0x3ul << CLK_PWRCTL_HXT_HF_ST_Pos)
#define | CLK_AHBCLK_GPIO_EN_Pos (0)
#define | CLK_AHBCLK_GPIO_EN_Msk (0x1ul << CLK_AHBCLK_GPIO_EN_Pos)
#define | CLK_AHBCLK_DMA_EN_Pos (1)
#define | CLK_AHBCLK_DMA_EN_Msk (0x1ul << CLK_AHBCLK_DMA_EN_Pos)
#define | CLK_AHBCLK_ISP_EN_Pos (2)
#define | CLK_AHBCLK_ISP_EN_Msk (0x1ul << CLK_AHBCLK_ISP_EN_Pos)
#define | CLK_AHBCLK_EBI_EN_Pos (3)
#define | CLK_AHBCLK_EBI_EN_Msk (0x1ul << CLK_AHBCLK_EBI_EN_Pos)
#define | CLK_AHBCLK_SRAM_EN_Pos (4)
#define | CLK_AHBCLK_SRAM_EN_Msk (0x1ul << CLK_AHBCLK_SRAM_EN_Pos)
#define | CLK_AHBCLK_TICK_EN_Pos (5)
#define | CLK_AHBCLK_TICK_EN_Msk (0x1ul << CLK_AHBCLK_TICK_EN_Pos)
#define | CLK_APBCLK_WDT_EN_Pos (0)
#define | CLK_APBCLK_WDT_EN_Msk (0x1ul << CLK_APBCLK_WDT_EN_Pos)
#define | CLK_APBCLK_RTC_EN_Pos (1)
#define | CLK_APBCLK_RTC_EN_Msk (0x1ul << CLK_APBCLK_RTC_EN_Pos)
#define | CLK_APBCLK_TMR0_EN_Pos (2)
#define | CLK_APBCLK_TMR0_EN_Msk (0x1ul << CLK_APBCLK_TMR0_EN_Pos)
#define | CLK_APBCLK_TMR1_EN_Pos (3)
#define | CLK_APBCLK_TMR1_EN_Msk (0x1ul << CLK_APBCLK_TMR1_EN_Pos)
#define | CLK_APBCLK_TMR2_EN_Pos (4)
#define | CLK_APBCLK_TMR2_EN_Msk (0x1ul << CLK_APBCLK_TMR2_EN_Pos)
#define | CLK_APBCLK_TMR3_EN_Pos (5)
#define | CLK_APBCLK_TMR3_EN_Msk (0x1ul << CLK_APBCLK_TMR3_EN_Pos)
#define | CLK_APBCLK_FDIV_EN_Pos (6)
#define | CLK_APBCLK_FDIV_EN_Msk (0x1ul << CLK_APBCLK_FDIV_EN_Pos)
#define | CLK_APBCLK_SC2_EN_Pos (7)
#define | CLK_APBCLK_SC2_EN_Msk (0x1ul << CLK_APBCLK_SC2_EN_Pos)
#define | CLK_APBCLK_I2C0_EN_Pos (8)
#define | CLK_APBCLK_I2C0_EN_Msk (0x1ul << CLK_APBCLK_I2C0_EN_Pos)
#define | CLK_APBCLK_I2C1_EN_Pos (9)
#define | CLK_APBCLK_I2C1_EN_Msk (0x1ul << CLK_APBCLK_I2C1_EN_Pos)
#define | CLK_APBCLK_SPI0_EN_Pos (12)
#define | CLK_APBCLK_SPI0_EN_Msk (0x1ul << CLK_APBCLK_SPI0_EN_Pos)
#define | CLK_APBCLK_SPI1_EN_Pos (13)
#define | CLK_APBCLK_SPI1_EN_Msk (0x1ul << CLK_APBCLK_SPI1_EN_Pos)
#define | CLK_APBCLK_SPI2_EN_Pos (14)
#define | CLK_APBCLK_SPI2_EN_Msk (0x1ul << CLK_APBCLK_SPI2_EN_Pos)
#define | CLK_APBCLK_UART0_EN_Pos (16)
#define | CLK_APBCLK_UART0_EN_Msk (0x1ul << CLK_APBCLK_UART0_EN_Pos)
#define | CLK_APBCLK_UART1_EN_Pos (17)
#define | CLK_APBCLK_UART1_EN_Msk (0x1ul << CLK_APBCLK_UART1_EN_Pos)
#define | CLK_APBCLK_PWM0_CH01_EN_Pos (20)
#define | CLK_APBCLK_PWM0_CH01_EN_Msk (0x1ul << CLK_APBCLK_PWM0_CH01_EN_Pos)
#define | CLK_APBCLK_PWM0_CH23_EN_Pos (21)
#define | CLK_APBCLK_PWM0_CH23_EN_Msk (0x1ul << CLK_APBCLK_PWM0_CH23_EN_Pos)
#define | CLK_APBCLK_PWM1_CH01_EN_Pos (22)
#define | CLK_APBCLK_PWM1_CH01_EN_Msk (0x1ul << CLK_APBCLK_PWM1_CH01_EN_Pos)
#define | CLK_APBCLK_PWM1_CH23_EN_Pos (23)
#define | CLK_APBCLK_PWM1_CH23_EN_Msk (0x1ul << CLK_APBCLK_PWM1_CH23_EN_Pos)
#define | CLK_APBCLK_DAC_EN_Pos (25)
#define | CLK_APBCLK_DAC_EN_Msk (0x1ul << CLK_APBCLK_DAC_EN_Pos)
#define | CLK_APBCLK_LCD_EN_Pos (26)
#define | CLK_APBCLK_LCD_EN_Msk (0x1ul << CLK_APBCLK_LCD_EN_Pos)
#define | CLK_APBCLK_USBD_EN_Pos (27)
#define | CLK_APBCLK_USBD_EN_Msk (0x1ul << CLK_APBCLK_USBD_EN_Pos)
#define | CLK_APBCLK_ADC_EN_Pos (28)
#define | CLK_APBCLK_ADC_EN_Msk (0x1ul << CLK_APBCLK_ADC_EN_Pos)
#define | CLK_APBCLK_I2S_EN_Pos (29)
#define | CLK_APBCLK_I2S_EN_Msk (0x1ul << CLK_APBCLK_I2S_EN_Pos)
#define | CLK_APBCLK_SC0_EN_Pos (30)
#define | CLK_APBCLK_SC0_EN_Msk (0x1ul << CLK_APBCLK_SC0_EN_Pos)
#define | CLK_APBCLK_SC1_EN_Pos (31)
#define | CLK_APBCLK_SC1_EN_Msk (0x1ul << CLK_APBCLK_SC1_EN_Pos)
#define | CLK_CLKSTATUS_HXT_STB_Pos (0)
#define | CLK_CLKSTATUS_HXT_STB_Msk (0x1ul << CLK_CLKSTATUS_HXT_STB_Pos)
#define | CLK_CLKSTATUS_LXT_STB_Pos (1)
#define | CLK_CLKSTATUS_LXT_STB_Msk (0x1ul << CLK_CLKSTATUS_LXT_STB_Pos)
#define | CLK_CLKSTATUS_PLL_STB_Pos (2)
#define | CLK_CLKSTATUS_PLL_STB_Msk (0x1ul << CLK_CLKSTATUS_PLL_STB_Pos)
#define | CLK_CLKSTATUS_LIRC_STB_Pos (3)
#define | CLK_CLKSTATUS_LIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_LIRC_STB_Pos)
#define | CLK_CLKSTATUS_HIRC_STB_Pos (4)
#define | CLK_CLKSTATUS_HIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_HIRC_STB_Pos)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Pos (7)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Msk (0x1ul << CLK_CLKSTATUS_CLK_SW_FAIL_Pos)
#define | CLK_CLKSEL0_HCLK_S_Pos (0)
#define | CLK_CLKSEL0_HCLK_S_Msk (0x7ul << CLK_CLKSEL0_HCLK_S_Pos)
#define | CLK_CLKSEL1_UART_S_Pos (0)
#define | CLK_CLKSEL1_UART_S_Msk (0x3ul << CLK_CLKSEL1_UART_S_Pos)
#define | CLK_CLKSEL1_ADC_S_Pos (2)
#define | CLK_CLKSEL1_ADC_S_Msk (0x3ul << CLK_CLKSEL1_ADC_S_Pos)
#define | CLK_CLKSEL1_PWM0_CH01_S_Pos (4)
#define | CLK_CLKSEL1_PWM0_CH01_S_Msk (0x3ul << CLK_CLKSEL1_PWM0_CH01_S_Pos)
#define | CLK_CLKSEL1_PWM0_CH23_S_Pos (6)
#define | CLK_CLKSEL1_PWM0_CH23_S_Msk (0x3ul << CLK_CLKSEL1_PWM0_CH23_S_Pos)
#define | CLK_CLKSEL1_TMR0_S_Pos (8)
#define | CLK_CLKSEL1_TMR0_S_Msk (0x7ul << CLK_CLKSEL1_TMR0_S_Pos)
#define | CLK_CLKSEL1_TMR1_S_Pos (12)
#define | CLK_CLKSEL1_TMR1_S_Msk (0x7ul << CLK_CLKSEL1_TMR1_S_Pos)
#define | CLK_CLKSEL1_LCD_S_Pos (18)
#define | CLK_CLKSEL1_LCD_S_Msk (0x1ul << CLK_CLKSEL1_LCD_S_Pos)
#define | CLK_CLKSEL2_FRQDIV_S_Pos (2)
#define | CLK_CLKSEL2_FRQDIV_S_Msk (0x3ul << CLK_CLKSEL2_FRQDIV_S_Pos)
#define | CLK_CLKSEL2_PWM1_CH01_S_Pos (4)
#define | CLK_CLKSEL2_PWM1_CH01_S_Msk (0x3ul << CLK_CLKSEL2_PWM1_CH01_S_Pos)
#define | CLK_CLKSEL2_PWM1_CH23_S_Pos (6)
#define | CLK_CLKSEL2_PWM1_CH23_S_Msk (0x3ul << CLK_CLKSEL2_PWM1_CH23_S_Pos)
#define | CLK_CLKSEL2_TMR2_S_Pos (8)
#define | CLK_CLKSEL2_TMR2_S_Msk (0x7ul << CLK_CLKSEL2_TMR2_S_Pos)
#define | CLK_CLKSEL2_TMR3_S_Pos (12)
#define | CLK_CLKSEL2_TMR3_S_Msk (0x7ul << CLK_CLKSEL2_TMR3_S_Pos)
#define | CLK_CLKSEL2_I2S_S_Pos (16)
#define | CLK_CLKSEL2_I2S_S_Msk (0x3ul << CLK_CLKSEL2_I2S_S_Pos)
#define | CLK_CLKSEL2_SC_S_Pos (18)
#define | CLK_CLKSEL2_SC_S_Msk (0x3ul << CLK_CLKSEL2_SC_S_Pos)
#define | CLK_CLKSEL2_SPI0_S_Pos (20)
#define | CLK_CLKSEL2_SPI0_S_Msk (0x1ul << CLK_CLKSEL2_SPI0_S_Pos)
#define | CLK_CLKSEL2_SPI1_S_Pos (21)
#define | CLK_CLKSEL2_SPI1_S_Msk (0x1ul << CLK_CLKSEL2_SPI1_S_Pos)
#define | CLK_CLKSEL2_SPI2_S_Pos (22)
#define | CLK_CLKSEL2_SPI2_S_Msk (0x1ul << CLK_CLKSEL2_SPI2_S_Pos)
#define | CLK_CLKDIV0_HCLK_N_Pos (0)
#define | CLK_CLKDIV0_HCLK_N_Msk (0xful << CLK_CLKDIV0_HCLK_N_Pos)
#define | CLK_CLKDIV0_USB_N_Pos (4)
#define | CLK_CLKDIV0_USB_N_Msk (0xful << CLK_CLKDIV0_USB_N_Pos)
#define | CLK_CLKDIV0_UART_N_Pos (8)
#define | CLK_CLKDIV0_UART_N_Msk (0xful << CLK_CLKDIV0_UART_N_Pos)
#define | CLK_CLKDIV0_I2S_N_Pos (12)
#define | CLK_CLKDIV0_I2S_N_Msk (0xful << CLK_CLKDIV0_I2S_N_Pos)
#define | CLK_CLKDIV0_ADC_N_Pos (16)
#define | CLK_CLKDIV0_ADC_N_Msk (0xfful << CLK_CLKDIV0_ADC_N_Pos)
#define | CLK_CLKDIV0_SC0_N_Pos (28)
#define | CLK_CLKDIV0_SC0_N_Msk (0xful << CLK_CLKDIV0_SC0_N_Pos)
#define | CLK_CLKDIV1_SC1_N_Pos (0)
#define | CLK_CLKDIV1_SC1_N_Msk (0xful << CLK_CLKDIV1_SC1_N_Pos)
#define | CLK_CLKDIV1_SC2_N_Pos (4)
#define | CLK_CLKDIV1_SC2_N_Msk (0xful << CLK_CLKDIV1_SC2_N_Pos)
#define | CLK_PLLCTL_FB_DV_Pos (0)
#define | CLK_PLLCTL_FB_DV_Msk (0x3ful << CLK_PLLCTL_FB_DV_Pos)
#define | CLK_PLLCTL_IN_DV_Pos (8)
#define | CLK_PLLCTL_IN_DV_Msk (0x3ul << CLK_PLLCTL_IN_DV_Pos)
#define | CLK_PLLCTL_OUT_DV_Pos (12)
#define | CLK_PLLCTL_OUT_DV_Msk (0x1ul << CLK_PLLCTL_OUT_DV_Pos)
#define | CLK_PLLCTL_PD_Pos (16)
#define | CLK_PLLCTL_PD_Msk (0x1ul << CLK_PLLCTL_PD_Pos)
#define | CLK_PLLCTL_PLL_SRC_Pos (17)
#define | CLK_PLLCTL_PLL_SRC_Msk (0x1ul << CLK_PLLCTL_PLL_SRC_Pos)
#define | CLK_FRQDIV_FSEL_Pos (0)
#define | CLK_FRQDIV_FSEL_Msk (0xful << CLK_FRQDIV_FSEL_Pos)
#define | CLK_FRQDIV_FDIV_EN_Pos (4)
#define | CLK_FRQDIV_FDIV_EN_Msk (0x1ul << CLK_FRQDIV_FDIV_EN_Pos)
#define | CLK_MCLKO_MCLK_SEL_Pos (0)
#define | CLK_MCLKO_MCLK_SEL_Msk (0x3ful << CLK_MCLKO_MCLK_SEL_Pos)
#define | CLK_MCLKO_MCLK_EN_Pos (7)
#define | CLK_MCLKO_MCLK_EN_Msk (0x1ul << CLK_MCLKO_MCLK_EN_Pos)
#define | CLK_WK_INTSTS_PD_WK_IS_Pos (0)
#define | CLK_WK_INTSTS_PD_WK_IS_Msk (0x1ul << CLK_WK_INTSTS_PD_WK_IS_Pos)
#define | DAC_CTL_DACEN_Pos (0)
#define | DAC_CTL_DACEN_Msk (0x1ul << DAC_CTL_DACEN_Pos)
#define | DAC_CTL_DACIE_Pos (1)
#define | DAC_CTL_DACIE_Msk (0x1ul << DAC_CTL_DACIE_Pos)
#define | DAC_CTL_DACLSEL_Pos (4)
#define | DAC_CTL_DACLSEL_Msk (0x7ul << DAC_CTL_DACLSEL_Pos)
#define | DAC_CTL_DACPWONSTBCNT_Pos (8)
#define | DAC_CTL_DACPWONSTBCNT_Msk (0x3ffful << DAC_CTL_DACPWONSTBCNT_Pos)
#define | DAC_DATA_DACData_Pos (0)
#define | DAC_DATA_DACData_Msk (0xffful << DAC_DATA_DACData_Pos)
#define | DAC_STS_DACIFG_Pos (0)
#define | DAC_STS_DACIFG_Msk (0x1ul << DAC_STS_DACIFG_Pos)
#define | DAC_STS_DACSTFG_Pos (1)
#define | DAC_STS_DACSTFG_Msk (0x1ul << DAC_STS_DACSTFG_Pos)
#define | DAC_STS_BUSY_Pos (2)
#define | DAC_STS_BUSY_Msk (0x1ul << DAC_STS_BUSY_Pos)
#define | DAC_COMCTL_WAITDACCONV_Pos (0)
#define | DAC_COMCTL_WAITDACCONV_Msk (0xfful << DAC_COMCTL_WAITDACCONV_Pos)
#define | DAC_COMCTL_DAC01GRP_Pos (8)
#define | DAC_COMCTL_DAC01GRP_Msk (0x1ul << DAC_COMCTL_DAC01GRP_Pos)
#define | DAC_COMCTL_REFSEL_Pos (9)
#define | DAC_COMCTL_REFSEL_Msk (0x3ul << DAC_COMCTL_REFSEL_Pos)
#define | EBI_EBICON_ExtEN_Pos (0)
#define | EBI_EBICON_ExtEN_Msk (0x1ul << EBI_EBICON_ExtEN_Pos)
#define | EBI_EBICON_ExtBW16_Pos (1)
#define | EBI_EBICON_ExtBW16_Msk (0x1ul << EBI_EBICON_ExtBW16_Pos)
#define | EBI_EBICON_MCLKDIV_Pos (8)
#define | EBI_EBICON_MCLKDIV_Msk (0x7ul << EBI_EBICON_MCLKDIV_Pos)
#define | EBI_EBICON_MCLKEN_Pos (11)
#define | EBI_EBICON_MCLKEN_Msk (0x1ul << EBI_EBICON_MCLKEN_Pos)
#define | EBI_EBICON_ExttALE_Pos (16)
#define | EBI_EBICON_ExttALE_Msk (0x7ul << EBI_EBICON_ExttALE_Pos)
#define | EBI_EXTIME_ExttACC_Pos (0)
#define | EBI_EXTIME_ExttACC_Msk (0x1ful << EBI_EXTIME_ExttACC_Pos)
#define | EBI_EXTIME_ExttAHD_Pos (8)
#define | EBI_EXTIME_ExttAHD_Msk (0x7ul << EBI_EXTIME_ExttAHD_Pos)
#define | EBI_EXTIME_ExtIW2X_Pos (12)
#define | EBI_EXTIME_ExtIW2X_Msk (0xful << EBI_EXTIME_ExtIW2X_Pos)
#define | EBI_EXTIME_ExtIR2W_Pos (16)
#define | EBI_EXTIME_ExtIR2W_Msk (0xful << EBI_EXTIME_ExtIR2W_Pos)
#define | EBI_EXTIME_ExtIR2R_Pos (24)
#define | EBI_EXTIME_ExtIR2R_Msk (0xful << EBI_EXTIME_ExtIR2R_Pos)
#define | FMC_ISPCON_ISPEN_Pos (0)
#define | FMC_ISPCON_ISPEN_Msk (0x1ul << FMC_ISPCON_ISPEN_Pos)
#define | FMC_ISPCON_BS_Pos (1)
#define | FMC_ISPCON_BS_Msk (0x1ul << FMC_ISPCON_BS_Pos)
#define | FMC_ISPCON_APUEN_Pos (3)
#define | FMC_ISPCON_APUEN_Msk (0x1ul << FMC_ISPCON_APUEN_Pos)
#define | FMC_ISPCON_CFGUEN_Pos (4)
#define | FMC_ISPCON_CFGUEN_Msk (0x1ul << FMC_ISPCON_CFGUEN_Pos)
#define | FMC_ISPCON_LDUEN_Pos (5)
#define | FMC_ISPCON_LDUEN_Msk (0x1ul << FMC_ISPCON_LDUEN_Pos)
#define | FMC_ISPCON_ISPFF_Pos (6)
#define | FMC_ISPCON_ISPFF_Msk (0x1ul << FMC_ISPCON_ISPFF_Pos)
#define | FMC_ISPADR_ISPADR_Pos (0)
#define | FMC_ISPADR_ISPADR_Msk (0xfffffffful << FMC_ISPADR_ISPADR_Pos)
#define | FMC_ISPDAT_ISPDAT_Pos (0)
#define | FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)
#define | FMC_ISPCMD_FCTRL_Pos (0)
#define | FMC_ISPCMD_FCTRL_Msk (0xful << FMC_ISPCMD_FCTRL_Pos)
#define | FMC_ISPCMD_FCEN_Pos (4)
#define | FMC_ISPCMD_FCEN_Msk (0x1ul << FMC_ISPCMD_FCEN_Pos)
#define | FMC_ISPCMD_FOEN_Pos (5)
#define | FMC_ISPCMD_FOEN_Msk (0x1ul << FMC_ISPCMD_FOEN_Pos)
#define | FMC_ISPTRG_ISPGO_Pos (0)
#define | FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)
#define | FMC_DFBADR_DFBA_Pos (0)
#define | FMC_DFBADR_DFBA_Msk (0xfffffffful << FMC_DFBADR_DFBA_Pos)
#define | FMC_ISPSTA_ISPBUSY_Pos (0)
#define | FMC_ISPSTA_ISPBUSY_Msk (0x1ul << FMC_ISPSTA_ISPBUSY_Pos)
#define | FMC_ISPSTA_CBS_Pos (1)
#define | FMC_ISPSTA_CBS_Msk (0x3ul << FMC_ISPSTA_CBS_Pos)
#define | FMC_ISPSTA_ISPFF_Pos (6)
#define | FMC_ISPSTA_ISPFF_Msk (0x1ul << FMC_ISPSTA_ISPFF_Pos)
#define | SYS_PDID_PDID_Pos (0)
#define | SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)
#define | SYS_RST_SRC_RSTS_POR_Pos (0)
#define | SYS_RST_SRC_RSTS_POR_Msk (0x1ul << SYS_RST_SRC_RSTS_POR_Pos)
#define | SYS_RST_SRC_RSTS_PAD_Pos (1)
#define | SYS_RST_SRC_RSTS_PAD_Msk (0x1ul << SYS_RST_SRC_RSTS_PAD_Pos)
#define | SYS_RST_SRC_RSTS_WDT_Pos (2)
#define | SYS_RST_SRC_RSTS_WDT_Msk (0x1ul << SYS_RST_SRC_RSTS_WDT_Pos)
#define | SYS_RST_SRC_RSTS_BOD_Pos (4)
#define | SYS_RST_SRC_RSTS_BOD_Msk (0x1ul << SYS_RST_SRC_RSTS_BOD_Pos)
#define | SYS_RST_SRC_RSTS_SYS_Pos (5)
#define | SYS_RST_SRC_RSTS_SYS_Msk (0x1ul << SYS_RST_SRC_RSTS_SYS_Pos)
#define | SYS_RST_SRC_RSTS_CPU_Pos (7)
#define | SYS_RST_SRC_RSTS_CPU_Msk (0x1ul << SYS_RST_SRC_RSTS_CPU_Pos)
#define | SYS_IPRST_CTL1_CHIP_RST_Pos (0)
#define | SYS_IPRST_CTL1_CHIP_RST_Msk (0x1ul << SYS_IPRST_CTL1_CHIP_RST_Pos)
#define | SYS_IPRST_CTL1_CPU_RST_Pos (1)
#define | SYS_IPRST_CTL1_CPU_RST_Msk (0x1ul << SYS_IPRST_CTL1_CPU_RST_Pos)
#define | SYS_IPRST_CTL1_DMA_RST_Pos (2)
#define | SYS_IPRST_CTL1_DMA_RST_Msk (0x1ul << SYS_IPRST_CTL1_DMA_RST_Pos)
#define | SYS_IPRST_CTL1_EBI_RST_Pos (3)
#define | SYS_IPRST_CTL1_EBI_RST_Msk (0x1ul << SYS_IPRST_CTL1_EBI_RST_Pos)
#define | SYS_IPRST_CTL2_GPIO_RST_Pos (1)
#define | SYS_IPRST_CTL2_GPIO_RST_Msk (0x1ul << SYS_IPRST_CTL2_GPIO_RST_Pos)
#define | SYS_IPRST_CTL2_TMR0_RST_Pos (2)
#define | SYS_IPRST_CTL2_TMR0_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR0_RST_Pos)
#define | SYS_IPRST_CTL2_TMR1_RST_Pos (3)
#define | SYS_IPRST_CTL2_TMR1_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR1_RST_Pos)
#define | SYS_IPRST_CTL2_TMR2_RST_Pos (4)
#define | SYS_IPRST_CTL2_TMR2_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR2_RST_Pos)
#define | SYS_IPRST_CTL2_TMR3_RST_Pos (5)
#define | SYS_IPRST_CTL2_TMR3_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR3_RST_Pos)
#define | SYS_IPRST_CTL2_SC2_RST_Pos (7)
#define | SYS_IPRST_CTL2_SC2_RST_Msk (0x1ul << SYS_IPRST_CTL2_SC2_RST_Pos)
#define | SYS_IPRST_CTL2_I2C0_RST_Pos (8)
#define | SYS_IPRST_CTL2_I2C0_RST_Msk (0x1ul << SYS_IPRST_CTL2_I2C0_RST_Pos)
#define | SYS_IPRST_CTL2_I2C1_RST_Pos (9)
#define | SYS_IPRST_CTL2_I2C1_RST_Msk (0x1ul << SYS_IPRST_CTL2_I2C1_RST_Pos)
#define | SYS_IPRST_CTL2_SPI0_RST_Pos (12)
#define | SYS_IPRST_CTL2_SPI0_RST_Msk (0x1ul << SYS_IPRST_CTL2_SPI0_RST_Pos)
#define | SYS_IPRST_CTL2_SPI1_RST_Pos (13)
#define | SYS_IPRST_CTL2_SPI1_RST_Msk (0x1ul << SYS_IPRST_CTL2_SPI1_RST_Pos)
#define | SYS_IPRST_CTL2_SPI2_RST_Pos (14)
#define | SYS_IPRST_CTL2_SPI2_RST_Msk (0x1ul << SYS_IPRST_CTL2_SPI2_RST_Pos)
#define | SYS_IPRST_CTL2_UART0_RST_Pos (16)
#define | SYS_IPRST_CTL2_UART0_RST_Msk (0x1ul << SYS_IPRST_CTL2_UART0_RST_Pos)
#define | SYS_IPRST_CTL2_UART1_RST_Pos (17)
#define | SYS_IPRST_CTL2_UART1_RST_Msk (0x1ul << SYS_IPRST_CTL2_UART1_RST_Pos)
#define | SYS_IPRST_CTL2_PWM0_RST_Pos (20)
#define | SYS_IPRST_CTL2_PWM0_RST_Msk (0x1ul << SYS_IPRST_CTL2_PWM0_RST_Pos)
#define | SYS_IPRST_CTL2_PWM1_RST_Pos (21)
#define | SYS_IPRST_CTL2_PWM1_RST_Msk (0x1ul << SYS_IPRST_CTL2_PWM1_RST_Pos)
#define | SYS_IPRST_CTL2_DAC_RST_Pos (25)
#define | SYS_IPRST_CTL2_DAC_RST_Msk (0x1ul << SYS_IPRST_CTL2_DAC_RST_Pos)
#define | SYS_IPRST_CTL2_LCD_RST_Pos (26)
#define | SYS_IPRST_CTL2_LCD_RST_Msk (0x1ul << SYS_IPRST_CTL2_LCD_RST_Pos)
#define | SYS_IPRST_CTL2_USBD_RST_Pos (27)
#define | SYS_IPRST_CTL2_USBD_RST_Msk (0x1ul << SYS_IPRST_CTL2_USBD_RST_Pos)
#define | SYS_IPRST_CTL2_ADC_RST_Pos (28)
#define | SYS_IPRST_CTL2_ADC_RST_Msk (0x1ul << SYS_IPRST_CTL2_ADC_RST_Pos)
#define | SYS_IPRST_CTL2_I2S_RST_Pos (29)
#define | SYS_IPRST_CTL2_I2S_RST_Msk (0x1ul << SYS_IPRST_CTL2_I2S_RST_Pos)
#define | SYS_IPRST_CTL2_SC0_RST_Pos (30)
#define | SYS_IPRST_CTL2_SC0_RST_Msk (0x1ul << SYS_IPRST_CTL2_SC0_RST_Pos)
#define | SYS_IPRST_CTL2_SC1_RST_Pos (31)
#define | SYS_IPRST_CTL2_SC1_RST_Msk (0x1ul << SYS_IPRST_CTL2_SC1_RST_Pos)
#define | SYS_TEMPCTL_VTEMP_EN_Pos (0)
#define | SYS_TEMPCTL_VTEMP_EN_Msk (0x1ul << SYS_TEMPCTL_VTEMP_EN_Pos)
#define | SYS_PA_L_MFP_PA0_MFP_Pos (0)
#define | SYS_PA_L_MFP_PA0_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA0_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_Pos (4)
#define | SYS_PA_L_MFP_PA1_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_Pos (8)
#define | SYS_PA_L_MFP_PA2_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_Pos (12)
#define | SYS_PA_L_MFP_PA3_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_Pos (16)
#define | SYS_PA_L_MFP_PA4_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_Pos (20)
#define | SYS_PA_L_MFP_PA5_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_Pos (24)
#define | SYS_PA_L_MFP_PA6_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_Pos (28)
#define | SYS_PA_L_MFP_PA7_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_Pos (0)
#define | SYS_PA_H_MFP_PA8_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_Pos (4)
#define | SYS_PA_H_MFP_PA9_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_Pos (8)
#define | SYS_PA_H_MFP_PA10_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_Pos (12)
#define | SYS_PA_H_MFP_PA11_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_Pos (16)
#define | SYS_PA_H_MFP_PA12_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_Pos (20)
#define | SYS_PA_H_MFP_PA13_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_Pos (24)
#define | SYS_PA_H_MFP_PA14_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_Pos (28)
#define | SYS_PA_H_MFP_PA15_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_Pos (0)
#define | SYS_PB_L_MFP_PB0_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_Pos (4)
#define | SYS_PB_L_MFP_PB1_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_Pos (8)
#define | SYS_PB_L_MFP_PB2_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_Pos (12)
#define | SYS_PB_L_MFP_PB3_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_Pos (16)
#define | SYS_PB_L_MFP_PB4_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_Pos (20)
#define | SYS_PB_L_MFP_PB5_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_Pos (24)
#define | SYS_PB_L_MFP_PB6_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_Pos (28)
#define | SYS_PB_L_MFP_PB7_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_Pos (0)
#define | SYS_PB_H_MFP_PB8_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_Pos (4)
#define | SYS_PB_H_MFP_PB9_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_Pos (8)
#define | SYS_PB_H_MFP_PB10_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_Pos (12)
#define | SYS_PB_H_MFP_PB11_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_Pos (16)
#define | SYS_PB_H_MFP_PB12_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_Pos (20)
#define | SYS_PB_H_MFP_PB13_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_Pos (24)
#define | SYS_PB_H_MFP_PB14_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_Pos (28)
#define | SYS_PB_H_MFP_PB15_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_Pos (0)
#define | SYS_PC_L_MFP_PC0_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_Pos (4)
#define | SYS_PC_L_MFP_PC1_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_Pos (8)
#define | SYS_PC_L_MFP_PC2_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_Pos (12)
#define | SYS_PC_L_MFP_PC3_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_Pos (16)
#define | SYS_PC_L_MFP_PC4_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_Pos (20)
#define | SYS_PC_L_MFP_PC5_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_Pos (24)
#define | SYS_PC_L_MFP_PC6_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_Pos (28)
#define | SYS_PC_L_MFP_PC7_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_Pos (0)
#define | SYS_PC_H_MFP_PC8_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_Pos (4)
#define | SYS_PC_H_MFP_PC9_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_Pos (8)
#define | SYS_PC_H_MFP_PC10_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_Pos (12)
#define | SYS_PC_H_MFP_PC11_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_Pos (16)
#define | SYS_PC_H_MFP_PC12_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_Pos (20)
#define | SYS_PC_H_MFP_PC13_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_Pos (24)
#define | SYS_PC_H_MFP_PC14_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_Pos (28)
#define | SYS_PC_H_MFP_PC15_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_Pos (0)
#define | SYS_PD_L_MFP_PD0_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_Pos (4)
#define | SYS_PD_L_MFP_PD1_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_Pos (8)
#define | SYS_PD_L_MFP_PD2_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_Pos (12)
#define | SYS_PD_L_MFP_PD3_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_Pos (16)
#define | SYS_PD_L_MFP_PD4_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_Pos (20)
#define | SYS_PD_L_MFP_PD5_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD6_MFP_Pos (24)
#define | SYS_PD_L_MFP_PD6_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD6_MFP_Pos)
#define | SYS_PD_L_MFP_PD7_MFP_Pos (28)
#define | SYS_PD_L_MFP_PD7_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD7_MFP_Pos)
#define | SYS_PD_H_MFP_PD8_MFP_Pos (0)
#define | SYS_PD_H_MFP_PD8_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD8_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_Pos (4)
#define | SYS_PD_H_MFP_PD9_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_Pos (8)
#define | SYS_PD_H_MFP_PD10_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_Pos (12)
#define | SYS_PD_H_MFP_PD11_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_Pos (16)
#define | SYS_PD_H_MFP_PD12_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD13_MFP_Pos (20)
#define | SYS_PD_H_MFP_PD13_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD13_MFP_Pos)
#define | SYS_PD_H_MFP_PD14_MFP_Pos (24)
#define | SYS_PD_H_MFP_PD14_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD14_MFP_Pos)
#define | SYS_PD_H_MFP_PD15_MFP_Pos (28)
#define | SYS_PD_H_MFP_PD15_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD15_MFP_Pos)
#define | SYS_PE_L_MFP_PE0_MFP_Pos (0)
#define | SYS_PE_L_MFP_PE0_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE0_MFP_Pos)
#define | SYS_PE_L_MFP_PE1_MFP_Pos (4)
#define | SYS_PE_L_MFP_PE1_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE1_MFP_Pos)
#define | SYS_PE_L_MFP_PE2_MFP_Pos (8)
#define | SYS_PE_L_MFP_PE2_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE2_MFP_Pos)
#define | SYS_PE_L_MFP_PE3_MFP_Pos (12)
#define | SYS_PE_L_MFP_PE3_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE3_MFP_Pos)
#define | SYS_PE_L_MFP_PE4_MFP_Pos (16)
#define | SYS_PE_L_MFP_PE4_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE4_MFP_Pos)
#define | SYS_PE_L_MFP_PE5_MFP_Pos (20)
#define | SYS_PE_L_MFP_PE5_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE5_MFP_Pos)
#define | SYS_PE_L_MFP_PE6_MFP_Pos (24)
#define | SYS_PE_L_MFP_PE6_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE6_MFP_Pos)
#define | SYS_PE_L_MFP_PE7_MFP_Pos (28)
#define | SYS_PE_L_MFP_PE7_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE7_MFP_Pos)
#define | SYS_PE_H_MFP_PE8_MFP_Pos (0)
#define | SYS_PE_H_MFP_PE8_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE8_MFP_Pos)
#define | SYS_PE_H_MFP_PE9_MFP_Pos (4)
#define | SYS_PE_H_MFP_PE9_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE9_MFP_Pos)
#define | SYS_PE_H_MFP_PE10_MFP_Pos (8)
#define | SYS_PE_H_MFP_PE10_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE10_MFP_Pos)
#define | SYS_PE_H_MFP_PE11_MFP_Pos (12)
#define | SYS_PE_H_MFP_PE11_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE11_MFP_Pos)
#define | SYS_PE_H_MFP_PE12_MFP_Pos (16)
#define | SYS_PE_H_MFP_PE12_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE12_MFP_Pos)
#define | SYS_PE_H_MFP_PE13_MFP_Pos (20)
#define | SYS_PE_H_MFP_PE13_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE13_MFP_Pos)
#define | SYS_PE_H_MFP_PE14_MFP_Pos (24)
#define | SYS_PE_H_MFP_PE14_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE14_MFP_Pos)
#define | SYS_PE_H_MFP_PE15_MFP_Pos (28)
#define | SYS_PE_H_MFP_PE15_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE15_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_Pos (0)
#define | SYS_PF_L_MFP_PF0_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF0_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_Pos (4)
#define | SYS_PF_L_MFP_PF1_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_Pos (8)
#define | SYS_PF_L_MFP_PF2_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_Pos (12)
#define | SYS_PF_L_MFP_PF3_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_Pos (16)
#define | SYS_PF_L_MFP_PF4_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_Pos (20)
#define | SYS_PF_L_MFP_PF5_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PORCTL_POR_DIS_CODE_Pos (0)
#define | SYS_PORCTL_POR_DIS_CODE_Msk (0xfffful << SYS_PORCTL_POR_DIS_CODE_Pos)
#define | SYS_BODCTL_BOD17_EN_Pos (0)
#define | SYS_BODCTL_BOD17_EN_Msk (0x1ul << SYS_BODCTL_BOD17_EN_Pos)
#define | SYS_BODCTL_BOD20_EN_Pos (1)
#define | SYS_BODCTL_BOD20_EN_Msk (0x1ul << SYS_BODCTL_BOD20_EN_Pos)
#define | SYS_BODCTL_BOD25_EN_Pos (2)
#define | SYS_BODCTL_BOD25_EN_Msk (0x1ul << SYS_BODCTL_BOD25_EN_Pos)
#define | SYS_BODCTL_BOD17_RST_EN_Pos (4)
#define | SYS_BODCTL_BOD17_RST_EN_Msk (0x1ul << SYS_BODCTL_BOD17_RST_EN_Pos)
#define | SYS_BODCTL_BOD20_RST_EN_Pos (5)
#define | SYS_BODCTL_BOD20_RST_EN_Msk (0x1ul << SYS_BODCTL_BOD20_RST_EN_Pos)
#define | SYS_BODCTL_BOD25_RST_EN_Pos (6)
#define | SYS_BODCTL_BOD25_RST_EN_Msk (0x1ul << SYS_BODCTL_BOD25_RST_EN_Pos)
#define | SYS_BODCTL_BOD17_INT_EN_Pos (8)
#define | SYS_BODCTL_BOD17_INT_EN_Msk (0x1ul << SYS_BODCTL_BOD17_INT_EN_Pos)
#define | SYS_BODCTL_BOD20_INT_EN_Pos (9)
#define | SYS_BODCTL_BOD20_INT_EN_Msk (0x1ul << SYS_BODCTL_BOD20_INT_EN_Pos)
#define | SYS_BODCTL_BOD25_INT_EN_Pos (10)
#define | SYS_BODCTL_BOD25_INT_EN_Msk (0x1ul << SYS_BODCTL_BOD25_INT_EN_Pos)
#define | SYS_BODSTS_BOD_INT_Pos (0)
#define | SYS_BODSTS_BOD_INT_Msk (0x1ul << SYS_BODSTS_BOD_INT_Pos)
#define | SYS_BODSTS_BOD17_drop_Pos (1)
#define | SYS_BODSTS_BOD17_drop_Msk (0x1ul << SYS_BODSTS_BOD17_drop_Pos)
#define | SYS_BODSTS_BOD20_drop_Pos (2)
#define | SYS_BODSTS_BOD20_drop_Msk (0x1ul << SYS_BODSTS_BOD20_drop_Pos)
#define | SYS_BODSTS_BOD25_drop_Pos (3)
#define | SYS_BODSTS_BOD25_drop_Msk (0x1ul << SYS_BODSTS_BOD25_drop_Pos)
#define | SYS_BODSTS_BOD17_rise_Pos (4)
#define | SYS_BODSTS_BOD17_rise_Msk (0x1ul << SYS_BODSTS_BOD17_rise_Pos)
#define | SYS_BODSTS_BOD20_rise_Pos (5)
#define | SYS_BODSTS_BOD20_rise_Msk (0x1ul << SYS_BODSTS_BOD20_rise_Pos)
#define | SYS_BODSTS_BOD25_rise_Pos (6)
#define | SYS_BODSTS_BOD25_rise_Msk (0x1ul << SYS_BODSTS_BOD25_rise_Pos)
#define | SYS_VREFCTL_BGP_EN_Pos (0)
#define | SYS_VREFCTL_BGP_EN_Msk (0x1ul << SYS_VREFCTL_BGP_EN_Pos)
#define | SYS_VREFCTL_REG_EN_Pos (1)
#define | SYS_VREFCTL_REG_EN_Msk (0x1ul << SYS_VREFCTL_REG_EN_Pos)
#define | SYS_VREFCTL_SEL25_Pos (2)
#define | SYS_VREFCTL_SEL25_Msk (0x1ul << SYS_VREFCTL_SEL25_Pos)
#define | SYS_VREFCTL_EXT_MODE_Pos (3)
#define | SYS_VREFCTL_EXT_MODE_Msk (0x1ul << SYS_VREFCTL_EXT_MODE_Pos)
#define | SYS_IRCTRIMCTL_TRIM_SEL_Pos (0)
#define | SYS_IRCTRIMCTL_TRIM_SEL_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_SEL_Pos)
#define | SYS_IRCTRIMCTL_TRIM_LOOP_Pos (4)
#define | SYS_IRCTRIMCTL_TRIM_LOOP_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos (6)
#define | SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)
#define | SYS_IRCTRIMCTL_ERR_STOP_Pos (8)
#define | SYS_IRCTRIMCTL_ERR_STOP_Msk (0x1ul << SYS_IRCTRIMCTL_ERR_STOP_Pos)
#define | SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos (1)
#define | SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos)
#define | SYS_IRCTRIMIEN_32K_ERR_IEN_Pos (2)
#define | SYS_IRCTRIMIEN_32K_ERR_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_32K_ERR_IEN_Pos)
#define | SYS_IRCTRIMINT_FREQ_LOCK_Pos (0)
#define | SYS_IRCTRIMINT_FREQ_LOCK_Msk (0x1ul << SYS_IRCTRIMINT_FREQ_LOCK_Pos)
#define | SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos (1)
#define | SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk (0x1ul << SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos)
#define | SYS_IRCTRIMINT_32K_ERR_INT_Pos (2)
#define | SYS_IRCTRIMINT_32K_ERR_INT_Msk (0x1ul << SYS_IRCTRIMINT_32K_ERR_INT_Pos)
#define | SYS_RegLockAddr_RegUnLock_Pos (0)
#define | SYS_RegLockAddr_RegUnLock_Msk (0x1ul << SYS_RegLockAddr_RegUnLock_Pos)
#define | GP_PMD_PMD0_Pos (0)
#define | GP_PMD_PMD0_Msk (0x3ul << GP_PMD_PMD0_Pos)
#define | GP_PMD_PMD1_Pos (2)
#define | GP_PMD_PMD1_Msk (0x3ul << GP_PMD_PMD1_Pos)
#define | GP_PMD_PMD2_Pos (4)
#define | GP_PMD_PMD2_Msk (0x3ul << GP_PMD_PMD2_Pos)
#define | GP_PMD_PMD3_Pos (6)
#define | GP_PMD_PMD3_Msk (0x3ul << GP_PMD_PMD3_Pos)
#define | GP_PMD_PMD4_Pos (8)
#define | GP_PMD_PMD4_Msk (0x3ul << GP_PMD_PMD4_Pos)
#define | GP_PMD_PMD5_Pos (10)
#define | GP_PMD_PMD5_Msk (0x3ul << GP_PMD_PMD5_Pos)
#define | GP_PMD_PMD6_Pos (12)
#define | GP_PMD_PMD6_Msk (0x3ul << GP_PMD_PMD6_Pos)
#define | GP_PMD_PMD7_Pos (14)
#define | GP_PMD_PMD7_Msk (0x3ul << GP_PMD_PMD7_Pos)
#define | GP_PMD_PMD8_Pos (16)
#define | GP_PMD_PMD8_Msk (0x3ul << GP_PMD_PMD8_Pos)
#define | GP_PMD_PMD9_Pos (18)
#define | GP_PMD_PMD9_Msk (0x3ul << GP_PMD_PMD9_Pos)
#define | GP_PMD_PMD10_Pos (20)
#define | GP_PMD_PMD10_Msk (0x3ul << GP_PMD_PMD10_Pos)
#define | GP_PMD_PMD11_Pos (22)
#define | GP_PMD_PMD11_Msk (0x3ul << GP_PMD_PMD11_Pos)
#define | GP_PMD_PMD12_Pos (24)
#define | GP_PMD_PMD12_Msk (0x3ul << GP_PMD_PMD12_Pos)
#define | GP_PMD_PMD13_Pos (26)
#define | GP_PMD_PMD13_Msk (0x3ul << GP_PMD_PMD13_Pos)
#define | GP_PMD_PMD14_Pos (28)
#define | GP_PMD_PMD14_Msk (0x3ul << GP_PMD_PMD14_Pos)
#define | GP_PMD_PMD15_Pos (30)
#define | GP_PMD_PMD15_Msk (0x3ul << GP_PMD_PMD15_Pos)
#define | GP_OFFD_OFFD_Pos (16)
#define | GP_OFFD_OFFD_Msk (0xfffful << GP_OFFD_OFFD_Pos)
#define | GP_DOUT_DOUT_Pos (0)
#define | GP_DOUT_DOUT_Msk (0xfffful << GP_DOUT_DOUT_Pos)
#define | GP_DMASK_DMASK_Pos (0)
#define | GP_DMASK_DMASK_Msk (0xfffful << GP_DMASK_DMASK_Pos)
#define | GP_PIN_PIN_Pos (0)
#define | GP_PIN_PIN_Msk (0xfffful << GP_PIN_PIN_Pos)
#define | GP_DBEN_DBEN_Pos (0)
#define | GP_DBEN_DBEN_Msk (0xfffful << GP_DBEN_DBEN_Pos)
#define | GP_IMD_IMD_Pos (0)
#define | GP_IMD_IMD_Msk (0xfffful << GP_IMD_IMD_Pos)
#define | GP_IER_FIER0_Pos (0)
#define | GP_IER_FIER0_Msk (0x1ul << GP_IER_FIER0_Pos)
#define | GP_IER_FIER1_Pos (1)
#define | GP_IER_FIER1_Msk (0x1ul << GP_IER_FIER1_Pos)
#define | GP_IER_FIER2_Pos (2)
#define | GP_IER_FIER2_Msk (0x1ul << GP_IER_FIER2_Pos)
#define | GP_IER_FIER3_Pos (3)
#define | GP_IER_FIER3_Msk (0x1ul << GP_IER_FIER3_Pos)
#define | GP_IER_FIER4_Pos (4)
#define | GP_IER_FIER4_Msk (0x1ul << GP_IER_FIER4_Pos)
#define | GP_IER_FIER5_Pos (5)
#define | GP_IER_FIER5_Msk (0x1ul << GP_IER_FIER5_Pos)
#define | GP_IER_FIER6_Pos (6)
#define | GP_IER_FIER6_Msk (0x1ul << GP_IER_FIER6_Pos)
#define | GP_IER_FIER7_Pos (7)
#define | GP_IER_FIER7_Msk (0x1ul << GP_IER_FIER7_Pos)
#define | GP_IER_FIER8_Pos (8)
#define | GP_IER_FIER8_Msk (0x1ul << GP_IER_FIER8_Pos)
#define | GP_IER_FIER9_Pos (9)
#define | GP_IER_FIER9_Msk (0x1ul << GP_IER_FIER9_Pos)
#define | GP_IER_FIER10_Pos (10)
#define | GP_IER_FIER10_Msk (0x1ul << GP_IER_FIER10_Pos)
#define | GP_IER_FIER11_Pos (11)
#define | GP_IER_FIER11_Msk (0x1ul << GP_IER_FIER11_Pos)
#define | GP_IER_FIER12_Pos (12)
#define | GP_IER_FIER12_Msk (0x1ul << GP_IER_FIER12_Pos)
#define | GP_IER_FIER13_Pos (13)
#define | GP_IER_FIER13_Msk (0x1ul << GP_IER_FIER13_Pos)
#define | GP_IER_FIER14_Pos (14)
#define | GP_IER_FIER14_Msk (0x1ul << GP_IER_FIER14_Pos)
#define | GP_IER_FIER15_Pos (15)
#define | GP_IER_FIER15_Msk (0x1ul << GP_IER_FIER15_Pos)
#define | GP_IER_RIER0_Pos (16)
#define | GP_IER_RIER0_Msk (0x1ul << GP_IER_RIER0_Pos)
#define | GP_IER_RIER1_Pos (17)
#define | GP_IER_RIER1_Msk (0x1ul << GP_IER_RIER1_Pos)
#define | GP_IER_RIER2_Pos (18)
#define | GP_IER_RIER2_Msk (0x1ul << GP_IER_RIER2_Pos)
#define | GP_IER_RIER3_Pos (19)
#define | GP_IER_RIER3_Msk (0x1ul << GP_IER_RIER3_Pos)
#define | GP_IER_RIER4_Pos (20)
#define | GP_IER_RIER4_Msk (0x1ul << GP_IER_RIER4_Pos)
#define | GP_IER_RIER5_Pos (21)
#define | GP_IER_RIER5_Msk (0x1ul << GP_IER_RIER5_Pos)
#define | GP_IER_RIER6_Pos (22)
#define | GP_IER_RIER6_Msk (0x1ul << GP_IER_RIER6_Pos)
#define | GP_IER_RIER7_Pos (23)
#define | GP_IER_RIER7_Msk (0x1ul << GP_IER_RIER7_Pos)
#define | GP_IER_RIER8_Pos (24)
#define | GP_IER_RIER8_Msk (0x1ul << GP_IER_RIER8_Pos)
#define | GP_IER_RIER9_Pos (25)
#define | GP_IER_RIER9_Msk (0x1ul << GP_IER_RIER9_Pos)
#define | GP_IER_RIER10_Pos (26)
#define | GP_IER_RIER10_Msk (0x1ul << GP_IER_RIER10_Pos)
#define | GP_IER_RIER11_Pos (27)
#define | GP_IER_RIER11_Msk (0x1ul << GP_IER_RIER11_Pos)
#define | GP_IER_RIER12_Pos (28)
#define | GP_IER_RIER12_Msk (0x1ul << GP_IER_RIER12_Pos)
#define | GP_IER_RIER13_Pos (29)
#define | GP_IER_RIER13_Msk (0x1ul << GP_IER_RIER13_Pos)
#define | GP_IER_RIER14_Pos (30)
#define | GP_IER_RIER14_Msk (0x1ul << GP_IER_RIER14_Pos)
#define | GP_IER_RIER15_Pos (31)
#define | GP_IER_RIER15_Msk (0x1ul << GP_IER_RIER15_Pos)
#define | GP_ISRC_ISRC_Pos (0)
#define | GP_ISRC_ISRC_Msk (0xfffful << GP_ISRC_ISRC_Pos)
#define | GP_PUEN_PUEN_Pos (0)
#define | GP_PUEN_PUEN_Msk (0xfffful << GP_PUEN_PUEN_Pos)
#define | GP_DBNCECON_DBCLKSEL_Pos (0)
#define | GP_DBNCECON_DBCLKSEL_Msk (0xful << GP_DBNCECON_DBCLKSEL_Pos)
#define | GP_DBNCECON_DBCLKSRC_Pos (4)
#define | GP_DBNCECON_DBCLKSRC_Msk (0x1ul << GP_DBNCECON_DBCLKSRC_Pos)
#define | GP_DBNCECON_DBCLK_ON_Pos (5)
#define | GP_DBNCECON_DBCLK_ON_Msk (0x1ul << GP_DBNCECON_DBCLK_ON_Pos)
#define | I2C_CON_IPEN_Pos (0)
#define | I2C_CON_IPEN_Msk (0x1ul << I2C_CON_IPEN_Pos)
#define | I2C_CON_ACK_Pos (1)
#define | I2C_CON_ACK_Msk (0x1ul << I2C_CON_ACK_Pos)
#define | I2C_CON_STOP_Pos (2)
#define | I2C_CON_STOP_Msk (0x1ul << I2C_CON_STOP_Pos)
#define | I2C_CON_START_Pos (3)
#define | I2C_CON_START_Msk (0x1ul << I2C_CON_START_Pos)
#define | I2C_CON_I2C_STS_Pos (4)
#define | I2C_CON_I2C_STS_Msk (0x1ul << I2C_CON_I2C_STS_Pos)
#define | I2C_CON_INTEN_Pos (7)
#define | I2C_CON_INTEN_Msk (0x1ul << I2C_CON_INTEN_Pos)
#define | I2C_INTSTS_INTSTS_Pos (0)
#define | I2C_INTSTS_INTSTS_Msk (0x1ul << I2C_INTSTS_INTSTS_Pos)
#define | I2C_INTSTS_TIF_Pos (1)
#define | I2C_INTSTS_TIF_Msk (0x1ul << I2C_INTSTS_TIF_Pos)
#define | I2C_STATUS_STATUS_Pos (0)
#define | I2C_STATUS_STATUS_Msk (0xfful << I2C_STATUS_STATUS_Pos)
#define | I2C_DIV_CLK_DIV_Pos (0)
#define | I2C_DIV_CLK_DIV_Msk (0xfful << I2C_DIV_CLK_DIV_Pos)
#define | I2C_TOUT_TOUTEN_Pos (0)
#define | I2C_TOUT_TOUTEN_Msk (0x1ul << I2C_TOUT_TOUTEN_Pos)
#define | I2C_TOUT_DIV4_Pos (1)
#define | I2C_TOUT_DIV4_Msk (0x1ul << I2C_TOUT_DIV4_Pos)
#define | I2C_DATA_DATA_Pos (0)
#define | I2C_DATA_DATA_Msk (0xfful << I2C_DATA_DATA_Pos)
#define | I2C_SADDR0_GCALL_Pos (0)
#define | I2C_SADDR0_GCALL_Msk (0x1ul << I2C_SADDR0_GCALL_Pos)
#define | I2C_SADDR0_SADDR_Pos (1)
#define | I2C_SADDR0_SADDR_Msk (0x7ful << I2C_SADDR0_SADDR_Pos)
#define | I2C_SADDR1_GCALL_Pos (0)
#define | I2C_SADDR1_GCALL_Msk (0x1ul << I2C_SADDR1_GCALL_Pos)
#define | I2C_SADDR1_SADDR_Pos (1)
#define | I2C_SADDR1_SADDR_Msk (0x7ful << I2C_SADDR1_SADDR_Pos)
#define | I2C_SAMASK0_SAMASK_Pos (1)
#define | I2C_SAMASK0_SAMASK_Msk (0x7ful << I2C_SAMASK0_SAMASK_Pos)
#define | I2C_SAMASK1_SAMASK_Pos (1)
#define | I2C_SAMASK1_SAMASK_Msk (0x7ful << I2C_SAMASK1_SAMASK_Pos)
#define | I2C_WKUPCON_WKUPEN_Pos (0)
#define | I2C_WKUPCON_WKUPEN_Msk (0x1ul << I2C_WKUPCON_WKUPEN_Pos)
#define | I2C_WKUPSTS_WKUPIF_Pos (0)
#define | I2C_WKUPSTS_WKUPIF_Msk (0x1ul << I2C_WKUPSTS_WKUPIF_Pos)
#define | I2S_CTRL_I2SEN_Pos (0)
#define | I2S_CTRL_I2SEN_Msk (0x1ul << I2S_CTRL_I2SEN_Pos)
#define | I2S_CTRL_TXEN_Pos (1)
#define | I2S_CTRL_TXEN_Msk (0x1ul << I2S_CTRL_TXEN_Pos)
#define | I2S_CTRL_RXEN_Pos (2)
#define | I2S_CTRL_RXEN_Msk (0x1ul << I2S_CTRL_RXEN_Pos)
#define | I2S_CTRL_MUTE_Pos (3)
#define | I2S_CTRL_MUTE_Msk (0x1ul << I2S_CTRL_MUTE_Pos)
#define | I2S_CTRL_WORDWIDTH_Pos (4)
#define | I2S_CTRL_WORDWIDTH_Msk (0x3ul << I2S_CTRL_WORDWIDTH_Pos)
#define | I2S_CTRL_MONO_Pos (6)
#define | I2S_CTRL_MONO_Msk (0x1ul << I2S_CTRL_MONO_Pos)
#define | I2S_CTRL_FORMAT_Pos (7)
#define | I2S_CTRL_FORMAT_Msk (0x1ul << I2S_CTRL_FORMAT_Pos)
#define | I2S_CTRL_SLAVE_Pos (8)
#define | I2S_CTRL_SLAVE_Msk (0x1ul << I2S_CTRL_SLAVE_Pos)
#define | I2S_CTRL_TXTH_Pos (9)
#define | I2S_CTRL_TXTH_Msk (0x7ul << I2S_CTRL_TXTH_Pos)
#define | I2S_CTRL_RXTH_Pos (12)
#define | I2S_CTRL_RXTH_Msk (0x7ul << I2S_CTRL_RXTH_Pos)
#define | I2S_CTRL_MCLKEN_Pos (15)
#define | I2S_CTRL_MCLKEN_Msk (0x1ul << I2S_CTRL_MCLKEN_Pos)
#define | I2S_CTRL_RCHZCEN_Pos (16)
#define | I2S_CTRL_RCHZCEN_Msk (0x1ul << I2S_CTRL_RCHZCEN_Pos)
#define | I2S_CTRL_LCHZCEN_Pos (17)
#define | I2S_CTRL_LCHZCEN_Msk (0x1ul << I2S_CTRL_LCHZCEN_Pos)
#define | I2S_CTRL_CLR_TXFIFO_Pos (18)
#define | I2S_CTRL_CLR_TXFIFO_Msk (0x1ul << I2S_CTRL_CLR_TXFIFO_Pos)
#define | I2S_CTRL_CLR_RXFIFO_Pos (19)
#define | I2S_CTRL_CLR_RXFIFO_Msk (0x1ul << I2S_CTRL_CLR_RXFIFO_Pos)
#define | I2S_CTRL_TXDMA_Pos (20)
#define | I2S_CTRL_TXDMA_Msk (0x1ul << I2S_CTRL_TXDMA_Pos)
#define | I2S_CTRL_RXDMA_Pos (21)
#define | I2S_CTRL_RXDMA_Msk (0x1ul << I2S_CTRL_RXDMA_Pos)
#define | I2S_CTRL_RXLCH_Pos (23)
#define | I2S_CTRL_RXLCH_Msk (0x1ul << I2S_CTRL_RXLCH_Pos)
#define | I2S_CLKDIV_MCLK_DIV_Pos (0)
#define | I2S_CLKDIV_MCLK_DIV_Msk (0x7ul << I2S_CLKDIV_MCLK_DIV_Pos)
#define | I2S_CLKDIV_BCLK_DIV_Pos (8)
#define | I2S_CLKDIV_BCLK_DIV_Msk (0xfful << I2S_CLKDIV_BCLK_DIV_Pos)
#define | I2S_INTEN_RXUDFIE_Pos (0)
#define | I2S_INTEN_RXUDFIE_Msk (0x1ul << I2S_INTEN_RXUDFIE_Pos)
#define | I2S_INTEN_RXOVFIE_Pos (1)
#define | I2S_INTEN_RXOVFIE_Msk (0x1ul << I2S_INTEN_RXOVFIE_Pos)
#define | I2S_INTEN_RXTHIE_Pos (2)
#define | I2S_INTEN_RXTHIE_Msk (0x1ul << I2S_INTEN_RXTHIE_Pos)
#define | I2S_INTEN_TXUDFIE_Pos (8)
#define | I2S_INTEN_TXUDFIE_Msk (0x1ul << I2S_INTEN_TXUDFIE_Pos)
#define | I2S_INTEN_TXOVFIE_Pos (9)
#define | I2S_INTEN_TXOVFIE_Msk (0x1ul << I2S_INTEN_TXOVFIE_Pos)
#define | I2S_INTEN_TXTHIE_Pos (10)
#define | I2S_INTEN_TXTHIE_Msk (0x1ul << I2S_INTEN_TXTHIE_Pos)
#define | I2S_INTEN_RZCIE_Pos (11)
#define | I2S_INTEN_RZCIE_Msk (0x1ul << I2S_INTEN_RZCIE_Pos)
#define | I2S_INTEN_LZCIE_Pos (12)
#define | I2S_INTEN_LZCIE_Msk (0x1ul << I2S_INTEN_LZCIE_Pos)
#define | I2S_STATUS_I2SINT_Pos (0)
#define | I2S_STATUS_I2SINT_Msk (0x1ul << I2S_STATUS_I2SINT_Pos)
#define | I2S_STATUS_I2SRXINT_Pos (1)
#define | I2S_STATUS_I2SRXINT_Msk (0x1ul << I2S_STATUS_I2SRXINT_Pos)
#define | I2S_STATUS_I2STXINT_Pos (2)
#define | I2S_STATUS_I2STXINT_Msk (0x1ul << I2S_STATUS_I2STXINT_Pos)
#define | I2S_STATUS_RIGHT_Pos (3)
#define | I2S_STATUS_RIGHT_Msk (0x1ul << I2S_STATUS_RIGHT_Pos)
#define | I2S_STATUS_RXUDF_Pos (8)
#define | I2S_STATUS_RXUDF_Msk (0x1ul << I2S_STATUS_RXUDF_Pos)
#define | I2S_STATUS_RXOVF_Pos (9)
#define | I2S_STATUS_RXOVF_Msk (0x1ul << I2S_STATUS_RXOVF_Pos)
#define | I2S_STATUS_RXTHF_Pos (10)
#define | I2S_STATUS_RXTHF_Msk (0x1ul << I2S_STATUS_RXTHF_Pos)
#define | I2S_STATUS_RXFULL_Pos (11)
#define | I2S_STATUS_RXFULL_Msk (0x1ul << I2S_STATUS_RXFULL_Pos)
#define | I2S_STATUS_RXEMPTY_Pos (12)
#define | I2S_STATUS_RXEMPTY_Msk (0x1ul << I2S_STATUS_RXEMPTY_Pos)
#define | I2S_STATUS_TXUDF_Pos (16)
#define | I2S_STATUS_TXUDF_Msk (0x1ul << I2S_STATUS_TXUDF_Pos)
#define | I2S_STATUS_TXOVF_Pos (17)
#define | I2S_STATUS_TXOVF_Msk (0x1ul << I2S_STATUS_TXOVF_Pos)
#define | I2S_STATUS_TXTHF_Pos (18)
#define | I2S_STATUS_TXTHF_Msk (0x1ul << I2S_STATUS_TXTHF_Pos)
#define | I2S_STATUS_TXFULL_Pos (19)
#define | I2S_STATUS_TXFULL_Msk (0x1ul << I2S_STATUS_TXFULL_Pos)
#define | I2S_STATUS_TXEMPTY_Pos (20)
#define | I2S_STATUS_TXEMPTY_Msk (0x1ul << I2S_STATUS_TXEMPTY_Pos)
#define | I2S_STATUS_TXBUSY_Pos (21)
#define | I2S_STATUS_TXBUSY_Msk (0x1ul << I2S_STATUS_TXBUSY_Pos)
#define | I2S_STATUS_RZCF_Pos (22)
#define | I2S_STATUS_RZCF_Msk (0x1ul << I2S_STATUS_RZCF_Pos)
#define | I2S_STATUS_LZCF_Pos (23)
#define | I2S_STATUS_LZCF_Msk (0x1ul << I2S_STATUS_LZCF_Pos)
#define | I2S_STATUS_RX_LEVEL_Pos (24)
#define | I2S_STATUS_RX_LEVEL_Msk (0xful << I2S_STATUS_RX_LEVEL_Pos)
#define | I2S_STATUS_TX_LEVEL_Pos (28)
#define | I2S_STATUS_TX_LEVEL_Msk (0xful << I2S_STATUS_TX_LEVEL_Pos)
#define | I2S_TXFIFO_TXFIFO_Pos (0)
#define | I2S_TXFIFO_TXFIFO_Msk (0xfffffffful << I2S_TXFIFO_TXFIFO_Pos)
#define | I2S_RXFIFO_RXFIFO_Pos (0)
#define | I2S_RXFIFO_RXFIFO_Msk (0xfffffffful << I2S_RXFIFO_RXFIFO_Pos)
#define | INTR_IRQSRC_INT_SRC_Pos (0)
#define | INTR_IRQSRC_INT_SRC_Msk (0xful << INTR_IRQ0SRC_INT_SRC_Pos)
#define | INTR_NMI_SEL_NMISEL_Pos (0)
#define | INTR_NMI_SEL_NMISEL_Msk (0x1ful << INTR_NMI_SEL_NMISEL_Pos)
#define | INTR_MCU_IRQ_MCU_IRQ_Pos (0)
#define | INTR_MCU_IRQ_MCU_IRQ_Msk (0xfffffffful << INTR_MCU_IRQ_MCU_IRQ_Pos)
#define | LCD_CTL_EN_Pos (0)
#define | LCD_CTL_EN_Msk (0x1ul << LCD_CTL_EN_Pos)
#define | LCD_CTL_MUX_Pos (1)
#define | LCD_CTL_MUX_Msk (0x7ul << LCD_CTL_MUX_Pos)
#define | LCD_CTL_FREQ_Pos (4)
#define | LCD_CTL_FREQ_Msk (0x7ul << LCD_CTL_FREQ_Pos)
#define | LCD_CTL_BLINK_Pos (7)
#define | LCD_CTL_BLINK_Msk (0x1ul << LCD_CTL_BLINK_Pos)
#define | LCD_CTL_PDDISP_EN_Pos (8)
#define | LCD_CTL_PDDISP_EN_Msk (0x1ul << LCD_CTL_PDDISP_EN_Pos)
#define | LCD_CTL_PDINT_EN_Pos (9)
#define | LCD_CTL_PDINT_EN_Msk (0x1ul << LCD_CTL_PDINT_EN_Pos)
#define | LCD_DISPCTL_CPUMP_EN_Pos (0)
#define | LCD_DISPCTL_CPUMP_EN_Msk (0x1ul << LCD_DISPCTL_CPUMP_EN_Pos)
#define | LCD_DISPCTL_BIAS_SEL_Pos (1)
#define | LCD_DISPCTL_BIAS_SEL_Msk (0x3ul << LCD_DISPCTL_BIAS_SEL_Pos)
#define | LCD_DISPCTL_IBRL_EN_Pos (4)
#define | LCD_DISPCTL_IBRL_EN_Msk (0x1ul << LCD_DISPCTL_IBRL_EN_Pos)
#define | LCD_DISPCTL_BV_SEL_Pos (6)
#define | LCD_DISPCTL_BV_SEL_Msk (0x1ul << LCD_DISPCTL_BV_SEL_Pos)
#define | LCD_DISPCTL_CPUMP_VOL_SET_Pos (8)
#define | LCD_DISPCTL_CPUMP_VOL_SET_Msk (0x7ul << LCD_DISPCTL_CPUMP_VOL_SET_Pos)
#define | LCD_DISPCTL_CPUMP_FREQ_Pos (11)
#define | LCD_DISPCTL_CPUMP_FREQ_Msk (0x7ul << LCD_DISPCTL_CPUMP_FREQ_Pos)
#define | LCD_MEM_0_SEG_0_4x_Pos (0)
#define | LCD_MEM_0_SEG_0_4x_Msk (0x3ful << LCD_MEM_0_SEG_0_4x_Pos)
#define | LCD_MEM_0_SEG_1_4x_Pos (8)
#define | LCD_MEM_0_SEG_1_4x_Msk (0x7ful << LCD_MEM_0_SEG_1_4x_Pos)
#define | LCD_MEM_0_SEG_2_4x_Pos (16)
#define | LCD_MEM_0_SEG_2_4x_Msk (0x3ful << LCD_MEM_0_SEG_2_4x_Pos)
#define | LCD_MEM_0_SEG_3_4x_Pos (24)
#define | LCD_MEM_0_SEG_3_4x_Msk (0x3ful << LCD_MEM_0_SEG_3_4x_Pos)
#define | LCD_MEM_1_SEG_0_4x_Pos (0)
#define | LCD_MEM_1_SEG_0_4x_Msk (0x3ful << LCD_MEM_1_SEG_0_4x_Pos)
#define | LCD_MEM_1_SEG_1_4x_Pos (8)
#define | LCD_MEM_1_SEG_1_4x_Msk (0x7ful << LCD_MEM_1_SEG_1_4x_Pos)
#define | LCD_MEM_1_SEG_2_4x_Pos (16)
#define | LCD_MEM_1_SEG_2_4x_Msk (0x3ful << LCD_MEM_1_SEG_2_4x_Pos)
#define | LCD_MEM_1_SEG_3_4x_Pos (24)
#define | LCD_MEM_1_SEG_3_4x_Msk (0x3ful << LCD_MEM_1_SEG_3_4x_Pos)
#define | LCD_MEM_2_SEG_0_4x_Pos (0)
#define | LCD_MEM_2_SEG_0_4x_Msk (0x3ful << LCD_MEM_2_SEG_0_4x_Pos)
#define | LCD_MEM_2_SEG_1_4x_Pos (8)
#define | LCD_MEM_2_SEG_1_4x_Msk (0x7ful << LCD_MEM_2_SEG_1_4x_Pos)
#define | LCD_MEM_2_SEG_2_4x_Pos (16)
#define | LCD_MEM_2_SEG_2_4x_Msk (0x3ful << LCD_MEM_2_SEG_2_4x_Pos)
#define | LCD_MEM_2_SEG_3_4x_Pos (24)
#define | LCD_MEM_2_SEG_3_4x_Msk (0x3ful << LCD_MEM_2_SEG_3_4x_Pos)
#define | LCD_MEM_3_SEG_0_4x_Pos (0)
#define | LCD_MEM_3_SEG_0_4x_Msk (0x3ful << LCD_MEM_3_SEG_0_4x_Pos)
#define | LCD_MEM_3_SEG_1_4x_Pos (8)
#define | LCD_MEM_3_SEG_1_4x_Msk (0x7ful << LCD_MEM_3_SEG_1_4x_Pos)
#define | LCD_MEM_3_SEG_2_4x_Pos (16)
#define | LCD_MEM_3_SEG_2_4x_Msk (0x3ful << LCD_MEM_3_SEG_2_4x_Pos)
#define | LCD_MEM_3_SEG_3_4x_Pos (24)
#define | LCD_MEM_3_SEG_3_4x_Msk (0x3ful << LCD_MEM_3_SEG_3_4x_Pos)
#define | LCD_MEM_4_SEG_0_4x_Pos (0)
#define | LCD_MEM_4_SEG_0_4x_Msk (0x3ful << LCD_MEM_4_SEG_0_4x_Pos)
#define | LCD_MEM_4_SEG_1_4x_Pos (8)
#define | LCD_MEM_4_SEG_1_4x_Msk (0x7ful << LCD_MEM_4_SEG_1_4x_Pos)
#define | LCD_MEM_4_SEG_2_4x_Pos (16)
#define | LCD_MEM_4_SEG_2_4x_Msk (0x3ful << LCD_MEM_4_SEG_2_4x_Pos)
#define | LCD_MEM_4_SEG_3_4x_Pos (24)
#define | LCD_MEM_4_SEG_3_4x_Msk (0x3ful << LCD_MEM_4_SEG_3_4x_Pos)
#define | LCD_MEM_5_SEG_0_4x_Pos (0)
#define | LCD_MEM_5_SEG_0_4x_Msk (0x3ful << LCD_MEM_5_SEG_0_4x_Pos)
#define | LCD_MEM_5_SEG_1_4x_Pos (8)
#define | LCD_MEM_5_SEG_1_4x_Msk (0x7ful << LCD_MEM_5_SEG_1_4x_Pos)
#define | LCD_MEM_5_SEG_2_4x_Pos (16)
#define | LCD_MEM_5_SEG_2_4x_Msk (0x3ful << LCD_MEM_5_SEG_2_4x_Pos)
#define | LCD_MEM_5_SEG_3_4x_Pos (24)
#define | LCD_MEM_5_SEG_3_4x_Msk (0x3ful << LCD_MEM_5_SEG_3_4x_Pos)
#define | LCD_MEM_6_SEG_0_4x_Pos (0)
#define | LCD_MEM_6_SEG_0_4x_Msk (0x3ful << LCD_MEM_6_SEG_0_4x_Pos)
#define | LCD_MEM_6_SEG_1_4x_Pos (8)
#define | LCD_MEM_6_SEG_1_4x_Msk (0x7ful << LCD_MEM_6_SEG_1_4x_Pos)
#define | LCD_MEM_6_SEG_2_4x_Pos (16)
#define | LCD_MEM_6_SEG_2_4x_Msk (0x3ful << LCD_MEM_6_SEG_2_4x_Pos)
#define | LCD_MEM_6_SEG_3_4x_Pos (24)
#define | LCD_MEM_6_SEG_3_4x_Msk (0x3ful << LCD_MEM_6_SEG_3_4x_Pos)
#define | LCD_MEM_7_SEG_0_4x_Pos (0)
#define | LCD_MEM_7_SEG_0_4x_Msk (0x3ful << LCD_MEM_7_SEG_0_4x_Pos)
#define | LCD_MEM_7_SEG_1_4x_Pos (8)
#define | LCD_MEM_7_SEG_1_4x_Msk (0x7ful << LCD_MEM_7_SEG_1_4x_Pos)
#define | LCD_MEM_7_SEG_2_4x_Pos (16)
#define | LCD_MEM_7_SEG_2_4x_Msk (0x3ful << LCD_MEM_7_SEG_2_4x_Pos)
#define | LCD_MEM_7_SEG_3_4x_Pos (24)
#define | LCD_MEM_7_SEG_3_4x_Msk (0x3ful << LCD_MEM_7_SEG_3_4x_Pos)
#define | LCD_MEM_8_SEG_0_4x_Pos (0)
#define | LCD_MEM_8_SEG_0_4x_Msk (0x3ful << LCD_MEM_8_SEG_0_4x_Pos)
#define | LCD_MEM_8_SEG_1_4x_Pos (8)
#define | LCD_MEM_8_SEG_1_4x_Msk (0x7ful << LCD_MEM_8_SEG_1_4x_Pos)
#define | LCD_MEM_8_SEG_2_4x_Pos (16)
#define | LCD_MEM_8_SEG_2_4x_Msk (0x3ful << LCD_MEM_8_SEG_2_4x_Pos)
#define | LCD_MEM_8_SEG_3_4x_Pos (24)
#define | LCD_MEM_8_SEG_3_4x_Msk (0x3ful << LCD_MEM_8_SEG_3_4x_Pos)
#define | LCD_MEM_9_SEG_0_4x_Pos (0)
#define | LCD_MEM_9_SEG_0_4x_Msk (0x3ful << LCD_MEM_9_SEG_0_4x_Pos)
#define | LCD_MEM_9_SEG_1_4x_Pos (8)
#define | LCD_MEM_9_SEG_1_4x_Msk (0x7ful << LCD_MEM_9_SEG_1_4x_Pos)
#define | LCD_MEM_9_SEG_2_4x_Pos (16)
#define | LCD_MEM_9_SEG_2_4x_Msk (0x3ful << LCD_MEM_9_SEG_2_4x_Pos)
#define | LCD_MEM_9_SEG_3_4x_Pos (24)
#define | LCD_MEM_9_SEG_3_4x_Msk (0x3ful << LCD_MEM_9_SEG_3_4x_Pos)
#define | LCD_FCR_FCEN_Pos (0)
#define | LCD_FCR_FCEN_Msk (0x1ul << LCD_FCR_FCEN_Pos)
#define | LCD_FCR_FCINTEN_Pos (1)
#define | LCD_FCR_FCINTEN_Msk (0x1ul << LCD_FCR_FCINTEN_Pos)
#define | LCD_FCR_PRESCL_Pos (2)
#define | LCD_FCR_PRESCL_Msk (0x3ul << LCD_FCR_PRESCL_Pos)
#define | LCD_FCR_FCV_Pos (4)
#define | LCD_FCR_FCV_Msk (0x3ful << LCD_FCR_FCV_Pos)
#define | LCD_FCSTS_FCSTS_Pos (0)
#define | LCD_FCSTS_FCSTS_Msk (0x1ul << LCD_FCSTS_FCSTS_Pos)
#define | LCD_FCSTS_PDSTS_Pos (1)
#define | LCD_FCSTS_PDSTS_Msk (0x1ul << LCD_FCSTS_PDSTS_Pos)
#define | DMA_CRC_CTL_CRCCEN_Pos (0)
#define | DMA_CRC_CTL_CRCCEN_Msk (0x1ul << DMA_CRC_CTL_CRCCEN_Pos)
#define | DMA_CRC_CTL_CRC_RST_Pos (1)
#define | DMA_CRC_CTL_CRC_RST_Msk (0x1ul << DMA_CRC_CTL_CRC_RST_Pos)
#define | DMA_CRC_CTL_TRIG_EN_Pos (23)
#define | DMA_CRC_CTL_TRIG_EN_Msk (0x1ul << DMA_CRC_CTL_TRIG_EN_Pos)
#define | DMA_CRC_CTL_WDATA_RVS_Pos (24)
#define | DMA_CRC_CTL_WDATA_RVS_Msk (0x1ul << DMA_CRC_CTL_WDATA_RVS_Pos)
#define | DMA_CRC_CTL_CHECKSUM_RVS_Pos (25)
#define | DMA_CRC_CTL_CHECKSUM_RVS_Msk (0x1ul << DMA_CRC_CTL_CHECKSUM_RVS_Pos)
#define | DMA_CRC_CTL_WDATA_COM_Pos (26)
#define | DMA_CRC_CTL_WDATA_COM_Msk (0x1ul << DMA_CRC_CTL_WDATA_COM_Pos)
#define | DMA_CRC_CTL_CHECKSUM_COM_Pos (27)
#define | DMA_CRC_CTL_CHECKSUM_COM_Msk (0x1ul << DMA_CRC_CTL_CHECKSUM_COM_Pos)
#define | DMA_CRC_CTL_CPU_WDLEN_Pos (28)
#define | DMA_CRC_CTL_CPU_WDLEN_Msk (0x3ul << DMA_CRC_CTL_CPU_WDLEN_Pos)
#define | DMA_CRC_CTL_CRC_MODE_Pos (30)
#define | DMA_CRC_CTL_CRC_MODE_Msk (0x3ul << DMA_CRC_CTL_CRC_MODE_Pos)
#define | DMA_CRC_DMASAR_CRC_DMASAR_Pos (0)
#define | DMA_CRC_DMASAR_CRC_DMASAR_Msk (0xfffffffful << DMA_CRC_DMASAR_CRC_DMASAR_Pos)
#define | DMA_CRC_DMABCR_CRC_DMABCR_Pos (0)
#define | DMA_CRC_DMABCR_CRC_DMABCR_Msk (0xfffful << DMA_CRC_DMABCR_CRC_DMABCR_Pos)
#define | DMA_CRC_DMACSAR_CRC_DMACSAR_Pos (0)
#define | DMA_CRC_DMACSAR_CRC_DMACSAR_Msk (0xfffffffful << DMA_CRC_DMACSAR_CRC_DMACSAR_Pos)
#define | DMA_CRC_DMACBCR_CRC_DMACBCR_Pos (0)
#define | DMA_CRC_DMACBCR_CRC_DMACBCR_Msk (0xfffful << DMA_CRC_DMACBCR_CRC_DMACBCR_Pos)
#define | DMA_CRC_DMAIER_TABORT_IE_Pos (0)
#define | DMA_CRC_DMAIER_TABORT_IE_Msk (0x1ul << DMA_CRC_DMAIER_TABORT_IE_Pos)
#define | DMA_CRC_DMAIER_BLKD_IE_Pos (1)
#define | DMA_CRC_DMAIER_BLKD_IE_Msk (0x1ul << DMA_CRC_DMAIER_BLKD_IE_Pos)
#define | DMA_CRC_DMAISR_TABORT_IF_Pos (0)
#define | DMA_CRC_DMAISR_TABORT_IF_Msk (0x1ul << DMA_CRC_DMAISR_TABORT_IF_Pos)
#define | DMA_CRC_DMAISR_BLKD_IF_Pos (1)
#define | DMA_CRC_DMAISR_BLKD_IF_Msk (0x1ul << DMA_CRC_DMAISR_BLKD_IF_Pos)
#define | DMA_CRC_WDATA_CRC_WDATA_Pos (0)
#define | DMA_CRC_WDATA_CRC_WDATA_Msk (0xfffffffful << DMA_CRC_WDATA_CRC_WDATA_Pos)
#define | DMA_CRC_SEED_CRC_SEED_Pos (0)
#define | DMA_CRC_SEED_CRC_SEED_Msk (0xfffffffful << DMA_CRC_SEED_CRC_SEED_Pos)
#define | DMA_CRC_CHECKSUM_CRC_CHECKSUM_Pos (0)
#define | DMA_CRC_CHECKSUM_CRC_CHECKSUM_Msk (0xfffffffful << DMA_CRC_CHECKSUM_CRC_CHECKSUM_Pos)
#define | DMA_GCR_GCRCSR_CLK0_EN_Pos (8)
#define | DMA_GCR_GCRCSR_CLK0_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK0_EN_Pos)
#define | DMA_GCR_GCRCSR_CLK1_EN_Pos (9)
#define | DMA_GCR_GCRCSR_CLK1_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK1_EN_Pos)
#define | DMA_GCR_GCRCSR_CLK2_EN_Pos (10)
#define | DMA_GCR_GCRCSR_CLK2_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK2_EN_Pos)
#define | DMA_GCR_GCRCSR_CLK3_EN_Pos (11)
#define | DMA_GCR_GCRCSR_CLK3_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK3_EN_Pos)
#define | DMA_GCR_GCRCSR_CLK4_EN_Pos (12)
#define | DMA_GCR_GCRCSR_CLK4_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK4_EN_Pos)
#define | DMA_GCR_GCRCSR_CLK5_EN_Pos (13)
#define | DMA_GCR_GCRCSR_CLK5_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK5_EN_Pos)
#define | DMA_GCR_GCRCSR_CLK6_EN_Pos (14)
#define | DMA_GCR_GCRCSR_CLK6_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK6_EN_Pos)
#define | DMA_GCR_GCRCSR_CRC_CLK_EN_Pos (24)
#define | DMA_GCR_GCRCSR_CRC_CLK_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CRC_CLK_EN_Pos)
#define | DMA_GCR_DSSR0_CH1_SEL_Pos (8)
#define | DMA_GCR_DSSR0_CH1_SEL_Msk (0x1ful << DMA_GCR_DSSR0_CH1_SEL_Pos)
#define | DMA_GCR_DSSR0_CH2_SEL_Pos (16)
#define | DMA_GCR_DSSR0_CH2_SEL_Msk (0x1ful << DMA_GCR_DSSR0_CH2_SEL_Pos)
#define | DMA_GCR_DSSR0_CH3_SEL_Pos (24)
#define | DMA_GCR_DSSR0_CH3_SEL_Msk (0x1ful << DMA_GCR_DSSR0_CH3_SEL_Pos)
#define | DMA_GCR_DSSR1_CH4_SEL_Pos (0)
#define | DMA_GCR_DSSR1_CH4_SEL_Msk (0x1ful << DMA_GCR_DSSR1_CH4_SEL_Pos)
#define | DMA_GCR_DSSR1_CH5_SEL_Pos (8)
#define | DMA_GCR_DSSR1_CH5_SEL_Msk (0x1ful << DMA_GCR_DSSR1_CH5_SEL_Pos)
#define | DMA_GCR_DSSR1_CH6_SEL_Pos (16)
#define | DMA_GCR_DSSR1_CH6_SEL_Msk (0x1ful << DMA_GCR_DSSR1_CH6_SEL_Pos)
#define | DMA_GCR_GCRISR_INTR0_Pos (0)
#define | DMA_GCR_GCRISR_INTR0_Msk (0x1ul << DMA_GCR_GCRISR_INTR0_Pos)
#define | DMA_GCR_GCRISR_INTR1_Pos (1)
#define | DMA_GCR_GCRISR_INTR1_Msk (0x1ul << DMA_GCR_GCRISR_INTR1_Pos)
#define | DMA_GCR_GCRISR_INTR2_Pos (2)
#define | DMA_GCR_GCRISR_INTR2_Msk (0x1ul << DMA_GCR_GCRISR_INTR2_Pos)
#define | DMA_GCR_GCRISR_INTR3_Pos (3)
#define | DMA_GCR_GCRISR_INTR3_Msk (0x1ul << DMA_GCR_GCRISR_INTR3_Pos)
#define | DMA_GCR_GCRISR_INTR4_Pos (4)
#define | DMA_GCR_GCRISR_INTR4_Msk (0x1ul << DMA_GCR_GCRISR_INTR4_Pos)
#define | DMA_GCR_GCRISR_INTR5_Pos (5)
#define | DMA_GCR_GCRISR_INTR5_Msk (0x1ul << DMA_GCR_GCRISR_INTR5_Pos)
#define | DMA_GCR_GCRISR_INTR6_Pos (6)
#define | DMA_GCR_GCRISR_INTR6_Msk (0x1ul << DMA_GCR_GCRISR_INTR6_Pos)
#define | DMA_GCR_GCRISR_CRC_INTR_Pos (16)
#define | DMA_GCR_GCRISR_CRC_INTR_Msk (0x1ul << DMA_GCR_GCRISR_CRC_INTR_Pos)
#define | PDMA_CSR_PDMACEN_Pos (0)
#define | PDMA_CSR_PDMACEN_Msk (0x1ul << PDMA_CSR_PDMACEN_Pos)
#define | PDMA_CSR_SW_RST_Pos (1)
#define | PDMA_CSR_SW_RST_Msk (0x1ul << PDMA_CSR_SW_RST_Pos)
#define | PDMA_CSR_MODE_SEL_Pos (2)
#define | PDMA_CSR_MODE_SEL_Msk (0x3ul << PDMA_CSR_MODE_SEL_Pos)
#define | PDMA_CSR_SAD_SEL_Pos (4)
#define | PDMA_CSR_SAD_SEL_Msk (0x3ul << PDMA_CSR_SAD_SEL_Pos)
#define | PDMA_CSR_DAD_SEL_Pos (6)
#define | PDMA_CSR_DAD_SEL_Msk (0x3ul << PDMA_CSR_DAD_SEL_Pos)
#define | PDMA_CSR_TO_EN_Pos (12)
#define | PDMA_CSR_TO_EN_Msk (0x1ul << PDMA_CSR_TO_EN_Pos)
#define | PDMA_CSR_APB_TWS_Pos (19)
#define | PDMA_CSR_APB_TWS_Msk (0x3ul << PDMA_CSR_APB_TWS_Pos)
#define | PDMA_CSR_TRIG_EN_Pos (23)
#define | PDMA_CSR_TRIG_EN_Msk (0x1ul << PDMA_CSR_TRIG_EN_Pos)
#define | PDMA_SAR_PDMA_SAR_Pos (0)
#define | PDMA_SAR_PDMA_SAR_Msk (0xfffffffful << PDMA_SAR_PDMA_SAR_Pos)
#define | PDMA_DAR_PDMA_DAR_Pos (0)
#define | PDMA_DAR_PDMA_DAR_Msk (0xfffffffful << PDMA_DAR_PDMA_DAR_Pos)
#define | PDMA_BCR_PDMA_BCR_Pos (0)
#define | PDMA_BCR_PDMA_BCR_Msk (0xfffful << PDMA_BCR_PDMA_BCR_Pos)
#define | PDMA_CSAR_PDMA_CSAR_Pos (0)
#define | PDMA_CSAR_PDMA_CSAR_Msk (0xfffffffful << PDMA_CSAR_PDMA_CSAR_Pos)
#define | PDMA_CDAR_PDMA_CDAR_Pos (0)
#define | PDMA_CDAR_PDMA_CDAR_Msk (0xfffffffful << PDMA_CDAR_PDMA_CDAR_Pos)
#define | PDMA_CBCR_PDMA_CBCR_Pos (0)
#define | PDMA_CBCR_PDMA_CBCR_Msk (0xfffffful << PDMA_CBCR_PDMA_CBCR_Pos)
#define | PDMA_IER_TABORT_IE_Pos (0)
#define | PDMA_IER_TABORT_IE_Msk (0x1ul << PDMA_IER_TABORT_IE_Pos)
#define | PDMA_IER_TD_IE_Pos (1)
#define | PDMA_IER_TD_IE_Msk (0x1ul << PDMA_IER_TD_IE_Pos)
#define | PDMA_IER_WRA_BCR_IE_Pos (2)
#define | PDMA_IER_WRA_BCR_IE_Msk (0xful << PDMA_IER_WRA_BCR_IE_Pos)
#define | PDMA_IER_TO_IE_Pos (6)
#define | PDMA_IER_TO_IE_Msk (0x1ul << PDMA_IER_TO_IE_Pos)
#define | PDMA_ISR_TABORT_IS_Pos (0)
#define | PDMA_ISR_TABORT_IS_Msk (0x1ul << PDMA_ISR_TABORT_IS_Pos)
#define | PDMA_ISR_TD_IS_Pos (1)
#define | PDMA_ISR_TD_IS_Msk (0x1ul << PDMA_ISR_TD_IS_Pos)
#define | PDMA_ISR_WRA_BCR_IS_Pos (2)
#define | PDMA_ISR_WRA_BCR_IS_Msk (0xful << PDMA_ISR_WRA_BCR_IS_Pos)
#define | PDMA_ISR_TO_IS_Pos (6)
#define | PDMA_ISR_TO_IS_Msk (0x1ul << PDMA_ISR_TO_IS_Pos)
#define | PDMA_TCR_PDMA_TCR_Pos (0)
#define | PDMA_TCR_PDMA_TCR_Msk (0xfffful << PDMA_TCR_PDMA_TCR_Pos)
#define | VDMA_CSR_VDMACEN_Pos (0)
#define | VDMA_CSR_VDMACEN_Msk (0x1ul << VDMA_CSR_VDMACEN_Pos)
#define | VDMA_CSR_SW_RST_Pos (1)
#define | VDMA_CSR_SW_RST_Msk (0x1ul << VDMA_CSR_SW_RST_Pos)
#define | VDMA_CSR_STRIDE_EN_Pos (10)
#define | VDMA_CSR_STRIDE_EN_Msk (0x1ul << VDMA_CSR_STRIDE_EN_Pos)
#define | VDMA_CSR_DIR_SEL_Pos (11)
#define | VDMA_CSR_DIR_SEL_Msk (0x1ul << VDMA_CSR_DIR_SEL_Pos)
#define | VDMA_CSR_TRIG_EN_Pos (23)
#define | VDMA_CSR_TRIG_EN_Msk (0x1ul << VDMA_CSR_TRIG_EN_Pos)
#define | VDMA_SAR_VDMA_SAR_Pos (0)
#define | VDMA_SAR_VDMA_SAR_Msk (0xfffffffful << VDMA_SAR_VDMA_SAR_Pos)
#define | VDMA_DAR_VDMA_DAR_Pos (0)
#define | VDMA_DAR_VDMA_DAR_Msk (0xfffffffful << VDMA_DAR_VDMA_DAR_Pos)
#define | VDMA_BCR_VDMA_BCR_Pos (0)
#define | VDMA_BCR_VDMA_BCR_Msk (0xfffful << VDMA_BCR_VDMA_BCR_Pos)
#define | VDMA_CSAR_VDMA_CSAR_Pos (0)
#define | VDMA_CSAR_VDMA_CSAR_Msk (0xfffffffful << VDMA_CSAR_VDMA_CSAR_Pos)
#define | VDMA_CDAR_VDMA_CDAR_Pos (0)
#define | VDMA_CDAR_VDMA_CDAR_Msk (0xfffffffful << VDMA_CDAR_VDMA_CDAR_Pos)
#define | VDMA_CBCR_VDMA_CBCR_Pos (0)
#define | VDMA_CBCR_VDMA_CBCR_Msk (0xfffful << VDMA_CBCR_VDMA_CBCR_Pos)
#define | VDMA_IER_TABORT_IE_Pos (0)
#define | VDMA_IER_TABORT_IE_Msk (0x1ul << VDMA_IER_TABORT_IE_Pos)
#define | VDMA_IER_TD_IE_Pos (1)
#define | VDMA_IER_TD_IE_Msk (0x1ul << VDMA_IER_TD_IE_Pos)
#define | VDMA_ISR_TABORT_IS_Pos (0)
#define | VDMA_ISR_TABORT_IS_Msk (0x1ul << VDMA_ISR_TABORT_IS_Pos)
#define | VDMA_ISR_TD_IS_Pos (1)
#define | VDMA_ISR_TD_IS_Msk (0x1ul << VDMA_ISR_TD_IS_Pos)
#define | VDMA_SASOCR_SASTOBL_Pos (0)
#define | VDMA_SASOCR_SASTOBL_Msk (0xfffful << VDMA_SASOCR_SASTOBL_Pos)
#define | VDMA_SASOCR_STBC_Pos (16)
#define | VDMA_SASOCR_STBC_Msk (0xfffful << VDMA_SASOCR_STBC_Pos)
#define | VDMA_DASOCR_DASTOBL_Pos (0)
#define | VDMA_DASOCR_DASTOBL_Msk (0xfffful << VDMA_DASOCR_DASTOBL_Pos)
#define | PWM_PRES_CP01_Pos (0)
#define | PWM_PRES_CP01_Msk (0xfful << PWM_PRES_CP01_Pos)
#define | PWM_PRES_CP23_Pos (8)
#define | PWM_PRES_CP23_Msk (0xfful << PWM_PRES_CP23_Pos)
#define | PWM_PRES_DZ01_Pos (16)
#define | PWM_PRES_DZ01_Msk (0xfful << PWM_PRES_DZ01_Pos)
#define | PWM_PRES_DZ23_Pos (24)
#define | PWM_PRES_DZ23_Msk (0xfful << PWM_PRES_DZ23_Pos)
#define | PWM_CLKSEL_CLKSEL0_Pos (0)
#define | PWM_CLKSEL_CLKSEL0_Msk (0x7ul << PWM_CLKSEL_CLKSEL0_Pos)
#define | PWM_CLKSEL_CLKSEL1_Pos (4)
#define | PWM_CLKSEL_CLKSEL1_Msk (0x7ul << PWM_CLKSEL_CLKSEL1_Pos)
#define | PWM_CLKSEL_CLKSEL2_Pos (8)
#define | PWM_CLKSEL_CLKSEL2_Msk (0x7ul << PWM_CLKSEL_CLKSEL2_Pos)
#define | PWM_CLKSEL_CLKSEL3_Pos (12)
#define | PWM_CLKSEL_CLKSEL3_Msk (0x7ul << PWM_CLKSEL_CLKSEL3_Pos)
#define | PWM_CTL_CH0EN_Pos (0)
#define | PWM_CTL_CH0EN_Msk (0x1ul << PWM_CTL_CH0EN_Pos)
#define | PWM_CTL_CH0INV_Pos (2)
#define | PWM_CTL_CH0INV_Msk (0x1ul << PWM_CTL_CH0INV_Pos)
#define | PWM_CTL_CH0MOD_Pos (3)
#define | PWM_CTL_CH0MOD_Msk (0x1ul << PWM_CTL_CH0MOD_Pos)
#define | PWM_CTL_DZEN01_Pos (4)
#define | PWM_CTL_DZEN01_Msk (0x1ul << PWM_CTL_DZEN01_Pos)
#define | PWM_CTL_DZEN23_Pos (5)
#define | PWM_CTL_DZEN23_Msk (0x1ul << PWM_CTL_DZEN23_Pos)
#define | PWM_CTL_CH1EN_Pos (8)
#define | PWM_CTL_CH1EN_Msk (0x1ul << PWM_CTL_CH1EN_Pos)
#define | PWM_CTL_CH1INV_Pos (10)
#define | PWM_CTL_CH1INV_Msk (0x1ul << PWM_CTL_CH1INV_Pos)
#define | PWM_CTL_CH1MOD_Pos (11)
#define | PWM_CTL_CH1MOD_Msk (0x1ul << PWM_CTL_CH1MOD_Pos)
#define | PWM_CTL_CH2EN_Pos (16)
#define | PWM_CTL_CH2EN_Msk (0x1ul << PWM_CTL_CH2EN_Pos)
#define | PWM_CTL_CH2INV_Pos (18)
#define | PWM_CTL_CH2INV_Msk (0x1ul << PWM_CTL_CH2INV_Pos)
#define | PWM_CTL_CH2MOD_Pos (19)
#define | PWM_CTL_CH2MOD_Msk (0x1ul << PWM_CTL_CH2MOD_Pos)
#define | PWM_CTL_CH3EN_Pos (24)
#define | PWM_CTL_CH3EN_Msk (0x1ul << PWM_CTL_CH3EN_Pos)
#define | PWM_CTL_CH3INV_Pos (26)
#define | PWM_CTL_CH3INV_Msk (0x1ul << PWM_CTL_CH3INV_Pos)
#define | PWM_CTL_CH3MOD_Pos (27)
#define | PWM_CTL_CH3MOD_Msk (0x1ul << PWM_CTL_CH3MOD_Pos)
#define | PWM_INTEN_TMIE0_Pos (0)
#define | PWM_INTEN_TMIE0_Msk (0x1ul << PWM_INTEN_TMIE0_Pos)
#define | PWM_INTEN_TMIE1_Pos (1)
#define | PWM_INTEN_TMIE1_Msk (0x1ul << PWM_INTEN_TMIE1_Pos)
#define | PWM_INTEN_TMIE2_Pos (2)
#define | PWM_INTEN_TMIE2_Msk (0x1ul << PWM_INTEN_TMIE2_Pos)
#define | PWM_INTEN_TMIE3_Pos (3)
#define | PWM_INTEN_TMIE3_Msk (0x1ul << PWM_INTEN_TMIE3_Pos)
#define | PWM_INTSTS_TMINT0_Pos (0)
#define | PWM_INTSTS_TMINT0_Msk (0x1ul << PWM_INTSTS_TMINT0_Pos)
#define | PWM_INTSTS_TMINT1_Pos (1)
#define | PWM_INTSTS_TMINT1_Msk (0x1ul << PWM_INTSTS_TMINT1_Pos)
#define | PWM_INTSTS_TMINT2_Pos (2)
#define | PWM_INTSTS_TMINT2_Msk (0x1ul << PWM_INTSTS_TMINT2_Pos)
#define | PWM_INTSTS_TMINT3_Pos (3)
#define | PWM_INTSTS_TMINT3_Msk (0x1ul << PWM_INTSTS_TMINT3_Pos)
#define | PWM_INTSTS_DUTY0SYNC_Pos (4)
#define | PWM_INTSTS_DUTY0SYNC_Msk (0x1ul << PWM_INTSTS_DUTY0SYNC_Pos)
#define | PWM_INTSTS_PRESSYNC_Pos (8)
#define | PWM_INTSTS_PRESSYNC_Msk (0x1ul << PWM_INTSTS_PRESSYNC_Pos)
#define | PWM_OE_CH0_OE_Pos (0)
#define | PWM_OE_CH0_OE_Msk (0x1ul << PWM_OE_CH0_OE_Pos)
#define | PWM_OE_CH1_OE_Pos (1)
#define | PWM_OE_CH1_OE_Msk (0x1ul << PWM_OE_CH1_OE_Pos)
#define | PWM_OE_CH2_OE_Pos (2)
#define | PWM_OE_CH2_OE_Msk (0x1ul << PWM_OE_CH2_OE_Pos)
#define | PWM_OE_CH3_OE_Pos (3)
#define | PWM_OE_CH3_OE_Msk (0x1ul << PWM_OE_CH3_OE_Pos)
#define | PWM_DUTY_CN_Pos (0)
#define | PWM_DUTY_CN_Msk (0xfffful << PWM_DUTY_CN_Pos)
#define | PWM_DUTY_CM_Pos (16)
#define | PWM_DUTY_CM_Msk (0xfffful << PWM_DUTY_CM_Pos)
#define | PWM_DATA0_PWMx_DATAy15_0_Pos (0)
#define | PWM_DATA0_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA0_PWMx_DATAy15_0_Pos)
#define | PWM_DATA0_PWMx_DATAy30_16_Pos (16)
#define | PWM_DATA0_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA0_PWMx_DATAy30_16_Pos)
#define | PWM_DATA0_sync_Pos (31)
#define | PWM_DATA0_sync_Msk (0x1ul << PWM_DATA0_sync_Pos)
#define | PWM_DUTY1_CN_Pos (0)
#define | PWM_DUTY1_CN_Msk (0xfffful << PWM_DUTY1_CN_Pos)
#define | PWM_DUTY1_CM_Pos (16)
#define | PWM_DUTY1_CM_Msk (0xfffful << PWM_DUTY1_CM_Pos)
#define | PWM_DATA1_PWMx_DATAy15_0_Pos (0)
#define | PWM_DATA1_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA1_PWMx_DATAy15_0_Pos)
#define | PWM_DATA1_PWMx_DATAy30_16_Pos (16)
#define | PWM_DATA1_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA1_PWMx_DATAy30_16_Pos)
#define | PWM_DATA1_sync_Pos (31)
#define | PWM_DATA1_sync_Msk (0x1ul << PWM_DATA1_sync_Pos)
#define | PWM_DUTY2_CN_Pos (0)
#define | PWM_DUTY2_CN_Msk (0xfffful << PWM_DUTY2_CN_Pos)
#define | PWM_DUTY2_CM_Pos (16)
#define | PWM_DUTY2_CM_Msk (0xfffful << PWM_DUTY2_CM_Pos)
#define | PWM_DATA2_PWMx_DATAy15_0_Pos (0)
#define | PWM_DATA2_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA2_PWMx_DATAy15_0_Pos)
#define | PWM_DATA2_PWMx_DATAy30_16_Pos (16)
#define | PWM_DATA2_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA2_PWMx_DATAy30_16_Pos)
#define | PWM_DATA2_sync_Pos (31)
#define | PWM_DATA2_sync_Msk (0x1ul << PWM_DATA2_sync_Pos)
#define | PWM_DUTY3_CN_Pos (0)
#define | PWM_DUTY3_CN_Msk (0xfffful << PWM_DUTY3_CN_Pos)
#define | PWM_DUTY3_CM_Pos (16)
#define | PWM_DUTY3_CM_Msk (0xfffful << PWM_DUTY3_CM_Pos)
#define | PWM_DATA3_PWMx_DATAy15_0_Pos (0)
#define | PWM_DATA3_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA3_PWMx_DATAy15_0_Pos)
#define | PWM_DATA3_PWMx_DATAy30_16_Pos (16)
#define | PWM_DATA3_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA3_PWMx_DATAy30_16_Pos)
#define | PWM_DATA3_sync_Pos (31)
#define | PWM_DATA3_sync_Msk (0x1ul << PWM_DATA3_sync_Pos)
#define | PWM_CAPCTL_INV0_Pos (0)
#define | PWM_CAPCTL_INV0_Msk (0x1ul << PWM_CAPCTL_INV0_Pos)
#define | PWM_CAPCTL_CAPCH0EN_Pos (1)
#define | PWM_CAPCTL_CAPCH0EN_Msk (0x1ul << PWM_CAPCTL_CAPCH0EN_Pos)
#define | PWM_CAPCTL_CAPCH0PADEN_Pos (2)
#define | PWM_CAPCTL_CAPCH0PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH0PADEN_Pos)
#define | PWM_CAPCTL_CH0PDMAEN_Pos (3)
#define | PWM_CAPCTL_CH0PDMAEN_Msk (0x1ul << PWM_CAPCTL_CH0PDMAEN_Pos)
#define | PWM_CAPCTL_PDMACAPMOD0_Pos (4)
#define | PWM_CAPCTL_PDMACAPMOD0_Msk (0x3ul << PWM_CAPCTL_PDMACAPMOD0_Pos)
#define | PWM_CAPCTL_CAPRELOADREN0_Pos (6)
#define | PWM_CAPCTL_CAPRELOADREN0_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN0_Pos)
#define | PWM_CAPCTL_CAPRELOADFEN0_Pos (7)
#define | PWM_CAPCTL_CAPRELOADFEN0_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN0_Pos)
#define | PWM_CAPCTL_INV1_Pos (8)
#define | PWM_CAPCTL_INV1_Msk (0x1ul << PWM_CAPCTL_INV1_Pos)
#define | PWM_CAPCTL_CAPCH1EN_Pos (9)
#define | PWM_CAPCTL_CAPCH1EN_Msk (0x1ul << PWM_CAPCTL_CAPCH1EN_Pos)
#define | PWM_CAPCTL_CAPCH1PADEN_Pos (10)
#define | PWM_CAPCTL_CAPCH1PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH1PADEN_Pos)
#define | PWM_CAPCTL_CH0RFORDER_Pos (12)
#define | PWM_CAPCTL_CH0RFORDER_Msk (0x1ul << PWM_CAPCTL_CH0RFORDER_Pos)
#define | PWM_CAPCTL_CH01CASK_Pos (13)
#define | PWM_CAPCTL_CH01CASK_Msk (0x1ul << PWM_CAPCTL_CH01CASK_Pos)
#define | PWM_CAPCTL_CAPRELOADREN1_Pos (14)
#define | PWM_CAPCTL_CAPRELOADREN1_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN1_Pos)
#define | PWM_CAPCTL_CAPRELOADFEN1_Pos (15)
#define | PWM_CAPCTL_CAPRELOADFEN1_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN1_Pos)
#define | PWM_CAPCTL_INV2_Pos (16)
#define | PWM_CAPCTL_INV2_Msk (0x1ul << PWM_CAPCTL_INV2_Pos)
#define | PWM_CAPCTL_CAPCH2EN_Pos (17)
#define | PWM_CAPCTL_CAPCH2EN_Msk (0x1ul << PWM_CAPCTL_CAPCH2EN_Pos)
#define | PWM_CAPCTL_CAPCH2PADEN_Pos (18)
#define | PWM_CAPCTL_CAPCH2PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH2PADEN_Pos)
#define | PWM_CAPCTL_CH2PDMAEN_Pos (19)
#define | PWM_CAPCTL_CH2PDMAEN_Msk (0x1ul << PWM_CAPCTL_CH2PDMAEN_Pos)
#define | PWM_CAPCTL_PDMACAPMOD2_Pos (20)
#define | PWM_CAPCTL_PDMACAPMOD2_Msk (0x3ul << PWM_CAPCTL_PDMACAPMOD2_Pos)
#define | PWM_CAPCTL_CAPRELOADREN2_Pos (22)
#define | PWM_CAPCTL_CAPRELOADREN2_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN2_Pos)
#define | PWM_CAPCTL_CAPRELOADFEN2_Pos (23)
#define | PWM_CAPCTL_CAPRELOADFEN2_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN2_Pos)
#define | PWM_CAPCTL_INV3_Pos (24)
#define | PWM_CAPCTL_INV3_Msk (0x1ul << PWM_CAPCTL_INV3_Pos)
#define | PWM_CAPCTL_CAPCH3EN_Pos (25)
#define | PWM_CAPCTL_CAPCH3EN_Msk (0x1ul << PWM_CAPCTL_CAPCH3EN_Pos)
#define | PWM_CAPCTL_CAPCH3PADEN_Pos (26)
#define | PWM_CAPCTL_CAPCH3PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH3PADEN_Pos)
#define | PWM_CAPCTL_CH2RFORDER_Pos (28)
#define | PWM_CAPCTL_CH2RFORDER_Msk (0x1ul << PWM_CAPCTL_CH2RFORDER_Pos)
#define | PWM_CAPCTL_CH23CASK_Pos (29)
#define | PWM_CAPCTL_CH23CASK_Msk (0x1ul << PWM_CAPCTL_CH23CASK_Pos)
#define | PWM_CAPCTL_CAPRELOADREN3_Pos (30)
#define | PWM_CAPCTL_CAPRELOADREN3_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN3_Pos)
#define | PWM_CAPCTL_CAPRELOADFEN3_Pos (31)
#define | PWM_CAPCTL_CAPRELOADFEN3_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN3_Pos)
#define | PWM_CAPINTEN_CRL_IE0_Pos (0)
#define | PWM_CAPINTEN_CRL_IE0_Msk (0x1ul << PWM_CAPINTEN_CRL_IE0_Pos)
#define | PWM_CAPINTEN_CFL_IE0_Pos (1)
#define | PWM_CAPINTEN_CFL_IE0_Msk (0x1ul << PWM_CAPINTEN_CFL_IE0_Pos)
#define | PWM_CAPINTEN_CRL_IE1_Pos (8)
#define | PWM_CAPINTEN_CRL_IE1_Msk (0x1ul << PWM_CAPINTEN_CRL_IE1_Pos)
#define | PWM_CAPINTEN_CFL_IE1_Pos (9)
#define | PWM_CAPINTEN_CFL_IE1_Msk (0x1ul << PWM_CAPINTEN_CFL_IE1_Pos)
#define | PWM_CAPINTEN_CRL_IE2_Pos (16)
#define | PWM_CAPINTEN_CRL_IE2_Msk (0x1ul << PWM_CAPINTEN_CRL_IE2_Pos)
#define | PWM_CAPINTEN_CFL_IE2_Pos (17)
#define | PWM_CAPINTEN_CFL_IE2_Msk (0x1ul << PWM_CAPINTEN_CFL_IE2_Pos)
#define | PWM_CAPINTEN_CRL_IE3_Pos (24)
#define | PWM_CAPINTEN_CRL_IE3_Msk (0x1ul << PWM_CAPINTEN_CRL_IE3_Pos)
#define | PWM_CAPINTEN_CFL_IE3_Pos (25)
#define | PWM_CAPINTEN_CFL_IE3_Msk (0x1ul << PWM_CAPINTEN_CFL_IE3_Pos)
#define | PWM_CAPINTSTS_CAPIF0_Pos (0)
#define | PWM_CAPINTSTS_CAPIF0_Msk (0x1ul << PWM_CAPINTSTS_CAPIF0_Pos)
#define | PWM_CAPINTSTS_CRLI0_Pos (1)
#define | PWM_CAPINTSTS_CRLI0_Msk (0x1ul << PWM_CAPINTSTS_CRLI0_Pos)
#define | PWM_CAPINTSTS_CFLRI0_Pos (2)
#define | PWM_CAPINTSTS_CFLRI0_Msk (0x1ul << PWM_CAPINTSTS_CFLRI0_Pos)
#define | PWM_CAPINTSTS_CAPOVR0_Pos (3)
#define | PWM_CAPINTSTS_CAPOVR0_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR0_Pos)
#define | PWM_CAPINTSTS_CAPOVF0_Pos (4)
#define | PWM_CAPINTSTS_CAPOVF0_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF0_Pos)
#define | PWM_CAPINTSTS_CAPIF1_Pos (8)
#define | PWM_CAPINTSTS_CAPIF1_Msk (0x1ul << PWM_CAPINTSTS_CAPIF1_Pos)
#define | PWM_CAPINTSTS_CRLI1_Pos (9)
#define | PWM_CAPINTSTS_CRLI1_Msk (0x1ul << PWM_CAPINTSTS_CRLI1_Pos)
#define | PWM_CAPINTSTS_CFLI1_Pos (10)
#define | PWM_CAPINTSTS_CFLI1_Msk (0x1ul << PWM_CAPINTSTS_CFLI1_Pos)
#define | PWM_CAPINTSTS_CAPOVR1_Pos (11)
#define | PWM_CAPINTSTS_CAPOVR1_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR1_Pos)
#define | PWM_CAPINTSTS_CAPOVF1_Pos (12)
#define | PWM_CAPINTSTS_CAPOVF1_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF1_Pos)
#define | PWM_CAPINTSTS_CAPIF2_Pos (16)
#define | PWM_CAPINTSTS_CAPIF2_Msk (0x1ul << PWM_CAPINTSTS_CAPIF2_Pos)
#define | PWM_CAPINTSTS_CRLI2_Pos (17)
#define | PWM_CAPINTSTS_CRLI2_Msk (0x1ul << PWM_CAPINTSTS_CRLI2_Pos)
#define | PWM_CAPINTSTS_CFLI2_Pos (18)
#define | PWM_CAPINTSTS_CFLI2_Msk (0x1ul << PWM_CAPINTSTS_CFLI2_Pos)
#define | PWM_CAPINTSTS_CAPOVR2_Pos (19)
#define | PWM_CAPINTSTS_CAPOVR2_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR2_Pos)
#define | PWM_CAPINTSTS_CAPOVF2_Pos (20)
#define | PWM_CAPINTSTS_CAPOVF2_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF2_Pos)
#define | PWM_CAPINTSTS_CAPIF3_Pos (24)
#define | PWM_CAPINTSTS_CAPIF3_Msk (0x1ul << PWM_CAPINTSTS_CAPIF3_Pos)
#define | PWM_CAPINTSTS_CRLI3_Pos (25)
#define | PWM_CAPINTSTS_CRLI3_Msk (0x1ul << PWM_CAPINTSTS_CRLI3_Pos)
#define | PWM_CAPINTSTS_CFLI3_Pos (26)
#define | PWM_CAPINTSTS_CFLI3_Msk (0x1ul << PWM_CAPINTSTS_CFLI3_Pos)
#define | PWM_CAPINTSTS_CAPOVR3_Pos (27)
#define | PWM_CAPINTSTS_CAPOVR3_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR3_Pos)
#define | PWM_CAPINTSTS_CAPOVF3_Pos (28)
#define | PWM_CAPINTSTS_CAPOVF3_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF3_Pos)
#define | PWM_CRL0_CRL15_0_Pos (0)
#define | PWM_CRL0_CRL15_0_Msk (0xfffful << PWM_CRL0_CRL15_0_Pos)
#define | PWM_CRL0_CRL31_16_Pos (16)
#define | PWM_CRL0_CRL31_16_Msk (0xfffful << PWM_CRL0_CRL31_16_Pos)
#define | PWM_CFL0_CFL15_0_Pos (0)
#define | PWM_CFL0_CFL15_0_Msk (0xfffful << PWM_CFL0_CFL15_0_Pos)
#define | PWM_CFL0_CFL31_16_Pos (16)
#define | PWM_CFL0_CFL31_16_Msk (0xfffful << PWM_CFL0_CFL31_16_Pos)
#define | PWM_CRL1_CRL15_0_Pos (0)
#define | PWM_CRL1_CRL15_0_Msk (0xfffful << PWM_CRL1_CRL15_0_Pos)
#define | PWM_CRL1_CRL31_16_Pos (16)
#define | PWM_CRL1_CRL31_16_Msk (0xfffful << PWM_CRL1_CRL31_16_Pos)
#define | PWM_CFL1_CFL15_0_Pos (0)
#define | PWM_CFL1_CFL15_0_Msk (0xfffful << PWM_CFL1_CFL15_0_Pos)
#define | PWM_CFL1_CFL31_16_Pos (16)
#define | PWM_CFL1_CFL31_16_Msk (0xfffful << PWM_CFL1_CFL31_16_Pos)
#define | PWM_CRL2_CRL15_0_Pos (0)
#define | PWM_CRL2_CRL15_0_Msk (0xfffful << PWM_CRL2_CRL15_0_Pos)
#define | PWM_CRL2_CRL31_16_Pos (16)
#define | PWM_CRL2_CRL31_16_Msk (0xfffful << PWM_CRL2_CRL31_16_Pos)
#define | PWM_CFL2_CFL15_0_Pos (0)
#define | PWM_CFL2_CFL15_0_Msk (0xfffful << PWM_CFL2_CFL15_0_Pos)
#define | PWM_CFL2_CFL31_16_Pos (16)
#define | PWM_CFL2_CFL31_16_Msk (0xfffful << PWM_CFL2_CFL31_16_Pos)
#define | PWM_CRL3_CRL15_0_Pos (0)
#define | PWM_CRL3_CRL15_0_Msk (0xfffful << PWM_CRL3_CRL15_0_Pos)
#define | PWM_CRL3_CRL31_16_Pos (16)
#define | PWM_CRL3_CRL31_16_Msk (0xfffful << PWM_CRL3_CRL31_16_Pos)
#define | PWM_CFL3_CFL15_0_Pos (0)
#define | PWM_CFL3_CFL15_0_Msk (0xfffful << PWM_CFL3_CFL15_0_Pos)
#define | PWM_CFL3_CFL31_16_Pos (16)
#define | PWM_CFL3_CFL31_16_Msk (0xfffful << PWM_CFL3_CFL31_16_Pos)
#define | PWM_PDMACH0_Captureddata7_0_Pos (0)
#define | PWM_PDMACH0_Captureddata7_0_Msk (0xfful << PWM_PDMACH0_Captureddata7_0_Pos)
#define | PWM_PDMACH0_Captureddata15_8_Pos (8)
#define | PWM_PDMACH0_Captureddata15_8_Msk (0xfful << PWM_PDMACH0_Captureddata15_8_Pos)
#define | PWM_PDMACH0_Captureddata23_16_Pos (16)
#define | PWM_PDMACH0_Captureddata23_16_Msk (0xfful << PWM_PDMACH0_Captureddata23_16_Pos)
#define | PWM_PDMACH0_Captureddata31_24_Pos (24)
#define | PWM_PDMACH0_Captureddata31_24_Msk (0xfful << PWM_PDMACH0_Captureddata31_24_Pos)
#define | PWM_PDMACH2_Captureddata7_0_Pos (0)
#define | PWM_PDMACH2_Captureddata7_0_Msk (0xfful << PWM_PDMACH2_Captureddata7_0_Pos)
#define | PWM_PDMACH2_Captureddata15_8_Pos (8)
#define | PWM_PDMACH2_Captureddata15_8_Msk (0xfful << PWM_PDMACH2_Captureddata15_8_Pos)
#define | PWM_PDMACH2_Captureddata23_16_Pos (16)
#define | PWM_PDMACH2_Captureddata23_16_Msk (0xfful << PWM_PDMACH2_Captureddata23_16_Pos)
#define | PWM_PDMACH2_Captureddata31_24_Pos (24)
#define | PWM_PDMACH2_Captureddata31_24_Msk (0xfful << PWM_PDMACH2_Captureddata31_24_Pos)
#define | RTC_INIR_ACTIVE_Pos (0)
#define | RTC_INIR_ACTIVE_Msk (0x1ul << RTC_INIR_ACTIVE_Pos)
#define | RTC_INIR_INIR_Pos (0)
#define | RTC_INIR_INIR_Msk (0xfffffffful << RTC_INIR_INIR_Pos)
#define | RTC_AER_AER_Pos (0)
#define | RTC_AER_AER_Msk (0xfffful << RTC_AER_AER_Pos)
#define | RTC_AER_ENF_Pos (16)
#define | RTC_AER_ENF_Msk (0x1ul << RTC_AER_ENF_Pos)
#define | RTC_FCR_FRACTION_Pos (0)
#define | RTC_FCR_FRACTION_Msk (0x3ful << RTC_FCR_FRACTION_Pos)
#define | RTC_FCR_INTEGER_Pos (8)
#define | RTC_FCR_INTEGER_Msk (0xful << RTC_FCR_INTEGER_Pos)
#define | RTC_TLR_1SEC_Pos (0)
#define | RTC_TLR_1SEC_Msk (0xful << RTC_TLR_1SEC_Pos)
#define | RTC_TLR_10SEC_Pos (4)
#define | RTC_TLR_10SEC_Msk (0x7ul << RTC_TLR_10SEC_Pos)
#define | RTC_TLR_1MIN_Pos (8)
#define | RTC_TLR_1MIN_Msk (0xful << RTC_TLR_1MIN_Pos)
#define | RTC_TLR_10MIN_Pos (12)
#define | RTC_TLR_10MIN_Msk (0x7ul << RTC_TLR_10MIN_Pos)
#define | RTC_TLR_1HR_Pos (16)
#define | RTC_TLR_1HR_Msk (0xful << RTC_TLR_1HR_Pos)
#define | RTC_TLR_10HR_Pos (20)
#define | RTC_TLR_10HR_Msk (0x3ul << RTC_TLR_10HR_Pos)
#define | RTC_CLR_1DAY_Pos (0)
#define | RTC_CLR_1DAY_Msk (0xful << RTC_CLR_1DAY_Pos)
#define | RTC_CLR_10DAY_Pos (4)
#define | RTC_CLR_10DAY_Msk (0x3ul << RTC_CLR_10DAY_Pos)
#define | RTC_CLR_1MON_Pos (8)
#define | RTC_CLR_1MON_Msk (0xful << RTC_CLR_1MON_Pos)
#define | RTC_CLR_10MON_Pos (12)
#define | RTC_CLR_10MON_Msk (0x1ul << RTC_CLR_10MON_Pos)
#define | RTC_CLR_1YEAR_Pos (16)
#define | RTC_CLR_1YEAR_Msk (0xful << RTC_CLR_1YEAR_Pos)
#define | RTC_CLR_10YEAR_Pos (20)
#define | RTC_CLR_10YEAR_Msk (0xful << RTC_CLR_10YEAR_Pos)
#define | RTC_TSSR_24H_12H_Pos (0)
#define | RTC_TSSR_24H_12H_Msk (0x1ul << RTC_TSSR_24H_12H_Pos)
#define | RTC_DWR_DWR_Pos (0)
#define | RTC_DWR_DWR_Msk (0x7ul << RTC_DWR_DWR_Pos)
#define | RTC_TAR_1SEC_Pos (0)
#define | RTC_TAR_1SEC_Msk (0xful << RTC_TAR_1SEC_Pos)
#define | RTC_TAR_10SEC_Pos (4)
#define | RTC_TAR_10SEC_Msk (0x7ul << RTC_TAR_10SEC_Pos)
#define | RTC_TAR_1MIN_Pos (8)
#define | RTC_TAR_1MIN_Msk (0xful << RTC_TAR_1MIN_Pos)
#define | RTC_TAR_10MIN_Pos (12)
#define | RTC_TAR_10MIN_Msk (0x7ul << RTC_TAR_10MIN_Pos)
#define | RTC_TAR_1HR_Pos (16)
#define | RTC_TAR_1HR_Msk (0xful << RTC_TAR_1HR_Pos)
#define | RTC_TAR_10HR_Pos (20)
#define | RTC_TAR_10HR_Msk (0x3ul << RTC_TAR_10HR_Pos)
#define | RTC_CAR_1DAY_Pos (0)
#define | RTC_CAR_1DAY_Msk (0xful << RTC_CAR_1DAY_Pos)
#define | RTC_CAR_10DAY_Pos (4)
#define | RTC_CAR_10DAY_Msk (0x3ul << RTC_CAR_10DAY_Pos)
#define | RTC_CAR_1MON_Pos (8)
#define | RTC_CAR_1MON_Msk (0xful << RTC_CAR_1MON_Pos)
#define | RTC_CAR_10MON_Pos (12)
#define | RTC_CAR_10MON_Msk (0x1ul << RTC_CAR_10MON_Pos)
#define | RTC_CAR_1YEAR_Pos (16)
#define | RTC_CAR_1YEAR_Msk (0xful << RTC_CAR_1YEAR_Pos)
#define | RTC_CAR_10YEAR_Pos (20)
#define | RTC_CAR_10YEAR_Msk (0xful << RTC_CAR_10YEAR_Pos)
#define | RTC_LIR_LIR_Pos (0)
#define | RTC_LIR_LIR_Msk (0x1ul << RTC_LIR_LIR_Pos)
#define | RTC_RIER_AIER_Pos (0)
#define | RTC_RIER_AIER_Msk (0x1ul << RTC_RIER_AIER_Pos)
#define | RTC_RIER_TIER_Pos (1)
#define | RTC_RIER_TIER_Msk (0x1ul << RTC_RIER_TIER_Pos)
#define | RTC_RIER_SNOOPIER_Pos (2)
#define | RTC_RIER_SNOOPIER_Msk (0x1ul << RTC_RIER_SNOOPIER_Pos)
#define | RTC_RIIR_AIF_Pos (0)
#define | RTC_RIIR_AIF_Msk (0x1ul << RTC_RIIR_AIF_Pos)
#define | RTC_RIIR_TIF_Pos (1)
#define | RTC_RIIR_TIF_Msk (0x1ul << RTC_RIIR_TIF_Pos)
#define | RTC_RIIR_SNOOPIF_Pos (2)
#define | RTC_RIIR_SNOOPIF_Msk (0x1ul << RTC_RIIR_SNOOPIF_Pos)
#define | RTC_TTR_TTR_Pos (0)
#define | RTC_TTR_TTR_Msk (0x7ul << RTC_TTR_TTR_Pos)
#define | RTC_TTR_TWKE_Pos (3)
#define | RTC_TTR_TWKE_Msk (0x1ul << RTC_TTR_TWKE_Pos)
#define | RTC_SPRCTL_SNOOPEN_Pos (0)
#define | RTC_SPRCTL_SNOOPEN_Msk (0x1ul << RTC_SPRCTL_SNOOPEN_Pos)
#define | RTC_SPRCTL_SNOOPEDGE_Pos (1)
#define | RTC_SPRCTL_SNOOPEDGE_Msk (0x1ul << RTC_SPRCTL_SNOOPEDGE_Pos)
#define | RTC_SPRCTL_SPRRDY_Pos (7)
#define | RTC_SPRCTL_SPRRDY_Msk (0x1ul << RTC_SPRCTL_SPRRDY_Pos)
#define | RTC_SPR0_SPARE_Pos (0)
#define | RTC_SPR0_SPARE_Msk (0xfffffffful << RTC_SPR0_SPARE_Pos)
#define | RTC_SPR1_SPARE_Pos (0)
#define | RTC_SPR1_SPARE_Msk (0xfffffffful << RTC_SPR1_SPARE_Pos)
#define | RTC_SPR2_SPARE_Pos (0)
#define | RTC_SPR2_SPARE_Msk (0xfffffffful << RTC_SPR2_SPARE_Pos)
#define | RTC_SPR3_SPARE_Pos (0)
#define | RTC_SPR3_SPARE_Msk (0xfffffffful << RTC_SPR3_SPARE_Pos)
#define | RTC_SPR4_SPARE_Pos (0)
#define | RTC_SPR4_SPARE_Msk (0xfffffffful << RTC_SPR4_SPARE_Pos)
#define | RTC_SPR5_SPARE_Pos (0)
#define | RTC_SPR5_SPARE_Msk (0xfffffffful << RTC_SPR5_SPARE_Pos)
#define | RTC_SPR6_SPARE_Pos (0)
#define | RTC_SPR6_SPARE_Msk (0xfffffffful << RTC_SPR6_SPARE_Pos)
#define | RTC_SPR7_SPARE_Pos (0)
#define | RTC_SPR7_SPARE_Msk (0xfffffffful << RTC_SPR7_SPARE_Pos)
#define | RTC_SPR8_SPARE_Pos (0)
#define | RTC_SPR8_SPARE_Msk (0xfffffffful << RTC_SPR8_SPARE_Pos)
#define | RTC_SPR9_SPARE_Pos (0)
#define | RTC_SPR9_SPARE_Msk (0xfffffffful << RTC_SPR9_SPARE_Pos)
#define | RTC_SPR10_SPARE_Pos (0)
#define | RTC_SPR10_SPARE_Msk (0xfffffffful << RTC_SPR10_SPARE_Pos)
#define | RTC_SPR11_SPARE_Pos (0)
#define | RTC_SPR11_SPARE_Msk (0xfffffffful << RTC_SPR11_SPARE_Pos)
#define | RTC_SPR12_SPARE_Pos (0)
#define | RTC_SPR12_SPARE_Msk (0xfffffffful << RTC_SPR12_SPARE_Pos)
#define | RTC_SPR13_SPARE_Pos (0)
#define | RTC_SPR13_SPARE_Msk (0xfffffffful << RTC_SPR13_SPARE_Pos)
#define | RTC_SPR14_SPARE_Pos (0)
#define | RTC_SPR14_SPARE_Msk (0xfffffffful << RTC_SPR14_SPARE_Pos)
#define | RTC_SPR15_SPARE_Pos (0)
#define | RTC_SPR15_SPARE_Msk (0xfffffffful << RTC_SPR15_SPARE_Pos)
#define | RTC_SPR16_SPARE_Pos (0)
#define | RTC_SPR16_SPARE_Msk (0xfffffffful << RTC_SPR16_SPARE_Pos)
#define | RTC_SPR17_SPARE_Pos (0)
#define | RTC_SPR17_SPARE_Msk (0xfffffffful << RTC_SPR17_SPARE_Pos)
#define | RTC_SPR18_SPARE_Pos (0)
#define | RTC_SPR18_SPARE_Msk (0xfffffffful << RTC_SPR18_SPARE_Pos)
#define | RTC_SPR19_SPARE_Pos (0)
#define | RTC_SPR19_SPARE_Msk (0xfffffffful << RTC_SPR19_SPARE_Pos)
#define | SC_DAT_DAT_Pos (0)
#define | SC_DAT_DAT_Msk (0xfful << SC_DAT_DAT_Pos)
#define | SC_CTL_SC_CEN_Pos (0)
#define | SC_CTL_SC_CEN_Msk (0x1ul << SC_CTL_SC_CEN_Pos)
#define | SC_CTL_DIS_RX_Pos (1)
#define | SC_CTL_DIS_RX_Msk (0x1ul << SC_CTL_DIS_RX_Pos)
#define | SC_CTL_DIS_TX_Pos (2)
#define | SC_CTL_DIS_TX_Msk (0x1ul << SC_CTL_DIS_TX_Pos)
#define | SC_CTL_AUTO_CON_EN_Pos (3)
#define | SC_CTL_AUTO_CON_EN_Msk (0x1ul << SC_CTL_AUTO_CON_EN_Pos)
#define | SC_CTL_CON_SEL_Pos (4)
#define | SC_CTL_CON_SEL_Msk (0x3ul << SC_CTL_CON_SEL_Pos)
#define | SC_CTL_RX_FTRI_LEV_Pos (6)
#define | SC_CTL_RX_FTRI_LEV_Msk (0x3ul << SC_CTL_RX_FTRI_LEV_Pos)
#define | SC_CTL_BGT_Pos (8)
#define | SC_CTL_BGT_Msk (0x1ful << SC_CTL_BGT_Pos)
#define | SC_CTL_TMR_SEL_Pos (13)
#define | SC_CTL_TMR_SEL_Msk (0x3ul << SC_CTL_TMR_SEL_Pos)
#define | SC_CTL_SLEN_Pos (15)
#define | SC_CTL_SLEN_Msk (0x1ul << SC_CTL_SLEN_Pos)
#define | SC_CTL_RX_ERETRY_Pos (16)
#define | SC_CTL_RX_ERETRY_Msk (0x7ul << SC_CTL_RX_ERETRY_Pos)
#define | SC_CTL_RX_ERETRY_EN_Pos (19)
#define | SC_CTL_RX_ERETRY_EN_Msk (0x1ul << SC_CTL_RX_ERETRY_EN_Pos)
#define | SC_CTL_TX_ERETRY_Pos (20)
#define | SC_CTL_TX_ERETRY_Msk (0x7ul << SC_CTL_TX_ERETRY_Pos)
#define | SC_CTL_TX_ERETRY_EN_Pos (23)
#define | SC_CTL_TX_ERETRY_EN_Msk (0x1ul << SC_CTL_TX_ERETRY_EN_Pos)
#define | SC_CTL_CD_DEB_SEL_Pos (24)
#define | SC_CTL_CD_DEB_SEL_Msk (0x3ul << SC_CTL_CD_DEB_SEL_Pos)
#define | SC_ALTCTL_TX_RST_Pos (0)
#define | SC_ALTCTL_TX_RST_Msk (0x1ul << SC_ALTCTL_TX_RST_Pos)
#define | SC_ALTCTL_RX_RST_Pos (1)
#define | SC_ALTCTL_RX_RST_Msk (0x1ul << SC_ALTCTL_RX_RST_Pos)
#define | SC_ALTCTL_DACT_EN_Pos (2)
#define | SC_ALTCTL_DACT_EN_Msk (0x1ul << SC_ALTCTL_DACT_EN_Pos)
#define | SC_ALTCTL_ACT_EN_Pos (3)
#define | SC_ALTCTL_ACT_EN_Msk (0x1ul << SC_ALTCTL_ACT_EN_Pos)
#define | SC_ALTCTL_WARST_EN_Pos (4)
#define | SC_ALTCTL_WARST_EN_Msk (0x1ul << SC_ALTCTL_WARST_EN_Pos)
#define | SC_ALTCTL_TMR0_SEN_Pos (5)
#define | SC_ALTCTL_TMR0_SEN_Msk (0x1ul << SC_ALTCTL_TMR0_SEN_Pos)
#define | SC_ALTCTL_TMR1_SEN_Pos (6)
#define | SC_ALTCTL_TMR1_SEN_Msk (0x1ul << SC_ALTCTL_TMR1_SEN_Pos)
#define | SC_ALTCTL_TMR2_SEN_Pos (7)
#define | SC_ALTCTL_TMR2_SEN_Msk (0x1ul << SC_ALTCTL_TMR2_SEN_Pos)
#define | SC_ALTCTL_INIT_SEL_Pos (8)
#define | SC_ALTCTL_INIT_SEL_Msk (0x3ul << SC_ALTCTL_INIT_SEL_Pos)
#define | SC_ALTCTL_RX_BGT_EN_Pos (12)
#define | SC_ALTCTL_RX_BGT_EN_Msk (0x1ul << SC_ALTCTL_RX_BGT_EN_Pos)
#define | SC_ALTCTL_TMR0_ATV_Pos (13)
#define | SC_ALTCTL_TMR0_ATV_Msk (0x1ul << SC_ALTCTL_TMR0_ATV_Pos)
#define | SC_ALTCTL_TMR1_ATV_Pos (14)
#define | SC_ALTCTL_TMR1_ATV_Msk (0x1ul << SC_ALTCTL_TMR1_ATV_Pos)
#define | SC_ALTCTL_TMR2_ATV_Pos (15)
#define | SC_ALTCTL_TMR2_ATV_Msk (0x1ul << SC_ALTCTL_TMR2_ATV_Pos)
#define | SC_EGTR_EGT_Pos (0)
#define | SC_EGTR_EGT_Msk (0xfful << SC_EGTR_EGT_Pos)
#define | SC_RFTMR_RFTM_Pos (0)
#define | SC_RFTMR_RFTM_Msk (0x1fful << SC_RFTMR_RFTM_Pos)
#define | SC_ETUCR_ETU_RDIV_Pos (0)
#define | SC_ETUCR_ETU_RDIV_Msk (0xffful << SC_ETUCR_ETU_RDIV_Pos)
#define | SC_ETUCR_COMPEN_EN_Pos (15)
#define | SC_ETUCR_COMPEN_EN_Msk (0x1ul << SC_ETUCR_COMPEN_EN_Pos)
#define | SC_IER_RDA_IE_Pos (0)
#define | SC_IER_RDA_IE_Msk (0x1ul << SC_IER_RDA_IE_Pos)
#define | SC_IER_TBE_IE_Pos (1)
#define | SC_IER_TBE_IE_Msk (0x1ul << SC_IER_TBE_IE_Pos)
#define | SC_IER_TERR_IE_Pos (2)
#define | SC_IER_TERR_IE_Msk (0x1ul << SC_IER_TERR_IE_Pos)
#define | SC_IER_TMR0_IE_Pos (3)
#define | SC_IER_TMR0_IE_Msk (0x1ul << SC_IER_TMR0_IE_Pos)
#define | SC_IER_TMR1_IE_Pos (4)
#define | SC_IER_TMR1_IE_Msk (0x1ul << SC_IER_TMR1_IE_Pos)
#define | SC_IER_TMR2_IE_Pos (5)
#define | SC_IER_TMR2_IE_Msk (0x1ul << SC_IER_TMR2_IE_Pos)
#define | SC_IER_BGT_IE_Pos (6)
#define | SC_IER_BGT_IE_Msk (0x1ul << SC_IER_BGT_IE_Pos)
#define | SC_IER_CD_IE_Pos (7)
#define | SC_IER_CD_IE_Msk (0x1ul << SC_IER_CD_IE_Pos)
#define | SC_IER_INIT_IE_Pos (8)
#define | SC_IER_INIT_IE_Msk (0x1ul << SC_IER_INIT_IE_Pos)
#define | SC_IER_RTMR_IE_Pos (9)
#define | SC_IER_RTMR_IE_Msk (0x1ul << SC_IER_RTMR_IE_Pos)
#define | SC_IER_ACON_ERR_IE_Pos (10)
#define | SC_IER_ACON_ERR_IE_Msk (0x1ul << SC_IER_ACON_ERR_IE_Pos)
#define | SC_ISR_RDA_IS_Pos (0)
#define | SC_ISR_RDA_IS_Msk (0x1ul << SC_ISR_RDA_IS_Pos)
#define | SC_ISR_TBE_IS_Pos (1)
#define | SC_ISR_TBE_IS_Msk (0x1ul << SC_ISR_TBE_IS_Pos)
#define | SC_ISR_TERR_IS_Pos (2)
#define | SC_ISR_TERR_IS_Msk (0x1ul << SC_ISR_TERR_IS_Pos)
#define | SC_ISR_TMR0_IS_Pos (3)
#define | SC_ISR_TMR0_IS_Msk (0x1ul << SC_ISR_TMR0_IS_Pos)
#define | SC_ISR_TMR1_IS_Pos (4)
#define | SC_ISR_TMR1_IS_Msk (0x1ul << SC_ISR_TMR1_IS_Pos)
#define | SC_ISR_TMR2_IS_Pos (5)
#define | SC_ISR_TMR2_IS_Msk (0x1ul << SC_ISR_TMR2_IS_Pos)
#define | SC_ISR_BGT_IS_Pos (6)
#define | SC_ISR_BGT_IS_Msk (0x1ul << SC_ISR_BGT_IS_Pos)
#define | SC_ISR_CD_IS_Pos (7)
#define | SC_ISR_CD_IS_Msk (0x1ul << SC_ISR_CD_IS_Pos)
#define | SC_ISR_INIT_IS_Pos (8)
#define | SC_ISR_INIT_IS_Msk (0x1ul << SC_ISR_INIT_IS_Pos)
#define | SC_ISR_RTMR_IS_Pos (9)
#define | SC_ISR_RTMR_IS_Msk (0x1ul << SC_ISR_RTMR_IS_Pos)
#define | SC_ISR_ACON_ERR_IS_Pos (10)
#define | SC_ISR_ACON_ERR_IS_Msk (0x1ul << SC_ISR_ACON_ERR_IS_Pos)
#define | SC_TRSR_RX_OVER_F_Pos (0)
#define | SC_TRSR_RX_OVER_F_Msk (0x1ul << SC_TRSR_RX_OVER_F_Pos)
#define | SC_TRSR_RX_EMPTY_F_Pos (1)
#define | SC_TRSR_RX_EMPTY_F_Msk (0x1ul << SC_TRSR_RX_EMPTY_F_Pos)
#define | SC_TRSR_RX_FULL_F_Pos (2)
#define | SC_TRSR_RX_FULL_F_Msk (0x1ul << SC_TRSR_RX_FULL_F_Pos)
#define | SC_TRSR_RX_EPA_F_Pos (4)
#define | SC_TRSR_RX_EPA_F_Msk (0x1ul << SC_TRSR_RX_EPA_F_Pos)
#define | SC_TRSR_RX_EFR_F_Pos (5)
#define | SC_TRSR_RX_EFR_F_Msk (0x1ul << SC_TRSR_RX_EFR_F_Pos)
#define | SC_TRSR_RX_EBR_F_Pos (6)
#define | SC_TRSR_RX_EBR_F_Msk (0x1ul << SC_TRSR_RX_EBR_F_Pos)
#define | SC_TRSR_TX_OVER_F_Pos (8)
#define | SC_TRSR_TX_OVER_F_Msk (0x1ul << SC_TRSR_TX_OVER_F_Pos)
#define | SC_TRSR_TX_EMPTY_F_Pos (9)
#define | SC_TRSR_TX_EMPTY_F_Msk (0x1ul << SC_TRSR_TX_EMPTY_F_Pos)
#define | SC_TRSR_TX_FULL_F_Pos (10)
#define | SC_TRSR_TX_FULL_F_Msk (0x1ul << SC_TRSR_TX_FULL_F_Pos)
#define | SC_TRSR_RX_POINT_F_Pos (16)
#define | SC_TRSR_RX_POINT_F_Msk (0x7ul << SC_TRSR_RX_POINT_F_Pos)
#define | SC_TRSR_RX_REERR_Pos (21)
#define | SC_TRSR_RX_REERR_Msk (0x1ul << SC_TRSR_RX_REERR_Pos)
#define | SC_TRSR_RX_OVER_ERETRY_Pos (22)
#define | SC_TRSR_RX_OVER_ERETRY_Msk (0x1ul << SC_TRSR_RX_OVER_ERETRY_Pos)
#define | SC_TRSR_RX_ATV_Pos (23)
#define | SC_TRSR_RX_ATV_Msk (0x1ul << SC_TRSR_RX_ATV_Pos)
#define | SC_TRSR_TX_POINT_F_Pos (24)
#define | SC_TRSR_TX_POINT_F_Msk (0x7ul << SC_TRSR_TX_POINT_F_Pos)
#define | SC_TRSR_TX_REERR_Pos (29)
#define | SC_TRSR_TX_REERR_Msk (0x1ul << SC_TRSR_TX_REERR_Pos)
#define | SC_TRSR_TX_OVER_ERETRY_Pos (30)
#define | SC_TRSR_TX_OVER_ERETRY_Msk (0x1ul << SC_TRSR_TX_OVER_ERETRY_Pos)
#define | SC_TRSR_TX_ATV_Pos (31)
#define | SC_TRSR_TX_ATV_Msk (0x1ul << SC_TRSR_TX_ATV_Pos)
#define | SC_PINCSR_POW_EN_Pos (0)
#define | SC_PINCSR_POW_EN_Msk (0x1ul << SC_PINCSR_POW_EN_Pos)
#define | SC_PINCSR_SC_RST_Pos (1)
#define | SC_PINCSR_SC_RST_Msk (0x1ul << SC_PINCSR_SC_RST_Pos)
#define | SC_PINCSR_CD_REM_F_Pos (2)
#define | SC_PINCSR_CD_REM_F_Msk (0x1ul << SC_PINCSR_CD_REM_F_Pos)
#define | SC_PINCSR_CD_INS_F_Pos (3)
#define | SC_PINCSR_CD_INS_F_Msk (0x1ul << SC_PINCSR_CD_INS_F_Pos)
#define | SC_PINCSR_CD_PIN_ST_Pos (4)
#define | SC_PINCSR_CD_PIN_ST_Msk (0x1ul << SC_PINCSR_CD_PIN_ST_Pos)
#define | SC_PINCSR_CLK_KEEP_Pos (6)
#define | SC_PINCSR_CLK_KEEP_Msk (0x1ul << SC_PINCSR_CLK_KEEP_Pos)
#define | SC_PINCSR_ADAC_CD_EN_Pos (7)
#define | SC_PINCSR_ADAC_CD_EN_Msk (0x1ul << SC_PINCSR_ADAC_CD_EN_Pos)
#define | SC_PINCSR_SC_OEN_ST_Pos (8)
#define | SC_PINCSR_SC_OEN_ST_Msk (0x1ul << SC_PINCSR_SC_OEN_ST_Pos)
#define | SC_PINCSR_SC_DATA_O_Pos (9)
#define | SC_PINCSR_SC_DATA_O_Msk (0x1ul << SC_PINCSR_SC_DATA_O_Pos)
#define | SC_PINCSR_CD_LEV_Pos (10)
#define | SC_PINCSR_CD_LEV_Msk (0x1ul << SC_PINCSR_CD_LEV_Pos)
#define | SC_PINCSR_POW_INV_Pos (11)
#define | SC_PINCSR_POW_INV_Msk (0x1ul << SC_PINCSR_POW_INV_Pos)
#define | SC_PINCSR_SC_DATA_I_ST_Pos (16)
#define | SC_PINCSR_SC_DATA_I_ST_Msk (0x1ul << SC_PINCSR_SC_DATA_I_ST_Pos)
#define | SC_TMR0_CNT_Pos (0)
#define | SC_TMR0_CNT_Msk (0xfffffful << SC_TMR0_CNT_Pos)
#define | SC_TMR0_MODE_Pos (24)
#define | SC_TMR0_MODE_Msk (0xful << SC_TMR0_MODE_Pos)
#define | SC_TMR1_CNT_Pos (0)
#define | SC_TMR1_CNT_Msk (0xfful << SC_TMR1_CNT_Pos)
#define | SC_TMR1_MODE_Pos (24)
#define | SC_TMR1_MODE_Msk (0xful << SC_TMR1_MODE_Pos)
#define | SC_TMR2_CNT_Pos (0)
#define | SC_TMR2_CNT_Msk (0xfful << SC_TMR2_CNT_Pos)
#define | SC_TMR2_MODE_Pos (24)
#define | SC_TMR2_MODE_Msk (0xful << SC_TMR2_MODE_Pos)
#define | SC_UACTL_UA_MODE_EN_Pos (0)
#define | SC_UACTL_UA_MODE_EN_Msk (0x1ul << SC_UACTL_UA_MODE_EN_Pos)
#define | SC_UACTL_DATA_LEN_Pos (4)
#define | SC_UACTL_DATA_LEN_Msk (0x3ul << SC_UACTL_DATA_LEN_Pos)
#define | SC_UACTL_PBDIS_Pos (6)
#define | SC_UACTL_PBDIS_Msk (0x1ul << SC_UACTL_PBDIS_Pos)
#define | SC_UACTL_OPE_Pos (7)
#define | SC_UACTL_OPE_Msk (0x1ul << SC_UACTL_OPE_Pos)
#define | SC_TDRA_TDR0_Pos (0)
#define | SC_TDRA_TDR0_Msk (0xfffffful << SC_TDRA_TDR0_Pos)
#define | SC_TDRB_TDR1_Pos (0)
#define | SC_TDRB_TDR1_Msk (0xfful << SC_TDRB_TDR1_Pos)
#define | SC_TDRB_TDR2_Pos (8)
#define | SC_TDRB_TDR2_Msk (0xfful << SC_TDRB_TDR2_Pos)
#define | SPI_CTL_GO_BUSY_Pos (0)
#define | SPI_CTL_GO_BUSY_Msk (0x1ul << SPI_CTL_GO_BUSY_Pos)
#define | SPI_CTL_RX_NEG_Pos (1)
#define | SPI_CTL_RX_NEG_Msk (0x1ul << SPI_CTL_RX_NEG_Pos)
#define | SPI_CTL_TX_NEG_Pos (2)
#define | SPI_CTL_TX_NEG_Msk (0x1ul << SPI_CTL_TX_NEG_Pos)
#define | SPI_CTL_TX_BIT_LEN_Pos (3)
#define | SPI_CTL_TX_BIT_LEN_Msk (0x1ful << SPI_CTL_TX_BIT_LEN_Pos)
#define | SPI_CTL_LSB_Pos (10)
#define | SPI_CTL_LSB_Msk (0x1ul << SPI_CTL_LSB_Pos)
#define | SPI_CTL_CLKP_Pos (11)
#define | SPI_CTL_CLKP_Msk (0x1ul << SPI_CTL_CLKP_Pos)
#define | SPI_CTL_SP_CYCLE_Pos (12)
#define | SPI_CTL_SP_CYCLE_Msk (0xful << SPI_CTL_SP_CYCLE_Pos)
#define | SPI_CTL_INTEN_Pos (17)
#define | SPI_CTL_INTEN_Msk (0x1ul << SPI_CTL_INTEN_Pos)
#define | SPI_CTL_SLAVE_Pos (18)
#define | SPI_CTL_SLAVE_Msk (0x1ul << SPI_CTL_SLAVE_Pos)
#define | SPI_CTL_REORDER_Pos (19)
#define | SPI_CTL_REORDER_Msk (0x1ul << SPI_CTL_REORDER_Pos)
#define | SPI_CTL_FIFOM_Pos (21)
#define | SPI_CTL_FIFOM_Msk (0x1ul << SPI_CTL_FIFOM_Pos)
#define | SPI_CTL_TWOB_Pos (22)
#define | SPI_CTL_TWOB_Msk (0x1ul << SPI_CTL_TWOB_Pos)
#define | SPI_CTL_VARCLK_EN_Pos (23)
#define | SPI_CTL_VARCLK_EN_Msk (0x1ul << SPI_CTL_VARCLK_EN_Pos)
#define | SPI_CTL_DUAL_IO_DIR_Pos (28)
#define | SPI_CTL_DUAL_IO_DIR_Msk (0x1ul << SPI_CTL_DUAL_IO_DIR_Pos)
#define | SPI_CTL_DUAL_IO_EN_Pos (29)
#define | SPI_CTL_DUAL_IO_EN_Msk (0x1ul << SPI_CTL_DUAL_IO_EN_Pos)
#define | SPI_CTL_WKEUP_EN_Pos (31)
#define | SPI_CTL_WKEUP_EN_Msk (0x1ul << SPI_CTL_WKEUP_EN_Pos)
#define | SPI_STATUS_RX_EMPTY_Pos (0)
#define | SPI_STATUS_RX_EMPTY_Msk (0x1ul << SPI_STATUS_RX_EMPTY_Pos)
#define | SPI_STATUS_RX_FULL_Pos (1)
#define | SPI_STATUS_RX_FULL_Msk (0x1ul << SPI_STATUS_RX_FULL_Pos)
#define | SPI_STATUS_TX_EMPTY_Pos (2)
#define | SPI_STATUS_TX_EMPTY_Msk (0x1ul << SPI_STATUS_TX_EMPTY_Pos)
#define | SPI_STATUS_TX_FULL_Pos (3)
#define | SPI_STATUS_TX_FULL_Msk (0x1ul << SPI_STATUS_TX_FULL_Pos)
#define | SPI_STATUS_LTRIG_FLAG_Pos (4)
#define | SPI_STATUS_LTRIG_FLAG_Msk (0x1ul << SPI_STATUS_LTRIG_FLAG_Pos)
#define | SPI_STATUS_SLV_START_INTSTS_Pos (6)
#define | SPI_STATUS_SLV_START_INTSTS_Msk (0x1ul << SPI_STATUS_SLV_START_INTSTS_Pos)
#define | SPI_STATUS_INTSTS_Pos (7)
#define | SPI_STATUS_INTSTS_Msk (0x1ul << SPI_STATUS_INTSTS_Pos)
#define | SPI_STATUS_RXINT_STS_Pos (8)
#define | SPI_STATUS_RXINT_STS_Msk (0x1ul << SPI_STATUS_RXINT_STS_Pos)
#define | SPI_STATUS_RX_OVER_RUN_Pos (9)
#define | SPI_STATUS_RX_OVER_RUN_Msk (0x1ul << SPI_STATUS_RX_OVER_RUN_Pos)
#define | SPI_STATUS_TXINT_STS_Pos (10)
#define | SPI_STATUS_TXINT_STS_Msk (0x1ul << SPI_STATUS_TXINT_STS_Pos)
#define | SPI_STATUS_TIME_OUT_STS_Pos (12)
#define | SPI_STATUS_TIME_OUT_STS_Msk (0x1ul << SPI_STATUS_TIME_OUT_STS_Pos)
#define | SPI_STATUS_RX_FIFO_CNT_Pos (16)
#define | SPI_STATUS_RX_FIFO_CNT_Msk (0xful << SPI_STATUS_RX_FIFO_CNT_Pos)
#define | SPI_STATUS_TX_FIFO_CNT_Pos (20)
#define | SPI_STATUS_TX_FIFO_CNT_Msk (0xful << SPI_STATUS_TX_FIFO_CNT_Pos)
#define | SPI_CLKDIV_DIVIDER1_Pos (0)
#define | SPI_CLKDIV_DIVIDER1_Msk (0xfful << SPI_CLKDIV_DIVIDER1_Pos)
#define | SPI_CLKDIV_DIVIDER2_Pos (16)
#define | SPI_CLKDIV_DIVIDER2_Msk (0xfful << SPI_CLKDIV_DIVIDER2_Pos)
#define | SPI_SSR_SSR_Pos (0)
#define | SPI_SSR_SSR_Msk (0x3ul << SPI_SSR_SSR_Pos)
#define | SPI_SSR_SS_LVL_Pos (2)
#define | SPI_SSR_SS_LVL_Msk (0x1ul << SPI_SSR_SS_LVL_Pos)
#define | SPI_SSR_AUTOSS_Pos (3)
#define | SPI_SSR_AUTOSS_Msk (0x1ul << SPI_SSR_AUTOSS_Pos)
#define | SPI_SSR_SS_LTRIG_Pos (4)
#define | SPI_SSR_SS_LTRIG_Msk (0x1ul << SPI_SSR_SS_LTRIG_Pos)
#define | SPI_SSR_NOSLVSEL_Pos (5)
#define | SPI_SSR_NOSLVSEL_Msk (0x1ul << SPI_SSR_NOSLVSEL_Pos)
#define | SPI_SSR_SLV_ABORT_Pos (8)
#define | SPI_SSR_SLV_ABORT_Msk (0x1ul << SPI_SSR_SLV_ABORT_Pos)
#define | SPI_SSR_SSTA_INTEN_Pos (9)
#define | SPI_SSR_SSTA_INTEN_Msk (0x1ul << SPI_SSR_SSTA_INTEN_Pos)
#define | SPI_SSR_SS_INT_OPT_Pos (16)
#define | SPI_SSR_SS_INT_OPT_Msk (0x1ul << SPI_SSR_SS_INT_OPT_Pos)
#define | SPI_RX0_RDATA_Pos (0)
#define | SPI_RX0_RDATA_Msk (0xfffffffful << SPI_RX0_RDATA_Pos)
#define | SPI_RX1_RDATA_Pos (0)
#define | SPI_RX1_RDATA_Msk (0xfffffffful << SPI_RX1_RDATA_Pos)
#define | SPI_TX0_TDATA_Pos (0)
#define | SPI_TX0_TDATA_Msk (0xfffffffful << SPI_TX0_TDATA_Pos)
#define | SPI_TX1_TDATA_Pos (0)
#define | SPI_TX1_TDATA_Msk (0xfffffffful << SPI_TX1_TDATA_Pos)
#define | SPI_VARCLK_VARCLK_Pos (0)
#define | SPI_VARCLK_VARCLK_Msk (0xfffffffful << SPI_VARCLK_VARCLK_Pos)
#define | SPI_DMA_TX_DMA_EN_Pos (0)
#define | SPI_DMA_TX_DMA_EN_Msk (0x1ul << SPI_DMA_TX_DMA_EN_Pos)
#define | SPI_DMA_RX_DMA_EN_Pos (1)
#define | SPI_DMA_RX_DMA_EN_Msk (0x1ul << SPI_DMA_RX_DMA_EN_Pos)
#define | SPI_DMA_PDMA_RST_Pos (2)
#define | SPI_DMA_PDMA_RST_Msk (0x1ul << SPI_DMA_PDMA_RST_Pos)
#define | SPI_FFCTL_RX_CLR_Pos (0)
#define | SPI_FFCTL_RX_CLR_Msk (0x1ul << SPI_FFCTL_RX_CLR_Pos)
#define | SPI_FFCTL_TX_CLR_Pos (1)
#define | SPI_FFCTL_TX_CLR_Msk (0x1ul << SPI_FFCTL_TX_CLR_Pos)
#define | SPI_FFCTL_RX_INTEN_Pos (2)
#define | SPI_FFCTL_RX_INTEN_Msk (0x1ul << SPI_FFCTL_RX_INTEN_Pos)
#define | SPI_FFCTL_TX_INTEN_Pos (3)
#define | SPI_FFCTL_TX_INTEN_Msk (0x1ul << SPI_FFCTL_TX_INTEN_Pos)
#define | SPI_FFCTL_RXOVR_INTEN_Pos (4)
#define | SPI_FFCTL_RXOVR_INTEN_Msk (0x1ul << SPI_FFCTL_RXOVR_INTEN_Pos)
#define | SPI_FFCTL_TIMEOUT_EN_Pos (7)
#define | SPI_FFCTL_TIMEOUT_EN_Msk (0x1ul << SPI_FFCTL_TIMEOUT_EN_Pos)
#define | SPI_FFCTL_RX_THRESHOLD_Pos (24)
#define | SPI_FFCTL_RX_THRESHOLD_Msk (0x7ul << SPI_FFCTL_RX_THRESHOLD_Pos)
#define | SPI_FFCTL_TX_THRESHOLD_Pos (28)
#define | SPI_FFCTL_TX_THRESHOLD_Msk (0x7ul << SPI_FFCTL_TX_THRESHOLD_Pos)
#define | TIMER_CTL_TMR_EN_Pos (0)
#define | TIMER_CTL_TMR_EN_Msk (0x1ul << TIMER_CTL_TMR_EN_Pos)
#define | TIMER_CTL_SW_RST_Pos (1)
#define | TIMER_CTL_SW_RST_Msk (0x1ul << TIMER_CTL_SW_RST_Pos)
#define | TIMER_CTL_WAKE_EN_Pos (2)
#define | TIMER_CTL_WAKE_EN_Msk (0x1ul << TIMER_CTL_WAKE_EN_Pos)
#define | TIMER_CTL_DBGACK_EN_Pos (3)
#define | TIMER_CTL_DBGACK_EN_Msk (0x1ul << TIMER_CTL_DBGACK_EN_Pos)
#define | TIMER_CTL_MODE_SEL_Pos (4)
#define | TIMER_CTL_MODE_SEL_Msk (0x3ul << TIMER_CTL_MODE_SEL_Pos)
#define | TIMER_CTL_TMR_ACT_Pos (7)
#define | TIMER_CTL_TMR_ACT_Msk (0x1ul << TIMER_CTL_TMR_ACT_Pos)
#define | TIMER_CTL_ADC_TEEN_Pos (8)
#define | TIMER_CTL_ADC_TEEN_Msk (0x1ul << TIMER_CTL_ADC_TEEN_Pos)
#define | TIMER_CTL_DAC_TEEN_Pos (9)
#define | TIMER_CTL_DAC_TEEN_Msk (0x1ul << TIMER_CTL_DAC_TEEN_Pos)
#define | TIMER_CTL_PDMA_TEEN_Pos (10)
#define | TIMER_CTL_PDMA_TEEN_Msk (0x1ul << TIMER_CTL_PDMA_TEEN_Pos)
#define | TIMER_CTL_CAP_TRG_EN_Pos (11)
#define | TIMER_CTL_CAP_TRG_EN_Msk (0x1ul << TIMER_CTL_CAP_TRG_EN_Pos)
#define | TIMER_CTL_EVENT_EN_Pos (12)
#define | TIMER_CTL_EVENT_EN_Msk (0x1ul << TIMER_CTL_EVENT_EN_Pos)
#define | TIMER_CTL_EVENT_EDGE_Pos (13)
#define | TIMER_CTL_EVENT_EDGE_Msk (0x1ul << TIMER_CTL_EVENT_EDGE_Pos)
#define | TIMER_CTL_EVNT_DEB_EN_Pos (14)
#define | TIMER_CTL_EVNT_DEB_EN_Msk (0x1ul << TIMER_CTL_EVNT_DEB_EN_Pos)
#define | TIMER_CTL_TCAP_EN_Pos (16)
#define | TIMER_CTL_TCAP_EN_Msk (0x1ul << TIMER_CTL_TCAP_EN_Pos)
#define | TIMER_CTL_TCAP_MODE_Pos (17)
#define | TIMER_CTL_TCAP_MODE_Msk (0x1ul << TIMER_CTL_TCAP_MODE_Pos)
#define | TIMER_CTL_TCAP_EDGE_Pos (18)
#define | TIMER_CTL_TCAP_EDGE_Msk (0x3ul << TIMER_CTL_TCAP_EDGE_Pos)
#define | TIMER_CTL_TCAP_CNT_MODE_Pos (20)
#define | TIMER_CTL_TCAP_CNT_MODE_Msk (0x1ul << TIMER_CTL_TCAP_CNT_MODE_Pos)
#define | TIMER_CTL_TCAP_DEB_EN_Pos (22)
#define | TIMER_CTL_TCAP_DEB_EN_Msk (0x1ul << TIMER_CTL_TCAP_DEB_EN_Pos)
#define | TIMER_CTL_INTR_TRG_EN_Pos (24)
#define | TIMER_CTL_INTR_TRG_EN_Msk (0x1ul << TIMER_CTL_INTR_TRG_EN_Pos)
#define | TIMER_PRECNT_PRESCALE_CNT_Pos (0)
#define | TIMER_PRECNT_PRESCALE_CNT_Msk (0xfful << TIMER_PRECNT_PRESCALE_CNT_Pos)
#define | TIMER_CMPR_TMR_CMP_Pos (0)
#define | TIMER_CMPR_TMR_CMP_Msk (0xfffffful << TIMER_CMPR_TMR_CMP_Pos)
#define | TIMER_IER_TMR_IE_Pos (0)
#define | TIMER_IER_TMR_IE_Msk (0x1ul << TIMER_IER_TMR_IE_Pos)
#define | TIMER_IER_TCAP_IE_Pos (1)
#define | TIMER_IER_TCAP_IE_Msk (0x1ul << TIMER_IER_TCAP_IE_Pos)
#define | TIMER_ISR_TMR_IS_Pos (0)
#define | TIMER_ISR_TMR_IS_Msk (0x1ul << TIMER_ISR_TMR_IS_Pos)
#define | TIMER_ISR_TCAP_IS_Pos (1)
#define | TIMER_ISR_TCAP_IS_Msk (0x1ul << TIMER_ISR_TCAP_IS_Pos)
#define | TIMER_ISR_TMR_WAKE_STS_Pos (4)
#define | TIMER_ISR_TMR_WAKE_STS_Msk (0x1ul << TIMER_ISR_TMR_WAKE_STS_Pos)
#define | TIMER_ISR_NCAP_DET_STS_Pos (5)
#define | TIMER_ISR_NCAP_DET_STS_Msk (0x1ul << TIMER_ISR_NCAP_DET_STS_Pos)
#define | TIMER_DR_TDR_Pos (0)
#define | TIMER_DR_TDR_Msk (0xfffffful << TIMER_DR_TDR_Pos)
#define | TIMER_TCAP_CAP_Pos (0)
#define | TIMER_TCAP_CAP_Msk (0xfffffful << TIMER_TCAP_CAP_Pos)
#define | UART_DAT_DAT_Pos (0)
#define | UART_DAT_DAT_Msk (0xfful << UART_DAT_DAT_Pos)
#define | UART_CTL_RX_RST_Pos (0)
#define | UART_CTL_RX_RST_Msk (0x1ul << UART_CTL_RX_RST_Pos)
#define | UART_CTL_TX_RST_Pos (1)
#define | UART_CTL_TX_RST_Msk (0x1ul << UART_CTL_TX_RST_Pos)
#define | UART_CTL_RX_DIS_Pos (2)
#define | UART_CTL_RX_DIS_Msk (0x1ul << UART_CTL_RX_DIS_Pos)
#define | UART_CTL_TX_DIS_Pos (3)
#define | UART_CTL_TX_DIS_Msk (0x1ul << UART_CTL_TX_DIS_Pos)
#define | UART_CTL_AUTO_RTS_EN_Pos (4)
#define | UART_CTL_AUTO_RTS_EN_Msk (0x1ul << UART_CTL_AUTO_RTS_EN_Pos)
#define | UART_CTL_AUTO_CTS_EN_Pos (5)
#define | UART_CTL_AUTO_CTS_EN_Msk (0x1ul << UART_CTL_AUTO_CTS_EN_Pos)
#define | UART_CTL_DMA_RX_EN_Pos (6)
#define | UART_CTL_DMA_RX_EN_Msk (0x1ul << UART_CTL_DMA_RX_EN_Pos)
#define | UART_CTL_DMA_TX_EN_Pos (7)
#define | UART_CTL_DMA_TX_EN_Msk (0x1ul << UART_CTL_DMA_TX_EN_Pos)
#define | UART_CTL_WAKE_CTS_EN_Pos (8)
#define | UART_CTL_WAKE_CTS_EN_Msk (0x1ul << UART_CTL_WAKE_CTS_EN_Pos)
#define | UART_CTL_WAKE_DATA_EN_Pos (9)
#define | UART_CTL_WAKE_DATA_EN_Msk (0x1ul << UART_CTL_WAKE_DATA_EN_Pos)
#define | UART_CTL_ABAUD_EN_Pos (12)
#define | UART_CTL_ABAUD_EN_Msk (0x1ul << UART_CTL_ABAUD_EN_Pos)
#define | UART_TLCTL_DATA_LEN_Pos (0)
#define | UART_TLCTL_DATA_LEN_Msk (0x3ul << UART_TLCTL_DATA_LEN_Pos)
#define | UART_TLCTL_NSB_Pos (2)
#define | UART_TLCTL_NSB_Msk (0x1ul << UART_TLCTL_NSB_Pos)
#define | UART_TLCTL_PBE_Pos (3)
#define | UART_TLCTL_PBE_Msk (0x1ul << UART_TLCTL_PBE_Pos)
#define | UART_TLCTL_EPE_Pos (4)
#define | UART_TLCTL_EPE_Msk (0x1ul << UART_TLCTL_EPE_Pos)
#define | UART_TLCTL_SPE_Pos (5)
#define | UART_TLCTL_SPE_Msk (0x1ul << UART_TLCTL_SPE_Pos)
#define | UART_TLCTL_BCB_Pos (6)
#define | UART_TLCTL_BCB_Msk (0x1ul << UART_TLCTL_BCB_Pos)
#define | UART_TLCTL_RFITL_Pos (8)
#define | UART_TLCTL_RFITL_Msk (0x3ul << UART_TLCTL_RFITL_Pos)
#define | UART_TLCTL_RTS_TRI_LEV_Pos (12)
#define | UART_TLCTL_RTS_TRI_LEV_Msk (0x3ul << UART_TLCTL_RTS_TRI_LEV_Pos)
#define | UART_IER_RDA_IE_Pos (0)
#define | UART_IER_RDA_IE_Msk (0x1ul << UART_IER_RDA_IE_Pos)
#define | UART_IER_THRE_IE_Pos (1)
#define | UART_IER_THRE_IE_Msk (0x1ul << UART_IER_THRE_IE_Pos)
#define | UART_IER_RLS_IE_Pos (2)
#define | UART_IER_RLS_IE_Msk (0x1ul << UART_IER_RLS_IE_Pos)
#define | UART_IER_MODEM_IE_Pos (3)
#define | UART_IER_MODEM_IE_Msk (0x1ul << UART_IER_MODEM_IE_Pos)
#define | UART_IER_RTO_IE_Pos (4)
#define | UART_IER_RTO_IE_Msk (0x1ul << UART_IER_RTO_IE_Pos)
#define | UART_IER_BUF_ERR_IE_Pos (5)
#define | UART_IER_BUF_ERR_IE_Msk (0x1ul << UART_IER_BUF_ERR_IE_Pos)
#define | UART_IER_WAKE_IE_Pos (6)
#define | UART_IER_WAKE_IE_Msk (0x1ul << UART_IER_WAKE_IE_Pos)
#define | UART_IER_ABAUD_IE_Pos (7)
#define | UART_IER_ABAUD_IE_Msk (0x1ul << UART_IER_ABAUD_IE_Pos)
#define | UART_IER_LIN_IE_Pos (8)
#define | UART_IER_LIN_IE_Msk (0x1ul << UART_IER_LIN_IE_Pos)
#define | UART_ISR_RDA_IS_Pos (0)
#define | UART_ISR_RDA_IS_Msk (0x1ul << UART_ISR_RDA_IS_Pos)
#define | UART_ISR_THRE_IS_Pos (1)
#define | UART_ISR_THRE_IS_Msk (0x1ul << UART_ISR_THRE_IS_Pos)
#define | UART_ISR_RLS_IS_Pos (2)
#define | UART_ISR_RLS_IS_Msk (0x1ul << UART_ISR_RLS_IS_Pos)
#define | UART_ISR_MODEM_IS_Pos (3)
#define | UART_ISR_MODEM_IS_Msk (0x1ul << UART_ISR_MODEM_IS_Pos)
#define | UART_ISR_RTO_IS_Pos (4)
#define | UART_ISR_RTO_IS_Msk (0x1ul << UART_ISR_RTO_IS_Pos)
#define | UART_ISR_BUF_ERR_IS_Pos (5)
#define | UART_ISR_BUF_ERR_IS_Msk (0x1ul << UART_ISR_BUF_ERR_IS_Pos)
#define | UART_ISR_WAKE_IS_Pos (6)
#define | UART_ISR_WAKE_IS_Msk (0x1ul << UART_ISR_WAKE_IS_Pos)
#define | UART_ISR_ABAUD_IS_Pos (7)
#define | UART_ISR_ABAUD_IS_Msk (0x1ul << UART_ISR_ABAUD_IS_Pos)
#define | UART_ISR_LIN_IS_Pos (8)
#define | UART_ISR_LIN_IS_Msk (0x1ul << UART_ISR_LIN_IS_Pos)
#define | UART_TRSR_RS485_ADDET_F_Pos (0)
#define | UART_TRSR_RS485_ADDET_F_Msk (0x1ul << UART_TRSR_RS485_ADDET_F_Pos)
#define | UART_TRSR_ABAUD_F_Pos (1)
#define | UART_TRSR_ABAUD_F_Msk (0x1ul << UART_TRSR_ABAUD_F_Pos)
#define | UART_TRSR_ABAUD_TOUT_F_Pos (2)
#define | UART_TRSR_ABAUD_TOUT_F_Msk (0x1ul << UART_TRSR_ABAUD_TOUT_F_Pos)
#define | UART_TRSR_LIN_TX_F_Pos (3)
#define | UART_TRSR_LIN_TX_F_Msk (0x1ul << UART_TRSR_LIN_TX_F_Pos)
#define | UART_TRSR_LIN_RX_F_Pos (4)
#define | UART_TRSR_LIN_RX_F_Msk (0x1ul << UART_TRSR_LIN_RX_F_Pos)
#define | UART_TRSR_BIT_ERR_F_Pos (5)
#define | UART_TRSR_BIT_ERR_F_Msk (0x1ul << UART_TRSR_BIT_ERR_F_Pos)
#define | UART_TRSR_LIN_RX_SYNC_ERR_F_Pos (8)
#define | UART_TRSR_LIN_RX_SYNC_ERR_F_Msk (0x1ul << UART_TRSR_LIN_RX_SYNC_ERR_F_Pos)
#define | UART_FSR_RX_OVER_F_Pos (0)
#define | UART_FSR_RX_OVER_F_Msk (0x1ul << UART_FSR_RX_OVER_F_Pos)
#define | UART_FSR_RX_EMPTY_F_Pos (1)
#define | UART_FSR_RX_EMPTY_F_Msk (0x1ul << UART_FSR_RX_EMPTY_F_Pos)
#define | UART_FSR_RX_FULL_F_Pos (2)
#define | UART_FSR_RX_FULL_F_Msk (0x1ul << UART_FSR_RX_FULL_F_Pos)
#define | UART_FSR_PE_F_Pos (4)
#define | UART_FSR_PE_F_Msk (0x1ul << UART_FSR_PE_F_Pos)
#define | UART_FSR_FE_F_Pos (5)
#define | UART_FSR_FE_F_Msk (0x1ul << UART_FSR_FE_F_Pos)
#define | UART_FSR_BI_F_Pos (6)
#define | UART_FSR_BI_F_Msk (0x1ul << UART_FSR_BI_F_Pos)
#define | UART_FSR_TX_OVER_F_Pos (8)
#define | UART_FSR_TX_OVER_F_Msk (0x1ul << UART_FSR_TX_OVER_F_Pos)
#define | UART_FSR_TX_EMPTY_F_Pos (9)
#define | UART_FSR_TX_EMPTY_F_Msk (0x1ul << UART_FSR_TX_EMPTY_F_Pos)
#define | UART_FSR_TX_FULL_F_Pos (10)
#define | UART_FSR_TX_FULL_F_Msk (0x1ul << UART_FSR_TX_FULL_F_Pos)
#define | UART_FSR_TE_F_Pos (11)
#define | UART_FSR_TE_F_Msk (0x1ul << UART_FSR_TE_F_Pos)
#define | UART_FSR_RX_POINTER_F_Pos (16)
#define | UART_FSR_RX_POINTER_F_Msk (0x1ful << UART_FSR_RX_POINTER_F_Pos)
#define | UART_FSR_TX_POINTER_F_Pos (24)
#define | UART_FSR_TX_POINTER_F_Msk (0x1ful << UART_FSR_TX_POINTER_F_Pos)
#define | UART_MCSR_LEV_RTS_Pos (0)
#define | UART_MCSR_LEV_RTS_Msk (0x1ul << UART_MCSR_LEV_RTS_Pos)
#define | UART_MCSR_RTS_ST_Pos (1)
#define | UART_MCSR_RTS_ST_Msk (0x1ul << UART_MCSR_RTS_ST_Pos)
#define | UART_MCSR_LEV_CTS_Pos (16)
#define | UART_MCSR_LEV_CTS_Msk (0x1ul << UART_MCSR_LEV_CTS_Pos)
#define | UART_MCSR_CTS_ST_Pos (17)
#define | UART_MCSR_CTS_ST_Msk (0x1ul << UART_MCSR_CTS_ST_Pos)
#define | UART_MCSR_DCT_F_Pos (18)
#define | UART_MCSR_DCT_F_Msk (0x1ul << UART_MCSR_DCT_F_Pos)
#define | UART_TMCTL_TOIC_Pos (0)
#define | UART_TMCTL_TOIC_Msk (0x1fful << UART_TMCTL_TOIC_Pos)
#define | UART_TMCTL_DLY_Pos (16)
#define | UART_TMCTL_DLY_Msk (0xfful << UART_TMCTL_DLY_Pos)
#define | UART_BAUD_BRD_Pos (0)
#define | UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)
#define | UART_BAUD_DIV_16_EN_Pos (31)
#define | UART_BAUD_DIV_16_EN_Msk (0x1ul << UART_BAUD_DIV_16_EN_Pos)
#define | UART_IRCR_TX_SELECT_Pos (1)
#define | UART_IRCR_TX_SELECT_Msk (0x1ul << UART_IRCR_TX_SELECT_Pos)
#define | UART_IRCR_INV_TX_Pos (5)
#define | UART_IRCR_INV_TX_Msk (0x1ul << UART_IRCR_INV_TX_Pos)
#define | UART_IRCR_INV_RX_Pos (6)
#define | UART_IRCR_INV_RX_Msk (0x1ul << UART_IRCR_INV_RX_Pos)
#define | UART_ALT_CTL_LIN_TX_BCNT_Pos (0)
#define | UART_ALT_CTL_LIN_TX_BCNT_Msk (0x7ul << UART_ALT_CTL_LIN_TX_BCNT_Pos)
#define | UART_ALT_CTL_LIN_HEAD_SEL_Pos (4)
#define | UART_ALT_CTL_LIN_HEAD_SEL_Msk (0x3ul << UART_ALT_CTL_LIN_HEAD_SEL_Pos)
#define | UART_ALT_CTL_LIN_RX_EN_Pos (6)
#define | UART_ALT_CTL_LIN_RX_EN_Msk (0x1ul << UART_ALT_CTL_LIN_RX_EN_Pos)
#define | UART_ALT_CTL_LIN_TX_EN_Pos (7)
#define | UART_ALT_CTL_LIN_TX_EN_Msk (0x1ul << UART_ALT_CTL_LIN_TX_EN_Pos)
#define | UART_ALT_CTL_Bit_ERR_EN_Pos (8)
#define | UART_ALT_CTL_Bit_ERR_EN_Msk (0x1ul << UART_ALT_CTL_Bit_ERR_EN_Pos)
#define | UART_ALT_CTL_RS485_NMM_Pos (16)
#define | UART_ALT_CTL_RS485_NMM_Msk (0x1ul << UART_ALT_CTL_RS485_NMM_Pos)
#define | UART_ALT_CTL_RS485_AAD_Pos (17)
#define | UART_ALT_CTL_RS485_AAD_Msk (0x1ul << UART_ALT_CTL_RS485_AAD_Pos)
#define | UART_ALT_CTL_RS485_AUD_Pos (18)
#define | UART_ALT_CTL_RS485_AUD_Msk (0x1ul << UART_ALT_CTL_RS485_AUD_Pos)
#define | UART_ALT_CTL_RS485_ADD_EN_Pos (19)
#define | UART_ALT_CTL_RS485_ADD_EN_Msk (0x1ul << UART_ALT_CTL_RS485_ADD_EN_Pos)
#define | UART_ALT_CTL_ADDR_PID_MATCH_Pos (24)
#define | UART_ALT_CTL_ADDR_PID_MATCH_Msk (0xfful << UART_ALT_CTL_ADDR_PID_MATCH_Pos)
#define | UART_FUN_SEL_FUN_SEL_Pos (0)
#define | UART_FUN_SEL_FUN_SEL_Msk (0x3ul << UART_FUN_SEL_FUN_SEL_Pos)
#define | USBD_CTL_USB_EN_Pos (0)
#define | USBD_CTL_USB_EN_Msk (0x1ul << USBD_CTL_USB_EN_Pos)
#define | USBD_CTL_PHY_EN_Pos (1)
#define | USBD_CTL_PHY_EN_Msk (0x1ul << USBD_CTL_PHY_EN_Pos)
#define | USBD_CTL_PWRDB_Pos (2)
#define | USBD_CTL_PWRDB_Msk (0x1ul << USBD_CTL_PWRDB_Pos)
#define | USBD_CTL_DPPU_EN_Pos (3)
#define | USBD_CTL_DPPU_EN_Msk (0x1ul << USBD_CTL_DPPU_EN_Pos)
#define | USBD_CTL_DRVSE0_Pos (4)
#define | USBD_CTL_DRVSE0_Msk (0x1ul << USBD_CTL_DRVSE0_Pos)
#define | USBD_CTL_RWAKEUP_Pos (8)
#define | USBD_CTL_RWAKEUP_Msk (0x1ul << USBD_CTL_RWAKEUP_Pos)
#define | USBD_CTL_WAKEUP_EN_Pos (9)
#define | USBD_CTL_WAKEUP_EN_Msk (0x1ul << USBD_CTL_WAKEUP_EN_Pos)
#define | USBD_BUSSTS_USBRST_Pos (0)
#define | USBD_BUSSTS_USBRST_Msk (0x1ul << USBD_BUSSTS_USBRST_Pos)
#define | USBD_BUSSTS_SUSPEND_Pos (1)
#define | USBD_BUSSTS_SUSPEND_Msk (0x1ul << USBD_BUSSTS_SUSPEND_Pos)
#define | USBD_BUSSTS_RESUME_Pos (2)
#define | USBD_BUSSTS_RESUME_Msk (0x1ul << USBD_BUSSTS_RESUME_Pos)
#define | USBD_BUSSTS_TIMEOUT_Pos (3)
#define | USBD_BUSSTS_TIMEOUT_Msk (0x1ul << USBD_BUSSTS_TIMEOUT_Pos)
#define | USBD_BUSSTS_FLDET_Pos (4)
#define | USBD_BUSSTS_FLDET_Msk (0x1ul << USBD_BUSSTS_FLDET_Pos)
#define | USBD_INTEN_BUSEVT_IE_Pos (0)
#define | USBD_INTEN_BUSEVT_IE_Msk (0x1ul << USBD_INTEN_BUSEVT_IE_Pos)
#define | USBD_INTEN_USBEVT_IE_Pos (1)
#define | USBD_INTEN_USBEVT_IE_Msk (0x1ul << USBD_INTEN_USBEVT_IE_Pos)
#define | USBD_INTEN_FLDET_IE_Pos (2)
#define | USBD_INTEN_FLDET_IE_Msk (0x1ul << USBD_INTEN_FLDET_IE_Pos)
#define | USBD_INTEN_WAKEUP_IE_Pos (3)
#define | USBD_INTEN_WAKEUP_IE_Msk (0x1ul << USBD_INTEN_WAKEUP_IE_Pos)
#define | USBD_INTSTS_BUS_STS_Pos (0)
#define | USBD_INTSTS_BUS_STS_Msk (0x1ul << USBD_INTSTS_BUS_STS_Pos)
#define | USBD_INTSTS_USB_STS_Pos (1)
#define | USBD_INTSTS_USB_STS_Msk (0x1ul << USBD_INTSTS_USB_STS_Pos)
#define | USBD_INTSTS_FLD_STS_Pos (2)
#define | USBD_INTSTS_FLD_STS_Msk (0x1ul << USBD_INTSTS_FLD_STS_Pos)
#define | USBD_INTSTS_WKEUP_STS_Pos (3)
#define | USBD_INTSTS_WKEUP_STS_Msk (0x1ul << USBD_INTSTS_WKEUP_STS_Pos)
#define | USBD_INTSTS_EPEVT0_Pos (16)
#define | USBD_INTSTS_EPEVT0_Msk (0x1ul << USBD_INTSTS_EPEVT0_Pos)
#define | USBD_INTSTS_EPEVT1_Pos (17)
#define | USBD_INTSTS_EPEVT1_Msk (0x1ul << USBD_INTSTS_EPEVT1_Pos)
#define | USBD_INTSTS_EPEVT2_Pos (18)
#define | USBD_INTSTS_EPEVT2_Msk (0x1ul << USBD_INTSTS_EPEVT2_Pos)
#define | USBD_INTSTS_EPEVT3_Pos (19)
#define | USBD_INTSTS_EPEVT3_Msk (0x1ul << USBD_INTSTS_EPEVT3_Pos)
#define | USBD_INTSTS_EPEVT4_Pos (20)
#define | USBD_INTSTS_EPEVT4_Msk (0x1ul << USBD_INTSTS_EPEVT4_Pos)
#define | USBD_INTSTS_EPEVT5_Pos (21)
#define | USBD_INTSTS_EPEVT5_Msk (0x1ul << USBD_INTSTS_EPEVT5_Pos)
#define | USBD_INTSTS_EPEVT6_Pos (22)
#define | USBD_INTSTS_EPEVT6_Msk (0x1ul << USBD_INTSTS_EPEVT6_Pos)
#define | USBD_INTSTS_EPEVT7_Pos (23)
#define | USBD_INTSTS_EPEVT7_Msk (0x1ul << USBD_INTSTS_EPEVT7_Pos)
#define | USBD_INTSTS_SETUP_Pos (31)
#define | USBD_INTSTS_SETUP_Msk (0x1ul << USBD_INTSTS_SETUP_Pos)
#define | USBD_FADDR_FADDR_Pos (0)
#define | USBD_FADDR_FADDR_Msk (0x7ful << USBD_FADDR_FADDR_Pos)
#define | USBD_EPSTS_OVERRUN_Pos (7)
#define | USBD_EPSTS_OVERRUN_Msk (0x1ul << USBD_EPSTS_OVERRUN_Pos)
#define | USBD_EPSTS_EPSTS0_Pos (8)
#define | USBD_EPSTS_EPSTS0_Msk (0xful << USBD_EPSTS_EPSTS0_Pos)
#define | USBD_EPSTS_EPSTS1_Pos (12)
#define | USBD_EPSTS_EPSTS1_Msk (0xful << USBD_EPSTS_EPSTS1_Pos)
#define | USBD_EPSTS_EPSTS2_Pos (16)
#define | USBD_EPSTS_EPSTS2_Msk (0xful << USBD_EPSTS_EPSTS2_Pos)
#define | USBD_EPSTS_EPSTS3_Pos (20)
#define | USBD_EPSTS_EPSTS3_Msk (0xful << USBD_EPSTS_EPSTS3_Pos)
#define | USBD_EPSTS_EPSTS4_Pos (24)
#define | USBD_EPSTS_EPSTS4_Msk (0xful << USBD_EPSTS_EPSTS4_Pos)
#define | USBD_EPSTS_EPSTS5_Pos (28)
#define | USBD_EPSTS_EPSTS5_Msk (0xful << USBD_EPSTS_EPSTS5_Pos)
#define | USBD_BUFSEG_BUFSEG_Pos (3)
#define | USBD_BUFSEG_BUFSEG_Msk (0x3ful << USBD_BUFSEG_BUFSEG_Pos)
#define | USBD_EPSTS2_EPSTS6_Pos (0)
#define | USBD_EPSTS2_EPSTS6_Msk (0x7ul << USBD_EPSTS2_EPSTS6_Pos)
#define | USBD_EPSTS2_EPSTS7_Pos (4)
#define | USBD_EPSTS2_EPSTS7_Msk (0x7ul << USBD_EPSTS2_EPSTS7_Pos)
#define | USBD_BUFSEG_BUFSEG_Pos (3)
#define | USBD_BUFSEG_BUFSEG_Msk (0x3ful << USBD_BUFSEG_BUFSEG_Pos)
#define | USBD_MXPLD_MXPLD_Pos (0)
#define | USBD_MXPLD_MXPLD_Msk (0x1fful << USBD_MXPLD_MXPLD_Pos)
#define | USBD_CFG_EP_NUM_Pos (0)
#define | USBD_CFG_EP_NUM_Msk (0xful << USBD_CFG_EP_NUM_Pos)
#define | USBD_CFG_ISOCH_Pos (4)
#define | USBD_CFG_ISOCH_Msk (0x1ul << USBD_CFG_ISOCH_Pos)
#define | USBD_CFG_EPMODE_Pos (5)
#define | USBD_CFG_EPMODE_Msk (0x3ul << USBD_CFG_EPMODE_Pos)
#define | USBD_CFG_DSQ_SYNC_Pos (7)
#define | USBD_CFG_DSQ_SYNC_Msk (0x1ul << USBD_CFG_DSQ_SYNC_Pos)
#define | USBD_CFG_CSTALL_Pos (8)
#define | USBD_CFG_CSTALL_Msk (0x1ul << USBD_CFG_CSTALL_Pos)
#define | USBD_CFG_SSTALL_Pos (9)
#define | USBD_CFG_SSTALL_Msk (0x1ul << USBD_CFG_SSTALL_Pos)
#define | USBD_CFG_CLRRDY_Pos (15)
#define | USBD_CFG_CLRRDY_Msk (0x1ul << USBD_CFG_CLRRDY_Pos)
#define | USBD_PDMA_PDMA_RW_Pos (0)
#define | USBD_PDMA_PDMA_RW_Msk (0x1ul << USBD_PDMA_PDMA_RW_Pos)
#define | USBD_PDMA_PDMA_TRG_Pos (1)
#define | USBD_PDMA_PDMA_TRG_Msk (0x1ul << USBD_PDMA_PDMA_TRG_Pos)
#define | USBD_PDMA_BYTEM_Pos (2)
#define | USBD_PDMA_BYTEM_Msk (0x1ul << USBD_PDMA_BYTEM_Pos)
#define | USBD_PDMA_PDMA_RST_Pos (3)
#define | USBD_PDMA_PDMA_RST_Msk (0x1ul << USBD_PDMA_PDMA_RST_Pos)
#define | WDT_CTL_WTR_Pos (0)
#define | WDT_CTL_WTR_Msk (0x1ul << WDT_CTL_WTR_Pos)
#define | WDT_CTL_WTRE_Pos (1)
#define | WDT_CTL_WTRE_Msk (0x1ul << WDT_CTL_WTRE_Pos)
#define | WDT_CTL_WTWKE_Pos (2)
#define | WDT_CTL_WTWKE_Msk (0x1ul << WDT_CTL_WTWKE_Pos)
#define | WDT_CTL_WTE_Pos (3)
#define | WDT_CTL_WTE_Msk (0x1ul << WDT_CTL_WTE_Pos)
#define | WDT_CTL_WTIS_Pos (4)
#define | WDT_CTL_WTIS_Msk (0x7ul << WDT_CTL_WTIS_Pos)
#define | WDT_CTL_WTRDSEL_Pos (8)
#define | WDT_CTL_WTRDSEL_Msk (0x3ul << WDT_CTL_WTRDSEL_Pos)
#define | WDT_IER_IE_Pos (0)
#define | WDT_IER_IE_Msk (0x1ul << WDT_IER_IE_Pos)
#define | WDT_ISR_IS_Pos (0)
#define | WDT_ISR_IS_Msk (0x1ul << WDT_ISR_IS_Pos)
#define | WDT_ISR_RST_IS_Pos (1)
#define | WDT_ISR_RST_IS_Msk (0x1ul << WDT_ISR_RST_IS_Pos)
#define | WDT_ISR_WAKE_IS_Pos (2)
#define | WDT_ISR_WAKE_IS_Msk (0x1ul << WDT_ISR_WAKE_IS_Pos)
#define | WWDT_RLD_WWDTRLD_Pos (0)
#define | WWDT_RLD_WWDTRLD_Msk (0xfffffffful << WWDT_RLD_RLD_Pos)
#define | WWDT_CR_WWDTEN_Pos (0)
#define | WWDT_CR_WWDTEN_Msk (0x1ul << WWDT_CR_WWDTEN_Pos)
#define | WWDT_CR_PERIODSEL_Pos (8)
#define | WWDT_CR_PERIODSEL_Msk (0xful << WWDT_CR_PERIODSEL_Pos)
#define | WWDT_CR_WINCMP_Pos (16)
#define | WWDT_CR_WINCMP_Msk (0x3ful << WWDT_CR_WINCMP_Pos)
#define | WWDT_CR_DBGEN_Pos (31)
#define | WWDT_CR_DBGEN_Msk (0x1ul << WWDT_CR_DBGEN_Pos)
#define | WWDT_IER_WWDTIE_Pos (0)
#define | WWDT_IER_WWDTIE_Msk (0x1ul << WWDT_IER_WWDTIE_Pos)
#define | WWDT_STS_IF_Pos (0)
#define | WWDT_STS_IF_Msk (0x1ul << WWDT_STS_IF_Pos)
#define | WWDT_STS_RF_Pos (1)
#define | WWDT_STS_RF_Msk (0x1ul << WWDT_STS_RF_Pos)
#define | WWDT_VAL_WWDTVAL_Pos (0)
#define | WWDT_VAL_WWDTVAL_Msk (0x3ful << WWDT_VAL_WWDTVAL_Pos)

## Typedefs
typedef enum IRQn | IRQn_Type
typedef volatile unsigned char | vu8
| Define 8-bit unsigned volatile data type. More...
typedef volatile unsigned short | vu16
| Define 16-bit unsigned volatile data type. More...
typedef volatile unsigned long | vu32
| Define 32-bit unsigned volatile data type. More...

## Enumerations
enum | IRQn { NonMaskableInt_IRQn = -14 , HardFault_IRQn = -13 , SVCall_IRQn = -5 , PendSV_IRQn = -2 , SysTick_IRQn = -1 , BOD_IRQn = 0 , WDT_IRQn = 1 , EINT0_IRQn = 2 , EINT1_IRQn = 3 , GPABC_IRQn = 4 , GPDEF_IRQn = 5 , PWM0_IRQn = 6 , PWM1_IRQn = 7 , TMR0_IRQn = 8 , TMR1_IRQn = 9 , TMR2_IRQn = 10 , TMR3_IRQn = 11 , UART0_IRQn = 12 , UART1_IRQn = 13 , SPI0_IRQn = 14 , SPI1_IRQn = 15 , SPI2_IRQn = 16 , HIRC_IRQn = 17 , I2C0_IRQn = 18 , I2C1_IRQn = 19 , SC2_IRQn = 20 , SC0_IRQn = 21 , SC1_IRQn = 22 , USBD_IRQn = 23 , LCD_IRQn = 25 , PDMA_IRQn = 26 , I2S_IRQn = 27 , PDWU_IRQn = 28 , ADC_IRQn = 29 , DAC_IRQn = 30 , RTC_IRQn = 31 }

## Detailed Description

Nano100 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Nano100 series MCU.

Version
  V1.00

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2018 Nuvoton Technology Corp. All rights reserved.

Definition in file Nano100Series.h.

## Macro Definition Documentation

## ◆ DMA_CRC_CHECKSUM_CRC_CHECKSUM_Msk

#define DMA_CRC_CHECKSUM_CRC_CHECKSUM_Msk (0xfffffffful << DMA_CRC_CHECKSUM_CRC_CHECKSUM_Pos)

DMA_CRC_T::CHECKSUM: CRC_CHECKSUM Mask

Definition at line 6357 of file Nano100Series.h.

## ◆ DMA_CRC_CHECKSUM_CRC_CHECKSUM_Pos

#define DMA_CRC_CHECKSUM_CRC_CHECKSUM_Pos (0)

DMA_CRC_T::CHECKSUM: CRC_CHECKSUM Position

Definition at line 6356 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CHECKSUM_COM_Msk

#define DMA_CRC_CTL_CHECKSUM_COM_Msk (0x1ul << DMA_CRC_CTL_CHECKSUM_COM_Pos)

DMA_CRC_T::CTL: CHECKSUM_COM Mask

Definition at line 6318 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CHECKSUM_COM_Pos

#define DMA_CRC_CTL_CHECKSUM_COM_Pos (27)

DMA_CRC_T::CTL: CHECKSUM_COM Position

Definition at line 6317 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CHECKSUM_RVS_Msk

#define DMA_CRC_CTL_CHECKSUM_RVS_Msk (0x1ul << DMA_CRC_CTL_CHECKSUM_RVS_Pos)

DMA_CRC_T::CTL: CHECKSUM_RVS Mask

Definition at line 6312 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CHECKSUM_RVS_Pos

#define DMA_CRC_CTL_CHECKSUM_RVS_Pos (25)

DMA_CRC_T::CTL: CHECKSUM_RVS Position

Definition at line 6311 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CPU_WDLEN_Msk

#define DMA_CRC_CTL_CPU_WDLEN_Msk (0x3ul << DMA_CRC_CTL_CPU_WDLEN_Pos)

DMA_CRC_T::CTL: CPU_WDLEN Mask

Definition at line 6321 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CPU_WDLEN_Pos

#define DMA_CRC_CTL_CPU_WDLEN_Pos (28)

DMA_CRC_T::CTL: CPU_WDLEN Position

Definition at line 6320 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CRC_MODE_Msk

#define DMA_CRC_CTL_CRC_MODE_Msk (0x3ul << DMA_CRC_CTL_CRC_MODE_Pos)

DMA_CRC_T::CTL: CRC_MODE Mask

Definition at line 6324 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CRC_MODE_Pos

#define DMA_CRC_CTL_CRC_MODE_Pos (30)

DMA_CRC_T::CTL: CRC_MODE Position

Definition at line 6323 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CRC_RST_Msk

#define DMA_CRC_CTL_CRC_RST_Msk (0x1ul << DMA_CRC_CTL_CRC_RST_Pos)

DMA_CRC_T::CTL: CRC_RST Mask

Definition at line 6303 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CRC_RST_Pos

#define DMA_CRC_CTL_CRC_RST_Pos (1)

DMA_CRC_T::CTL: CRC_RST Position

Definition at line 6302 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CRCCEN_Msk

#define DMA_CRC_CTL_CRCCEN_Msk (0x1ul << DMA_CRC_CTL_CRCCEN_Pos)

DMA_CRC_T::CTL: CRCCEN Mask

Definition at line 6300 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_CRCCEN_Pos

#define DMA_CRC_CTL_CRCCEN_Pos (0)

    @addtogroup DMA_CRC_CONST DMA_CRC Bit Field Definition
    Constant Definitions for DMA_CRC Controller

DMA_CRC_T::CTL: CRCCEN Position

Definition at line 6299 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_TRIG_EN_Msk

#define DMA_CRC_CTL_TRIG_EN_Msk (0x1ul << DMA_CRC_CTL_TRIG_EN_Pos)

DMA_CRC_T::CTL: TRIG_EN Mask

Definition at line 6306 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_TRIG_EN_Pos

#define DMA_CRC_CTL_TRIG_EN_Pos (23)

DMA_CRC_T::CTL: TRIG_EN Position

Definition at line 6305 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_WDATA_COM_Msk

#define DMA_CRC_CTL_WDATA_COM_Msk (0x1ul << DMA_CRC_CTL_WDATA_COM_Pos)

DMA_CRC_T::CTL: WDATA_COM Mask

Definition at line 6315 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_WDATA_COM_Pos

#define DMA_CRC_CTL_WDATA_COM_Pos (26)

DMA_CRC_T::CTL: WDATA_COM Position

Definition at line 6314 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_WDATA_RVS_Msk

#define DMA_CRC_CTL_WDATA_RVS_Msk (0x1ul << DMA_CRC_CTL_WDATA_RVS_Pos)

DMA_CRC_T::CTL: WDATA_RVS Mask

Definition at line 6309 of file Nano100Series.h.

## ◆ DMA_CRC_CTL_WDATA_RVS_Pos

#define DMA_CRC_CTL_WDATA_RVS_Pos (24)

DMA_CRC_T::CTL: WDATA_RVS Position

Definition at line 6308 of file Nano100Series.h.

## ◆ DMA_CRC_DMABCR_CRC_DMABCR_Msk

#define DMA_CRC_DMABCR_CRC_DMABCR_Msk (0xfffful << DMA_CRC_DMABCR_CRC_DMABCR_Pos)

DMA_CRC_T::DMABCR: CRC_DMABCR Mask

Definition at line 6330 of file Nano100Series.h.

## ◆ DMA_CRC_DMABCR_CRC_DMABCR_Pos

#define DMA_CRC_DMABCR_CRC_DMABCR_Pos (0)

DMA_CRC_T::DMABCR: CRC_DMABCR Position

Definition at line 6329 of file Nano100Series.h.

## ◆ DMA_CRC_DMACBCR_CRC_DMACBCR_Msk

#define DMA_CRC_DMACBCR_CRC_DMACBCR_Msk (0xfffful << DMA_CRC_DMACBCR_CRC_DMACBCR_Pos)

DMA_CRC_T::DMACBCR: CRC_DMACBCR Mask

Definition at line 6336 of file Nano100Series.h.

## ◆ DMA_CRC_DMACBCR_CRC_DMACBCR_Pos

#define DMA_CRC_DMACBCR_CRC_DMACBCR_Pos (0)

DMA_CRC_T::DMACBCR: CRC_DMACBCR Position

Definition at line 6335 of file Nano100Series.h.

## ◆ DMA_CRC_DMACSAR_CRC_DMACSAR_Msk

#define DMA_CRC_DMACSAR_CRC_DMACSAR_Msk (0xfffffffful << DMA_CRC_DMACSAR_CRC_DMACSAR_Pos)

DMA_CRC_T::DMACSAR: CRC_DMACSAR Mask

Definition at line 6333 of file Nano100Series.h.

## ◆ DMA_CRC_DMACSAR_CRC_DMACSAR_Pos

#define DMA_CRC_DMACSAR_CRC_DMACSAR_Pos (0)

DMA_CRC_T::DMACSAR: CRC_DMACSAR Position

Definition at line 6332 of file Nano100Series.h.

## ◆ DMA_CRC_DMAIER_BLKD_IE_Msk

#define DMA_CRC_DMAIER_BLKD_IE_Msk (0x1ul << DMA_CRC_DMAIER_BLKD_IE_Pos)

DMA_CRC_T::DMAIER: BLKD_IE Mask

Definition at line 6342 of file Nano100Series.h.

## ◆ DMA_CRC_DMAIER_BLKD_IE_Pos

#define DMA_CRC_DMAIER_BLKD_IE_Pos (1)

DMA_CRC_T::DMAIER: BLKD_IE Position

Definition at line 6341 of file Nano100Series.h.

## ◆ DMA_CRC_DMAIER_TABORT_IE_Msk

#define DMA_CRC_DMAIER_TABORT_IE_Msk (0x1ul << DMA_CRC_DMAIER_TABORT_IE_Pos)

DMA_CRC_T::DMAIER: TABORT_IE Mask

Definition at line 6339 of file Nano100Series.h.

## ◆ DMA_CRC_DMAIER_TABORT_IE_Pos

#define DMA_CRC_DMAIER_TABORT_IE_Pos (0)

DMA_CRC_T::DMAIER: TABORT_IE Position

Definition at line 6338 of file Nano100Series.h.

## ◆ DMA_CRC_DMAISR_BLKD_IF_Msk

#define DMA_CRC_DMAISR_BLKD_IF_Msk (0x1ul << DMA_CRC_DMAISR_BLKD_IF_Pos)

DMA_CRC_T::DMAISR: BLKD_IF Mask

Definition at line 6348 of file Nano100Series.h.

## ◆ DMA_CRC_DMAISR_BLKD_IF_Pos

#define DMA_CRC_DMAISR_BLKD_IF_Pos (1)

DMA_CRC_T::DMAISR: BLKD_IF Position

Definition at line 6347 of file Nano100Series.h.

## ◆ DMA_CRC_DMAISR_TABORT_IF_Msk

#define DMA_CRC_DMAISR_TABORT_IF_Msk (0x1ul << DMA_CRC_DMAISR_TABORT_IF_Pos)

DMA_CRC_T::DMAISR: TABORT_IF Mask

Definition at line 6345 of file Nano100Series.h.

## ◆ DMA_CRC_DMAISR_TABORT_IF_Pos

#define DMA_CRC_DMAISR_TABORT_IF_Pos (0)

DMA_CRC_T::DMAISR: TABORT_IF Position

Definition at line 6344 of file Nano100Series.h.

## ◆ DMA_CRC_DMASAR_CRC_DMASAR_Msk

#define DMA_CRC_DMASAR_CRC_DMASAR_Msk (0xfffffffful << DMA_CRC_DMASAR_CRC_DMASAR_Pos)

DMA_CRC_T::DMASAR: CRC_DMASAR Mask

Definition at line 6327 of file Nano100Series.h.

## ◆ DMA_CRC_DMASAR_CRC_DMASAR_Pos

#define DMA_CRC_DMASAR_CRC_DMASAR_Pos (0)

DMA_CRC_T::DMASAR: CRC_DMASAR Position

Definition at line 6326 of file Nano100Series.h.

## ◆ DMA_CRC_SEED_CRC_SEED_Msk

#define DMA_CRC_SEED_CRC_SEED_Msk (0xfffffffful << DMA_CRC_SEED_CRC_SEED_Pos)

DMA_CRC_T::SEED: CRC_SEED Mask

Definition at line 6354 of file Nano100Series.h.

## ◆ DMA_CRC_SEED_CRC_SEED_Pos

#define DMA_CRC_SEED_CRC_SEED_Pos (0)

DMA_CRC_T::SEED: CRC_SEED Position

Definition at line 6353 of file Nano100Series.h.

## ◆ DMA_CRC_WDATA_CRC_WDATA_Msk

#define DMA_CRC_WDATA_CRC_WDATA_Msk (0xfffffffful << DMA_CRC_WDATA_CRC_WDATA_Pos)

DMA_CRC_T::WDATA: CRC_WDATA Mask

Definition at line 6351 of file Nano100Series.h.

## ◆ DMA_CRC_WDATA_CRC_WDATA_Pos

#define DMA_CRC_WDATA_CRC_WDATA_Pos (0)

DMA_CRC_T::WDATA: CRC_WDATA Position

Definition at line 6350 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR0_CH1_SEL_Msk

#define DMA_GCR_DSSR0_CH1_SEL_Msk (0x1ful << DMA_GCR_DSSR0_CH1_SEL_Pos)

DMA_GCR_T::DSSR0: CH1_SEL Mask

Definition at line 6392 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR0_CH1_SEL_Pos

#define DMA_GCR_DSSR0_CH1_SEL_Pos (8)

DMA_GCR_T::DSSR0: CH1_SEL Position

Definition at line 6391 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR0_CH2_SEL_Msk

#define DMA_GCR_DSSR0_CH2_SEL_Msk (0x1ful << DMA_GCR_DSSR0_CH2_SEL_Pos)

DMA_GCR_T::DSSR0: CH2_SEL Mask

Definition at line 6395 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR0_CH2_SEL_Pos

#define DMA_GCR_DSSR0_CH2_SEL_Pos (16)

DMA_GCR_T::DSSR0: CH2_SEL Position

Definition at line 6394 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR0_CH3_SEL_Msk

#define DMA_GCR_DSSR0_CH3_SEL_Msk (0x1ful << DMA_GCR_DSSR0_CH3_SEL_Pos)

DMA_GCR_T::DSSR0: CH3_SEL Mask

Definition at line 6398 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR0_CH3_SEL_Pos

#define DMA_GCR_DSSR0_CH3_SEL_Pos (24)

DMA_GCR_T::DSSR0: CH3_SEL Position

Definition at line 6397 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR1_CH4_SEL_Msk

#define DMA_GCR_DSSR1_CH4_SEL_Msk (0x1ful << DMA_GCR_DSSR1_CH4_SEL_Pos)

DMA_GCR_T::DSSR1: CH4_SEL Mask

Definition at line 6401 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR1_CH4_SEL_Pos

#define DMA_GCR_DSSR1_CH4_SEL_Pos (0)

DMA_GCR_T::DSSR1: CH4_SEL Position

Definition at line 6400 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR1_CH5_SEL_Msk

#define DMA_GCR_DSSR1_CH5_SEL_Msk (0x1ful << DMA_GCR_DSSR1_CH5_SEL_Pos)

DMA_GCR_T::DSSR1: CH5_SEL Mask

Definition at line 6404 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR1_CH5_SEL_Pos

#define DMA_GCR_DSSR1_CH5_SEL_Pos (8)

DMA_GCR_T::DSSR1: CH5_SEL Position

Definition at line 6403 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR1_CH6_SEL_Msk

#define DMA_GCR_DSSR1_CH6_SEL_Msk (0x1ful << DMA_GCR_DSSR1_CH6_SEL_Pos)

DMA_GCR_T::DSSR1: CH6_SEL Mask

Definition at line 6407 of file Nano100Series.h.

## ◆ DMA_GCR_DSSR1_CH6_SEL_Pos

#define DMA_GCR_DSSR1_CH6_SEL_Pos (16)

DMA_GCR_T::DSSR1: CH6_SEL Position

Definition at line 6406 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK0_EN_Msk

#define DMA_GCR_GCRCSR_CLK0_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK0_EN_Pos)

DMA_GCR_T::GCRCSR: CLK0_EN Mask

Definition at line 6368 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK0_EN_Pos

#define DMA_GCR_GCRCSR_CLK0_EN_Pos (8)

    @addtogroup DMA_GCR_CONST DMA_GCR Bit Field Definition
    Constant Definitions for DMA_GCR Controller

DMA_GCR_T::GCRCSR: CLK0_EN Position

Definition at line 6367 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK1_EN_Msk

#define DMA_GCR_GCRCSR_CLK1_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK1_EN_Pos)

DMA_GCR_T::GCRCSR: CLK1_EN Mask

Definition at line 6371 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK1_EN_Pos

#define DMA_GCR_GCRCSR_CLK1_EN_Pos (9)

DMA_GCR_T::GCRCSR: CLK1_EN Position

Definition at line 6370 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK2_EN_Msk

#define DMA_GCR_GCRCSR_CLK2_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK2_EN_Pos)

DMA_GCR_T::GCRCSR: CLK2_EN Mask

Definition at line 6374 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK2_EN_Pos

#define DMA_GCR_GCRCSR_CLK2_EN_Pos (10)

DMA_GCR_T::GCRCSR: CLK2_EN Position

Definition at line 6373 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK3_EN_Msk

#define DMA_GCR_GCRCSR_CLK3_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK3_EN_Pos)

DMA_GCR_T::GCRCSR: CLK3_EN Mask

Definition at line 6377 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK3_EN_Pos

#define DMA_GCR_GCRCSR_CLK3_EN_Pos (11)

DMA_GCR_T::GCRCSR: CLK3_EN Position

Definition at line 6376 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK4_EN_Msk

#define DMA_GCR_GCRCSR_CLK4_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK4_EN_Pos)

DMA_GCR_T::GCRCSR: CLK4_EN Mask

Definition at line 6380 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK4_EN_Pos

#define DMA_GCR_GCRCSR_CLK4_EN_Pos (12)

DMA_GCR_T::GCRCSR: CLK4_EN Position

Definition at line 6379 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK5_EN_Msk

#define DMA_GCR_GCRCSR_CLK5_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK5_EN_Pos)

DMA_GCR_T::GCRCSR: CLK5_EN Mask

Definition at line 6383 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK5_EN_Pos

#define DMA_GCR_GCRCSR_CLK5_EN_Pos (13)

DMA_GCR_T::GCRCSR: CLK5_EN Position

Definition at line 6382 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK6_EN_Msk

#define DMA_GCR_GCRCSR_CLK6_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CLK6_EN_Pos)

DMA_GCR_T::GCRCSR: CLK6_EN Mask

Definition at line 6386 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CLK6_EN_Pos

#define DMA_GCR_GCRCSR_CLK6_EN_Pos (14)

DMA_GCR_T::GCRCSR: CLK6_EN Position

Definition at line 6385 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CRC_CLK_EN_Msk

#define DMA_GCR_GCRCSR_CRC_CLK_EN_Msk (0x1ul << DMA_GCR_GCRCSR_CRC_CLK_EN_Pos)

DMA_GCR_T::GCRCSR: CRC_CLK_EN Mask

Definition at line 6389 of file Nano100Series.h.

## ◆ DMA_GCR_GCRCSR_CRC_CLK_EN_Pos

#define DMA_GCR_GCRCSR_CRC_CLK_EN_Pos (24)

DMA_GCR_T::GCRCSR: CRC_CLK_EN Position

Definition at line 6388 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_CRC_INTR_Msk

#define DMA_GCR_GCRISR_CRC_INTR_Msk (0x1ul << DMA_GCR_GCRISR_CRC_INTR_Pos)

DMA_GCR_T::GCRISR: CRC_INTR Mask

Definition at line 6431 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_CRC_INTR_Pos

#define DMA_GCR_GCRISR_CRC_INTR_Pos (16)

DMA_GCR_T::GCRISR: CRC_INTR Position

Definition at line 6430 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR0_Msk

#define DMA_GCR_GCRISR_INTR0_Msk (0x1ul << DMA_GCR_GCRISR_INTR0_Pos)

DMA_GCR_T::GCRISR: INTR0 Mask

Definition at line 6410 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR0_Pos

#define DMA_GCR_GCRISR_INTR0_Pos (0)

DMA_GCR_T::GCRISR: INTR0 Position

Definition at line 6409 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR1_Msk

#define DMA_GCR_GCRISR_INTR1_Msk (0x1ul << DMA_GCR_GCRISR_INTR1_Pos)

DMA_GCR_T::GCRISR: INTR1 Mask

Definition at line 6413 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR1_Pos

#define DMA_GCR_GCRISR_INTR1_Pos (1)

DMA_GCR_T::GCRISR: INTR1 Position

Definition at line 6412 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR2_Msk

#define DMA_GCR_GCRISR_INTR2_Msk (0x1ul << DMA_GCR_GCRISR_INTR2_Pos)

DMA_GCR_T::GCRISR: INTR2 Mask

Definition at line 6416 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR2_Pos

#define DMA_GCR_GCRISR_INTR2_Pos (2)

DMA_GCR_T::GCRISR: INTR2 Position

Definition at line 6415 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR3_Msk

#define DMA_GCR_GCRISR_INTR3_Msk (0x1ul << DMA_GCR_GCRISR_INTR3_Pos)

DMA_GCR_T::GCRISR: INTR3 Mask

Definition at line 6419 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR3_Pos

#define DMA_GCR_GCRISR_INTR3_Pos (3)

DMA_GCR_T::GCRISR: INTR3 Position

Definition at line 6418 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR4_Msk

#define DMA_GCR_GCRISR_INTR4_Msk (0x1ul << DMA_GCR_GCRISR_INTR4_Pos)

DMA_GCR_T::GCRISR: INTR4 Mask

Definition at line 6422 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR4_Pos

#define DMA_GCR_GCRISR_INTR4_Pos (4)

DMA_GCR_T::GCRISR: INTR4 Position

Definition at line 6421 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR5_Msk

#define DMA_GCR_GCRISR_INTR5_Msk (0x1ul << DMA_GCR_GCRISR_INTR5_Pos)

DMA_GCR_T::GCRISR: INTR5 Mask

Definition at line 6425 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR5_Pos

#define DMA_GCR_GCRISR_INTR5_Pos (5)

DMA_GCR_T::GCRISR: INTR5 Position

Definition at line 6424 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR6_Msk

#define DMA_GCR_GCRISR_INTR6_Msk (0x1ul << DMA_GCR_GCRISR_INTR6_Pos)

DMA_GCR_T::GCRISR: INTR6 Mask

Definition at line 6428 of file Nano100Series.h.

## ◆ DMA_GCR_GCRISR_INTR6_Pos

#define DMA_GCR_GCRISR_INTR6_Pos (6)

DMA_GCR_T::GCRISR: INTR6 Position

Definition at line 6427 of file Nano100Series.h.

## ◆ EBI_EBICON_ExtBW16_Msk

#define EBI_EBICON_ExtBW16_Msk (0x1ul << EBI_EBICON_ExtBW16_Pos)

EBI_T::EBICON: ExtBW16 Mask

Definition at line 1756 of file Nano100Series.h.

## ◆ EBI_EBICON_ExtBW16_Pos

#define EBI_EBICON_ExtBW16_Pos (1)

EBI_T::EBICON: ExtBW16 Position

Definition at line 1755 of file Nano100Series.h.

## ◆ EBI_EBICON_ExtEN_Msk

#define EBI_EBICON_ExtEN_Msk (0x1ul << EBI_EBICON_ExtEN_Pos)

EBI_T::EBICON: ExtEN Mask

Definition at line 1753 of file Nano100Series.h.

## ◆ EBI_EBICON_ExtEN_Pos

#define EBI_EBICON_ExtEN_Pos (0)

    @addtogroup EBI_CONST EBI Bit Field Definition
    Constant Definitions for EBI Controller

EBI_T::EBICON: ExtEN Position

Definition at line 1752 of file Nano100Series.h.

## ◆ EBI_EBICON_ExttALE_Msk

#define EBI_EBICON_ExttALE_Msk (0x7ul << EBI_EBICON_ExttALE_Pos)

EBI_T::EBICON: ExttALE Mask

Definition at line 1765 of file Nano100Series.h.

## ◆ EBI_EBICON_ExttALE_Pos

#define EBI_EBICON_ExttALE_Pos (16)

EBI_T::EBICON: ExttALE Position

Definition at line 1764 of file Nano100Series.h.

## ◆ EBI_EBICON_MCLKDIV_Msk

#define EBI_EBICON_MCLKDIV_Msk (0x7ul << EBI_EBICON_MCLKDIV_Pos)

EBI_T::EBICON: MCLKDIV Mask

Definition at line 1759 of file Nano100Series.h.

## ◆ EBI_EBICON_MCLKDIV_Pos

#define EBI_EBICON_MCLKDIV_Pos (8)

EBI_T::EBICON: MCLKDIV Position

Definition at line 1758 of file Nano100Series.h.

## ◆ EBI_EBICON_MCLKEN_Msk

#define EBI_EBICON_MCLKEN_Msk (0x1ul << EBI_EBICON_MCLKEN_Pos)

EBI_T::EBICON: MCLKEN Mask

Definition at line 1762 of file Nano100Series.h.

## ◆ EBI_EBICON_MCLKEN_Pos

#define EBI_EBICON_MCLKEN_Pos (11)

EBI_T::EBICON: MCLKEN Position

Definition at line 1761 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExtIR2R_Msk

#define EBI_EXTIME_ExtIR2R_Msk (0xful << EBI_EXTIME_ExtIR2R_Pos)

EBI_T::EXTIME: ExtIR2R Mask

Definition at line 1780 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExtIR2R_Pos

#define EBI_EXTIME_ExtIR2R_Pos (24)

EBI_T::EXTIME: ExtIR2R Position

Definition at line 1779 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExtIR2W_Msk

#define EBI_EXTIME_ExtIR2W_Msk (0xful << EBI_EXTIME_ExtIR2W_Pos)

EBI_T::EXTIME: ExtIR2W Mask

Definition at line 1777 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExtIR2W_Pos

#define EBI_EXTIME_ExtIR2W_Pos (16)

EBI_T::EXTIME: ExtIR2W Position

Definition at line 1776 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExtIW2X_Msk

#define EBI_EXTIME_ExtIW2X_Msk (0xful << EBI_EXTIME_ExtIW2X_Pos)

EBI_T::EXTIME: ExtIW2X Mask

Definition at line 1774 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExtIW2X_Pos

#define EBI_EXTIME_ExtIW2X_Pos (12)

EBI_T::EXTIME: ExtIW2X Position

Definition at line 1773 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExttACC_Msk

#define EBI_EXTIME_ExttACC_Msk (0x1ful << EBI_EXTIME_ExttACC_Pos)

EBI_T::EXTIME: ExttACC Mask

Definition at line 1768 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExttACC_Pos

#define EBI_EXTIME_ExttACC_Pos (0)

EBI_T::EXTIME: ExttACC Position

Definition at line 1767 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExttAHD_Msk

#define EBI_EXTIME_ExttAHD_Msk (0x7ul << EBI_EXTIME_ExttAHD_Pos)

EBI_T::EXTIME: ExttAHD Mask

Definition at line 1771 of file Nano100Series.h.

## ◆ EBI_EXTIME_ExttAHD_Pos

#define EBI_EXTIME_ExttAHD_Pos (8)

EBI_T::EXTIME: ExttAHD Position

Definition at line 1770 of file Nano100Series.h.

## ◆ FMC_DFBADR_DFBA_Msk

#define FMC_DFBADR_DFBA_Msk (0xfffffffful << FMC_DFBADR_DFBA_Pos)

FMC_T::DFBADR: DFBA Mask

Definition at line 1972 of file Nano100Series.h.

## ◆ FMC_DFBADR_DFBA_Pos

#define FMC_DFBADR_DFBA_Pos (0)

FMC_T::DFBADR: DFBA Position

Definition at line 1971 of file Nano100Series.h.

## ◆ FMC_ISPADR_ISPADR_Msk

#define FMC_ISPADR_ISPADR_Msk (0xfffffffful << FMC_ISPADR_ISPADR_Pos)

FMC_T::ISPADR: ISPADR Mask

Definition at line 1954 of file Nano100Series.h.

## ◆ FMC_ISPADR_ISPADR_Pos

#define FMC_ISPADR_ISPADR_Pos (0)

FMC_T::ISPADR: ISPADR Position

Definition at line 1953 of file Nano100Series.h.

## ◆ FMC_ISPCMD_FCEN_Msk

#define FMC_ISPCMD_FCEN_Msk (0x1ul << FMC_ISPCMD_FCEN_Pos)

FMC_T::ISPCMD: FCEN Mask

Definition at line 1963 of file Nano100Series.h.

## ◆ FMC_ISPCMD_FCEN_Pos

#define FMC_ISPCMD_FCEN_Pos (4)

FMC_T::ISPCMD: FCEN Position

Definition at line 1962 of file Nano100Series.h.

## ◆ FMC_ISPCMD_FCTRL_Msk

#define FMC_ISPCMD_FCTRL_Msk (0xful << FMC_ISPCMD_FCTRL_Pos)

FMC_T::ISPCMD: FCTRL Mask

Definition at line 1960 of file Nano100Series.h.

## ◆ FMC_ISPCMD_FCTRL_Pos

#define FMC_ISPCMD_FCTRL_Pos (0)

FMC_T::ISPCMD: FCTRL Position

Definition at line 1959 of file Nano100Series.h.

## ◆ FMC_ISPCMD_FOEN_Msk

#define FMC_ISPCMD_FOEN_Msk (0x1ul << FMC_ISPCMD_FOEN_Pos)

FMC_T::ISPCMD: FOEN Mask

Definition at line 1966 of file Nano100Series.h.

## ◆ FMC_ISPCMD_FOEN_Pos

#define FMC_ISPCMD_FOEN_Pos (5)

FMC_T::ISPCMD: FOEN Position

Definition at line 1965 of file Nano100Series.h.

## ◆ FMC_ISPCON_APUEN_Msk

#define FMC_ISPCON_APUEN_Msk (0x1ul << FMC_ISPCON_APUEN_Pos)

FMC_T::ISPCON: APUEN Mask

Definition at line 1942 of file Nano100Series.h.

## ◆ FMC_ISPCON_APUEN_Pos

#define FMC_ISPCON_APUEN_Pos (3)

FMC_T::ISPCON: APUEN Position

Definition at line 1941 of file Nano100Series.h.

## ◆ FMC_ISPCON_BS_Msk

#define FMC_ISPCON_BS_Msk (0x1ul << FMC_ISPCON_BS_Pos)

FMC_T::ISPCON: BS Mask

Definition at line 1939 of file Nano100Series.h.

## ◆ FMC_ISPCON_BS_Pos

#define FMC_ISPCON_BS_Pos (1)

FMC_T::ISPCON: BS Position

Definition at line 1938 of file Nano100Series.h.

## ◆ FMC_ISPCON_CFGUEN_Msk

#define FMC_ISPCON_CFGUEN_Msk (0x1ul << FMC_ISPCON_CFGUEN_Pos)

FMC_T::ISPCON: CFGUEN Mask

Definition at line 1945 of file Nano100Series.h.

## ◆ FMC_ISPCON_CFGUEN_Pos

#define FMC_ISPCON_CFGUEN_Pos (4)

FMC_T::ISPCON: CFGUEN Position

Definition at line 1944 of file Nano100Series.h.

## ◆ FMC_ISPCON_ISPEN_Msk

#define FMC_ISPCON_ISPEN_Msk (0x1ul << FMC_ISPCON_ISPEN_Pos)

FMC_T::ISPCON: ISPEN Mask

Definition at line 1936 of file Nano100Series.h.

## ◆ FMC_ISPCON_ISPEN_Pos

#define FMC_ISPCON_ISPEN_Pos (0)

    @addtogroup FMC_CONST FMC Bit Field Definition
    Constant Definitions for FMC Controller

FMC_T::ISPCON: ISPEN Position

Definition at line 1935 of file Nano100Series.h.

## ◆ FMC_ISPCON_ISPFF_Msk

#define FMC_ISPCON_ISPFF_Msk (0x1ul << FMC_ISPCON_ISPFF_Pos)

FMC_T::ISPCON: ISPFF Mask

Definition at line 1951 of file Nano100Series.h.

## ◆ FMC_ISPCON_ISPFF_Pos

#define FMC_ISPCON_ISPFF_Pos (6)

FMC_T::ISPCON: ISPFF Position

Definition at line 1950 of file Nano100Series.h.

## ◆ FMC_ISPCON_LDUEN_Msk

#define FMC_ISPCON_LDUEN_Msk (0x1ul << FMC_ISPCON_LDUEN_Pos)

FMC_T::ISPCON: LDUEN Mask

Definition at line 1948 of file Nano100Series.h.

## ◆ FMC_ISPCON_LDUEN_Pos

#define FMC_ISPCON_LDUEN_Pos (5)

FMC_T::ISPCON: LDUEN Position

Definition at line 1947 of file Nano100Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Msk

#define FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)

FMC_T::ISPDAT: ISPDAT Mask

Definition at line 1957 of file Nano100Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Pos

#define FMC_ISPDAT_ISPDAT_Pos (0)

FMC_T::ISPDAT: ISPDAT Position

Definition at line 1956 of file Nano100Series.h.

## ◆ FMC_ISPSTA_CBS_Msk

#define FMC_ISPSTA_CBS_Msk (0x3ul << FMC_ISPSTA_CBS_Pos)

FMC_T::ISPSTA: CBS Mask

Definition at line 1978 of file Nano100Series.h.

## ◆ FMC_ISPSTA_CBS_Pos

#define FMC_ISPSTA_CBS_Pos (1)

FMC_T::ISPSTA: CBS Position

Definition at line 1977 of file Nano100Series.h.

## ◆ FMC_ISPSTA_ISPBUSY_Msk

#define FMC_ISPSTA_ISPBUSY_Msk (0x1ul << FMC_ISPSTA_ISPBUSY_Pos)

FMC_T::ISPSTA: ISPBUSY Mask

Definition at line 1975 of file Nano100Series.h.

## ◆ FMC_ISPSTA_ISPBUSY_Pos

#define FMC_ISPSTA_ISPBUSY_Pos (0)

FMC_T::ISPSTA: ISPBUSY Position

Definition at line 1974 of file Nano100Series.h.

## ◆ FMC_ISPSTA_ISPFF_Msk

#define FMC_ISPSTA_ISPFF_Msk (0x1ul << FMC_ISPSTA_ISPFF_Pos)

FMC_T::ISPSTA: ISPFF Mask

Definition at line 1981 of file Nano100Series.h.

## ◆ FMC_ISPSTA_ISPFF_Pos

#define FMC_ISPSTA_ISPFF_Pos (6)

FMC_T::ISPSTA: ISPFF Position

Definition at line 1980 of file Nano100Series.h.

## ◆ FMC_ISPTRG_ISPGO_Msk

#define FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)

FMC_T::ISPTRG: ISPGO Mask

Definition at line 1969 of file Nano100Series.h.

## ◆ FMC_ISPTRG_ISPGO_Pos

#define FMC_ISPTRG_ISPGO_Pos (0)

FMC_T::ISPTRG: ISPGO Position

Definition at line 1968 of file Nano100Series.h.

## ◆ GP_DBEN_DBEN_Msk

#define GP_DBEN_DBEN_Msk (0xfffful << GP_DBEN_DBEN_Pos)

GPIO_T::DBEN: DBEN Mask

Definition at line 4082 of file Nano100Series.h.

## ◆ GP_DBEN_DBEN_Pos

#define GP_DBEN_DBEN_Pos (0)

GPIO_T::DBEN: DBEN Position

Definition at line 4081 of file Nano100Series.h.

## ◆ GP_DBNCECON_DBCLK_ON_Msk

#define GP_DBNCECON_DBCLK_ON_Msk (0x1ul << GP_DBNCECON_DBCLK_ON_Pos)

GP_DB_T::DBNCECON: DBCLK_ON Mask

Definition at line 4201 of file Nano100Series.h.

## ◆ GP_DBNCECON_DBCLK_ON_Pos

#define GP_DBNCECON_DBCLK_ON_Pos (5)

GP_DB_T::DBNCECON: DBCLK_ON Position

Definition at line 4200 of file Nano100Series.h.

## ◆ GP_DBNCECON_DBCLKSEL_Msk

#define GP_DBNCECON_DBCLKSEL_Msk (0xful << GP_DBNCECON_DBCLKSEL_Pos)

GP_DB_T::DBNCECON: DBCLKSEL Mask

Definition at line 4195 of file Nano100Series.h.

## ◆ GP_DBNCECON_DBCLKSEL_Pos

#define GP_DBNCECON_DBCLKSEL_Pos (0)

    @addtogroup GP_DB_CONST GP_DB Bit Field Definition
    Constant Definitions for GP_DB Controller

GP_DB_T::DBNCECON: DBCLKSEL Position

Definition at line 4194 of file Nano100Series.h.

## ◆ GP_DBNCECON_DBCLKSRC_Msk

#define GP_DBNCECON_DBCLKSRC_Msk (0x1ul << GP_DBNCECON_DBCLKSRC_Pos)

GP_DB_T::DBNCECON: DBCLKSRC Mask

Definition at line 4198 of file Nano100Series.h.

## ◆ GP_DBNCECON_DBCLKSRC_Pos

#define GP_DBNCECON_DBCLKSRC_Pos (4)

GP_DB_T::DBNCECON: DBCLKSRC Position

Definition at line 4197 of file Nano100Series.h.

## ◆ GP_DMASK_DMASK_Msk

#define GP_DMASK_DMASK_Msk (0xfffful << GP_DMASK_DMASK_Pos)

GPIO_T::DMASK: DMASK Mask

Definition at line 4076 of file Nano100Series.h.

## ◆ GP_DMASK_DMASK_Pos

#define GP_DMASK_DMASK_Pos (0)

GPIO_T::DMASK: DMASK Position

Definition at line 4075 of file Nano100Series.h.

## ◆ GP_DOUT_DOUT_Msk

#define GP_DOUT_DOUT_Msk (0xfffful << GP_DOUT_DOUT_Pos)

GPIO_T::DOUT: DOUT Mask

Definition at line 4073 of file Nano100Series.h.

## ◆ GP_DOUT_DOUT_Pos

#define GP_DOUT_DOUT_Pos (0)

GPIO_T::DOUT: DOUT Position

Definition at line 4072 of file Nano100Series.h.

## ◆ GP_IER_FIER0_Msk

#define GP_IER_FIER0_Msk (0x1ul << GP_IER_FIER0_Pos)

GPIO_T::IER: FIER0 Mask

Definition at line 4088 of file Nano100Series.h.

## ◆ GP_IER_FIER0_Pos

#define GP_IER_FIER0_Pos (0)

GPIO_T::IER: FIER0 Position

Definition at line 4087 of file Nano100Series.h.

## ◆ GP_IER_FIER10_Msk

#define GP_IER_FIER10_Msk (0x1ul << GP_IER_FIER10_Pos)

GPIO_T::IER: FIER10 Mask

Definition at line 4118 of file Nano100Series.h.

## ◆ GP_IER_FIER10_Pos

#define GP_IER_FIER10_Pos (10)

GPIO_T::IER: FIER10 Position

Definition at line 4117 of file Nano100Series.h.

## ◆ GP_IER_FIER11_Msk

#define GP_IER_FIER11_Msk (0x1ul << GP_IER_FIER11_Pos)

GPIO_T::IER: FIER11 Mask

Definition at line 4121 of file Nano100Series.h.

## ◆ GP_IER_FIER11_Pos

#define GP_IER_FIER11_Pos (11)

GPIO_T::IER: FIER11 Position

Definition at line 4120 of file Nano100Series.h.

## ◆ GP_IER_FIER12_Msk

#define GP_IER_FIER12_Msk (0x1ul << GP_IER_FIER12_Pos)

GPIO_T::IER: FIER12 Mask

Definition at line 4124 of file Nano100Series.h.

## ◆ GP_IER_FIER12_Pos

#define GP_IER_FIER12_Pos (12)

GPIO_T::IER: FIER12 Position

Definition at line 4123 of file Nano100Series.h.

## ◆ GP_IER_FIER13_Msk

#define GP_IER_FIER13_Msk (0x1ul << GP_IER_FIER13_Pos)

GPIO_T::IER: FIER13 Mask

Definition at line 4127 of file Nano100Series.h.

## ◆ GP_IER_FIER13_Pos

#define GP_IER_FIER13_Pos (13)

GPIO_T::IER: FIER13 Position

Definition at line 4126 of file Nano100Series.h.

## ◆ GP_IER_FIER14_Msk

#define GP_IER_FIER14_Msk (0x1ul << GP_IER_FIER14_Pos)

GPIO_T::IER: FIER14 Mask

Definition at line 4130 of file Nano100Series.h.

## ◆ GP_IER_FIER14_Pos

#define GP_IER_FIER14_Pos (14)

GPIO_T::IER: FIER14 Position

Definition at line 4129 of file Nano100Series.h.

## ◆ GP_IER_FIER15_Msk

#define GP_IER_FIER15_Msk (0x1ul << GP_IER_FIER15_Pos)

GPIO_T::IER: FIER15 Mask

Definition at line 4133 of file Nano100Series.h.

## ◆ GP_IER_FIER15_Pos

#define GP_IER_FIER15_Pos (15)

GPIO_T::IER: FIER15 Position

Definition at line 4132 of file Nano100Series.h.

## ◆ GP_IER_FIER1_Msk

#define GP_IER_FIER1_Msk (0x1ul << GP_IER_FIER1_Pos)

GPIO_T::IER: FIER1 Mask

Definition at line 4091 of file Nano100Series.h.

## ◆ GP_IER_FIER1_Pos

#define GP_IER_FIER1_Pos (1)

GPIO_T::IER: FIER1 Position

Definition at line 4090 of file Nano100Series.h.

## ◆ GP_IER_FIER2_Msk

#define GP_IER_FIER2_Msk (0x1ul << GP_IER_FIER2_Pos)

GPIO_T::IER: FIER2 Mask

Definition at line 4094 of file Nano100Series.h.

## ◆ GP_IER_FIER2_Pos

#define GP_IER_FIER2_Pos (2)

GPIO_T::IER: FIER2 Position

Definition at line 4093 of file Nano100Series.h.

## ◆ GP_IER_FIER3_Msk

#define GP_IER_FIER3_Msk (0x1ul << GP_IER_FIER3_Pos)

GPIO_T::IER: FIER3 Mask

Definition at line 4097 of file Nano100Series.h.

## ◆ GP_IER_FIER3_Pos

#define GP_IER_FIER3_Pos (3)

GPIO_T::IER: FIER3 Position

Definition at line 4096 of file Nano100Series.h.

## ◆ GP_IER_FIER4_Msk

#define GP_IER_FIER4_Msk (0x1ul << GP_IER_FIER4_Pos)

GPIO_T::IER: FIER4 Mask

Definition at line 4100 of file Nano100Series.h.

## ◆ GP_IER_FIER4_Pos

#define GP_IER_FIER4_Pos (4)

GPIO_T::IER: FIER4 Position

Definition at line 4099 of file Nano100Series.h.

## ◆ GP_IER_FIER5_Msk

#define GP_IER_FIER5_Msk (0x1ul << GP_IER_FIER5_Pos)

GPIO_T::IER: FIER5 Mask

Definition at line 4103 of file Nano100Series.h.

## ◆ GP_IER_FIER5_Pos

#define GP_IER_FIER5_Pos (5)

GPIO_T::IER: FIER5 Position

Definition at line 4102 of file Nano100Series.h.

## ◆ GP_IER_FIER6_Msk

#define GP_IER_FIER6_Msk (0x1ul << GP_IER_FIER6_Pos)

GPIO_T::IER: FIER6 Mask

Definition at line 4106 of file Nano100Series.h.

## ◆ GP_IER_FIER6_Pos

#define GP_IER_FIER6_Pos (6)

GPIO_T::IER: FIER6 Position

Definition at line 4105 of file Nano100Series.h.

## ◆ GP_IER_FIER7_Msk

#define GP_IER_FIER7_Msk (0x1ul << GP_IER_FIER7_Pos)

GPIO_T::IER: FIER7 Mask

Definition at line 4109 of file Nano100Series.h.

## ◆ GP_IER_FIER7_Pos

#define GP_IER_FIER7_Pos (7)

GPIO_T::IER: FIER7 Position

Definition at line 4108 of file Nano100Series.h.

## ◆ GP_IER_FIER8_Msk

#define GP_IER_FIER8_Msk (0x1ul << GP_IER_FIER8_Pos)

GPIO_T::IER: FIER8 Mask

Definition at line 4112 of file Nano100Series.h.

## ◆ GP_IER_FIER8_Pos

#define GP_IER_FIER8_Pos (8)

GPIO_T::IER: FIER8 Position

Definition at line 4111 of file Nano100Series.h.

## ◆ GP_IER_FIER9_Msk

#define GP_IER_FIER9_Msk (0x1ul << GP_IER_FIER9_Pos)

GPIO_T::IER: FIER9 Mask

Definition at line 4115 of file Nano100Series.h.

## ◆ GP_IER_FIER9_Pos

#define GP_IER_FIER9_Pos (9)

GPIO_T::IER: FIER9 Position

Definition at line 4114 of file Nano100Series.h.

## ◆ GP_IER_RIER0_Msk

#define GP_IER_RIER0_Msk (0x1ul << GP_IER_RIER0_Pos)

GPIO_T::IER: RIER0 Mask

Definition at line 4136 of file Nano100Series.h.

## ◆ GP_IER_RIER0_Pos

#define GP_IER_RIER0_Pos (16)

GPIO_T::IER: RIER0 Position

Definition at line 4135 of file Nano100Series.h.

## ◆ GP_IER_RIER10_Msk

#define GP_IER_RIER10_Msk (0x1ul << GP_IER_RIER10_Pos)

GPIO_T::IER: RIER10 Mask

Definition at line 4166 of file Nano100Series.h.

## ◆ GP_IER_RIER10_Pos

#define GP_IER_RIER10_Pos (26)

GPIO_T::IER: RIER10 Position

Definition at line 4165 of file Nano100Series.h.

## ◆ GP_IER_RIER11_Msk

#define GP_IER_RIER11_Msk (0x1ul << GP_IER_RIER11_Pos)

GPIO_T::IER: RIER11 Mask

Definition at line 4169 of file Nano100Series.h.

## ◆ GP_IER_RIER11_Pos

#define GP_IER_RIER11_Pos (27)

GPIO_T::IER: RIER11 Position

Definition at line 4168 of file Nano100Series.h.

## ◆ GP_IER_RIER12_Msk

#define GP_IER_RIER12_Msk (0x1ul << GP_IER_RIER12_Pos)

GPIO_T::IER: RIER12 Mask

Definition at line 4172 of file Nano100Series.h.

## ◆ GP_IER_RIER12_Pos

#define GP_IER_RIER12_Pos (28)

GPIO_T::IER: RIER12 Position

Definition at line 4171 of file Nano100Series.h.

## ◆ GP_IER_RIER13_Msk

#define GP_IER_RIER13_Msk (0x1ul << GP_IER_RIER13_Pos)

GPIO_T::IER: RIER13 Mask

Definition at line 4175 of file Nano100Series.h.

## ◆ GP_IER_RIER13_Pos

#define GP_IER_RIER13_Pos (29)

GPIO_T::IER: RIER13 Position

Definition at line 4174 of file Nano100Series.h.

## ◆ GP_IER_RIER14_Msk

#define GP_IER_RIER14_Msk (0x1ul << GP_IER_RIER14_Pos)

GPIO_T::IER: RIER14 Mask

Definition at line 4178 of file Nano100Series.h.

## ◆ GP_IER_RIER14_Pos

#define GP_IER_RIER14_Pos (30)

GPIO_T::IER: RIER14 Position

Definition at line 4177 of file Nano100Series.h.

## ◆ GP_IER_RIER15_Msk

#define GP_IER_RIER15_Msk (0x1ul << GP_IER_RIER15_Pos)

GPIO_T::IER: RIER15 Mask

Definition at line 4181 of file Nano100Series.h.

## ◆ GP_IER_RIER15_Pos

#define GP_IER_RIER15_Pos (31)

GPIO_T::IER: RIER15 Position

Definition at line 4180 of file Nano100Series.h.

## ◆ GP_IER_RIER1_Msk

#define GP_IER_RIER1_Msk (0x1ul << GP_IER_RIER1_Pos)

GPIO_T::IER: RIER1 Mask

Definition at line 4139 of file Nano100Series.h.

## ◆ GP_IER_RIER1_Pos

#define GP_IER_RIER1_Pos (17)

GPIO_T::IER: RIER1 Position

Definition at line 4138 of file Nano100Series.h.

## ◆ GP_IER_RIER2_Msk

#define GP_IER_RIER2_Msk (0x1ul << GP_IER_RIER2_Pos)

GPIO_T::IER: RIER2 Mask

Definition at line 4142 of file Nano100Series.h.

## ◆ GP_IER_RIER2_Pos

#define GP_IER_RIER2_Pos (18)

GPIO_T::IER: RIER2 Position

Definition at line 4141 of file Nano100Series.h.

## ◆ GP_IER_RIER3_Msk

#define GP_IER_RIER3_Msk (0x1ul << GP_IER_RIER3_Pos)

GPIO_T::IER: RIER3 Mask

Definition at line 4145 of file Nano100Series.h.

## ◆ GP_IER_RIER3_Pos

#define GP_IER_RIER3_Pos (19)

GPIO_T::IER: RIER3 Position

Definition at line 4144 of file Nano100Series.h.

## ◆ GP_IER_RIER4_Msk

#define GP_IER_RIER4_Msk (0x1ul << GP_IER_RIER4_Pos)

GPIO_T::IER: RIER4 Mask

Definition at line 4148 of file Nano100Series.h.

## ◆ GP_IER_RIER4_Pos

#define GP_IER_RIER4_Pos (20)

GPIO_T::IER: RIER4 Position

Definition at line 4147 of file Nano100Series.h.

## ◆ GP_IER_RIER5_Msk

#define GP_IER_RIER5_Msk (0x1ul << GP_IER_RIER5_Pos)

GPIO_T::IER: RIER5 Mask

Definition at line 4151 of file Nano100Series.h.

## ◆ GP_IER_RIER5_Pos

#define GP_IER_RIER5_Pos (21)

GPIO_T::IER: RIER5 Position

Definition at line 4150 of file Nano100Series.h.

## ◆ GP_IER_RIER6_Msk

#define GP_IER_RIER6_Msk (0x1ul << GP_IER_RIER6_Pos)

GPIO_T::IER: RIER6 Mask

Definition at line 4154 of file Nano100Series.h.

## ◆ GP_IER_RIER6_Pos

#define GP_IER_RIER6_Pos (22)

GPIO_T::IER: RIER6 Position

Definition at line 4153 of file Nano100Series.h.

## ◆ GP_IER_RIER7_Msk

#define GP_IER_RIER7_Msk (0x1ul << GP_IER_RIER7_Pos)

GPIO_T::IER: RIER7 Mask

Definition at line 4157 of file Nano100Series.h.

## ◆ GP_IER_RIER7_Pos

#define GP_IER_RIER7_Pos (23)

GPIO_T::IER: RIER7 Position

Definition at line 4156 of file Nano100Series.h.

## ◆ GP_IER_RIER8_Msk

#define GP_IER_RIER8_Msk (0x1ul << GP_IER_RIER8_Pos)

GPIO_T::IER: RIER8 Mask

Definition at line 4160 of file Nano100Series.h.

## ◆ GP_IER_RIER8_Pos

#define GP_IER_RIER8_Pos (24)

GPIO_T::IER: RIER8 Position

Definition at line 4159 of file Nano100Series.h.

## ◆ GP_IER_RIER9_Msk

#define GP_IER_RIER9_Msk (0x1ul << GP_IER_RIER9_Pos)

GPIO_T::IER: RIER9 Mask

Definition at line 4163 of file Nano100Series.h.

## ◆ GP_IER_RIER9_Pos

#define GP_IER_RIER9_Pos (25)

GPIO_T::IER: RIER9 Position

Definition at line 4162 of file Nano100Series.h.

## ◆ GP_IMD_IMD_Msk

#define GP_IMD_IMD_Msk (0xfffful << GP_IMD_IMD_Pos)

GPIO_T::IMD: IMD Mask

Definition at line 4085 of file Nano100Series.h.

## ◆ GP_IMD_IMD_Pos

#define GP_IMD_IMD_Pos (0)

GPIO_T::IMD: IMD Position

Definition at line 4084 of file Nano100Series.h.

## ◆ GP_ISRC_ISRC_Msk

#define GP_ISRC_ISRC_Msk (0xfffful << GP_ISRC_ISRC_Pos)

GPIO_T::ISRC: ISRC Mask

Definition at line 4184 of file Nano100Series.h.

## ◆ GP_ISRC_ISRC_Pos

#define GP_ISRC_ISRC_Pos (0)

GPIO_T::ISRC: ISRC Position

Definition at line 4183 of file Nano100Series.h.

## ◆ GP_OFFD_OFFD_Msk

#define GP_OFFD_OFFD_Msk (0xfffful << GP_OFFD_OFFD_Pos)

GPIO_T::OFFD: OFFD Mask

Definition at line 4070 of file Nano100Series.h.

## ◆ GP_OFFD_OFFD_Pos

#define GP_OFFD_OFFD_Pos (16)

GPIO_T::OFFD: OFFD Position

Definition at line 4069 of file Nano100Series.h.

## ◆ GP_PIN_PIN_Msk

#define GP_PIN_PIN_Msk (0xfffful << GP_PIN_PIN_Pos)

GPIO_T::PIN: PIN Mask

Definition at line 4079 of file Nano100Series.h.

## ◆ GP_PIN_PIN_Pos

#define GP_PIN_PIN_Pos (0)

GPIO_T::PIN: PIN Position

Definition at line 4078 of file Nano100Series.h.

## ◆ GP_PMD_PMD0_Msk

#define GP_PMD_PMD0_Msk (0x3ul << GP_PMD_PMD0_Pos)

GPIO_T::PMD: PMD0 Mask

Definition at line 4022 of file Nano100Series.h.

## ◆ GP_PMD_PMD0_Pos

#define GP_PMD_PMD0_Pos (0)

    @addtogroup GPIO_CONST GPIO Bit Field Definition
    Constant Definitions for GPIO Controller

GPIO_T::PMD: PMD0 Position

Definition at line 4021 of file Nano100Series.h.

## ◆ GP_PMD_PMD10_Msk

#define GP_PMD_PMD10_Msk (0x3ul << GP_PMD_PMD10_Pos)

GPIO_T::PMD: PMD10 Mask

Definition at line 4052 of file Nano100Series.h.

## ◆ GP_PMD_PMD10_Pos

#define GP_PMD_PMD10_Pos (20)

GPIO_T::PMD: PMD10 Position

Definition at line 4051 of file Nano100Series.h.

## ◆ GP_PMD_PMD11_Msk

#define GP_PMD_PMD11_Msk (0x3ul << GP_PMD_PMD11_Pos)

GPIO_T::PMD: PMD11 Mask

Definition at line 4055 of file Nano100Series.h.

## ◆ GP_PMD_PMD11_Pos

#define GP_PMD_PMD11_Pos (22)

GPIO_T::PMD: PMD11 Position

Definition at line 4054 of file Nano100Series.h.

## ◆ GP_PMD_PMD12_Msk

#define GP_PMD_PMD12_Msk (0x3ul << GP_PMD_PMD12_Pos)

GPIO_T::PMD: PMD12 Mask

Definition at line 4058 of file Nano100Series.h.

## ◆ GP_PMD_PMD12_Pos

#define GP_PMD_PMD12_Pos (24)

GPIO_T::PMD: PMD12 Position

Definition at line 4057 of file Nano100Series.h.

## ◆ GP_PMD_PMD13_Msk

#define GP_PMD_PMD13_Msk (0x3ul << GP_PMD_PMD13_Pos)

GPIO_T::PMD: PMD13 Mask

Definition at line 4061 of file Nano100Series.h.

## ◆ GP_PMD_PMD13_Pos

#define GP_PMD_PMD13_Pos (26)

GPIO_T::PMD: PMD13 Position

Definition at line 4060 of file Nano100Series.h.

## ◆ GP_PMD_PMD14_Msk

#define GP_PMD_PMD14_Msk (0x3ul << GP_PMD_PMD14_Pos)

GPIO_T::PMD: PMD14 Mask

Definition at line 4064 of file Nano100Series.h.

## ◆ GP_PMD_PMD14_Pos

#define GP_PMD_PMD14_Pos (28)

GPIO_T::PMD: PMD14 Position

Definition at line 4063 of file Nano100Series.h.

## ◆ GP_PMD_PMD15_Msk

#define GP_PMD_PMD15_Msk (0x3ul << GP_PMD_PMD15_Pos)

GPIO_T::PMD: PMD15 Mask

Definition at line 4067 of file Nano100Series.h.

## ◆ GP_PMD_PMD15_Pos

#define GP_PMD_PMD15_Pos (30)

GPIO_T::PMD: PMD15 Position

Definition at line 4066 of file Nano100Series.h.

## ◆ GP_PMD_PMD1_Msk

#define GP_PMD_PMD1_Msk (0x3ul << GP_PMD_PMD1_Pos)

GPIO_T::PMD: PMD1 Mask

Definition at line 4025 of file Nano100Series.h.

## ◆ GP_PMD_PMD1_Pos

#define GP_PMD_PMD1_Pos (2)

GPIO_T::PMD: PMD1 Position

Definition at line 4024 of file Nano100Series.h.

## ◆ GP_PMD_PMD2_Msk

#define GP_PMD_PMD2_Msk (0x3ul << GP_PMD_PMD2_Pos)

GPIO_T::PMD: PMD2 Mask

Definition at line 4028 of file Nano100Series.h.

## ◆ GP_PMD_PMD2_Pos

#define GP_PMD_PMD2_Pos (4)

GPIO_T::PMD: PMD2 Position

Definition at line 4027 of file Nano100Series.h.

## ◆ GP_PMD_PMD3_Msk

#define GP_PMD_PMD3_Msk (0x3ul << GP_PMD_PMD3_Pos)

GPIO_T::PMD: PMD3 Mask

Definition at line 4031 of file Nano100Series.h.

## ◆ GP_PMD_PMD3_Pos

#define GP_PMD_PMD3_Pos (6)

GPIO_T::PMD: PMD3 Position

Definition at line 4030 of file Nano100Series.h.

## ◆ GP_PMD_PMD4_Msk

#define GP_PMD_PMD4_Msk (0x3ul << GP_PMD_PMD4_Pos)

GPIO_T::PMD: PMD4 Mask

Definition at line 4034 of file Nano100Series.h.

## ◆ GP_PMD_PMD4_Pos

#define GP_PMD_PMD4_Pos (8)

GPIO_T::PMD: PMD4 Position

Definition at line 4033 of file Nano100Series.h.

## ◆ GP_PMD_PMD5_Msk

#define GP_PMD_PMD5_Msk (0x3ul << GP_PMD_PMD5_Pos)

GPIO_T::PMD: PMD5 Mask

Definition at line 4037 of file Nano100Series.h.

## ◆ GP_PMD_PMD5_Pos

#define GP_PMD_PMD5_Pos (10)

GPIO_T::PMD: PMD5 Position

Definition at line 4036 of file Nano100Series.h.

## ◆ GP_PMD_PMD6_Msk

#define GP_PMD_PMD6_Msk (0x3ul << GP_PMD_PMD6_Pos)

GPIO_T::PMD: PMD6 Mask

Definition at line 4040 of file Nano100Series.h.

## ◆ GP_PMD_PMD6_Pos

#define GP_PMD_PMD6_Pos (12)

GPIO_T::PMD: PMD6 Position

Definition at line 4039 of file Nano100Series.h.

## ◆ GP_PMD_PMD7_Msk

#define GP_PMD_PMD7_Msk (0x3ul << GP_PMD_PMD7_Pos)

GPIO_T::PMD: PMD7 Mask

Definition at line 4043 of file Nano100Series.h.

## ◆ GP_PMD_PMD7_Pos

#define GP_PMD_PMD7_Pos (14)

GPIO_T::PMD: PMD7 Position

Definition at line 4042 of file Nano100Series.h.

## ◆ GP_PMD_PMD8_Msk

#define GP_PMD_PMD8_Msk (0x3ul << GP_PMD_PMD8_Pos)

GPIO_T::PMD: PMD8 Mask

Definition at line 4046 of file Nano100Series.h.

## ◆ GP_PMD_PMD8_Pos

#define GP_PMD_PMD8_Pos (16)

GPIO_T::PMD: PMD8 Position

Definition at line 4045 of file Nano100Series.h.

## ◆ GP_PMD_PMD9_Msk

#define GP_PMD_PMD9_Msk (0x3ul << GP_PMD_PMD9_Pos)

GPIO_T::PMD: PMD9 Mask

Definition at line 4049 of file Nano100Series.h.

## ◆ GP_PMD_PMD9_Pos

#define GP_PMD_PMD9_Pos (18)

GPIO_T::PMD: PMD9 Position

Definition at line 4048 of file Nano100Series.h.

## ◆ GP_PUEN_PUEN_Msk

#define GP_PUEN_PUEN_Msk (0xfffful << GP_PUEN_PUEN_Pos)

GPIO_T::PUEN: PUEN Mask

Definition at line 4187 of file Nano100Series.h.

## ◆ GP_PUEN_PUEN_Pos

#define GP_PUEN_PUEN_Pos (0)

GPIO_T::PUEN: PUEN Position

Definition at line 4186 of file Nano100Series.h.

## ◆ I2C_CON_ACK_Msk

#define I2C_CON_ACK_Msk (0x1ul << I2C_CON_ACK_Pos)

I2C_T::CON: ACK Mask

Definition at line 4461 of file Nano100Series.h.

## ◆ I2C_CON_ACK_Pos

#define I2C_CON_ACK_Pos (1)

I2C_T::CON: ACK Position

Definition at line 4460 of file Nano100Series.h.

## ◆ I2C_CON_I2C_STS_Msk

#define I2C_CON_I2C_STS_Msk (0x1ul << I2C_CON_I2C_STS_Pos)

I2C_T::CON: I2C_STS Mask

Definition at line 4470 of file Nano100Series.h.

## ◆ I2C_CON_I2C_STS_Pos

#define I2C_CON_I2C_STS_Pos (4)

I2C_T::CON: I2C_STS Position

Definition at line 4469 of file Nano100Series.h.

## ◆ I2C_CON_INTEN_Msk

#define I2C_CON_INTEN_Msk (0x1ul << I2C_CON_INTEN_Pos)

I2C_T::CON: INTEN Mask

Definition at line 4473 of file Nano100Series.h.

## ◆ I2C_CON_INTEN_Pos

#define I2C_CON_INTEN_Pos (7)

I2C_T::CON: INTEN Position

Definition at line 4472 of file Nano100Series.h.

## ◆ I2C_CON_IPEN_Msk

#define I2C_CON_IPEN_Msk (0x1ul << I2C_CON_IPEN_Pos)

I2C_T::CON: IPEN Mask

Definition at line 4458 of file Nano100Series.h.

## ◆ I2C_CON_IPEN_Pos

#define I2C_CON_IPEN_Pos (0)

    @addtogroup I2C_CONST I2C Bit Field Definition
    Constant Definitions for I2C Controller

I2C_T::CON: IPEN Position

Definition at line 4457 of file Nano100Series.h.

## ◆ I2C_CON_START_Msk

#define I2C_CON_START_Msk (0x1ul << I2C_CON_START_Pos)

I2C_T::CON: START Mask

Definition at line 4467 of file Nano100Series.h.

## ◆ I2C_CON_START_Pos

#define I2C_CON_START_Pos (3)

I2C_T::CON: START Position

Definition at line 4466 of file Nano100Series.h.

## ◆ I2C_CON_STOP_Msk

#define I2C_CON_STOP_Msk (0x1ul << I2C_CON_STOP_Pos)

I2C_T::CON: STOP Mask

Definition at line 4464 of file Nano100Series.h.

## ◆ I2C_CON_STOP_Pos

#define I2C_CON_STOP_Pos (2)

I2C_T::CON: STOP Position

Definition at line 4463 of file Nano100Series.h.

## ◆ I2C_DATA_DATA_Msk

#define I2C_DATA_DATA_Msk (0xfful << I2C_DATA_DATA_Pos)

I2C_T::DATA: DATA Mask

Definition at line 4494 of file Nano100Series.h.

## ◆ I2C_DATA_DATA_Pos

#define I2C_DATA_DATA_Pos (0)

I2C_T::DATA: DATA Position

Definition at line 4493 of file Nano100Series.h.

## ◆ I2C_DIV_CLK_DIV_Msk

#define I2C_DIV_CLK_DIV_Msk (0xfful << I2C_DIV_CLK_DIV_Pos)

I2C_T::DIV: CLK_DIV Mask

Definition at line 4485 of file Nano100Series.h.

## ◆ I2C_DIV_CLK_DIV_Pos

#define I2C_DIV_CLK_DIV_Pos (0)

I2C_T::DIV: CLK_DIV Position

Definition at line 4484 of file Nano100Series.h.

## ◆ I2C_INTSTS_INTSTS_Msk

#define I2C_INTSTS_INTSTS_Msk (0x1ul << I2C_INTSTS_INTSTS_Pos)

I2C_T::INTSTS: INTSTS Mask

Definition at line 4476 of file Nano100Series.h.

## ◆ I2C_INTSTS_INTSTS_Pos

#define I2C_INTSTS_INTSTS_Pos (0)

I2C_T::INTSTS: INTSTS Position

Definition at line 4475 of file Nano100Series.h.

## ◆ I2C_INTSTS_TIF_Msk

#define I2C_INTSTS_TIF_Msk (0x1ul << I2C_INTSTS_TIF_Pos)

I2C_T::INTSTS: TIF Mask

Definition at line 4479 of file Nano100Series.h.

## ◆ I2C_INTSTS_TIF_Pos

#define I2C_INTSTS_TIF_Pos (1)

I2C_T::INTSTS: TIF Position

Definition at line 4478 of file Nano100Series.h.

## ◆ I2C_SADDR0_GCALL_Msk

#define I2C_SADDR0_GCALL_Msk (0x1ul << I2C_SADDR0_GCALL_Pos)

I2C_T::SADDR0: GCALL Mask

Definition at line 4497 of file Nano100Series.h.

## ◆ I2C_SADDR0_GCALL_Pos

#define I2C_SADDR0_GCALL_Pos (0)

I2C_T::SADDR0: GCALL Position

Definition at line 4496 of file Nano100Series.h.

## ◆ I2C_SADDR0_SADDR_Msk

#define I2C_SADDR0_SADDR_Msk (0x7ful << I2C_SADDR0_SADDR_Pos)

I2C_T::SADDR0: SADDR Mask

Definition at line 4500 of file Nano100Series.h.

## ◆ I2C_SADDR0_SADDR_Pos

#define I2C_SADDR0_SADDR_Pos (1)

I2C_T::SADDR0: SADDR Position

Definition at line 4499 of file Nano100Series.h.

## ◆ I2C_SADDR1_GCALL_Msk

#define I2C_SADDR1_GCALL_Msk (0x1ul << I2C_SADDR1_GCALL_Pos)

I2C_T::SADDR1: GCALL Mask

Definition at line 4503 of file Nano100Series.h.

## ◆ I2C_SADDR1_GCALL_Pos

#define I2C_SADDR1_GCALL_Pos (0)

I2C_T::SADDR1: GCALL Position

Definition at line 4502 of file Nano100Series.h.

## ◆ I2C_SADDR1_SADDR_Msk

#define I2C_SADDR1_SADDR_Msk (0x7ful << I2C_SADDR1_SADDR_Pos)

I2C_T::SADDR1: SADDR Mask

Definition at line 4506 of file Nano100Series.h.

## ◆ I2C_SADDR1_SADDR_Pos

#define I2C_SADDR1_SADDR_Pos (1)

I2C_T::SADDR1: SADDR Position

Definition at line 4505 of file Nano100Series.h.

## ◆ I2C_SAMASK0_SAMASK_Msk

#define I2C_SAMASK0_SAMASK_Msk (0x7ful << I2C_SAMASK0_SAMASK_Pos)

I2C_T::SAMASK0: SAMASK Mask

Definition at line 4509 of file Nano100Series.h.

## ◆ I2C_SAMASK0_SAMASK_Pos

#define I2C_SAMASK0_SAMASK_Pos (1)

I2C_T::SAMASK0: SAMASK Position

Definition at line 4508 of file Nano100Series.h.

## ◆ I2C_SAMASK1_SAMASK_Msk

#define I2C_SAMASK1_SAMASK_Msk (0x7ful << I2C_SAMASK1_SAMASK_Pos)

I2C_T::SAMASK1: SAMASK Mask

Definition at line 4512 of file Nano100Series.h.

## ◆ I2C_SAMASK1_SAMASK_Pos

#define I2C_SAMASK1_SAMASK_Pos (1)

I2C_T::SAMASK1: SAMASK Position

Definition at line 4511 of file Nano100Series.h.

## ◆ I2C_STATUS_STATUS_Msk

#define I2C_STATUS_STATUS_Msk (0xfful << I2C_STATUS_STATUS_Pos)

I2C_T::STATUS: STATUS Mask

Definition at line 4482 of file Nano100Series.h.

## ◆ I2C_STATUS_STATUS_Pos

#define I2C_STATUS_STATUS_Pos (0)

I2C_T::STATUS: STATUS Position

Definition at line 4481 of file Nano100Series.h.

## ◆ I2C_TOUT_DIV4_Msk

#define I2C_TOUT_DIV4_Msk (0x1ul << I2C_TOUT_DIV4_Pos)

I2C_T::TOUT: DIV4 Mask

Definition at line 4491 of file Nano100Series.h.

## ◆ I2C_TOUT_DIV4_Pos

#define I2C_TOUT_DIV4_Pos (1)

I2C_T::TOUT: DIV4 Position

Definition at line 4490 of file Nano100Series.h.

## ◆ I2C_TOUT_TOUTEN_Msk

#define I2C_TOUT_TOUTEN_Msk (0x1ul << I2C_TOUT_TOUTEN_Pos)

I2C_T::TOUT: TOUTEN Mask

Definition at line 4488 of file Nano100Series.h.

## ◆ I2C_TOUT_TOUTEN_Pos

#define I2C_TOUT_TOUTEN_Pos (0)

I2C_T::TOUT: TOUTEN Position

Definition at line 4487 of file Nano100Series.h.

## ◆ I2C_WKUPCON_WKUPEN_Msk

#define I2C_WKUPCON_WKUPEN_Msk (0x1ul << I2C_WKUPCON_WKUPEN_Pos)

I2C_T::WKUPCON: WKUPEN Mask

Definition at line 4515 of file Nano100Series.h.

## ◆ I2C_WKUPCON_WKUPEN_Pos

#define I2C_WKUPCON_WKUPEN_Pos (0)

I2C_T::WKUPCON: WKUPEN Position

Definition at line 4514 of file Nano100Series.h.

## ◆ I2C_WKUPSTS_WKUPIF_Msk

#define I2C_WKUPSTS_WKUPIF_Msk (0x1ul << I2C_WKUPSTS_WKUPIF_Pos)

I2C_T::WKUPSTS: WKUPIF Mask

Definition at line 4518 of file Nano100Series.h.

## ◆ I2C_WKUPSTS_WKUPIF_Pos

#define I2C_WKUPSTS_WKUPIF_Pos (0)

I2C_T::WKUPSTS: WKUPIF Position

Definition at line 4517 of file Nano100Series.h.

## ◆ I2S_CLKDIV_BCLK_DIV_Msk

#define I2S_CLKDIV_BCLK_DIV_Msk (0xfful << I2S_CLKDIV_BCLK_DIV_Pos)

I2S_T::CLKDIV: BCLK_DIV Mask

Definition at line 4883 of file Nano100Series.h.

## ◆ I2S_CLKDIV_BCLK_DIV_Pos

#define I2S_CLKDIV_BCLK_DIV_Pos (8)

I2S_T::CLKDIV: BCLK_DIV Position

Definition at line 4882 of file Nano100Series.h.

## ◆ I2S_CLKDIV_MCLK_DIV_Msk

#define I2S_CLKDIV_MCLK_DIV_Msk (0x7ul << I2S_CLKDIV_MCLK_DIV_Pos)

I2S_T::CLKDIV: MCLK_DIV Mask

Definition at line 4880 of file Nano100Series.h.

## ◆ I2S_CLKDIV_MCLK_DIV_Pos

#define I2S_CLKDIV_MCLK_DIV_Pos (0)

I2S_T::CLKDIV: MCLK_DIV Position

Definition at line 4879 of file Nano100Series.h.

## ◆ I2S_CTRL_CLR_RXFIFO_Msk

#define I2S_CTRL_CLR_RXFIFO_Msk (0x1ul << I2S_CTRL_CLR_RXFIFO_Pos)

I2S_T::CTRL: CLR_RXFIFO Mask

Definition at line 4868 of file Nano100Series.h.

## ◆ I2S_CTRL_CLR_RXFIFO_Pos

#define I2S_CTRL_CLR_RXFIFO_Pos (19)

I2S_T::CTRL: CLR_RXFIFO Position

Definition at line 4867 of file Nano100Series.h.

## ◆ I2S_CTRL_CLR_TXFIFO_Msk

#define I2S_CTRL_CLR_TXFIFO_Msk (0x1ul << I2S_CTRL_CLR_TXFIFO_Pos)

I2S_T::CTRL: CLR_TXFIFO Mask

Definition at line 4865 of file Nano100Series.h.

## ◆ I2S_CTRL_CLR_TXFIFO_Pos

#define I2S_CTRL_CLR_TXFIFO_Pos (18)

I2S_T::CTRL: CLR_TXFIFO Position

Definition at line 4864 of file Nano100Series.h.

## ◆ I2S_CTRL_FORMAT_Msk

#define I2S_CTRL_FORMAT_Msk (0x1ul << I2S_CTRL_FORMAT_Pos)

I2S_T::CTRL: FORMAT Mask

Definition at line 4844 of file Nano100Series.h.

## ◆ I2S_CTRL_FORMAT_Pos

#define I2S_CTRL_FORMAT_Pos (7)

I2S_T::CTRL: FORMAT Position

Definition at line 4843 of file Nano100Series.h.

## ◆ I2S_CTRL_I2SEN_Msk

#define I2S_CTRL_I2SEN_Msk (0x1ul << I2S_CTRL_I2SEN_Pos)

I2S_T::CTRL: I2SEN Mask

Definition at line 4826 of file Nano100Series.h.

## ◆ I2S_CTRL_I2SEN_Pos

#define I2S_CTRL_I2SEN_Pos (0)

    @addtogroup I2S_CONST I2S Bit Field Definition
    Constant Definitions for I2S Controller

I2S_T::CTRL: I2SEN Position

Definition at line 4825 of file Nano100Series.h.

## ◆ I2S_CTRL_LCHZCEN_Msk

#define I2S_CTRL_LCHZCEN_Msk (0x1ul << I2S_CTRL_LCHZCEN_Pos)

I2S_T::CTRL: LCHZCEN Mask

Definition at line 4862 of file Nano100Series.h.

## ◆ I2S_CTRL_LCHZCEN_Pos

#define I2S_CTRL_LCHZCEN_Pos (17)

I2S_T::CTRL: LCHZCEN Position

Definition at line 4861 of file Nano100Series.h.

## ◆ I2S_CTRL_MCLKEN_Msk

#define I2S_CTRL_MCLKEN_Msk (0x1ul << I2S_CTRL_MCLKEN_Pos)

I2S_T::CTRL: MCLKEN Mask

Definition at line 4856 of file Nano100Series.h.

## ◆ I2S_CTRL_MCLKEN_Pos

#define I2S_CTRL_MCLKEN_Pos (15)

I2S_T::CTRL: MCLKEN Position

Definition at line 4855 of file Nano100Series.h.

## ◆ I2S_CTRL_MONO_Msk

#define I2S_CTRL_MONO_Msk (0x1ul << I2S_CTRL_MONO_Pos)

I2S_T::CTRL: MONO Mask

Definition at line 4841 of file Nano100Series.h.

## ◆ I2S_CTRL_MONO_Pos

#define I2S_CTRL_MONO_Pos (6)

I2S_T::CTRL: MONO Position

Definition at line 4840 of file Nano100Series.h.

## ◆ I2S_CTRL_MUTE_Msk

#define I2S_CTRL_MUTE_Msk (0x1ul << I2S_CTRL_MUTE_Pos)

I2S_T::CTRL: MUTE Mask

Definition at line 4835 of file Nano100Series.h.

## ◆ I2S_CTRL_MUTE_Pos

#define I2S_CTRL_MUTE_Pos (3)

I2S_T::CTRL: MUTE Position

Definition at line 4834 of file Nano100Series.h.

## ◆ I2S_CTRL_RCHZCEN_Msk

#define I2S_CTRL_RCHZCEN_Msk (0x1ul << I2S_CTRL_RCHZCEN_Pos)

I2S_T::CTRL: RCHZCEN Mask

Definition at line 4859 of file Nano100Series.h.

## ◆ I2S_CTRL_RCHZCEN_Pos

#define I2S_CTRL_RCHZCEN_Pos (16)

I2S_T::CTRL: RCHZCEN Position

Definition at line 4858 of file Nano100Series.h.

## ◆ I2S_CTRL_RXDMA_Msk

#define I2S_CTRL_RXDMA_Msk (0x1ul << I2S_CTRL_RXDMA_Pos)

I2S_T::CTRL: RXDMA Mask

Definition at line 4874 of file Nano100Series.h.

## ◆ I2S_CTRL_RXDMA_Pos

#define I2S_CTRL_RXDMA_Pos (21)

I2S_T::CTRL: RXDMA Position

Definition at line 4873 of file Nano100Series.h.

## ◆ I2S_CTRL_RXEN_Msk

#define I2S_CTRL_RXEN_Msk (0x1ul << I2S_CTRL_RXEN_Pos)

I2S_T::CTRL: RXEN Mask

Definition at line 4832 of file Nano100Series.h.

## ◆ I2S_CTRL_RXEN_Pos

#define I2S_CTRL_RXEN_Pos (2)

I2S_T::CTRL: RXEN Position

Definition at line 4831 of file Nano100Series.h.

## ◆ I2S_CTRL_RXLCH_Msk

#define I2S_CTRL_RXLCH_Msk (0x1ul << I2S_CTRL_RXLCH_Pos)

I2S_T::CTRL: RXLCH Mask

Definition at line 4877 of file Nano100Series.h.

## ◆ I2S_CTRL_RXLCH_Pos

#define I2S_CTRL_RXLCH_Pos (23)

I2S_T::CTRL: RXLCH Position

Definition at line 4876 of file Nano100Series.h.

## ◆ I2S_CTRL_RXTH_Msk

#define I2S_CTRL_RXTH_Msk (0x7ul << I2S_CTRL_RXTH_Pos)

I2S_T::CTRL: RXTH Mask

Definition at line 4853 of file Nano100Series.h.

## ◆ I2S_CTRL_RXTH_Pos

#define I2S_CTRL_RXTH_Pos (12)

I2S_T::CTRL: RXTH Position

Definition at line 4852 of file Nano100Series.h.

## ◆ I2S_CTRL_SLAVE_Msk

#define I2S_CTRL_SLAVE_Msk (0x1ul << I2S_CTRL_SLAVE_Pos)

I2S_T::CTRL: SLAVE Mask

Definition at line 4847 of file Nano100Series.h.

## ◆ I2S_CTRL_SLAVE_Pos

#define I2S_CTRL_SLAVE_Pos (8)

I2S_T::CTRL: SLAVE Position

Definition at line 4846 of file Nano100Series.h.

## ◆ I2S_CTRL_TXDMA_Msk

#define I2S_CTRL_TXDMA_Msk (0x1ul << I2S_CTRL_TXDMA_Pos)

I2S_T::CTRL: TXDMA Mask

Definition at line 4871 of file Nano100Series.h.

## ◆ I2S_CTRL_TXDMA_Pos

#define I2S_CTRL_TXDMA_Pos (20)

I2S_T::CTRL: TXDMA Position

Definition at line 4870 of file Nano100Series.h.

## ◆ I2S_CTRL_TXEN_Msk

#define I2S_CTRL_TXEN_Msk (0x1ul << I2S_CTRL_TXEN_Pos)

I2S_T::CTRL: TXEN Mask

Definition at line 4829 of file Nano100Series.h.

## ◆ I2S_CTRL_TXEN_Pos

#define I2S_CTRL_TXEN_Pos (1)

I2S_T::CTRL: TXEN Position

Definition at line 4828 of file Nano100Series.h.

## ◆ I2S_CTRL_TXTH_Msk

#define I2S_CTRL_TXTH_Msk (0x7ul << I2S_CTRL_TXTH_Pos)

I2S_T::CTRL: TXTH Mask

Definition at line 4850 of file Nano100Series.h.

## ◆ I2S_CTRL_TXTH_Pos

#define I2S_CTRL_TXTH_Pos (9)

I2S_T::CTRL: TXTH Position

Definition at line 4849 of file Nano100Series.h.

## ◆ I2S_CTRL_WORDWIDTH_Msk

#define I2S_CTRL_WORDWIDTH_Msk (0x3ul << I2S_CTRL_WORDWIDTH_Pos)

I2S_T::CTRL: WORDWIDTH Mask

Definition at line 4838 of file Nano100Series.h.

## ◆ I2S_CTRL_WORDWIDTH_Pos

#define I2S_CTRL_WORDWIDTH_Pos (4)

I2S_T::CTRL: WORDWIDTH Position

Definition at line 4837 of file Nano100Series.h.

## ◆ I2S_INTEN_LZCIE_Msk

#define I2S_INTEN_LZCIE_Msk (0x1ul << I2S_INTEN_LZCIE_Pos)

I2S_T::INTEN: LZCIE Mask

Definition at line 4907 of file Nano100Series.h.

## ◆ I2S_INTEN_LZCIE_Pos

#define I2S_INTEN_LZCIE_Pos (12)

I2S_T::INTEN: LZCIE Position

Definition at line 4906 of file Nano100Series.h.

## ◆ I2S_INTEN_RXOVFIE_Msk

#define I2S_INTEN_RXOVFIE_Msk (0x1ul << I2S_INTEN_RXOVFIE_Pos)

I2S_T::INTEN: RXOVFIE Mask

Definition at line 4889 of file Nano100Series.h.

## ◆ I2S_INTEN_RXOVFIE_Pos

#define I2S_INTEN_RXOVFIE_Pos (1)

I2S_T::INTEN: RXOVFIE Position

Definition at line 4888 of file Nano100Series.h.

## ◆ I2S_INTEN_RXTHIE_Msk

#define I2S_INTEN_RXTHIE_Msk (0x1ul << I2S_INTEN_RXTHIE_Pos)

I2S_T::INTEN: RXTHIE Mask

Definition at line 4892 of file Nano100Series.h.

## ◆ I2S_INTEN_RXTHIE_Pos

#define I2S_INTEN_RXTHIE_Pos (2)

I2S_T::INTEN: RXTHIE Position

Definition at line 4891 of file Nano100Series.h.

## ◆ I2S_INTEN_RXUDFIE_Msk

#define I2S_INTEN_RXUDFIE_Msk (0x1ul << I2S_INTEN_RXUDFIE_Pos)

I2S_T::INTEN: RXUDFIE Mask

Definition at line 4886 of file Nano100Series.h.

## ◆ I2S_INTEN_RXUDFIE_Pos

#define I2S_INTEN_RXUDFIE_Pos (0)

I2S_T::INTEN: RXUDFIE Position

Definition at line 4885 of file Nano100Series.h.

## ◆ I2S_INTEN_RZCIE_Msk

#define I2S_INTEN_RZCIE_Msk (0x1ul << I2S_INTEN_RZCIE_Pos)

I2S_T::INTEN: RZCIE Mask

Definition at line 4904 of file Nano100Series.h.

## ◆ I2S_INTEN_RZCIE_Pos

#define I2S_INTEN_RZCIE_Pos (11)

I2S_T::INTEN: RZCIE Position

Definition at line 4903 of file Nano100Series.h.

## ◆ I2S_INTEN_TXOVFIE_Msk

#define I2S_INTEN_TXOVFIE_Msk (0x1ul << I2S_INTEN_TXOVFIE_Pos)

I2S_T::INTEN: TXOVFIE Mask

Definition at line 4898 of file Nano100Series.h.

## ◆ I2S_INTEN_TXOVFIE_Pos

#define I2S_INTEN_TXOVFIE_Pos (9)

I2S_T::INTEN: TXOVFIE Position

Definition at line 4897 of file Nano100Series.h.

## ◆ I2S_INTEN_TXTHIE_Msk

#define I2S_INTEN_TXTHIE_Msk (0x1ul << I2S_INTEN_TXTHIE_Pos)

I2S_T::INTEN: TXTHIE Mask

Definition at line 4901 of file Nano100Series.h.

## ◆ I2S_INTEN_TXTHIE_Pos

#define I2S_INTEN_TXTHIE_Pos (10)

I2S_T::INTEN: TXTHIE Position

Definition at line 4900 of file Nano100Series.h.

## ◆ I2S_INTEN_TXUDFIE_Msk

#define I2S_INTEN_TXUDFIE_Msk (0x1ul << I2S_INTEN_TXUDFIE_Pos)

I2S_T::INTEN: TXUDFIE Mask

Definition at line 4895 of file Nano100Series.h.

## ◆ I2S_INTEN_TXUDFIE_Pos

#define I2S_INTEN_TXUDFIE_Pos (8)

I2S_T::INTEN: TXUDFIE Position

Definition at line 4894 of file Nano100Series.h.

## ◆ I2S_RXFIFO_RXFIFO_Msk

#define I2S_RXFIFO_RXFIFO_Msk (0xfffffffful << I2S_RXFIFO_RXFIFO_Pos)

I2S_T::RXFIFO: RXFIFO Mask

Definition at line 4970 of file Nano100Series.h.

## ◆ I2S_RXFIFO_RXFIFO_Pos

#define I2S_RXFIFO_RXFIFO_Pos (0)

I2S_T::RXFIFO: RXFIFO Position

Definition at line 4969 of file Nano100Series.h.

## ◆ I2S_STATUS_I2SINT_Msk

#define I2S_STATUS_I2SINT_Msk (0x1ul << I2S_STATUS_I2SINT_Pos)

I2S_T::STATUS: I2SINT Mask

Definition at line 4910 of file Nano100Series.h.

## ◆ I2S_STATUS_I2SINT_Pos

#define I2S_STATUS_I2SINT_Pos (0)

I2S_T::STATUS: I2SINT Position

Definition at line 4909 of file Nano100Series.h.

## ◆ I2S_STATUS_I2SRXINT_Msk

#define I2S_STATUS_I2SRXINT_Msk (0x1ul << I2S_STATUS_I2SRXINT_Pos)

I2S_T::STATUS: I2SRXINT Mask

Definition at line 4913 of file Nano100Series.h.

## ◆ I2S_STATUS_I2SRXINT_Pos

#define I2S_STATUS_I2SRXINT_Pos (1)

I2S_T::STATUS: I2SRXINT Position

Definition at line 4912 of file Nano100Series.h.

## ◆ I2S_STATUS_I2STXINT_Msk

#define I2S_STATUS_I2STXINT_Msk (0x1ul << I2S_STATUS_I2STXINT_Pos)

I2S_T::STATUS: I2STXINT Mask

Definition at line 4916 of file Nano100Series.h.

## ◆ I2S_STATUS_I2STXINT_Pos

#define I2S_STATUS_I2STXINT_Pos (2)

I2S_T::STATUS: I2STXINT Position

Definition at line 4915 of file Nano100Series.h.

## ◆ I2S_STATUS_LZCF_Msk

#define I2S_STATUS_LZCF_Msk (0x1ul << I2S_STATUS_LZCF_Pos)

I2S_T::STATUS: LZCF Mask

Definition at line 4958 of file Nano100Series.h.

## ◆ I2S_STATUS_LZCF_Pos

#define I2S_STATUS_LZCF_Pos (23)

I2S_T::STATUS: LZCF Position

Definition at line 4957 of file Nano100Series.h.

## ◆ I2S_STATUS_RIGHT_Msk

#define I2S_STATUS_RIGHT_Msk (0x1ul << I2S_STATUS_RIGHT_Pos)

I2S_T::STATUS: RIGHT Mask

Definition at line 4919 of file Nano100Series.h.

## ◆ I2S_STATUS_RIGHT_Pos

#define I2S_STATUS_RIGHT_Pos (3)

I2S_T::STATUS: RIGHT Position

Definition at line 4918 of file Nano100Series.h.

## ◆ I2S_STATUS_RX_LEVEL_Msk

#define I2S_STATUS_RX_LEVEL_Msk (0xful << I2S_STATUS_RX_LEVEL_Pos)

I2S_T::STATUS: RX_LEVEL Mask

Definition at line 4961 of file Nano100Series.h.

## ◆ I2S_STATUS_RX_LEVEL_Pos

#define I2S_STATUS_RX_LEVEL_Pos (24)

I2S_T::STATUS: RX_LEVEL Position

Definition at line 4960 of file Nano100Series.h.

## ◆ I2S_STATUS_RXEMPTY_Msk

#define I2S_STATUS_RXEMPTY_Msk (0x1ul << I2S_STATUS_RXEMPTY_Pos)

I2S_T::STATUS: RXEMPTY Mask

Definition at line 4934 of file Nano100Series.h.

## ◆ I2S_STATUS_RXEMPTY_Pos

#define I2S_STATUS_RXEMPTY_Pos (12)

I2S_T::STATUS: RXEMPTY Position

Definition at line 4933 of file Nano100Series.h.

## ◆ I2S_STATUS_RXFULL_Msk

#define I2S_STATUS_RXFULL_Msk (0x1ul << I2S_STATUS_RXFULL_Pos)

I2S_T::STATUS: RXFULL Mask

Definition at line 4931 of file Nano100Series.h.

## ◆ I2S_STATUS_RXFULL_Pos

#define I2S_STATUS_RXFULL_Pos (11)

I2S_T::STATUS: RXFULL Position

Definition at line 4930 of file Nano100Series.h.

## ◆ I2S_STATUS_RXOVF_Msk

#define I2S_STATUS_RXOVF_Msk (0x1ul << I2S_STATUS_RXOVF_Pos)

I2S_T::STATUS: RXOVF Mask

Definition at line 4925 of file Nano100Series.h.

## ◆ I2S_STATUS_RXOVF_Pos

#define I2S_STATUS_RXOVF_Pos (9)

I2S_T::STATUS: RXOVF Position

Definition at line 4924 of file Nano100Series.h.

## ◆ I2S_STATUS_RXTHF_Msk

#define I2S_STATUS_RXTHF_Msk (0x1ul << I2S_STATUS_RXTHF_Pos)

I2S_T::STATUS: RXTHF Mask

Definition at line 4928 of file Nano100Series.h.

## ◆ I2S_STATUS_RXTHF_Pos

#define I2S_STATUS_RXTHF_Pos (10)

I2S_T::STATUS: RXTHF Position

Definition at line 4927 of file Nano100Series.h.

## ◆ I2S_STATUS_RXUDF_Msk

#define I2S_STATUS_RXUDF_Msk (0x1ul << I2S_STATUS_RXUDF_Pos)

I2S_T::STATUS: RXUDF Mask

Definition at line 4922 of file Nano100Series.h.

## ◆ I2S_STATUS_RXUDF_Pos

#define I2S_STATUS_RXUDF_Pos (8)

I2S_T::STATUS: RXUDF Position

Definition at line 4921 of file Nano100Series.h.

## ◆ I2S_STATUS_RZCF_Msk

#define I2S_STATUS_RZCF_Msk (0x1ul << I2S_STATUS_RZCF_Pos)

I2S_T::STATUS: RZCF Mask

Definition at line 4955 of file Nano100Series.h.

## ◆ I2S_STATUS_RZCF_Pos

#define I2S_STATUS_RZCF_Pos (22)

I2S_T::STATUS: RZCF Position

Definition at line 4954 of file Nano100Series.h.

## ◆ I2S_STATUS_TX_LEVEL_Msk

#define I2S_STATUS_TX_LEVEL_Msk (0xful << I2S_STATUS_TX_LEVEL_Pos)

I2S_T::STATUS: TX_LEVEL Mask

Definition at line 4964 of file Nano100Series.h.

## ◆ I2S_STATUS_TX_LEVEL_Pos

#define I2S_STATUS_TX_LEVEL_Pos (28)

I2S_T::STATUS: TX_LEVEL Position

Definition at line 4963 of file Nano100Series.h.

## ◆ I2S_STATUS_TXBUSY_Msk

#define I2S_STATUS_TXBUSY_Msk (0x1ul << I2S_STATUS_TXBUSY_Pos)

I2S_T::STATUS: TXBUSY Mask

Definition at line 4952 of file Nano100Series.h.

## ◆ I2S_STATUS_TXBUSY_Pos

#define I2S_STATUS_TXBUSY_Pos (21)

I2S_T::STATUS: TXBUSY Position

Definition at line 4951 of file Nano100Series.h.

## ◆ I2S_STATUS_TXEMPTY_Msk

#define I2S_STATUS_TXEMPTY_Msk (0x1ul << I2S_STATUS_TXEMPTY_Pos)

I2S_T::STATUS: TXEMPTY Mask

Definition at line 4949 of file Nano100Series.h.

## ◆ I2S_STATUS_TXEMPTY_Pos

#define I2S_STATUS_TXEMPTY_Pos (20)

I2S_T::STATUS: TXEMPTY Position

Definition at line 4948 of file Nano100Series.h.

## ◆ I2S_STATUS_TXFULL_Msk

#define I2S_STATUS_TXFULL_Msk (0x1ul << I2S_STATUS_TXFULL_Pos)

I2S_T::STATUS: TXFULL Mask

Definition at line 4946 of file Nano100Series.h.

## ◆ I2S_STATUS_TXFULL_Pos

#define I2S_STATUS_TXFULL_Pos (19)

I2S_T::STATUS: TXFULL Position

Definition at line 4945 of file Nano100Series.h.

## ◆ I2S_STATUS_TXOVF_Msk

#define I2S_STATUS_TXOVF_Msk (0x1ul << I2S_STATUS_TXOVF_Pos)

I2S_T::STATUS: TXOVF Mask

Definition at line 4940 of file Nano100Series.h.

## ◆ I2S_STATUS_TXOVF_Pos

#define I2S_STATUS_TXOVF_Pos (17)

I2S_T::STATUS: TXOVF Position

Definition at line 4939 of file Nano100Series.h.

## ◆ I2S_STATUS_TXTHF_Msk

#define I2S_STATUS_TXTHF_Msk (0x1ul << I2S_STATUS_TXTHF_Pos)

I2S_T::STATUS: TXTHF Mask

Definition at line 4943 of file Nano100Series.h.

## ◆ I2S_STATUS_TXTHF_Pos

#define I2S_STATUS_TXTHF_Pos (18)

I2S_T::STATUS: TXTHF Position

Definition at line 4942 of file Nano100Series.h.

## ◆ I2S_STATUS_TXUDF_Msk

#define I2S_STATUS_TXUDF_Msk (0x1ul << I2S_STATUS_TXUDF_Pos)

I2S_T::STATUS: TXUDF Mask

Definition at line 4937 of file Nano100Series.h.

## ◆ I2S_STATUS_TXUDF_Pos

#define I2S_STATUS_TXUDF_Pos (16)

I2S_T::STATUS: TXUDF Position

Definition at line 4936 of file Nano100Series.h.

## ◆ I2S_TXFIFO_TXFIFO_Msk

#define I2S_TXFIFO_TXFIFO_Msk (0xfffffffful << I2S_TXFIFO_TXFIFO_Pos)

I2S_T::TXFIFO: TXFIFO Mask

Definition at line 4967 of file Nano100Series.h.

## ◆ I2S_TXFIFO_TXFIFO_Pos

#define I2S_TXFIFO_TXFIFO_Pos (0)

I2S_T::TXFIFO: TXFIFO Position

Definition at line 4966 of file Nano100Series.h.

## ◆ INTR_IRQSRC_INT_SRC_Msk

#define INTR_IRQSRC_INT_SRC_Msk (0xful << INTR_IRQ0SRC_INT_SRC_Pos)

INTR_T::IRQSRC: INT_SRC Mask

Definition at line 5038 of file Nano100Series.h.

## ◆ INTR_IRQSRC_INT_SRC_Pos

#define INTR_IRQSRC_INT_SRC_Pos (0)

    @addtogroup INT_CONST INT Bit Field Definition
    Constant Definitions for INT Controller

INTR_T::IRQSRC: INT_SRC Position

Definition at line 5037 of file Nano100Series.h.

## ◆ INTR_MCU_IRQ_MCU_IRQ_Msk

#define INTR_MCU_IRQ_MCU_IRQ_Msk (0xfffffffful << INTR_MCU_IRQ_MCU_IRQ_Pos)

INTR_T::MCU_IRQ: MCU_IRQ Mask

Definition at line 5044 of file Nano100Series.h.

## ◆ INTR_MCU_IRQ_MCU_IRQ_Pos

#define INTR_MCU_IRQ_MCU_IRQ_Pos (0)

INTR_T::MCU_IRQ: MCU_IRQ Position

Definition at line 5043 of file Nano100Series.h.

## ◆ INTR_NMI_SEL_NMISEL_Msk

#define INTR_NMI_SEL_NMISEL_Msk (0x1ful << INTR_NMI_SEL_NMISEL_Pos)

INTR_T::NMI_SEL: NMISEL Mask

Definition at line 5041 of file Nano100Series.h.

## ◆ INTR_NMI_SEL_NMISEL_Pos

#define INTR_NMI_SEL_NMISEL_Pos (0)

INTR_T::NMI_SEL: NMISEL Position

Definition at line 5040 of file Nano100Series.h.

## ◆ LCD_CTL_BLINK_Msk

#define LCD_CTL_BLINK_Msk (0x1ul << LCD_CTL_BLINK_Pos)

LCD_T::CTL: BLINK Mask

Definition at line 5386 of file Nano100Series.h.

## ◆ LCD_CTL_BLINK_Pos

#define LCD_CTL_BLINK_Pos (7)

LCD_T::CTL: BLINK Position

Definition at line 5385 of file Nano100Series.h.

## ◆ LCD_CTL_EN_Msk

#define LCD_CTL_EN_Msk (0x1ul << LCD_CTL_EN_Pos)

LCD_T::CTL: EN Mask

Definition at line 5377 of file Nano100Series.h.

## ◆ LCD_CTL_EN_Pos

#define LCD_CTL_EN_Pos (0)

    @addtogroup LCD_CONST LCD Bit Field Definition
    Constant Definitions for LCD Controller

LCD_T::CTL: EN Position

Definition at line 5376 of file Nano100Series.h.

## ◆ LCD_CTL_FREQ_Msk

#define LCD_CTL_FREQ_Msk (0x7ul << LCD_CTL_FREQ_Pos)

LCD_T::CTL: FREQ Mask

Definition at line 5383 of file Nano100Series.h.

## ◆ LCD_CTL_FREQ_Pos

#define LCD_CTL_FREQ_Pos (4)

LCD_T::CTL: FREQ Position

Definition at line 5382 of file Nano100Series.h.

## ◆ LCD_CTL_MUX_Msk

#define LCD_CTL_MUX_Msk (0x7ul << LCD_CTL_MUX_Pos)

LCD_T::CTL: MUX Mask

Definition at line 5380 of file Nano100Series.h.

## ◆ LCD_CTL_MUX_Pos

#define LCD_CTL_MUX_Pos (1)

LCD_T::CTL: MUX Position

Definition at line 5379 of file Nano100Series.h.

## ◆ LCD_CTL_PDDISP_EN_Msk

#define LCD_CTL_PDDISP_EN_Msk (0x1ul << LCD_CTL_PDDISP_EN_Pos)

LCD_T::CTL: PDDISP_EN Mask

Definition at line 5389 of file Nano100Series.h.

## ◆ LCD_CTL_PDDISP_EN_Pos

#define LCD_CTL_PDDISP_EN_Pos (8)

LCD_T::CTL: PDDISP_EN Position

Definition at line 5388 of file Nano100Series.h.

## ◆ LCD_CTL_PDINT_EN_Msk

#define LCD_CTL_PDINT_EN_Msk (0x1ul << LCD_CTL_PDINT_EN_Pos)

LCD_T::CTL: PDINT_EN Mask

Definition at line 5392 of file Nano100Series.h.

## ◆ LCD_CTL_PDINT_EN_Pos

#define LCD_CTL_PDINT_EN_Pos (9)

LCD_T::CTL: PDINT_EN Position

Definition at line 5391 of file Nano100Series.h.

## ◆ LCD_DISPCTL_BIAS_SEL_Msk

#define LCD_DISPCTL_BIAS_SEL_Msk (0x3ul << LCD_DISPCTL_BIAS_SEL_Pos)

LCD_T::DISPCTL: BIAS_SEL Mask

Definition at line 5398 of file Nano100Series.h.

## ◆ LCD_DISPCTL_BIAS_SEL_Pos

#define LCD_DISPCTL_BIAS_SEL_Pos (1)

LCD_T::DISPCTL: BIAS_SEL Position

Definition at line 5397 of file Nano100Series.h.

## ◆ LCD_DISPCTL_BV_SEL_Msk

#define LCD_DISPCTL_BV_SEL_Msk (0x1ul << LCD_DISPCTL_BV_SEL_Pos)

LCD_T::DISPCTL: BV_SEL Mask

Definition at line 5404 of file Nano100Series.h.

## ◆ LCD_DISPCTL_BV_SEL_Pos

#define LCD_DISPCTL_BV_SEL_Pos (6)

LCD_T::DISPCTL: BV_SEL Position

Definition at line 5403 of file Nano100Series.h.

## ◆ LCD_DISPCTL_CPUMP_EN_Msk

#define LCD_DISPCTL_CPUMP_EN_Msk (0x1ul << LCD_DISPCTL_CPUMP_EN_Pos)

LCD_T::DISPCTL: CPUMP_EN Mask

Definition at line 5395 of file Nano100Series.h.

## ◆ LCD_DISPCTL_CPUMP_EN_Pos

#define LCD_DISPCTL_CPUMP_EN_Pos (0)

LCD_T::DISPCTL: CPUMP_EN Position

Definition at line 5394 of file Nano100Series.h.

## ◆ LCD_DISPCTL_CPUMP_FREQ_Msk

#define LCD_DISPCTL_CPUMP_FREQ_Msk (0x7ul << LCD_DISPCTL_CPUMP_FREQ_Pos)

LCD_T::DISPCTL: CPUMP_FREQ Mask

Definition at line 5410 of file Nano100Series.h.

## ◆ LCD_DISPCTL_CPUMP_FREQ_Pos

#define LCD_DISPCTL_CPUMP_FREQ_Pos (11)

LCD_T::DISPCTL: CPUMP_FREQ Position

Definition at line 5409 of file Nano100Series.h.

## ◆ LCD_DISPCTL_CPUMP_VOL_SET_Msk

#define LCD_DISPCTL_CPUMP_VOL_SET_Msk (0x7ul << LCD_DISPCTL_CPUMP_VOL_SET_Pos)

LCD_T::DISPCTL: CPUMP_VOL_SET Mask

Definition at line 5407 of file Nano100Series.h.

## ◆ LCD_DISPCTL_CPUMP_VOL_SET_Pos

#define LCD_DISPCTL_CPUMP_VOL_SET_Pos (8)

LCD_T::DISPCTL: CPUMP_VOL_SET Position

Definition at line 5406 of file Nano100Series.h.

## ◆ LCD_DISPCTL_IBRL_EN_Msk

#define LCD_DISPCTL_IBRL_EN_Msk (0x1ul << LCD_DISPCTL_IBRL_EN_Pos)

LCD_T::DISPCTL: IBRL_EN Mask

Definition at line 5401 of file Nano100Series.h.

## ◆ LCD_DISPCTL_IBRL_EN_Pos

#define LCD_DISPCTL_IBRL_EN_Pos (4)

LCD_T::DISPCTL: IBRL_EN Position

Definition at line 5400 of file Nano100Series.h.

## ◆ LCD_FCR_FCEN_Msk

#define LCD_FCR_FCEN_Msk (0x1ul << LCD_FCR_FCEN_Pos)

LCD_T::FCR: FCEN Mask

Definition at line 5533 of file Nano100Series.h.

## ◆ LCD_FCR_FCEN_Pos

#define LCD_FCR_FCEN_Pos (0)

LCD_T::FCR: FCEN Position

Definition at line 5532 of file Nano100Series.h.

## ◆ LCD_FCR_FCINTEN_Msk

#define LCD_FCR_FCINTEN_Msk (0x1ul << LCD_FCR_FCINTEN_Pos)

LCD_T::FCR: FCINTEN Mask

Definition at line 5536 of file Nano100Series.h.

## ◆ LCD_FCR_FCINTEN_Pos

#define LCD_FCR_FCINTEN_Pos (1)

LCD_T::FCR: FCINTEN Position

Definition at line 5535 of file Nano100Series.h.

## ◆ LCD_FCR_FCV_Msk

#define LCD_FCR_FCV_Msk (0x3ful << LCD_FCR_FCV_Pos)

LCD_T::FCR: FCV Mask

Definition at line 5542 of file Nano100Series.h.

## ◆ LCD_FCR_FCV_Pos

#define LCD_FCR_FCV_Pos (4)

LCD_T::FCR: FCV Position

Definition at line 5541 of file Nano100Series.h.

## ◆ LCD_FCR_PRESCL_Msk

#define LCD_FCR_PRESCL_Msk (0x3ul << LCD_FCR_PRESCL_Pos)

LCD_T::FCR: PRESCL Mask

Definition at line 5539 of file Nano100Series.h.

## ◆ LCD_FCR_PRESCL_Pos

#define LCD_FCR_PRESCL_Pos (2)

LCD_T::FCR: PRESCL Position

Definition at line 5538 of file Nano100Series.h.

## ◆ LCD_FCSTS_FCSTS_Msk

#define LCD_FCSTS_FCSTS_Msk (0x1ul << LCD_FCSTS_FCSTS_Pos)

LCD_T::FCSTS: FCSTS Mask

Definition at line 5545 of file Nano100Series.h.

## ◆ LCD_FCSTS_FCSTS_Pos

#define LCD_FCSTS_FCSTS_Pos (0)

LCD_T::FCSTS: FCSTS Position

Definition at line 5544 of file Nano100Series.h.

## ◆ LCD_FCSTS_PDSTS_Msk

#define LCD_FCSTS_PDSTS_Msk (0x1ul << LCD_FCSTS_PDSTS_Pos)

LCD_T::FCSTS: PDSTS Mask

Definition at line 5548 of file Nano100Series.h.

## ◆ LCD_FCSTS_PDSTS_Pos

#define LCD_FCSTS_PDSTS_Pos (1)

LCD_T::FCSTS: PDSTS Position

Definition at line 5547 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_0_4x_Msk

#define LCD_MEM_0_SEG_0_4x_Msk (0x3ful << LCD_MEM_0_SEG_0_4x_Pos)

LCD_T::MEM_0: SEG_0_4x Mask

Definition at line 5413 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_0_4x_Pos

#define LCD_MEM_0_SEG_0_4x_Pos (0)

LCD_T::MEM_0: SEG_0_4x Position

Definition at line 5412 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_1_4x_Msk

#define LCD_MEM_0_SEG_1_4x_Msk (0x7ful << LCD_MEM_0_SEG_1_4x_Pos)

LCD_T::MEM_0: SEG_1_4x Mask

Definition at line 5416 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_1_4x_Pos

#define LCD_MEM_0_SEG_1_4x_Pos (8)

LCD_T::MEM_0: SEG_1_4x Position

Definition at line 5415 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_2_4x_Msk

#define LCD_MEM_0_SEG_2_4x_Msk (0x3ful << LCD_MEM_0_SEG_2_4x_Pos)

LCD_T::MEM_0: SEG_2_4x Mask

Definition at line 5419 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_2_4x_Pos

#define LCD_MEM_0_SEG_2_4x_Pos (16)

LCD_T::MEM_0: SEG_2_4x Position

Definition at line 5418 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_3_4x_Msk

#define LCD_MEM_0_SEG_3_4x_Msk (0x3ful << LCD_MEM_0_SEG_3_4x_Pos)

LCD_T::MEM_0: SEG_3_4x Mask

Definition at line 5422 of file Nano100Series.h.

## ◆ LCD_MEM_0_SEG_3_4x_Pos

#define LCD_MEM_0_SEG_3_4x_Pos (24)

LCD_T::MEM_0: SEG_3_4x Position

Definition at line 5421 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_0_4x_Msk

#define LCD_MEM_1_SEG_0_4x_Msk (0x3ful << LCD_MEM_1_SEG_0_4x_Pos)

LCD_T::MEM_1: SEG_0_4x Mask

Definition at line 5425 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_0_4x_Pos

#define LCD_MEM_1_SEG_0_4x_Pos (0)

LCD_T::MEM_1: SEG_0_4x Position

Definition at line 5424 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_1_4x_Msk

#define LCD_MEM_1_SEG_1_4x_Msk (0x7ful << LCD_MEM_1_SEG_1_4x_Pos)

LCD_T::MEM_1: SEG_1_4x Mask

Definition at line 5428 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_1_4x_Pos

#define LCD_MEM_1_SEG_1_4x_Pos (8)

LCD_T::MEM_1: SEG_1_4x Position

Definition at line 5427 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_2_4x_Msk

#define LCD_MEM_1_SEG_2_4x_Msk (0x3ful << LCD_MEM_1_SEG_2_4x_Pos)

LCD_T::MEM_1: SEG_2_4x Mask

Definition at line 5431 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_2_4x_Pos

#define LCD_MEM_1_SEG_2_4x_Pos (16)

LCD_T::MEM_1: SEG_2_4x Position

Definition at line 5430 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_3_4x_Msk

#define LCD_MEM_1_SEG_3_4x_Msk (0x3ful << LCD_MEM_1_SEG_3_4x_Pos)

LCD_T::MEM_1: SEG_3_4x Mask

Definition at line 5434 of file Nano100Series.h.

## ◆ LCD_MEM_1_SEG_3_4x_Pos

#define LCD_MEM_1_SEG_3_4x_Pos (24)

LCD_T::MEM_1: SEG_3_4x Position

Definition at line 5433 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_0_4x_Msk

#define LCD_MEM_2_SEG_0_4x_Msk (0x3ful << LCD_MEM_2_SEG_0_4x_Pos)

LCD_T::MEM_2: SEG_0_4x Mask

Definition at line 5437 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_0_4x_Pos

#define LCD_MEM_2_SEG_0_4x_Pos (0)

LCD_T::MEM_2: SEG_0_4x Position

Definition at line 5436 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_1_4x_Msk

#define LCD_MEM_2_SEG_1_4x_Msk (0x7ful << LCD_MEM_2_SEG_1_4x_Pos)

LCD_T::MEM_2: SEG_1_4x Mask

Definition at line 5440 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_1_4x_Pos

#define LCD_MEM_2_SEG_1_4x_Pos (8)

LCD_T::MEM_2: SEG_1_4x Position

Definition at line 5439 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_2_4x_Msk

#define LCD_MEM_2_SEG_2_4x_Msk (0x3ful << LCD_MEM_2_SEG_2_4x_Pos)

LCD_T::MEM_2: SEG_2_4x Mask

Definition at line 5443 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_2_4x_Pos

#define LCD_MEM_2_SEG_2_4x_Pos (16)

LCD_T::MEM_2: SEG_2_4x Position

Definition at line 5442 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_3_4x_Msk

#define LCD_MEM_2_SEG_3_4x_Msk (0x3ful << LCD_MEM_2_SEG_3_4x_Pos)

LCD_T::MEM_2: SEG_3_4x Mask

Definition at line 5446 of file Nano100Series.h.

## ◆ LCD_MEM_2_SEG_3_4x_Pos

#define LCD_MEM_2_SEG_3_4x_Pos (24)

LCD_T::MEM_2: SEG_3_4x Position

Definition at line 5445 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_0_4x_Msk

#define LCD_MEM_3_SEG_0_4x_Msk (0x3ful << LCD_MEM_3_SEG_0_4x_Pos)

LCD_T::MEM_3: SEG_0_4x Mask

Definition at line 5449 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_0_4x_Pos

#define LCD_MEM_3_SEG_0_4x_Pos (0)

LCD_T::MEM_3: SEG_0_4x Position

Definition at line 5448 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_1_4x_Msk

#define LCD_MEM_3_SEG_1_4x_Msk (0x7ful << LCD_MEM_3_SEG_1_4x_Pos)

LCD_T::MEM_3: SEG_1_4x Mask

Definition at line 5452 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_1_4x_Pos

#define LCD_MEM_3_SEG_1_4x_Pos (8)

LCD_T::MEM_3: SEG_1_4x Position

Definition at line 5451 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_2_4x_Msk

#define LCD_MEM_3_SEG_2_4x_Msk (0x3ful << LCD_MEM_3_SEG_2_4x_Pos)

LCD_T::MEM_3: SEG_2_4x Mask

Definition at line 5455 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_2_4x_Pos

#define LCD_MEM_3_SEG_2_4x_Pos (16)

LCD_T::MEM_3: SEG_2_4x Position

Definition at line 5454 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_3_4x_Msk

#define LCD_MEM_3_SEG_3_4x_Msk (0x3ful << LCD_MEM_3_SEG_3_4x_Pos)

LCD_T::MEM_3: SEG_3_4x Mask

Definition at line 5458 of file Nano100Series.h.

## ◆ LCD_MEM_3_SEG_3_4x_Pos

#define LCD_MEM_3_SEG_3_4x_Pos (24)

LCD_T::MEM_3: SEG_3_4x Position

Definition at line 5457 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_0_4x_Msk

#define LCD_MEM_4_SEG_0_4x_Msk (0x3ful << LCD_MEM_4_SEG_0_4x_Pos)

LCD_T::MEM_4: SEG_0_4x Mask

Definition at line 5461 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_0_4x_Pos

#define LCD_MEM_4_SEG_0_4x_Pos (0)

LCD_T::MEM_4: SEG_0_4x Position

Definition at line 5460 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_1_4x_Msk

#define LCD_MEM_4_SEG_1_4x_Msk (0x7ful << LCD_MEM_4_SEG_1_4x_Pos)

LCD_T::MEM_4: SEG_1_4x Mask

Definition at line 5464 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_1_4x_Pos

#define LCD_MEM_4_SEG_1_4x_Pos (8)

LCD_T::MEM_4: SEG_1_4x Position

Definition at line 5463 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_2_4x_Msk

#define LCD_MEM_4_SEG_2_4x_Msk (0x3ful << LCD_MEM_4_SEG_2_4x_Pos)

LCD_T::MEM_4: SEG_2_4x Mask

Definition at line 5467 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_2_4x_Pos

#define LCD_MEM_4_SEG_2_4x_Pos (16)

LCD_T::MEM_4: SEG_2_4x Position

Definition at line 5466 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_3_4x_Msk

#define LCD_MEM_4_SEG_3_4x_Msk (0x3ful << LCD_MEM_4_SEG_3_4x_Pos)

LCD_T::MEM_4: SEG_3_4x Mask

Definition at line 5470 of file Nano100Series.h.

## ◆ LCD_MEM_4_SEG_3_4x_Pos

#define LCD_MEM_4_SEG_3_4x_Pos (24)

LCD_T::MEM_4: SEG_3_4x Position

Definition at line 5469 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_0_4x_Msk

#define LCD_MEM_5_SEG_0_4x_Msk (0x3ful << LCD_MEM_5_SEG_0_4x_Pos)

LCD_T::MEM_5: SEG_0_4x Mask

Definition at line 5473 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_0_4x_Pos

#define LCD_MEM_5_SEG_0_4x_Pos (0)

LCD_T::MEM_5: SEG_0_4x Position

Definition at line 5472 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_1_4x_Msk

#define LCD_MEM_5_SEG_1_4x_Msk (0x7ful << LCD_MEM_5_SEG_1_4x_Pos)

LCD_T::MEM_5: SEG_1_4x Mask

Definition at line 5476 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_1_4x_Pos

#define LCD_MEM_5_SEG_1_4x_Pos (8)

LCD_T::MEM_5: SEG_1_4x Position

Definition at line 5475 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_2_4x_Msk

#define LCD_MEM_5_SEG_2_4x_Msk (0x3ful << LCD_MEM_5_SEG_2_4x_Pos)

LCD_T::MEM_5: SEG_2_4x Mask

Definition at line 5479 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_2_4x_Pos

#define LCD_MEM_5_SEG_2_4x_Pos (16)

LCD_T::MEM_5: SEG_2_4x Position

Definition at line 5478 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_3_4x_Msk

#define LCD_MEM_5_SEG_3_4x_Msk (0x3ful << LCD_MEM_5_SEG_3_4x_Pos)

LCD_T::MEM_5: SEG_3_4x Mask

Definition at line 5482 of file Nano100Series.h.

## ◆ LCD_MEM_5_SEG_3_4x_Pos

#define LCD_MEM_5_SEG_3_4x_Pos (24)

LCD_T::MEM_5: SEG_3_4x Position

Definition at line 5481 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_0_4x_Msk

#define LCD_MEM_6_SEG_0_4x_Msk (0x3ful << LCD_MEM_6_SEG_0_4x_Pos)

LCD_T::MEM_6: SEG_0_4x Mask

Definition at line 5485 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_0_4x_Pos

#define LCD_MEM_6_SEG_0_4x_Pos (0)

LCD_T::MEM_6: SEG_0_4x Position

Definition at line 5484 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_1_4x_Msk

#define LCD_MEM_6_SEG_1_4x_Msk (0x7ful << LCD_MEM_6_SEG_1_4x_Pos)

LCD_T::MEM_6: SEG_1_4x Mask

Definition at line 5488 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_1_4x_Pos

#define LCD_MEM_6_SEG_1_4x_Pos (8)

LCD_T::MEM_6: SEG_1_4x Position

Definition at line 5487 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_2_4x_Msk

#define LCD_MEM_6_SEG_2_4x_Msk (0x3ful << LCD_MEM_6_SEG_2_4x_Pos)

LCD_T::MEM_6: SEG_2_4x Mask

Definition at line 5491 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_2_4x_Pos

#define LCD_MEM_6_SEG_2_4x_Pos (16)

LCD_T::MEM_6: SEG_2_4x Position

Definition at line 5490 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_3_4x_Msk

#define LCD_MEM_6_SEG_3_4x_Msk (0x3ful << LCD_MEM_6_SEG_3_4x_Pos)

LCD_T::MEM_6: SEG_3_4x Mask

Definition at line 5494 of file Nano100Series.h.

## ◆ LCD_MEM_6_SEG_3_4x_Pos

#define LCD_MEM_6_SEG_3_4x_Pos (24)

LCD_T::MEM_6: SEG_3_4x Position

Definition at line 5493 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_0_4x_Msk

#define LCD_MEM_7_SEG_0_4x_Msk (0x3ful << LCD_MEM_7_SEG_0_4x_Pos)

LCD_T::MEM_7: SEG_0_4x Mask

Definition at line 5497 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_0_4x_Pos

#define LCD_MEM_7_SEG_0_4x_Pos (0)

LCD_T::MEM_7: SEG_0_4x Position

Definition at line 5496 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_1_4x_Msk

#define LCD_MEM_7_SEG_1_4x_Msk (0x7ful << LCD_MEM_7_SEG_1_4x_Pos)

LCD_T::MEM_7: SEG_1_4x Mask

Definition at line 5500 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_1_4x_Pos

#define LCD_MEM_7_SEG_1_4x_Pos (8)

LCD_T::MEM_7: SEG_1_4x Position

Definition at line 5499 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_2_4x_Msk

#define LCD_MEM_7_SEG_2_4x_Msk (0x3ful << LCD_MEM_7_SEG_2_4x_Pos)

LCD_T::MEM_7: SEG_2_4x Mask

Definition at line 5503 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_2_4x_Pos

#define LCD_MEM_7_SEG_2_4x_Pos (16)

LCD_T::MEM_7: SEG_2_4x Position

Definition at line 5502 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_3_4x_Msk

#define LCD_MEM_7_SEG_3_4x_Msk (0x3ful << LCD_MEM_7_SEG_3_4x_Pos)

LCD_T::MEM_7: SEG_3_4x Mask

Definition at line 5506 of file Nano100Series.h.

## ◆ LCD_MEM_7_SEG_3_4x_Pos

#define LCD_MEM_7_SEG_3_4x_Pos (24)

LCD_T::MEM_7: SEG_3_4x Position

Definition at line 5505 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_0_4x_Msk

#define LCD_MEM_8_SEG_0_4x_Msk (0x3ful << LCD_MEM_8_SEG_0_4x_Pos)

LCD_T::MEM_8: SEG_0_4x Mask

Definition at line 5509 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_0_4x_Pos

#define LCD_MEM_8_SEG_0_4x_Pos (0)

LCD_T::MEM_8: SEG_0_4x Position

Definition at line 5508 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_1_4x_Msk

#define LCD_MEM_8_SEG_1_4x_Msk (0x7ful << LCD_MEM_8_SEG_1_4x_Pos)

LCD_T::MEM_8: SEG_1_4x Mask

Definition at line 5512 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_1_4x_Pos

#define LCD_MEM_8_SEG_1_4x_Pos (8)

LCD_T::MEM_8: SEG_1_4x Position

Definition at line 5511 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_2_4x_Msk

#define LCD_MEM_8_SEG_2_4x_Msk (0x3ful << LCD_MEM_8_SEG_2_4x_Pos)

LCD_T::MEM_8: SEG_2_4x Mask

Definition at line 5515 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_2_4x_Pos

#define LCD_MEM_8_SEG_2_4x_Pos (16)

LCD_T::MEM_8: SEG_2_4x Position

Definition at line 5514 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_3_4x_Msk

#define LCD_MEM_8_SEG_3_4x_Msk (0x3ful << LCD_MEM_8_SEG_3_4x_Pos)

LCD_T::MEM_8: SEG_3_4x Mask

Definition at line 5518 of file Nano100Series.h.

## ◆ LCD_MEM_8_SEG_3_4x_Pos

#define LCD_MEM_8_SEG_3_4x_Pos (24)

LCD_T::MEM_8: SEG_3_4x Position

Definition at line 5517 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_0_4x_Msk

#define LCD_MEM_9_SEG_0_4x_Msk (0x3ful << LCD_MEM_9_SEG_0_4x_Pos)

LCD_T::MEM_9: SEG_0_4x Mask

Definition at line 5521 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_0_4x_Pos

#define LCD_MEM_9_SEG_0_4x_Pos (0)

LCD_T::MEM_9: SEG_0_4x Position

Definition at line 5520 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_1_4x_Msk

#define LCD_MEM_9_SEG_1_4x_Msk (0x7ful << LCD_MEM_9_SEG_1_4x_Pos)

LCD_T::MEM_9: SEG_1_4x Mask

Definition at line 5524 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_1_4x_Pos

#define LCD_MEM_9_SEG_1_4x_Pos (8)

LCD_T::MEM_9: SEG_1_4x Position

Definition at line 5523 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_2_4x_Msk

#define LCD_MEM_9_SEG_2_4x_Msk (0x3ful << LCD_MEM_9_SEG_2_4x_Pos)

LCD_T::MEM_9: SEG_2_4x Mask

Definition at line 5527 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_2_4x_Pos

#define LCD_MEM_9_SEG_2_4x_Pos (16)

LCD_T::MEM_9: SEG_2_4x Position

Definition at line 5526 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_3_4x_Msk

#define LCD_MEM_9_SEG_3_4x_Msk (0x3ful << LCD_MEM_9_SEG_3_4x_Pos)

LCD_T::MEM_9: SEG_3_4x Mask

Definition at line 5530 of file Nano100Series.h.

## ◆ LCD_MEM_9_SEG_3_4x_Pos

#define LCD_MEM_9_SEG_3_4x_Pos (24)

LCD_T::MEM_9: SEG_3_4x Position

Definition at line 5529 of file Nano100Series.h.

## ◆ PDMA_BCR_PDMA_BCR_Msk

#define PDMA_BCR_PDMA_BCR_Msk (0xfffful << PDMA_BCR_PDMA_BCR_Pos)

PDMA_T::BCR: PDMA_BCR Mask

Definition at line 6472 of file Nano100Series.h.

## ◆ PDMA_BCR_PDMA_BCR_Pos

#define PDMA_BCR_PDMA_BCR_Pos (0)

PDMA_T::BCR: PDMA_BCR Position

Definition at line 6471 of file Nano100Series.h.

## ◆ PDMA_CBCR_PDMA_CBCR_Msk

#define PDMA_CBCR_PDMA_CBCR_Msk (0xfffffful << PDMA_CBCR_PDMA_CBCR_Pos)

PDMA_T::CBCR: PDMA_CBCR Mask

Definition at line 6481 of file Nano100Series.h.

## ◆ PDMA_CBCR_PDMA_CBCR_Pos

#define PDMA_CBCR_PDMA_CBCR_Pos (0)

PDMA_T::CBCR: PDMA_CBCR Position

Definition at line 6480 of file Nano100Series.h.

## ◆ PDMA_CDAR_PDMA_CDAR_Msk

#define PDMA_CDAR_PDMA_CDAR_Msk (0xfffffffful << PDMA_CDAR_PDMA_CDAR_Pos)

PDMA_T::CDAR: PDMA_CDAR Mask

Definition at line 6478 of file Nano100Series.h.

## ◆ PDMA_CDAR_PDMA_CDAR_Pos

#define PDMA_CDAR_PDMA_CDAR_Pos (0)

PDMA_T::CDAR: PDMA_CDAR Position

Definition at line 6477 of file Nano100Series.h.

## ◆ PDMA_CSAR_PDMA_CSAR_Msk

#define PDMA_CSAR_PDMA_CSAR_Msk (0xfffffffful << PDMA_CSAR_PDMA_CSAR_Pos)

PDMA_T::CSAR: PDMA_CSAR Mask

Definition at line 6475 of file Nano100Series.h.

## ◆ PDMA_CSAR_PDMA_CSAR_Pos

#define PDMA_CSAR_PDMA_CSAR_Pos (0)

PDMA_T::CSAR: PDMA_CSAR Position

Definition at line 6474 of file Nano100Series.h.

## ◆ PDMA_CSR_APB_TWS_Msk

#define PDMA_CSR_APB_TWS_Msk (0x3ul << PDMA_CSR_APB_TWS_Pos)

PDMA_T::CSR: APB_TWS Mask

Definition at line 6460 of file Nano100Series.h.

## ◆ PDMA_CSR_APB_TWS_Pos

#define PDMA_CSR_APB_TWS_Pos (19)

PDMA_T::CSR: APB_TWS Position

Definition at line 6459 of file Nano100Series.h.

## ◆ PDMA_CSR_DAD_SEL_Msk

#define PDMA_CSR_DAD_SEL_Msk (0x3ul << PDMA_CSR_DAD_SEL_Pos)

PDMA_T::CSR: DAD_SEL Mask

Definition at line 6454 of file Nano100Series.h.

## ◆ PDMA_CSR_DAD_SEL_Pos

#define PDMA_CSR_DAD_SEL_Pos (6)

PDMA_T::CSR: DAD_SEL Position

Definition at line 6453 of file Nano100Series.h.

## ◆ PDMA_CSR_MODE_SEL_Msk

#define PDMA_CSR_MODE_SEL_Msk (0x3ul << PDMA_CSR_MODE_SEL_Pos)

PDMA_T::CSR: MODE_SEL Mask

Definition at line 6448 of file Nano100Series.h.

## ◆ PDMA_CSR_MODE_SEL_Pos

#define PDMA_CSR_MODE_SEL_Pos (2)

PDMA_T::CSR: MODE_SEL Position

Definition at line 6447 of file Nano100Series.h.

## ◆ PDMA_CSR_PDMACEN_Msk

#define PDMA_CSR_PDMACEN_Msk (0x1ul << PDMA_CSR_PDMACEN_Pos)

PDMA_T::CSR: PDMACEN Mask

Definition at line 6442 of file Nano100Series.h.

## ◆ PDMA_CSR_PDMACEN_Pos

#define PDMA_CSR_PDMACEN_Pos (0)

    @addtogroup PDMA_CONST PDMA Bit Field Definition
    Constant Definitions for PDMA Controller

PDMA_T::CSR: PDMACEN Position

Definition at line 6441 of file Nano100Series.h.

## ◆ PDMA_CSR_SAD_SEL_Msk

#define PDMA_CSR_SAD_SEL_Msk (0x3ul << PDMA_CSR_SAD_SEL_Pos)

PDMA_T::CSR: SAD_SEL Mask

Definition at line 6451 of file Nano100Series.h.

## ◆ PDMA_CSR_SAD_SEL_Pos

#define PDMA_CSR_SAD_SEL_Pos (4)

PDMA_T::CSR: SAD_SEL Position

Definition at line 6450 of file Nano100Series.h.

## ◆ PDMA_CSR_SW_RST_Msk

#define PDMA_CSR_SW_RST_Msk (0x1ul << PDMA_CSR_SW_RST_Pos)

PDMA_T::CSR: SW_RST Mask

Definition at line 6445 of file Nano100Series.h.

## ◆ PDMA_CSR_SW_RST_Pos

#define PDMA_CSR_SW_RST_Pos (1)

PDMA_T::CSR: SW_RST Position

Definition at line 6444 of file Nano100Series.h.

## ◆ PDMA_CSR_TO_EN_Msk

#define PDMA_CSR_TO_EN_Msk (0x1ul << PDMA_CSR_TO_EN_Pos)

PDMA_T::CSR: TO_EN Mask

Definition at line 6457 of file Nano100Series.h.

## ◆ PDMA_CSR_TO_EN_Pos

#define PDMA_CSR_TO_EN_Pos (12)

PDMA_T::CSR: TO_EN Position

Definition at line 6456 of file Nano100Series.h.

## ◆ PDMA_CSR_TRIG_EN_Msk

#define PDMA_CSR_TRIG_EN_Msk (0x1ul << PDMA_CSR_TRIG_EN_Pos)

PDMA_T::CSR: TRIG_EN Mask

Definition at line 6463 of file Nano100Series.h.

## ◆ PDMA_CSR_TRIG_EN_Pos

#define PDMA_CSR_TRIG_EN_Pos (23)

PDMA_T::CSR: TRIG_EN Position

Definition at line 6462 of file Nano100Series.h.

## ◆ PDMA_DAR_PDMA_DAR_Msk

#define PDMA_DAR_PDMA_DAR_Msk (0xfffffffful << PDMA_DAR_PDMA_DAR_Pos)

PDMA_T::DAR: PDMA_DAR Mask

Definition at line 6469 of file Nano100Series.h.

## ◆ PDMA_DAR_PDMA_DAR_Pos

#define PDMA_DAR_PDMA_DAR_Pos (0)

PDMA_T::DAR: PDMA_DAR Position

Definition at line 6468 of file Nano100Series.h.

## ◆ PDMA_IER_TABORT_IE_Msk

#define PDMA_IER_TABORT_IE_Msk (0x1ul << PDMA_IER_TABORT_IE_Pos)

PDMA_T::IER: TABORT_IE Mask

Definition at line 6484 of file Nano100Series.h.

## ◆ PDMA_IER_TABORT_IE_Pos

#define PDMA_IER_TABORT_IE_Pos (0)

PDMA_T::IER: TABORT_IE Position

Definition at line 6483 of file Nano100Series.h.

## ◆ PDMA_IER_TD_IE_Msk

#define PDMA_IER_TD_IE_Msk (0x1ul << PDMA_IER_TD_IE_Pos)

PDMA_T::IER: TD_IE Mask

Definition at line 6487 of file Nano100Series.h.

## ◆ PDMA_IER_TD_IE_Pos

#define PDMA_IER_TD_IE_Pos (1)

PDMA_T::IER: TD_IE Position

Definition at line 6486 of file Nano100Series.h.

## ◆ PDMA_IER_TO_IE_Msk

#define PDMA_IER_TO_IE_Msk (0x1ul << PDMA_IER_TO_IE_Pos)

PDMA_T::IER: TO_IE Mask

Definition at line 6493 of file Nano100Series.h.

## ◆ PDMA_IER_TO_IE_Pos

#define PDMA_IER_TO_IE_Pos (6)

PDMA_T::IER: TO_IE Position

Definition at line 6492 of file Nano100Series.h.

## ◆ PDMA_IER_WRA_BCR_IE_Msk

#define PDMA_IER_WRA_BCR_IE_Msk (0xful << PDMA_IER_WRA_BCR_IE_Pos)

PDMA_T::IER: WRA_BCR_IE Mask

Definition at line 6490 of file Nano100Series.h.

## ◆ PDMA_IER_WRA_BCR_IE_Pos

#define PDMA_IER_WRA_BCR_IE_Pos (2)

PDMA_T::IER: WRA_BCR_IE Position

Definition at line 6489 of file Nano100Series.h.

## ◆ PDMA_ISR_TABORT_IS_Msk

#define PDMA_ISR_TABORT_IS_Msk (0x1ul << PDMA_ISR_TABORT_IS_Pos)

PDMA_T::ISR: TABORT_IS Mask

Definition at line 6496 of file Nano100Series.h.

## ◆ PDMA_ISR_TABORT_IS_Pos

#define PDMA_ISR_TABORT_IS_Pos (0)

PDMA_T::ISR: TABORT_IS Position

Definition at line 6495 of file Nano100Series.h.

## ◆ PDMA_ISR_TD_IS_Msk

#define PDMA_ISR_TD_IS_Msk (0x1ul << PDMA_ISR_TD_IS_Pos)

PDMA_T::ISR: TD_IS Mask

Definition at line 6499 of file Nano100Series.h.

## ◆ PDMA_ISR_TD_IS_Pos

#define PDMA_ISR_TD_IS_Pos (1)

PDMA_T::ISR: TD_IS Position

Definition at line 6498 of file Nano100Series.h.

## ◆ PDMA_ISR_TO_IS_Msk

#define PDMA_ISR_TO_IS_Msk (0x1ul << PDMA_ISR_TO_IS_Pos)

PDMA_T::ISR: TO_IS Mask

Definition at line 6505 of file Nano100Series.h.

## ◆ PDMA_ISR_TO_IS_Pos

#define PDMA_ISR_TO_IS_Pos (6)

PDMA_T::ISR: TO_IS Position

Definition at line 6504 of file Nano100Series.h.

## ◆ PDMA_ISR_WRA_BCR_IS_Msk

#define PDMA_ISR_WRA_BCR_IS_Msk (0xful << PDMA_ISR_WRA_BCR_IS_Pos)

PDMA_T::ISR: WRA_BCR_IS Mask

Definition at line 6502 of file Nano100Series.h.

## ◆ PDMA_ISR_WRA_BCR_IS_Pos

#define PDMA_ISR_WRA_BCR_IS_Pos (2)

PDMA_T::ISR: WRA_BCR_IS Position

Definition at line 6501 of file Nano100Series.h.

## ◆ PDMA_SAR_PDMA_SAR_Msk

#define PDMA_SAR_PDMA_SAR_Msk (0xfffffffful << PDMA_SAR_PDMA_SAR_Pos)

PDMA_T::SAR: PDMA_SAR Mask

Definition at line 6466 of file Nano100Series.h.

## ◆ PDMA_SAR_PDMA_SAR_Pos

#define PDMA_SAR_PDMA_SAR_Pos (0)

PDMA_T::SAR: PDMA_SAR Position

Definition at line 6465 of file Nano100Series.h.

## ◆ PDMA_TCR_PDMA_TCR_Msk

#define PDMA_TCR_PDMA_TCR_Msk (0xfffful << PDMA_TCR_PDMA_TCR_Pos)

PDMA_T::TCR: PDMA_TCR Mask

Definition at line 6508 of file Nano100Series.h.

## ◆ PDMA_TCR_PDMA_TCR_Pos

#define PDMA_TCR_PDMA_TCR_Pos (0)

PDMA_T::TCR: PDMA_TCR Position

Definition at line 6507 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH0EN_Msk

#define PWM_CAPCTL_CAPCH0EN_Msk (0x1ul << PWM_CAPCTL_CAPCH0EN_Pos)

PWM_T::CAPCTL: CAPCH0EN Mask

Definition at line 7526 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH0EN_Pos

#define PWM_CAPCTL_CAPCH0EN_Pos (1)

PWM_T::CAPCTL: CAPCH0EN Position

Definition at line 7525 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH0PADEN_Msk

#define PWM_CAPCTL_CAPCH0PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH0PADEN_Pos)

PWM_T::CAPCTL: CAPCH0PADEN Mask

Definition at line 7529 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH0PADEN_Pos

#define PWM_CAPCTL_CAPCH0PADEN_Pos (2)

PWM_T::CAPCTL: CAPCH0PADEN Position

Definition at line 7528 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH1EN_Msk

#define PWM_CAPCTL_CAPCH1EN_Msk (0x1ul << PWM_CAPCTL_CAPCH1EN_Pos)

PWM_T::CAPCTL: CAPCH1EN Mask

Definition at line 7547 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH1EN_Pos

#define PWM_CAPCTL_CAPCH1EN_Pos (9)

PWM_T::CAPCTL: CAPCH1EN Position

Definition at line 7546 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH1PADEN_Msk

#define PWM_CAPCTL_CAPCH1PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH1PADEN_Pos)

PWM_T::CAPCTL: CAPCH1PADEN Mask

Definition at line 7550 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH1PADEN_Pos

#define PWM_CAPCTL_CAPCH1PADEN_Pos (10)

PWM_T::CAPCTL: CAPCH1PADEN Position

Definition at line 7549 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH2EN_Msk

#define PWM_CAPCTL_CAPCH2EN_Msk (0x1ul << PWM_CAPCTL_CAPCH2EN_Pos)

PWM_T::CAPCTL: CAPCH2EN Mask

Definition at line 7568 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH2EN_Pos

#define PWM_CAPCTL_CAPCH2EN_Pos (17)

PWM_T::CAPCTL: CAPCH2EN Position

Definition at line 7567 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH2PADEN_Msk

#define PWM_CAPCTL_CAPCH2PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH2PADEN_Pos)

PWM_T::CAPCTL: CAPCH2PADEN Mask

Definition at line 7571 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH2PADEN_Pos

#define PWM_CAPCTL_CAPCH2PADEN_Pos (18)

PWM_T::CAPCTL: CAPCH2PADEN Position

Definition at line 7570 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH3EN_Msk

#define PWM_CAPCTL_CAPCH3EN_Msk (0x1ul << PWM_CAPCTL_CAPCH3EN_Pos)

PWM_T::CAPCTL: CAPCH3EN Mask

Definition at line 7589 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH3EN_Pos

#define PWM_CAPCTL_CAPCH3EN_Pos (25)

PWM_T::CAPCTL: CAPCH3EN Position

Definition at line 7588 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH3PADEN_Msk

#define PWM_CAPCTL_CAPCH3PADEN_Msk (0x1ul << PWM_CAPCTL_CAPCH3PADEN_Pos)

PWM_T::CAPCTL: CAPCH3PADEN Mask

Definition at line 7592 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPCH3PADEN_Pos

#define PWM_CAPCTL_CAPCH3PADEN_Pos (26)

PWM_T::CAPCTL: CAPCH3PADEN Position

Definition at line 7591 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN0_Msk

#define PWM_CAPCTL_CAPRELOADFEN0_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN0_Pos)

PWM_T::CAPCTL: CAPRELOADFEN0 Mask

Definition at line 7541 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN0_Pos

#define PWM_CAPCTL_CAPRELOADFEN0_Pos (7)

PWM_T::CAPCTL: CAPRELOADFEN0 Position

Definition at line 7540 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN1_Msk

#define PWM_CAPCTL_CAPRELOADFEN1_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN1_Pos)

PWM_T::CAPCTL: CAPRELOADFEN1 Mask

Definition at line 7562 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN1_Pos

#define PWM_CAPCTL_CAPRELOADFEN1_Pos (15)

PWM_T::CAPCTL: CAPRELOADFEN1 Position

Definition at line 7561 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN2_Msk

#define PWM_CAPCTL_CAPRELOADFEN2_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN2_Pos)

PWM_T::CAPCTL: CAPRELOADFEN2 Mask

Definition at line 7583 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN2_Pos

#define PWM_CAPCTL_CAPRELOADFEN2_Pos (23)

PWM_T::CAPCTL: CAPRELOADFEN2 Position

Definition at line 7582 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN3_Msk

#define PWM_CAPCTL_CAPRELOADFEN3_Msk (0x1ul << PWM_CAPCTL_CAPRELOADFEN3_Pos)

PWM_T::CAPCTL: CAPRELOADFEN3 Mask

Definition at line 7604 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADFEN3_Pos

#define PWM_CAPCTL_CAPRELOADFEN3_Pos (31)

PWM_T::CAPCTL: CAPRELOADFEN3 Position

Definition at line 7603 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN0_Msk

#define PWM_CAPCTL_CAPRELOADREN0_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN0_Pos)

PWM_T::CAPCTL: CAPRELOADREN0 Mask

Definition at line 7538 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN0_Pos

#define PWM_CAPCTL_CAPRELOADREN0_Pos (6)

PWM_T::CAPCTL: CAPRELOADREN0 Position

Definition at line 7537 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN1_Msk

#define PWM_CAPCTL_CAPRELOADREN1_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN1_Pos)

PWM_T::CAPCTL: CAPRELOADREN1 Mask

Definition at line 7559 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN1_Pos

#define PWM_CAPCTL_CAPRELOADREN1_Pos (14)

PWM_T::CAPCTL: CAPRELOADREN1 Position

Definition at line 7558 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN2_Msk

#define PWM_CAPCTL_CAPRELOADREN2_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN2_Pos)

PWM_T::CAPCTL: CAPRELOADREN2 Mask

Definition at line 7580 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN2_Pos

#define PWM_CAPCTL_CAPRELOADREN2_Pos (22)

PWM_T::CAPCTL: CAPRELOADREN2 Position

Definition at line 7579 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN3_Msk

#define PWM_CAPCTL_CAPRELOADREN3_Msk (0x1ul << PWM_CAPCTL_CAPRELOADREN3_Pos)

PWM_T::CAPCTL: CAPRELOADREN3 Mask

Definition at line 7601 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CAPRELOADREN3_Pos

#define PWM_CAPCTL_CAPRELOADREN3_Pos (30)

PWM_T::CAPCTL: CAPRELOADREN3 Position

Definition at line 7600 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH01CASK_Msk

#define PWM_CAPCTL_CH01CASK_Msk (0x1ul << PWM_CAPCTL_CH01CASK_Pos)

PWM_T::CAPCTL: CH01CASK Mask

Definition at line 7556 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH01CASK_Pos

#define PWM_CAPCTL_CH01CASK_Pos (13)

PWM_T::CAPCTL: CH01CASK Position

Definition at line 7555 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH0PDMAEN_Msk

#define PWM_CAPCTL_CH0PDMAEN_Msk (0x1ul << PWM_CAPCTL_CH0PDMAEN_Pos)

PWM_T::CAPCTL: CH0PDMAEN Mask

Definition at line 7532 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH0PDMAEN_Pos

#define PWM_CAPCTL_CH0PDMAEN_Pos (3)

PWM_T::CAPCTL: CH0PDMAEN Position

Definition at line 7531 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH0RFORDER_Msk

#define PWM_CAPCTL_CH0RFORDER_Msk (0x1ul << PWM_CAPCTL_CH0RFORDER_Pos)

PWM_T::CAPCTL: CH0RFORDER Mask

Definition at line 7553 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH0RFORDER_Pos

#define PWM_CAPCTL_CH0RFORDER_Pos (12)

PWM_T::CAPCTL: CH0RFORDER Position

Definition at line 7552 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH23CASK_Msk

#define PWM_CAPCTL_CH23CASK_Msk (0x1ul << PWM_CAPCTL_CH23CASK_Pos)

PWM_T::CAPCTL: CH23CASK Mask

Definition at line 7598 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH23CASK_Pos

#define PWM_CAPCTL_CH23CASK_Pos (29)

PWM_T::CAPCTL: CH23CASK Position

Definition at line 7597 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH2PDMAEN_Msk

#define PWM_CAPCTL_CH2PDMAEN_Msk (0x1ul << PWM_CAPCTL_CH2PDMAEN_Pos)

PWM_T::CAPCTL: CH2PDMAEN Mask

Definition at line 7574 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH2PDMAEN_Pos

#define PWM_CAPCTL_CH2PDMAEN_Pos (19)

PWM_T::CAPCTL: CH2PDMAEN Position

Definition at line 7573 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH2RFORDER_Msk

#define PWM_CAPCTL_CH2RFORDER_Msk (0x1ul << PWM_CAPCTL_CH2RFORDER_Pos)

PWM_T::CAPCTL: CH2RFORDER Mask

Definition at line 7595 of file Nano100Series.h.

## ◆ PWM_CAPCTL_CH2RFORDER_Pos

#define PWM_CAPCTL_CH2RFORDER_Pos (28)

PWM_T::CAPCTL: CH2RFORDER Position

Definition at line 7594 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV0_Msk

#define PWM_CAPCTL_INV0_Msk (0x1ul << PWM_CAPCTL_INV0_Pos)

PWM_T::CAPCTL: INV0 Mask

Definition at line 7523 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV0_Pos

#define PWM_CAPCTL_INV0_Pos (0)

PWM_T::CAPCTL: INV0 Position

Definition at line 7522 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV1_Msk

#define PWM_CAPCTL_INV1_Msk (0x1ul << PWM_CAPCTL_INV1_Pos)

PWM_T::CAPCTL: INV1 Mask

Definition at line 7544 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV1_Pos

#define PWM_CAPCTL_INV1_Pos (8)

PWM_T::CAPCTL: INV1 Position

Definition at line 7543 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV2_Msk

#define PWM_CAPCTL_INV2_Msk (0x1ul << PWM_CAPCTL_INV2_Pos)

PWM_T::CAPCTL: INV2 Mask

Definition at line 7565 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV2_Pos

#define PWM_CAPCTL_INV2_Pos (16)

PWM_T::CAPCTL: INV2 Position

Definition at line 7564 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV3_Msk

#define PWM_CAPCTL_INV3_Msk (0x1ul << PWM_CAPCTL_INV3_Pos)

PWM_T::CAPCTL: INV3 Mask

Definition at line 7586 of file Nano100Series.h.

## ◆ PWM_CAPCTL_INV3_Pos

#define PWM_CAPCTL_INV3_Pos (24)

PWM_T::CAPCTL: INV3 Position

Definition at line 7585 of file Nano100Series.h.

## ◆ PWM_CAPCTL_PDMACAPMOD0_Msk

#define PWM_CAPCTL_PDMACAPMOD0_Msk (0x3ul << PWM_CAPCTL_PDMACAPMOD0_Pos)

PWM_T::CAPCTL: PDMACAPMOD0 Mask

Definition at line 7535 of file Nano100Series.h.

## ◆ PWM_CAPCTL_PDMACAPMOD0_Pos

#define PWM_CAPCTL_PDMACAPMOD0_Pos (4)

PWM_T::CAPCTL: PDMACAPMOD0 Position

Definition at line 7534 of file Nano100Series.h.

## ◆ PWM_CAPCTL_PDMACAPMOD2_Msk

#define PWM_CAPCTL_PDMACAPMOD2_Msk (0x3ul << PWM_CAPCTL_PDMACAPMOD2_Pos)

PWM_T::CAPCTL: PDMACAPMOD2 Mask

Definition at line 7577 of file Nano100Series.h.

## ◆ PWM_CAPCTL_PDMACAPMOD2_Pos

#define PWM_CAPCTL_PDMACAPMOD2_Pos (20)

PWM_T::CAPCTL: PDMACAPMOD2 Position

Definition at line 7576 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE0_Msk

#define PWM_CAPINTEN_CFL_IE0_Msk (0x1ul << PWM_CAPINTEN_CFL_IE0_Pos)

PWM_T::CAPINTEN: CFL_IE0 Mask

Definition at line 7610 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE0_Pos

#define PWM_CAPINTEN_CFL_IE0_Pos (1)

PWM_T::CAPINTEN: CFL_IE0 Position

Definition at line 7609 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE1_Msk

#define PWM_CAPINTEN_CFL_IE1_Msk (0x1ul << PWM_CAPINTEN_CFL_IE1_Pos)

PWM_T::CAPINTEN: CFL_IE1 Mask

Definition at line 7616 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE1_Pos

#define PWM_CAPINTEN_CFL_IE1_Pos (9)

PWM_T::CAPINTEN: CFL_IE1 Position

Definition at line 7615 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE2_Msk

#define PWM_CAPINTEN_CFL_IE2_Msk (0x1ul << PWM_CAPINTEN_CFL_IE2_Pos)

PWM_T::CAPINTEN: CFL_IE2 Mask

Definition at line 7622 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE2_Pos

#define PWM_CAPINTEN_CFL_IE2_Pos (17)

PWM_T::CAPINTEN: CFL_IE2 Position

Definition at line 7621 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE3_Msk

#define PWM_CAPINTEN_CFL_IE3_Msk (0x1ul << PWM_CAPINTEN_CFL_IE3_Pos)

PWM_T::CAPINTEN: CFL_IE3 Mask

Definition at line 7628 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CFL_IE3_Pos

#define PWM_CAPINTEN_CFL_IE3_Pos (25)

PWM_T::CAPINTEN: CFL_IE3 Position

Definition at line 7627 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE0_Msk

#define PWM_CAPINTEN_CRL_IE0_Msk (0x1ul << PWM_CAPINTEN_CRL_IE0_Pos)

PWM_T::CAPINTEN: CRL_IE0 Mask

Definition at line 7607 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE0_Pos

#define PWM_CAPINTEN_CRL_IE0_Pos (0)

PWM_T::CAPINTEN: CRL_IE0 Position

Definition at line 7606 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE1_Msk

#define PWM_CAPINTEN_CRL_IE1_Msk (0x1ul << PWM_CAPINTEN_CRL_IE1_Pos)

PWM_T::CAPINTEN: CRL_IE1 Mask

Definition at line 7613 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE1_Pos

#define PWM_CAPINTEN_CRL_IE1_Pos (8)

PWM_T::CAPINTEN: CRL_IE1 Position

Definition at line 7612 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE2_Msk

#define PWM_CAPINTEN_CRL_IE2_Msk (0x1ul << PWM_CAPINTEN_CRL_IE2_Pos)

PWM_T::CAPINTEN: CRL_IE2 Mask

Definition at line 7619 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE2_Pos

#define PWM_CAPINTEN_CRL_IE2_Pos (16)

PWM_T::CAPINTEN: CRL_IE2 Position

Definition at line 7618 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE3_Msk

#define PWM_CAPINTEN_CRL_IE3_Msk (0x1ul << PWM_CAPINTEN_CRL_IE3_Pos)

PWM_T::CAPINTEN: CRL_IE3 Mask

Definition at line 7625 of file Nano100Series.h.

## ◆ PWM_CAPINTEN_CRL_IE3_Pos

#define PWM_CAPINTEN_CRL_IE3_Pos (24)

PWM_T::CAPINTEN: CRL_IE3 Position

Definition at line 7624 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF0_Msk

#define PWM_CAPINTSTS_CAPIF0_Msk (0x1ul << PWM_CAPINTSTS_CAPIF0_Pos)

PWM_T::CAPINTSTS: CAPIF0 Mask

Definition at line 7631 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF0_Pos

#define PWM_CAPINTSTS_CAPIF0_Pos (0)

PWM_T::CAPINTSTS: CAPIF0 Position

Definition at line 7630 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF1_Msk

#define PWM_CAPINTSTS_CAPIF1_Msk (0x1ul << PWM_CAPINTSTS_CAPIF1_Pos)

PWM_T::CAPINTSTS: CAPIF1 Mask

Definition at line 7646 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF1_Pos

#define PWM_CAPINTSTS_CAPIF1_Pos (8)

PWM_T::CAPINTSTS: CAPIF1 Position

Definition at line 7645 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF2_Msk

#define PWM_CAPINTSTS_CAPIF2_Msk (0x1ul << PWM_CAPINTSTS_CAPIF2_Pos)

PWM_T::CAPINTSTS: CAPIF2 Mask

Definition at line 7661 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF2_Pos

#define PWM_CAPINTSTS_CAPIF2_Pos (16)

PWM_T::CAPINTSTS: CAPIF2 Position

Definition at line 7660 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF3_Msk

#define PWM_CAPINTSTS_CAPIF3_Msk (0x1ul << PWM_CAPINTSTS_CAPIF3_Pos)

PWM_T::CAPINTSTS: CAPIF3 Mask

Definition at line 7676 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPIF3_Pos

#define PWM_CAPINTSTS_CAPIF3_Pos (24)

PWM_T::CAPINTSTS: CAPIF3 Position

Definition at line 7675 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF0_Msk

#define PWM_CAPINTSTS_CAPOVF0_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF0_Pos)

PWM_T::CAPINTSTS: CAPOVF0 Mask

Definition at line 7643 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF0_Pos

#define PWM_CAPINTSTS_CAPOVF0_Pos (4)

PWM_T::CAPINTSTS: CAPOVF0 Position

Definition at line 7642 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF1_Msk

#define PWM_CAPINTSTS_CAPOVF1_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF1_Pos)

PWM_T::CAPINTSTS: CAPOVF1 Mask

Definition at line 7658 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF1_Pos

#define PWM_CAPINTSTS_CAPOVF1_Pos (12)

PWM_T::CAPINTSTS: CAPOVF1 Position

Definition at line 7657 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF2_Msk

#define PWM_CAPINTSTS_CAPOVF2_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF2_Pos)

PWM_T::CAPINTSTS: CAPOVF2 Mask

Definition at line 7673 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF2_Pos

#define PWM_CAPINTSTS_CAPOVF2_Pos (20)

PWM_T::CAPINTSTS: CAPOVF2 Position

Definition at line 7672 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF3_Msk

#define PWM_CAPINTSTS_CAPOVF3_Msk (0x1ul << PWM_CAPINTSTS_CAPOVF3_Pos)

PWM_T::CAPINTSTS: CAPOVF3 Mask

Definition at line 7688 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVF3_Pos

#define PWM_CAPINTSTS_CAPOVF3_Pos (28)

PWM_T::CAPINTSTS: CAPOVF3 Position

Definition at line 7687 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR0_Msk

#define PWM_CAPINTSTS_CAPOVR0_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR0_Pos)

PWM_T::CAPINTSTS: CAPOVR0 Mask

Definition at line 7640 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR0_Pos

#define PWM_CAPINTSTS_CAPOVR0_Pos (3)

PWM_T::CAPINTSTS: CAPOVR0 Position

Definition at line 7639 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR1_Msk

#define PWM_CAPINTSTS_CAPOVR1_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR1_Pos)

PWM_T::CAPINTSTS: CAPOVR1 Mask

Definition at line 7655 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR1_Pos

#define PWM_CAPINTSTS_CAPOVR1_Pos (11)

PWM_T::CAPINTSTS: CAPOVR1 Position

Definition at line 7654 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR2_Msk

#define PWM_CAPINTSTS_CAPOVR2_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR2_Pos)

PWM_T::CAPINTSTS: CAPOVR2 Mask

Definition at line 7670 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR2_Pos

#define PWM_CAPINTSTS_CAPOVR2_Pos (19)

PWM_T::CAPINTSTS: CAPOVR2 Position

Definition at line 7669 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR3_Msk

#define PWM_CAPINTSTS_CAPOVR3_Msk (0x1ul << PWM_CAPINTSTS_CAPOVR3_Pos)

PWM_T::CAPINTSTS: CAPOVR3 Mask

Definition at line 7685 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CAPOVR3_Pos

#define PWM_CAPINTSTS_CAPOVR3_Pos (27)

PWM_T::CAPINTSTS: CAPOVR3 Position

Definition at line 7684 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLI1_Msk

#define PWM_CAPINTSTS_CFLI1_Msk (0x1ul << PWM_CAPINTSTS_CFLI1_Pos)

PWM_T::CAPINTSTS: CFLI1 Mask

Definition at line 7652 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLI1_Pos

#define PWM_CAPINTSTS_CFLI1_Pos (10)

PWM_T::CAPINTSTS: CFLI1 Position

Definition at line 7651 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLI2_Msk

#define PWM_CAPINTSTS_CFLI2_Msk (0x1ul << PWM_CAPINTSTS_CFLI2_Pos)

PWM_T::CAPINTSTS: CFLI2 Mask

Definition at line 7667 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLI2_Pos

#define PWM_CAPINTSTS_CFLI2_Pos (18)

PWM_T::CAPINTSTS: CFLI2 Position

Definition at line 7666 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLI3_Msk

#define PWM_CAPINTSTS_CFLI3_Msk (0x1ul << PWM_CAPINTSTS_CFLI3_Pos)

PWM_T::CAPINTSTS: CFLI3 Mask

Definition at line 7682 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLI3_Pos

#define PWM_CAPINTSTS_CFLI3_Pos (26)

PWM_T::CAPINTSTS: CFLI3 Position

Definition at line 7681 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLRI0_Msk

#define PWM_CAPINTSTS_CFLRI0_Msk (0x1ul << PWM_CAPINTSTS_CFLRI0_Pos)

PWM_T::CAPINTSTS: CFLRI0 Mask

Definition at line 7637 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CFLRI0_Pos

#define PWM_CAPINTSTS_CFLRI0_Pos (2)

PWM_T::CAPINTSTS: CFLRI0 Position

Definition at line 7636 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI0_Msk

#define PWM_CAPINTSTS_CRLI0_Msk (0x1ul << PWM_CAPINTSTS_CRLI0_Pos)

PWM_T::CAPINTSTS: CRLI0 Mask

Definition at line 7634 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI0_Pos

#define PWM_CAPINTSTS_CRLI0_Pos (1)

PWM_T::CAPINTSTS: CRLI0 Position

Definition at line 7633 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI1_Msk

#define PWM_CAPINTSTS_CRLI1_Msk (0x1ul << PWM_CAPINTSTS_CRLI1_Pos)

PWM_T::CAPINTSTS: CRLI1 Mask

Definition at line 7649 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI1_Pos

#define PWM_CAPINTSTS_CRLI1_Pos (9)

PWM_T::CAPINTSTS: CRLI1 Position

Definition at line 7648 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI2_Msk

#define PWM_CAPINTSTS_CRLI2_Msk (0x1ul << PWM_CAPINTSTS_CRLI2_Pos)

PWM_T::CAPINTSTS: CRLI2 Mask

Definition at line 7664 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI2_Pos

#define PWM_CAPINTSTS_CRLI2_Pos (17)

PWM_T::CAPINTSTS: CRLI2 Position

Definition at line 7663 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI3_Msk

#define PWM_CAPINTSTS_CRLI3_Msk (0x1ul << PWM_CAPINTSTS_CRLI3_Pos)

PWM_T::CAPINTSTS: CRLI3 Mask

Definition at line 7679 of file Nano100Series.h.

## ◆ PWM_CAPINTSTS_CRLI3_Pos

#define PWM_CAPINTSTS_CRLI3_Pos (25)

PWM_T::CAPINTSTS: CRLI3 Position

Definition at line 7678 of file Nano100Series.h.

## ◆ PWM_CFL0_CFL15_0_Msk

#define PWM_CFL0_CFL15_0_Msk (0xfffful << PWM_CFL0_CFL15_0_Pos)

PWM_T::CFL0: CFL15_0 Mask

Definition at line 7697 of file Nano100Series.h.

## ◆ PWM_CFL0_CFL15_0_Pos

#define PWM_CFL0_CFL15_0_Pos (0)

PWM_T::CFL0: CFL15_0 Position

Definition at line 7696 of file Nano100Series.h.

## ◆ PWM_CFL0_CFL31_16_Msk

#define PWM_CFL0_CFL31_16_Msk (0xfffful << PWM_CFL0_CFL31_16_Pos)

PWM_T::CFL0: CFL31_16 Mask

Definition at line 7700 of file Nano100Series.h.

## ◆ PWM_CFL0_CFL31_16_Pos

#define PWM_CFL0_CFL31_16_Pos (16)

PWM_T::CFL0: CFL31_16 Position

Definition at line 7699 of file Nano100Series.h.

## ◆ PWM_CFL1_CFL15_0_Msk

#define PWM_CFL1_CFL15_0_Msk (0xfffful << PWM_CFL1_CFL15_0_Pos)

PWM_T::CFL1: CFL15_0 Mask

Definition at line 7709 of file Nano100Series.h.

## ◆ PWM_CFL1_CFL15_0_Pos

#define PWM_CFL1_CFL15_0_Pos (0)

PWM_T::CFL1: CFL15_0 Position

Definition at line 7708 of file Nano100Series.h.

## ◆ PWM_CFL1_CFL31_16_Msk

#define PWM_CFL1_CFL31_16_Msk (0xfffful << PWM_CFL1_CFL31_16_Pos)

PWM_T::CFL1: CFL31_16 Mask

Definition at line 7712 of file Nano100Series.h.

## ◆ PWM_CFL1_CFL31_16_Pos

#define PWM_CFL1_CFL31_16_Pos (16)

PWM_T::CFL1: CFL31_16 Position

Definition at line 7711 of file Nano100Series.h.

## ◆ PWM_CFL2_CFL15_0_Msk

#define PWM_CFL2_CFL15_0_Msk (0xfffful << PWM_CFL2_CFL15_0_Pos)

PWM_T::CFL2: CFL15_0 Mask

Definition at line 7721 of file Nano100Series.h.

## ◆ PWM_CFL2_CFL15_0_Pos

#define PWM_CFL2_CFL15_0_Pos (0)

PWM_T::CFL2: CFL15_0 Position

Definition at line 7720 of file Nano100Series.h.

## ◆ PWM_CFL2_CFL31_16_Msk

#define PWM_CFL2_CFL31_16_Msk (0xfffful << PWM_CFL2_CFL31_16_Pos)

PWM_T::CFL2: CFL31_16 Mask

Definition at line 7724 of file Nano100Series.h.

## ◆ PWM_CFL2_CFL31_16_Pos

#define PWM_CFL2_CFL31_16_Pos (16)

PWM_T::CFL2: CFL31_16 Position

Definition at line 7723 of file Nano100Series.h.

## ◆ PWM_CFL3_CFL15_0_Msk

#define PWM_CFL3_CFL15_0_Msk (0xfffful << PWM_CFL3_CFL15_0_Pos)

PWM_T::CFL3: CFL15_0 Mask

Definition at line 7733 of file Nano100Series.h.

## ◆ PWM_CFL3_CFL15_0_Pos

#define PWM_CFL3_CFL15_0_Pos (0)

PWM_T::CFL3: CFL15_0 Position

Definition at line 7732 of file Nano100Series.h.

## ◆ PWM_CFL3_CFL31_16_Msk

#define PWM_CFL3_CFL31_16_Msk (0xfffful << PWM_CFL3_CFL31_16_Pos)

PWM_T::CFL3: CFL31_16 Mask

Definition at line 7736 of file Nano100Series.h.

## ◆ PWM_CFL3_CFL31_16_Pos

#define PWM_CFL3_CFL31_16_Pos (16)

PWM_T::CFL3: CFL31_16 Position

Definition at line 7735 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL0_Msk

#define PWM_CLKSEL_CLKSEL0_Msk (0x7ul << PWM_CLKSEL_CLKSEL0_Pos)

PWM_T::CLKSEL: CLKSEL0 Mask

Definition at line 7367 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL0_Pos

#define PWM_CLKSEL_CLKSEL0_Pos (0)

PWM_T::CLKSEL: CLKSEL0 Position

Definition at line 7366 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL1_Msk

#define PWM_CLKSEL_CLKSEL1_Msk (0x7ul << PWM_CLKSEL_CLKSEL1_Pos)

PWM_T::CLKSEL: CLKSEL1 Mask

Definition at line 7370 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL1_Pos

#define PWM_CLKSEL_CLKSEL1_Pos (4)

PWM_T::CLKSEL: CLKSEL1 Position

Definition at line 7369 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL2_Msk

#define PWM_CLKSEL_CLKSEL2_Msk (0x7ul << PWM_CLKSEL_CLKSEL2_Pos)

PWM_T::CLKSEL: CLKSEL2 Mask

Definition at line 7373 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL2_Pos

#define PWM_CLKSEL_CLKSEL2_Pos (8)

PWM_T::CLKSEL: CLKSEL2 Position

Definition at line 7372 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL3_Msk

#define PWM_CLKSEL_CLKSEL3_Msk (0x7ul << PWM_CLKSEL_CLKSEL3_Pos)

PWM_T::CLKSEL: CLKSEL3 Mask

Definition at line 7376 of file Nano100Series.h.

## ◆ PWM_CLKSEL_CLKSEL3_Pos

#define PWM_CLKSEL_CLKSEL3_Pos (12)

PWM_T::CLKSEL: CLKSEL3 Position

Definition at line 7375 of file Nano100Series.h.

## ◆ PWM_CRL0_CRL15_0_Msk

#define PWM_CRL0_CRL15_0_Msk (0xfffful << PWM_CRL0_CRL15_0_Pos)

PWM_T::CRL0: CRL15_0 Mask

Definition at line 7691 of file Nano100Series.h.

## ◆ PWM_CRL0_CRL15_0_Pos

#define PWM_CRL0_CRL15_0_Pos (0)

PWM_T::CRL0: CRL15_0 Position

Definition at line 7690 of file Nano100Series.h.

## ◆ PWM_CRL0_CRL31_16_Msk

#define PWM_CRL0_CRL31_16_Msk (0xfffful << PWM_CRL0_CRL31_16_Pos)

PWM_T::CRL0: CRL31_16 Mask

Definition at line 7694 of file Nano100Series.h.

## ◆ PWM_CRL0_CRL31_16_Pos

#define PWM_CRL0_CRL31_16_Pos (16)

PWM_T::CRL0: CRL31_16 Position

Definition at line 7693 of file Nano100Series.h.

## ◆ PWM_CRL1_CRL15_0_Msk

#define PWM_CRL1_CRL15_0_Msk (0xfffful << PWM_CRL1_CRL15_0_Pos)

PWM_T::CRL1: CRL15_0 Mask

Definition at line 7703 of file Nano100Series.h.

## ◆ PWM_CRL1_CRL15_0_Pos

#define PWM_CRL1_CRL15_0_Pos (0)

PWM_T::CRL1: CRL15_0 Position

Definition at line 7702 of file Nano100Series.h.

## ◆ PWM_CRL1_CRL31_16_Msk

#define PWM_CRL1_CRL31_16_Msk (0xfffful << PWM_CRL1_CRL31_16_Pos)

PWM_T::CRL1: CRL31_16 Mask

Definition at line 7706 of file Nano100Series.h.

## ◆ PWM_CRL1_CRL31_16_Pos

#define PWM_CRL1_CRL31_16_Pos (16)

PWM_T::CRL1: CRL31_16 Position

Definition at line 7705 of file Nano100Series.h.

## ◆ PWM_CRL2_CRL15_0_Msk

#define PWM_CRL2_CRL15_0_Msk (0xfffful << PWM_CRL2_CRL15_0_Pos)

PWM_T::CRL2: CRL15_0 Mask

Definition at line 7715 of file Nano100Series.h.

## ◆ PWM_CRL2_CRL15_0_Pos

#define PWM_CRL2_CRL15_0_Pos (0)

PWM_T::CRL2: CRL15_0 Position

Definition at line 7714 of file Nano100Series.h.

## ◆ PWM_CRL2_CRL31_16_Msk

#define PWM_CRL2_CRL31_16_Msk (0xfffful << PWM_CRL2_CRL31_16_Pos)

PWM_T::CRL2: CRL31_16 Mask

Definition at line 7718 of file Nano100Series.h.

## ◆ PWM_CRL2_CRL31_16_Pos

#define PWM_CRL2_CRL31_16_Pos (16)

PWM_T::CRL2: CRL31_16 Position

Definition at line 7717 of file Nano100Series.h.

## ◆ PWM_CRL3_CRL15_0_Msk

#define PWM_CRL3_CRL15_0_Msk (0xfffful << PWM_CRL3_CRL15_0_Pos)

PWM_T::CRL3: CRL15_0 Mask

Definition at line 7727 of file Nano100Series.h.

## ◆ PWM_CRL3_CRL15_0_Pos

#define PWM_CRL3_CRL15_0_Pos (0)

PWM_T::CRL3: CRL15_0 Position

Definition at line 7726 of file Nano100Series.h.

## ◆ PWM_CRL3_CRL31_16_Msk

#define PWM_CRL3_CRL31_16_Msk (0xfffful << PWM_CRL3_CRL31_16_Pos)

PWM_T::CRL3: CRL31_16 Mask

Definition at line 7730 of file Nano100Series.h.

## ◆ PWM_CRL3_CRL31_16_Pos

#define PWM_CRL3_CRL31_16_Pos (16)

PWM_T::CRL3: CRL31_16 Position

Definition at line 7729 of file Nano100Series.h.

## ◆ PWM_CTL_CH0EN_Msk

#define PWM_CTL_CH0EN_Msk (0x1ul << PWM_CTL_CH0EN_Pos)

PWM_T::CTL: CH0EN Mask

Definition at line 7379 of file Nano100Series.h.

## ◆ PWM_CTL_CH0EN_Pos

#define PWM_CTL_CH0EN_Pos (0)

PWM_T::CTL: CH0EN Position

Definition at line 7378 of file Nano100Series.h.

## ◆ PWM_CTL_CH0INV_Msk

#define PWM_CTL_CH0INV_Msk (0x1ul << PWM_CTL_CH0INV_Pos)

PWM_T::CTL: CH0INV Mask

Definition at line 7382 of file Nano100Series.h.

## ◆ PWM_CTL_CH0INV_Pos

#define PWM_CTL_CH0INV_Pos (2)

PWM_T::CTL: CH0INV Position

Definition at line 7381 of file Nano100Series.h.

## ◆ PWM_CTL_CH0MOD_Msk

#define PWM_CTL_CH0MOD_Msk (0x1ul << PWM_CTL_CH0MOD_Pos)

PWM_T::CTL: CH0MOD Mask

Definition at line 7385 of file Nano100Series.h.

## ◆ PWM_CTL_CH0MOD_Pos

#define PWM_CTL_CH0MOD_Pos (3)

PWM_T::CTL: CH0MOD Position

Definition at line 7384 of file Nano100Series.h.

## ◆ PWM_CTL_CH1EN_Msk

#define PWM_CTL_CH1EN_Msk (0x1ul << PWM_CTL_CH1EN_Pos)

PWM_T::CTL: CH1EN Mask

Definition at line 7394 of file Nano100Series.h.

## ◆ PWM_CTL_CH1EN_Pos

#define PWM_CTL_CH1EN_Pos (8)

PWM_T::CTL: CH1EN Position

Definition at line 7393 of file Nano100Series.h.

## ◆ PWM_CTL_CH1INV_Msk

#define PWM_CTL_CH1INV_Msk (0x1ul << PWM_CTL_CH1INV_Pos)

PWM_T::CTL: CH1INV Mask

Definition at line 7397 of file Nano100Series.h.

## ◆ PWM_CTL_CH1INV_Pos

#define PWM_CTL_CH1INV_Pos (10)

PWM_T::CTL: CH1INV Position

Definition at line 7396 of file Nano100Series.h.

## ◆ PWM_CTL_CH1MOD_Msk

#define PWM_CTL_CH1MOD_Msk (0x1ul << PWM_CTL_CH1MOD_Pos)

PWM_T::CTL: CH1MOD Mask

Definition at line 7400 of file Nano100Series.h.

## ◆ PWM_CTL_CH1MOD_Pos

#define PWM_CTL_CH1MOD_Pos (11)

PWM_T::CTL: CH1MOD Position

Definition at line 7399 of file Nano100Series.h.

## ◆ PWM_CTL_CH2EN_Msk

#define PWM_CTL_CH2EN_Msk (0x1ul << PWM_CTL_CH2EN_Pos)

PWM_T::CTL: CH2EN Mask

Definition at line 7403 of file Nano100Series.h.

## ◆ PWM_CTL_CH2EN_Pos

#define PWM_CTL_CH2EN_Pos (16)

PWM_T::CTL: CH2EN Position

Definition at line 7402 of file Nano100Series.h.

## ◆ PWM_CTL_CH2INV_Msk

#define PWM_CTL_CH2INV_Msk (0x1ul << PWM_CTL_CH2INV_Pos)

PWM_T::CTL: CH2INV Mask

Definition at line 7406 of file Nano100Series.h.

## ◆ PWM_CTL_CH2INV_Pos

#define PWM_CTL_CH2INV_Pos (18)

PWM_T::CTL: CH2INV Position

Definition at line 7405 of file Nano100Series.h.

## ◆ PWM_CTL_CH2MOD_Msk

#define PWM_CTL_CH2MOD_Msk (0x1ul << PWM_CTL_CH2MOD_Pos)

PWM_T::CTL: CH2MOD Mask

Definition at line 7409 of file Nano100Series.h.

## ◆ PWM_CTL_CH2MOD_Pos

#define PWM_CTL_CH2MOD_Pos (19)

PWM_T::CTL: CH2MOD Position

Definition at line 7408 of file Nano100Series.h.

## ◆ PWM_CTL_CH3EN_Msk

#define PWM_CTL_CH3EN_Msk (0x1ul << PWM_CTL_CH3EN_Pos)

PWM_T::CTL: CH3EN Mask

Definition at line 7412 of file Nano100Series.h.

## ◆ PWM_CTL_CH3EN_Pos

#define PWM_CTL_CH3EN_Pos (24)

PWM_T::CTL: CH3EN Position

Definition at line 7411 of file Nano100Series.h.

## ◆ PWM_CTL_CH3INV_Msk

#define PWM_CTL_CH3INV_Msk (0x1ul << PWM_CTL_CH3INV_Pos)

PWM_T::CTL: CH3INV Mask

Definition at line 7415 of file Nano100Series.h.

## ◆ PWM_CTL_CH3INV_Pos

#define PWM_CTL_CH3INV_Pos (26)

PWM_T::CTL: CH3INV Position

Definition at line 7414 of file Nano100Series.h.

## ◆ PWM_CTL_CH3MOD_Msk

#define PWM_CTL_CH3MOD_Msk (0x1ul << PWM_CTL_CH3MOD_Pos)

PWM_T::CTL: CH3MOD Mask

Definition at line 7418 of file Nano100Series.h.

## ◆ PWM_CTL_CH3MOD_Pos

#define PWM_CTL_CH3MOD_Pos (27)

PWM_T::CTL: CH3MOD Position

Definition at line 7417 of file Nano100Series.h.

## ◆ PWM_CTL_DZEN01_Msk

#define PWM_CTL_DZEN01_Msk (0x1ul << PWM_CTL_DZEN01_Pos)

PWM_T::CTL: DZEN01 Mask

Definition at line 7388 of file Nano100Series.h.

## ◆ PWM_CTL_DZEN01_Pos

#define PWM_CTL_DZEN01_Pos (4)

PWM_T::CTL: DZEN01 Position

Definition at line 7387 of file Nano100Series.h.

## ◆ PWM_CTL_DZEN23_Msk

#define PWM_CTL_DZEN23_Msk (0x1ul << PWM_CTL_DZEN23_Pos)

PWM_T::CTL: DZEN23 Mask

Definition at line 7391 of file Nano100Series.h.

## ◆ PWM_CTL_DZEN23_Pos

#define PWM_CTL_DZEN23_Pos (5)

PWM_T::CTL: DZEN23 Position

Definition at line 7390 of file Nano100Series.h.

## ◆ PWM_DATA0_PWMx_DATAy15_0_Msk

#define PWM_DATA0_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA0_PWMx_DATAy15_0_Pos)

PWM_T::DATA0: PWMx_DATAy15_0 Mask

Definition at line 7469 of file Nano100Series.h.

## ◆ PWM_DATA0_PWMx_DATAy15_0_Pos

#define PWM_DATA0_PWMx_DATAy15_0_Pos (0)

PWM_T::DATA0: PWMx_DATAy15_0 Position

Definition at line 7468 of file Nano100Series.h.

## ◆ PWM_DATA0_PWMx_DATAy30_16_Msk

#define PWM_DATA0_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA0_PWMx_DATAy30_16_Pos)

PWM_T::DATA0: PWMx_DATAy30_16 Mask

Definition at line 7472 of file Nano100Series.h.

## ◆ PWM_DATA0_PWMx_DATAy30_16_Pos

#define PWM_DATA0_PWMx_DATAy30_16_Pos (16)

PWM_T::DATA0: PWMx_DATAy30_16 Position

Definition at line 7471 of file Nano100Series.h.

## ◆ PWM_DATA0_sync_Msk

#define PWM_DATA0_sync_Msk (0x1ul << PWM_DATA0_sync_Pos)

PWM_T::DATA0: sync Mask

Definition at line 7475 of file Nano100Series.h.

## ◆ PWM_DATA0_sync_Pos

#define PWM_DATA0_sync_Pos (31)

PWM_T::DATA0: sync Position

Definition at line 7474 of file Nano100Series.h.

## ◆ PWM_DATA1_PWMx_DATAy15_0_Msk

#define PWM_DATA1_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA1_PWMx_DATAy15_0_Pos)

PWM_T::DATA1: PWMx_DATAy15_0 Mask

Definition at line 7484 of file Nano100Series.h.

## ◆ PWM_DATA1_PWMx_DATAy15_0_Pos

#define PWM_DATA1_PWMx_DATAy15_0_Pos (0)

PWM_T::DATA1: PWMx_DATAy15_0 Position

Definition at line 7483 of file Nano100Series.h.

## ◆ PWM_DATA1_PWMx_DATAy30_16_Msk

#define PWM_DATA1_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA1_PWMx_DATAy30_16_Pos)

PWM_T::DATA1: PWMx_DATAy30_16 Mask

Definition at line 7487 of file Nano100Series.h.

## ◆ PWM_DATA1_PWMx_DATAy30_16_Pos

#define PWM_DATA1_PWMx_DATAy30_16_Pos (16)

PWM_T::DATA1: PWMx_DATAy30_16 Position

Definition at line 7486 of file Nano100Series.h.

## ◆ PWM_DATA1_sync_Msk

#define PWM_DATA1_sync_Msk (0x1ul << PWM_DATA1_sync_Pos)

PWM_T::DATA1: sync Mask

Definition at line 7490 of file Nano100Series.h.

## ◆ PWM_DATA1_sync_Pos

#define PWM_DATA1_sync_Pos (31)

PWM_T::DATA1: sync Position

Definition at line 7489 of file Nano100Series.h.

## ◆ PWM_DATA2_PWMx_DATAy15_0_Msk

#define PWM_DATA2_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA2_PWMx_DATAy15_0_Pos)

PWM_T::DATA2: PWMx_DATAy15_0 Mask

Definition at line 7499 of file Nano100Series.h.

## ◆ PWM_DATA2_PWMx_DATAy15_0_Pos

#define PWM_DATA2_PWMx_DATAy15_0_Pos (0)

PWM_T::DATA2: PWMx_DATAy15_0 Position

Definition at line 7498 of file Nano100Series.h.

## ◆ PWM_DATA2_PWMx_DATAy30_16_Msk

#define PWM_DATA2_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA2_PWMx_DATAy30_16_Pos)

PWM_T::DATA2: PWMx_DATAy30_16 Mask

Definition at line 7502 of file Nano100Series.h.

## ◆ PWM_DATA2_PWMx_DATAy30_16_Pos

#define PWM_DATA2_PWMx_DATAy30_16_Pos (16)

PWM_T::DATA2: PWMx_DATAy30_16 Position

Definition at line 7501 of file Nano100Series.h.

## ◆ PWM_DATA2_sync_Msk

#define PWM_DATA2_sync_Msk (0x1ul << PWM_DATA2_sync_Pos)

PWM_T::DATA2: sync Mask

Definition at line 7505 of file Nano100Series.h.

## ◆ PWM_DATA2_sync_Pos

#define PWM_DATA2_sync_Pos (31)

PWM_T::DATA2: sync Position

Definition at line 7504 of file Nano100Series.h.

## ◆ PWM_DATA3_PWMx_DATAy15_0_Msk

#define PWM_DATA3_PWMx_DATAy15_0_Msk (0xfffful << PWM_DATA3_PWMx_DATAy15_0_Pos)

PWM_T::DATA3: PWMx_DATAy15_0 Mask

Definition at line 7514 of file Nano100Series.h.

## ◆ PWM_DATA3_PWMx_DATAy15_0_Pos

#define PWM_DATA3_PWMx_DATAy15_0_Pos (0)

PWM_T::DATA3: PWMx_DATAy15_0 Position

Definition at line 7513 of file Nano100Series.h.

## ◆ PWM_DATA3_PWMx_DATAy30_16_Msk

#define PWM_DATA3_PWMx_DATAy30_16_Msk (0x7ffful << PWM_DATA3_PWMx_DATAy30_16_Pos)

PWM_T::DATA3: PWMx_DATAy30_16 Mask

Definition at line 7517 of file Nano100Series.h.

## ◆ PWM_DATA3_PWMx_DATAy30_16_Pos

#define PWM_DATA3_PWMx_DATAy30_16_Pos (16)

PWM_T::DATA3: PWMx_DATAy30_16 Position

Definition at line 7516 of file Nano100Series.h.

## ◆ PWM_DATA3_sync_Msk

#define PWM_DATA3_sync_Msk (0x1ul << PWM_DATA3_sync_Pos)

PWM_T::DATA3: sync Mask

Definition at line 7520 of file Nano100Series.h.

## ◆ PWM_DATA3_sync_Pos

#define PWM_DATA3_sync_Pos (31)

PWM_T::DATA3: sync Position

Definition at line 7519 of file Nano100Series.h.

## ◆ PWM_DUTY1_CM_Msk

#define PWM_DUTY1_CM_Msk (0xfffful << PWM_DUTY1_CM_Pos)

PWM_T::DUTY1: CM Mask

Definition at line 7481 of file Nano100Series.h.

## ◆ PWM_DUTY1_CM_Pos

#define PWM_DUTY1_CM_Pos (16)

PWM_T::DUTY1: CM Position

Definition at line 7480 of file Nano100Series.h.

## ◆ PWM_DUTY1_CN_Msk

#define PWM_DUTY1_CN_Msk (0xfffful << PWM_DUTY1_CN_Pos)

PWM_T::DUTY1: CN Mask

Definition at line 7478 of file Nano100Series.h.

## ◆ PWM_DUTY1_CN_Pos

#define PWM_DUTY1_CN_Pos (0)

PWM_T::DUTY1: CN Position

Definition at line 7477 of file Nano100Series.h.

## ◆ PWM_DUTY2_CM_Msk

#define PWM_DUTY2_CM_Msk (0xfffful << PWM_DUTY2_CM_Pos)

PWM_T::DUTY2: CM Mask

Definition at line 7496 of file Nano100Series.h.

## ◆ PWM_DUTY2_CM_Pos

#define PWM_DUTY2_CM_Pos (16)

PWM_T::DUTY2: CM Position

Definition at line 7495 of file Nano100Series.h.

## ◆ PWM_DUTY2_CN_Msk

#define PWM_DUTY2_CN_Msk (0xfffful << PWM_DUTY2_CN_Pos)

PWM_T::DUTY2: CN Mask

Definition at line 7493 of file Nano100Series.h.

## ◆ PWM_DUTY2_CN_Pos

#define PWM_DUTY2_CN_Pos (0)

PWM_T::DUTY2: CN Position

Definition at line 7492 of file Nano100Series.h.

## ◆ PWM_DUTY3_CM_Msk

#define PWM_DUTY3_CM_Msk (0xfffful << PWM_DUTY3_CM_Pos)

PWM_T::DUTY3: CM Mask

Definition at line 7511 of file Nano100Series.h.

## ◆ PWM_DUTY3_CM_Pos

#define PWM_DUTY3_CM_Pos (16)

PWM_T::DUTY3: CM Position

Definition at line 7510 of file Nano100Series.h.

## ◆ PWM_DUTY3_CN_Msk

#define PWM_DUTY3_CN_Msk (0xfffful << PWM_DUTY3_CN_Pos)

PWM_T::DUTY3: CN Mask

Definition at line 7508 of file Nano100Series.h.

## ◆ PWM_DUTY3_CN_Pos

#define PWM_DUTY3_CN_Pos (0)

PWM_T::DUTY3: CN Position

Definition at line 7507 of file Nano100Series.h.

## ◆ PWM_DUTY_CM_Msk

#define PWM_DUTY_CM_Msk (0xfffful << PWM_DUTY_CM_Pos)

PWM_T::DUTY0: CM Mask

Definition at line 7466 of file Nano100Series.h.

## ◆ PWM_DUTY_CM_Pos

#define PWM_DUTY_CM_Pos (16)

PWM_T::DUTY0: CM Position

Definition at line 7465 of file Nano100Series.h.

## ◆ PWM_DUTY_CN_Msk

#define PWM_DUTY_CN_Msk (0xfffful << PWM_DUTY_CN_Pos)

PWM_T::DUTY0: CN Mask

Definition at line 7463 of file Nano100Series.h.

## ◆ PWM_DUTY_CN_Pos

#define PWM_DUTY_CN_Pos (0)

PWM_T::DUTY0: CN Position

Definition at line 7462 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE0_Msk

#define PWM_INTEN_TMIE0_Msk (0x1ul << PWM_INTEN_TMIE0_Pos)

PWM_T::INTEN: TMIE0 Mask

Definition at line 7421 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE0_Pos

#define PWM_INTEN_TMIE0_Pos (0)

PWM_T::INTEN: TMIE0 Position

Definition at line 7420 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE1_Msk

#define PWM_INTEN_TMIE1_Msk (0x1ul << PWM_INTEN_TMIE1_Pos)

PWM_T::INTEN: TMIE1 Mask

Definition at line 7424 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE1_Pos

#define PWM_INTEN_TMIE1_Pos (1)

PWM_T::INTEN: TMIE1 Position

Definition at line 7423 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE2_Msk

#define PWM_INTEN_TMIE2_Msk (0x1ul << PWM_INTEN_TMIE2_Pos)

PWM_T::INTEN: TMIE2 Mask

Definition at line 7427 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE2_Pos

#define PWM_INTEN_TMIE2_Pos (2)

PWM_T::INTEN: TMIE2 Position

Definition at line 7426 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE3_Msk

#define PWM_INTEN_TMIE3_Msk (0x1ul << PWM_INTEN_TMIE3_Pos)

PWM_T::INTEN: TMIE3 Mask

Definition at line 7430 of file Nano100Series.h.

## ◆ PWM_INTEN_TMIE3_Pos

#define PWM_INTEN_TMIE3_Pos (3)

PWM_T::INTEN: TMIE3 Position

Definition at line 7429 of file Nano100Series.h.

## ◆ PWM_INTSTS_DUTY0SYNC_Msk

#define PWM_INTSTS_DUTY0SYNC_Msk (0x1ul << PWM_INTSTS_DUTY0SYNC_Pos)

PWM_T::INTSTS: DUTY0SYNC Mask

Definition at line 7445 of file Nano100Series.h.

## ◆ PWM_INTSTS_DUTY0SYNC_Pos

#define PWM_INTSTS_DUTY0SYNC_Pos (4)

PWM_T::INTSTS: DUTY0SYNC Position

Definition at line 7444 of file Nano100Series.h.

## ◆ PWM_INTSTS_PRESSYNC_Msk

#define PWM_INTSTS_PRESSYNC_Msk (0x1ul << PWM_INTSTS_PRESSYNC_Pos)

PWM_T::INTSTS: PRESSYNC Mask

Definition at line 7448 of file Nano100Series.h.

## ◆ PWM_INTSTS_PRESSYNC_Pos

#define PWM_INTSTS_PRESSYNC_Pos (8)

PWM_T::INTSTS: PRESSYNC Position

Definition at line 7447 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT0_Msk

#define PWM_INTSTS_TMINT0_Msk (0x1ul << PWM_INTSTS_TMINT0_Pos)

PWM_T::INTSTS: TMINT0 Mask

Definition at line 7433 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT0_Pos

#define PWM_INTSTS_TMINT0_Pos (0)

PWM_T::INTSTS: TMINT0 Position

Definition at line 7432 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT1_Msk

#define PWM_INTSTS_TMINT1_Msk (0x1ul << PWM_INTSTS_TMINT1_Pos)

PWM_T::INTSTS: TMINT1 Mask

Definition at line 7436 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT1_Pos

#define PWM_INTSTS_TMINT1_Pos (1)

PWM_T::INTSTS: TMINT1 Position

Definition at line 7435 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT2_Msk

#define PWM_INTSTS_TMINT2_Msk (0x1ul << PWM_INTSTS_TMINT2_Pos)

PWM_T::INTSTS: TMINT2 Mask

Definition at line 7439 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT2_Pos

#define PWM_INTSTS_TMINT2_Pos (2)

PWM_T::INTSTS: TMINT2 Position

Definition at line 7438 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT3_Msk

#define PWM_INTSTS_TMINT3_Msk (0x1ul << PWM_INTSTS_TMINT3_Pos)

PWM_T::INTSTS: TMINT3 Mask

Definition at line 7442 of file Nano100Series.h.

## ◆ PWM_INTSTS_TMINT3_Pos

#define PWM_INTSTS_TMINT3_Pos (3)

PWM_T::INTSTS: TMINT3 Position

Definition at line 7441 of file Nano100Series.h.

## ◆ PWM_OE_CH0_OE_Msk

#define PWM_OE_CH0_OE_Msk (0x1ul << PWM_OE_CH0_OE_Pos)

PWM_T::OE: CH0_OE Mask

Definition at line 7451 of file Nano100Series.h.

## ◆ PWM_OE_CH0_OE_Pos

#define PWM_OE_CH0_OE_Pos (0)

PWM_T::OE: CH0_OE Position

Definition at line 7450 of file Nano100Series.h.

## ◆ PWM_OE_CH1_OE_Msk

#define PWM_OE_CH1_OE_Msk (0x1ul << PWM_OE_CH1_OE_Pos)

PWM_T::OE: CH1_OE Mask

Definition at line 7454 of file Nano100Series.h.

## ◆ PWM_OE_CH1_OE_Pos

#define PWM_OE_CH1_OE_Pos (1)

PWM_T::OE: CH1_OE Position

Definition at line 7453 of file Nano100Series.h.

## ◆ PWM_OE_CH2_OE_Msk

#define PWM_OE_CH2_OE_Msk (0x1ul << PWM_OE_CH2_OE_Pos)

PWM_T::OE: CH2_OE Mask

Definition at line 7457 of file Nano100Series.h.

## ◆ PWM_OE_CH2_OE_Pos

#define PWM_OE_CH2_OE_Pos (2)

PWM_T::OE: CH2_OE Position

Definition at line 7456 of file Nano100Series.h.

## ◆ PWM_OE_CH3_OE_Msk

#define PWM_OE_CH3_OE_Msk (0x1ul << PWM_OE_CH3_OE_Pos)

PWM_T::OE: CH3_OE Mask

Definition at line 7460 of file Nano100Series.h.

## ◆ PWM_OE_CH3_OE_Pos

#define PWM_OE_CH3_OE_Pos (3)

PWM_T::OE: CH3_OE Position

Definition at line 7459 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata15_8_Msk

#define PWM_PDMACH0_Captureddata15_8_Msk (0xfful << PWM_PDMACH0_Captureddata15_8_Pos)

PWM_T::PDMACH0: Captureddata15_8 Mask

Definition at line 7742 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata15_8_Pos

#define PWM_PDMACH0_Captureddata15_8_Pos (8)

PWM_T::PDMACH0: Captureddata15_8 Position

Definition at line 7741 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata23_16_Msk

#define PWM_PDMACH0_Captureddata23_16_Msk (0xfful << PWM_PDMACH0_Captureddata23_16_Pos)

PWM_T::PDMACH0: Captureddata23_16 Mask

Definition at line 7745 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata23_16_Pos

#define PWM_PDMACH0_Captureddata23_16_Pos (16)

PWM_T::PDMACH0: Captureddata23_16 Position

Definition at line 7744 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata31_24_Msk

#define PWM_PDMACH0_Captureddata31_24_Msk (0xfful << PWM_PDMACH0_Captureddata31_24_Pos)

PWM_T::PDMACH0: Captureddata31_24 Mask

Definition at line 7748 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata31_24_Pos

#define PWM_PDMACH0_Captureddata31_24_Pos (24)

PWM_T::PDMACH0: Captureddata31_24 Position

Definition at line 7747 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata7_0_Msk

#define PWM_PDMACH0_Captureddata7_0_Msk (0xfful << PWM_PDMACH0_Captureddata7_0_Pos)

PWM_T::PDMACH0: Captureddata7_0 Mask

Definition at line 7739 of file Nano100Series.h.

## ◆ PWM_PDMACH0_Captureddata7_0_Pos

#define PWM_PDMACH0_Captureddata7_0_Pos (0)

PWM_T::PDMACH0: Captureddata7_0 Position

Definition at line 7738 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata15_8_Msk

#define PWM_PDMACH2_Captureddata15_8_Msk (0xfful << PWM_PDMACH2_Captureddata15_8_Pos)

PWM_T::PDMACH2: Captureddata15_8 Mask

Definition at line 7754 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata15_8_Pos

#define PWM_PDMACH2_Captureddata15_8_Pos (8)

PWM_T::PDMACH2: Captureddata15_8 Position

Definition at line 7753 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata23_16_Msk

#define PWM_PDMACH2_Captureddata23_16_Msk (0xfful << PWM_PDMACH2_Captureddata23_16_Pos)

PWM_T::PDMACH2: Captureddata23_16 Mask

Definition at line 7757 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata23_16_Pos

#define PWM_PDMACH2_Captureddata23_16_Pos (16)

PWM_T::PDMACH2: Captureddata23_16 Position

Definition at line 7756 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata31_24_Msk

#define PWM_PDMACH2_Captureddata31_24_Msk (0xfful << PWM_PDMACH2_Captureddata31_24_Pos)

PWM_T::PDMACH2: Captureddata31_24 Mask

Definition at line 7760 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata31_24_Pos

#define PWM_PDMACH2_Captureddata31_24_Pos (24)

PWM_T::PDMACH2: Captureddata31_24 Position

Definition at line 7759 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata7_0_Msk

#define PWM_PDMACH2_Captureddata7_0_Msk (0xfful << PWM_PDMACH2_Captureddata7_0_Pos)

PWM_T::PDMACH2: Captureddata7_0 Mask

Definition at line 7751 of file Nano100Series.h.

## ◆ PWM_PDMACH2_Captureddata7_0_Pos

#define PWM_PDMACH2_Captureddata7_0_Pos (0)

PWM_T::PDMACH2: Captureddata7_0 Position

Definition at line 7750 of file Nano100Series.h.

## ◆ PWM_PRES_CP01_Msk

#define PWM_PRES_CP01_Msk (0xfful << PWM_PRES_CP01_Pos)

PWM_T::PRES: CP01 Mask

Definition at line 7355 of file Nano100Series.h.

## ◆ PWM_PRES_CP01_Pos

#define PWM_PRES_CP01_Pos (0)

    @addtogroup PWM_CONST PWM Bit Field Definition
    Constant Definitions for PWM Controller

PWM_T::PRES: CP01 Position

Definition at line 7354 of file Nano100Series.h.

## ◆ PWM_PRES_CP23_Msk

#define PWM_PRES_CP23_Msk (0xfful << PWM_PRES_CP23_Pos)

PWM_T::PRES: CP23 Mask

Definition at line 7358 of file Nano100Series.h.

## ◆ PWM_PRES_CP23_Pos

#define PWM_PRES_CP23_Pos (8)

PWM_T::PRES: CP23 Position

Definition at line 7357 of file Nano100Series.h.

## ◆ PWM_PRES_DZ01_Msk

#define PWM_PRES_DZ01_Msk (0xfful << PWM_PRES_DZ01_Pos)

PWM_T::PRES: DZ01 Mask

Definition at line 7361 of file Nano100Series.h.

## ◆ PWM_PRES_DZ01_Pos

#define PWM_PRES_DZ01_Pos (16)

PWM_T::PRES: DZ01 Position

Definition at line 7360 of file Nano100Series.h.

## ◆ PWM_PRES_DZ23_Msk

#define PWM_PRES_DZ23_Msk (0xfful << PWM_PRES_DZ23_Pos)

PWM_T::PRES: DZ23 Mask

Definition at line 7364 of file Nano100Series.h.

## ◆ PWM_PRES_DZ23_Pos

#define PWM_PRES_DZ23_Pos (24)

PWM_T::PRES: DZ23 Position

Definition at line 7363 of file Nano100Series.h.

## ◆ RTC_AER_AER_Msk

#define RTC_AER_AER_Msk (0xfffful << RTC_AER_AER_Pos)

RTC_T::AER: AER Mask

Definition at line 8078 of file Nano100Series.h.

## ◆ RTC_AER_AER_Pos

#define RTC_AER_AER_Pos (0)

RTC_T::AER: AER Position

Definition at line 8077 of file Nano100Series.h.

## ◆ RTC_AER_ENF_Msk

#define RTC_AER_ENF_Msk (0x1ul << RTC_AER_ENF_Pos)

RTC_T::AER: ENF Mask

Definition at line 8081 of file Nano100Series.h.

## ◆ RTC_AER_ENF_Pos

#define RTC_AER_ENF_Pos (16)

RTC_T::AER: ENF Position

Definition at line 8080 of file Nano100Series.h.

## ◆ RTC_CAR_10DAY_Msk

#define RTC_CAR_10DAY_Msk (0x3ul << RTC_CAR_10DAY_Pos)

RTC_T::CAR: 10DAY Mask

Definition at line 8153 of file Nano100Series.h.

## ◆ RTC_CAR_10DAY_Pos

#define RTC_CAR_10DAY_Pos (4)

RTC_T::CAR: 10DAY Position

Definition at line 8152 of file Nano100Series.h.

## ◆ RTC_CAR_10MON_Msk

#define RTC_CAR_10MON_Msk (0x1ul << RTC_CAR_10MON_Pos)

RTC_T::CAR: 10MON Mask

Definition at line 8159 of file Nano100Series.h.

## ◆ RTC_CAR_10MON_Pos

#define RTC_CAR_10MON_Pos (12)

RTC_T::CAR: 10MON Position

Definition at line 8158 of file Nano100Series.h.

## ◆ RTC_CAR_10YEAR_Msk

#define RTC_CAR_10YEAR_Msk (0xful << RTC_CAR_10YEAR_Pos)

RTC_T::CAR: 10YEAR Mask

Definition at line 8165 of file Nano100Series.h.

## ◆ RTC_CAR_10YEAR_Pos

#define RTC_CAR_10YEAR_Pos (20)

RTC_T::CAR: 10YEAR Position

Definition at line 8164 of file Nano100Series.h.

## ◆ RTC_CAR_1DAY_Msk

#define RTC_CAR_1DAY_Msk (0xful << RTC_CAR_1DAY_Pos)

RTC_T::CAR: 1DAY Mask

Definition at line 8150 of file Nano100Series.h.

## ◆ RTC_CAR_1DAY_Pos

#define RTC_CAR_1DAY_Pos (0)

RTC_T::CAR: 1DAY Position

Definition at line 8149 of file Nano100Series.h.

## ◆ RTC_CAR_1MON_Msk

#define RTC_CAR_1MON_Msk (0xful << RTC_CAR_1MON_Pos)

RTC_T::CAR: 1MON Mask

Definition at line 8156 of file Nano100Series.h.

## ◆ RTC_CAR_1MON_Pos

#define RTC_CAR_1MON_Pos (8)

RTC_T::CAR: 1MON Position

Definition at line 8155 of file Nano100Series.h.

## ◆ RTC_CAR_1YEAR_Msk

#define RTC_CAR_1YEAR_Msk (0xful << RTC_CAR_1YEAR_Pos)

RTC_T::CAR: 1YEAR Mask

Definition at line 8162 of file Nano100Series.h.

## ◆ RTC_CAR_1YEAR_Pos

#define RTC_CAR_1YEAR_Pos (16)

RTC_T::CAR: 1YEAR Position

Definition at line 8161 of file Nano100Series.h.

## ◆ RTC_CLR_10DAY_Msk

#define RTC_CLR_10DAY_Msk (0x3ul << RTC_CLR_10DAY_Pos)

RTC_T::CLR: 10DAY Mask

Definition at line 8111 of file Nano100Series.h.

## ◆ RTC_CLR_10DAY_Pos

#define RTC_CLR_10DAY_Pos (4)

RTC_T::CLR: 10DAY Position

Definition at line 8110 of file Nano100Series.h.

## ◆ RTC_CLR_10MON_Msk

#define RTC_CLR_10MON_Msk (0x1ul << RTC_CLR_10MON_Pos)

RTC_T::CLR: 10MON Mask

Definition at line 8117 of file Nano100Series.h.

## ◆ RTC_CLR_10MON_Pos

#define RTC_CLR_10MON_Pos (12)

RTC_T::CLR: 10MON Position

Definition at line 8116 of file Nano100Series.h.

## ◆ RTC_CLR_10YEAR_Msk

#define RTC_CLR_10YEAR_Msk (0xful << RTC_CLR_10YEAR_Pos)

RTC_T::CLR: 10YEAR Mask

Definition at line 8123 of file Nano100Series.h.

## ◆ RTC_CLR_10YEAR_Pos

#define RTC_CLR_10YEAR_Pos (20)

RTC_T::CLR: 10YEAR Position

Definition at line 8122 of file Nano100Series.h.

## ◆ RTC_CLR_1DAY_Msk

#define RTC_CLR_1DAY_Msk (0xful << RTC_CLR_1DAY_Pos)

RTC_T::CLR: 1DAY Mask

Definition at line 8108 of file Nano100Series.h.

## ◆ RTC_CLR_1DAY_Pos

#define RTC_CLR_1DAY_Pos (0)

RTC_T::CLR: 1DAY Position

Definition at line 8107 of file Nano100Series.h.

## ◆ RTC_CLR_1MON_Msk

#define RTC_CLR_1MON_Msk (0xful << RTC_CLR_1MON_Pos)

RTC_T::CLR: 1MON Mask

Definition at line 8114 of file Nano100Series.h.

## ◆ RTC_CLR_1MON_Pos

#define RTC_CLR_1MON_Pos (8)

RTC_T::CLR: 1MON Position

Definition at line 8113 of file Nano100Series.h.

## ◆ RTC_CLR_1YEAR_Msk

#define RTC_CLR_1YEAR_Msk (0xful << RTC_CLR_1YEAR_Pos)

RTC_T::CLR: 1YEAR Mask

Definition at line 8120 of file Nano100Series.h.

## ◆ RTC_CLR_1YEAR_Pos

#define RTC_CLR_1YEAR_Pos (16)

RTC_T::CLR: 1YEAR Position

Definition at line 8119 of file Nano100Series.h.

## ◆ RTC_DWR_DWR_Msk

#define RTC_DWR_DWR_Msk (0x7ul << RTC_DWR_DWR_Pos)

RTC_T::DWR: DWR Mask

Definition at line 8129 of file Nano100Series.h.

## ◆ RTC_DWR_DWR_Pos

#define RTC_DWR_DWR_Pos (0)

RTC_T::DWR: DWR Position

Definition at line 8128 of file Nano100Series.h.

## ◆ RTC_FCR_FRACTION_Msk

#define RTC_FCR_FRACTION_Msk (0x3ful << RTC_FCR_FRACTION_Pos)

RTC_T::FCR: FRACTION Mask

Definition at line 8084 of file Nano100Series.h.

## ◆ RTC_FCR_FRACTION_Pos

#define RTC_FCR_FRACTION_Pos (0)

RTC_T::FCR: FRACTION Position

Definition at line 8083 of file Nano100Series.h.

## ◆ RTC_FCR_INTEGER_Msk

#define RTC_FCR_INTEGER_Msk (0xful << RTC_FCR_INTEGER_Pos)

RTC_T::FCR: INTEGER Mask

Definition at line 8087 of file Nano100Series.h.

## ◆ RTC_FCR_INTEGER_Pos

#define RTC_FCR_INTEGER_Pos (8)

RTC_T::FCR: INTEGER Position

Definition at line 8086 of file Nano100Series.h.

## ◆ RTC_INIR_ACTIVE_Msk

#define RTC_INIR_ACTIVE_Msk (0x1ul << RTC_INIR_ACTIVE_Pos)

RTC_T::INIR: ACTIVE Mask

Definition at line 8072 of file Nano100Series.h.

## ◆ RTC_INIR_ACTIVE_Pos

#define RTC_INIR_ACTIVE_Pos (0)

    @addtogroup RTC_CONST RTC Bit Field Definition
    Constant Definitions for RTC Controller

RTC_T::INIR: ACTIVE Position

Definition at line 8071 of file Nano100Series.h.

## ◆ RTC_INIR_INIR_Msk

#define RTC_INIR_INIR_Msk (0xfffffffful << RTC_INIR_INIR_Pos)

RTC_T::INIR: INIR Mask

Definition at line 8075 of file Nano100Series.h.

## ◆ RTC_INIR_INIR_Pos

#define RTC_INIR_INIR_Pos (0)

RTC_T::INIR: INIR Position

Definition at line 8074 of file Nano100Series.h.

## ◆ RTC_LIR_LIR_Msk

#define RTC_LIR_LIR_Msk (0x1ul << RTC_LIR_LIR_Pos)

RTC_T::LIR: LIR Mask

Definition at line 8168 of file Nano100Series.h.

## ◆ RTC_LIR_LIR_Pos

#define RTC_LIR_LIR_Pos (0)

RTC_T::LIR: LIR Position

Definition at line 8167 of file Nano100Series.h.

## ◆ RTC_RIER_AIER_Msk

#define RTC_RIER_AIER_Msk (0x1ul << RTC_RIER_AIER_Pos)

RTC_T::RIER: AIER Mask

Definition at line 8171 of file Nano100Series.h.

## ◆ RTC_RIER_AIER_Pos

#define RTC_RIER_AIER_Pos (0)

RTC_T::RIER: AIER Position

Definition at line 8170 of file Nano100Series.h.

## ◆ RTC_RIER_SNOOPIER_Msk

#define RTC_RIER_SNOOPIER_Msk (0x1ul << RTC_RIER_SNOOPIER_Pos)

RTC_T::RIER: SNOOPIER Mask

Definition at line 8177 of file Nano100Series.h.

## ◆ RTC_RIER_SNOOPIER_Pos

#define RTC_RIER_SNOOPIER_Pos (2)

RTC_T::RIER: SNOOPIER Position

Definition at line 8176 of file Nano100Series.h.

## ◆ RTC_RIER_TIER_Msk

#define RTC_RIER_TIER_Msk (0x1ul << RTC_RIER_TIER_Pos)

RTC_T::RIER: TIER Mask

Definition at line 8174 of file Nano100Series.h.

## ◆ RTC_RIER_TIER_Pos

#define RTC_RIER_TIER_Pos (1)

RTC_T::RIER: TIER Position

Definition at line 8173 of file Nano100Series.h.

## ◆ RTC_RIIR_AIF_Msk

#define RTC_RIIR_AIF_Msk (0x1ul << RTC_RIIR_AIF_Pos)

RTC_T::RIIR: AIF Mask

Definition at line 8180 of file Nano100Series.h.

## ◆ RTC_RIIR_AIF_Pos

#define RTC_RIIR_AIF_Pos (0)

RTC_T::RIIR: AIF Position

Definition at line 8179 of file Nano100Series.h.

## ◆ RTC_RIIR_SNOOPIF_Msk

#define RTC_RIIR_SNOOPIF_Msk (0x1ul << RTC_RIIR_SNOOPIF_Pos)

RTC_T::RIIR: SNOOPIF Mask

Definition at line 8186 of file Nano100Series.h.

## ◆ RTC_RIIR_SNOOPIF_Pos

#define RTC_RIIR_SNOOPIF_Pos (2)

RTC_T::RIIR: SNOOPIF Position

Definition at line 8185 of file Nano100Series.h.

## ◆ RTC_RIIR_TIF_Msk

#define RTC_RIIR_TIF_Msk (0x1ul << RTC_RIIR_TIF_Pos)

RTC_T::RIIR: TIF Mask

Definition at line 8183 of file Nano100Series.h.

## ◆ RTC_RIIR_TIF_Pos

#define RTC_RIIR_TIF_Pos (1)

RTC_T::RIIR: TIF Position

Definition at line 8182 of file Nano100Series.h.

## ◆ RTC_SPR0_SPARE_Msk

#define RTC_SPR0_SPARE_Msk (0xfffffffful << RTC_SPR0_SPARE_Pos)

RTC_T::SPR0: SPARE Mask

Definition at line 8204 of file Nano100Series.h.

## ◆ RTC_SPR0_SPARE_Pos

#define RTC_SPR0_SPARE_Pos (0)

RTC_T::SPR0: SPARE Position

Definition at line 8203 of file Nano100Series.h.

## ◆ RTC_SPR10_SPARE_Msk

#define RTC_SPR10_SPARE_Msk (0xfffffffful << RTC_SPR10_SPARE_Pos)

RTC_T::SPR10: SPARE Mask

Definition at line 8234 of file Nano100Series.h.

## ◆ RTC_SPR10_SPARE_Pos

#define RTC_SPR10_SPARE_Pos (0)

RTC_T::SPR10: SPARE Position

Definition at line 8233 of file Nano100Series.h.

## ◆ RTC_SPR11_SPARE_Msk

#define RTC_SPR11_SPARE_Msk (0xfffffffful << RTC_SPR11_SPARE_Pos)

RTC_T::SPR11: SPARE Mask

Definition at line 8237 of file Nano100Series.h.

## ◆ RTC_SPR11_SPARE_Pos

#define RTC_SPR11_SPARE_Pos (0)

RTC_T::SPR11: SPARE Position

Definition at line 8236 of file Nano100Series.h.

## ◆ RTC_SPR12_SPARE_Msk

#define RTC_SPR12_SPARE_Msk (0xfffffffful << RTC_SPR12_SPARE_Pos)

RTC_T::SPR12: SPARE Mask

Definition at line 8240 of file Nano100Series.h.

## ◆ RTC_SPR12_SPARE_Pos

#define RTC_SPR12_SPARE_Pos (0)

RTC_T::SPR12: SPARE Position

Definition at line 8239 of file Nano100Series.h.

## ◆ RTC_SPR13_SPARE_Msk

#define RTC_SPR13_SPARE_Msk (0xfffffffful << RTC_SPR13_SPARE_Pos)

RTC_T::SPR13: SPARE Mask

Definition at line 8243 of file Nano100Series.h.

## ◆ RTC_SPR13_SPARE_Pos

#define RTC_SPR13_SPARE_Pos (0)

RTC_T::SPR13: SPARE Position

Definition at line 8242 of file Nano100Series.h.

## ◆ RTC_SPR14_SPARE_Msk

#define RTC_SPR14_SPARE_Msk (0xfffffffful << RTC_SPR14_SPARE_Pos)

RTC_T::SPR14: SPARE Mask

Definition at line 8246 of file Nano100Series.h.

## ◆ RTC_SPR14_SPARE_Pos

#define RTC_SPR14_SPARE_Pos (0)

RTC_T::SPR14: SPARE Position

Definition at line 8245 of file Nano100Series.h.

## ◆ RTC_SPR15_SPARE_Msk

#define RTC_SPR15_SPARE_Msk (0xfffffffful << RTC_SPR15_SPARE_Pos)

RTC_T::SPR15: SPARE Mask

Definition at line 8249 of file Nano100Series.h.

## ◆ RTC_SPR15_SPARE_Pos

#define RTC_SPR15_SPARE_Pos (0)

RTC_T::SPR15: SPARE Position

Definition at line 8248 of file Nano100Series.h.

## ◆ RTC_SPR16_SPARE_Msk

#define RTC_SPR16_SPARE_Msk (0xfffffffful << RTC_SPR16_SPARE_Pos)

RTC_T::SPR16: SPARE Mask

Definition at line 8252 of file Nano100Series.h.

## ◆ RTC_SPR16_SPARE_Pos

#define RTC_SPR16_SPARE_Pos (0)

RTC_T::SPR16: SPARE Position

Definition at line 8251 of file Nano100Series.h.

## ◆ RTC_SPR17_SPARE_Msk

#define RTC_SPR17_SPARE_Msk (0xfffffffful << RTC_SPR17_SPARE_Pos)

RTC_T::SPR17: SPARE Mask

Definition at line 8255 of file Nano100Series.h.

## ◆ RTC_SPR17_SPARE_Pos

#define RTC_SPR17_SPARE_Pos (0)

RTC_T::SPR17: SPARE Position

Definition at line 8254 of file Nano100Series.h.

## ◆ RTC_SPR18_SPARE_Msk

#define RTC_SPR18_SPARE_Msk (0xfffffffful << RTC_SPR18_SPARE_Pos)

RTC_T::SPR18: SPARE Mask

Definition at line 8258 of file Nano100Series.h.

## ◆ RTC_SPR18_SPARE_Pos

#define RTC_SPR18_SPARE_Pos (0)

RTC_T::SPR18: SPARE Position

Definition at line 8257 of file Nano100Series.h.

## ◆ RTC_SPR19_SPARE_Msk

#define RTC_SPR19_SPARE_Msk (0xfffffffful << RTC_SPR19_SPARE_Pos)

RTC_T::SPR19: SPARE Mask

Definition at line 8261 of file Nano100Series.h.

## ◆ RTC_SPR19_SPARE_Pos

#define RTC_SPR19_SPARE_Pos (0)

RTC_T::SPR19: SPARE Position

Definition at line 8260 of file Nano100Series.h.

## ◆ RTC_SPR1_SPARE_Msk

#define RTC_SPR1_SPARE_Msk (0xfffffffful << RTC_SPR1_SPARE_Pos)

RTC_T::SPR1: SPARE Mask

Definition at line 8207 of file Nano100Series.h.

## ◆ RTC_SPR1_SPARE_Pos

#define RTC_SPR1_SPARE_Pos (0)

RTC_T::SPR1: SPARE Position

Definition at line 8206 of file Nano100Series.h.

## ◆ RTC_SPR2_SPARE_Msk

#define RTC_SPR2_SPARE_Msk (0xfffffffful << RTC_SPR2_SPARE_Pos)

RTC_T::SPR2: SPARE Mask

Definition at line 8210 of file Nano100Series.h.

## ◆ RTC_SPR2_SPARE_Pos

#define RTC_SPR2_SPARE_Pos (0)

RTC_T::SPR2: SPARE Position

Definition at line 8209 of file Nano100Series.h.

## ◆ RTC_SPR3_SPARE_Msk

#define RTC_SPR3_SPARE_Msk (0xfffffffful << RTC_SPR3_SPARE_Pos)

RTC_T::SPR3: SPARE Mask

Definition at line 8213 of file Nano100Series.h.

## ◆ RTC_SPR3_SPARE_Pos

#define RTC_SPR3_SPARE_Pos (0)

RTC_T::SPR3: SPARE Position

Definition at line 8212 of file Nano100Series.h.

## ◆ RTC_SPR4_SPARE_Msk

#define RTC_SPR4_SPARE_Msk (0xfffffffful << RTC_SPR4_SPARE_Pos)

RTC_T::SPR4: SPARE Mask

Definition at line 8216 of file Nano100Series.h.

## ◆ RTC_SPR4_SPARE_Pos

#define RTC_SPR4_SPARE_Pos (0)

RTC_T::SPR4: SPARE Position

Definition at line 8215 of file Nano100Series.h.

## ◆ RTC_SPR5_SPARE_Msk

#define RTC_SPR5_SPARE_Msk (0xfffffffful << RTC_SPR5_SPARE_Pos)

RTC_T::SPR5: SPARE Mask

Definition at line 8219 of file Nano100Series.h.

## ◆ RTC_SPR5_SPARE_Pos

#define RTC_SPR5_SPARE_Pos (0)

RTC_T::SPR5: SPARE Position

Definition at line 8218 of file Nano100Series.h.

## ◆ RTC_SPR6_SPARE_Msk

#define RTC_SPR6_SPARE_Msk (0xfffffffful << RTC_SPR6_SPARE_Pos)

RTC_T::SPR6: SPARE Mask

Definition at line 8222 of file Nano100Series.h.

## ◆ RTC_SPR6_SPARE_Pos

#define RTC_SPR6_SPARE_Pos (0)

RTC_T::SPR6: SPARE Position

Definition at line 8221 of file Nano100Series.h.

## ◆ RTC_SPR7_SPARE_Msk

#define RTC_SPR7_SPARE_Msk (0xfffffffful << RTC_SPR7_SPARE_Pos)

RTC_T::SPR7: SPARE Mask

Definition at line 8225 of file Nano100Series.h.

## ◆ RTC_SPR7_SPARE_Pos

#define RTC_SPR7_SPARE_Pos (0)

RTC_T::SPR7: SPARE Position

Definition at line 8224 of file Nano100Series.h.

## ◆ RTC_SPR8_SPARE_Msk

#define RTC_SPR8_SPARE_Msk (0xfffffffful << RTC_SPR8_SPARE_Pos)

RTC_T::SPR8: SPARE Mask

Definition at line 8228 of file Nano100Series.h.

## ◆ RTC_SPR8_SPARE_Pos

#define RTC_SPR8_SPARE_Pos (0)

RTC_T::SPR8: SPARE Position

Definition at line 8227 of file Nano100Series.h.

## ◆ RTC_SPR9_SPARE_Msk

#define RTC_SPR9_SPARE_Msk (0xfffffffful << RTC_SPR9_SPARE_Pos)

RTC_T::SPR9: SPARE Mask

Definition at line 8231 of file Nano100Series.h.

## ◆ RTC_SPR9_SPARE_Pos

#define RTC_SPR9_SPARE_Pos (0)

RTC_T::SPR9: SPARE Position

Definition at line 8230 of file Nano100Series.h.

## ◆ RTC_SPRCTL_SNOOPEDGE_Msk

#define RTC_SPRCTL_SNOOPEDGE_Msk (0x1ul << RTC_SPRCTL_SNOOPEDGE_Pos)

RTC_T::SPRCTL: SNOOPEDGE Mask

Definition at line 8198 of file Nano100Series.h.

## ◆ RTC_SPRCTL_SNOOPEDGE_Pos

#define RTC_SPRCTL_SNOOPEDGE_Pos (1)

RTC_T::SPRCTL: SNOOPEDGE Position

Definition at line 8197 of file Nano100Series.h.

## ◆ RTC_SPRCTL_SNOOPEN_Msk

#define RTC_SPRCTL_SNOOPEN_Msk (0x1ul << RTC_SPRCTL_SNOOPEN_Pos)

RTC_T::SPRCTL: SNOOPEN Mask

Definition at line 8195 of file Nano100Series.h.

## ◆ RTC_SPRCTL_SNOOPEN_Pos

#define RTC_SPRCTL_SNOOPEN_Pos (0)

RTC_T::SPRCTL: SNOOPEN Position

Definition at line 8194 of file Nano100Series.h.

## ◆ RTC_SPRCTL_SPRRDY_Msk

#define RTC_SPRCTL_SPRRDY_Msk (0x1ul << RTC_SPRCTL_SPRRDY_Pos)

RTC_T::SPRCTL: SPRRDY Mask

Definition at line 8201 of file Nano100Series.h.

## ◆ RTC_SPRCTL_SPRRDY_Pos

#define RTC_SPRCTL_SPRRDY_Pos (7)

RTC_T::SPRCTL: SPRRDY Position

Definition at line 8200 of file Nano100Series.h.

## ◆ RTC_TAR_10HR_Msk

#define RTC_TAR_10HR_Msk (0x3ul << RTC_TAR_10HR_Pos)

RTC_T::TAR: 10HR Mask

Definition at line 8147 of file Nano100Series.h.

## ◆ RTC_TAR_10HR_Pos

#define RTC_TAR_10HR_Pos (20)

RTC_T::TAR: 10HR Position

Definition at line 8146 of file Nano100Series.h.

## ◆ RTC_TAR_10MIN_Msk

#define RTC_TAR_10MIN_Msk (0x7ul << RTC_TAR_10MIN_Pos)

RTC_T::TAR: 10MIN Mask

Definition at line 8141 of file Nano100Series.h.

## ◆ RTC_TAR_10MIN_Pos

#define RTC_TAR_10MIN_Pos (12)

RTC_T::TAR: 10MIN Position

Definition at line 8140 of file Nano100Series.h.

## ◆ RTC_TAR_10SEC_Msk

#define RTC_TAR_10SEC_Msk (0x7ul << RTC_TAR_10SEC_Pos)

RTC_T::TAR: 10SEC Mask

Definition at line 8135 of file Nano100Series.h.

## ◆ RTC_TAR_10SEC_Pos

#define RTC_TAR_10SEC_Pos (4)

RTC_T::TAR: 10SEC Position

Definition at line 8134 of file Nano100Series.h.

## ◆ RTC_TAR_1HR_Msk

#define RTC_TAR_1HR_Msk (0xful << RTC_TAR_1HR_Pos)

RTC_T::TAR: 1HR Mask

Definition at line 8144 of file Nano100Series.h.

## ◆ RTC_TAR_1HR_Pos

#define RTC_TAR_1HR_Pos (16)

RTC_T::TAR: 1HR Position

Definition at line 8143 of file Nano100Series.h.

## ◆ RTC_TAR_1MIN_Msk

#define RTC_TAR_1MIN_Msk (0xful << RTC_TAR_1MIN_Pos)

RTC_T::TAR: 1MIN Mask

Definition at line 8138 of file Nano100Series.h.

## ◆ RTC_TAR_1MIN_Pos

#define RTC_TAR_1MIN_Pos (8)

RTC_T::TAR: 1MIN Position

Definition at line 8137 of file Nano100Series.h.

## ◆ RTC_TAR_1SEC_Msk

#define RTC_TAR_1SEC_Msk (0xful << RTC_TAR_1SEC_Pos)

RTC_T::TAR: 1SEC Mask

Definition at line 8132 of file Nano100Series.h.

## ◆ RTC_TAR_1SEC_Pos

#define RTC_TAR_1SEC_Pos (0)

RTC_T::TAR: 1SEC Position

Definition at line 8131 of file Nano100Series.h.

## ◆ RTC_TLR_10HR_Msk

#define RTC_TLR_10HR_Msk (0x3ul << RTC_TLR_10HR_Pos)

RTC_T::TLR: 10HR Mask

Definition at line 8105 of file Nano100Series.h.

## ◆ RTC_TLR_10HR_Pos

#define RTC_TLR_10HR_Pos (20)

RTC_T::TLR: 10HR Position

Definition at line 8104 of file Nano100Series.h.

## ◆ RTC_TLR_10MIN_Msk

#define RTC_TLR_10MIN_Msk (0x7ul << RTC_TLR_10MIN_Pos)

RTC_T::TLR: 10MIN Mask

Definition at line 8099 of file Nano100Series.h.

## ◆ RTC_TLR_10MIN_Pos

#define RTC_TLR_10MIN_Pos (12)

RTC_T::TLR: 10MIN Position

Definition at line 8098 of file Nano100Series.h.

## ◆ RTC_TLR_10SEC_Msk

#define RTC_TLR_10SEC_Msk (0x7ul << RTC_TLR_10SEC_Pos)

RTC_T::TLR: 10SEC Mask

Definition at line 8093 of file Nano100Series.h.

## ◆ RTC_TLR_10SEC_Pos

#define RTC_TLR_10SEC_Pos (4)

RTC_T::TLR: 10SEC Position

Definition at line 8092 of file Nano100Series.h.

## ◆ RTC_TLR_1HR_Msk

#define RTC_TLR_1HR_Msk (0xful << RTC_TLR_1HR_Pos)

RTC_T::TLR: 1HR Mask

Definition at line 8102 of file Nano100Series.h.

## ◆ RTC_TLR_1HR_Pos

#define RTC_TLR_1HR_Pos (16)

RTC_T::TLR: 1HR Position

Definition at line 8101 of file Nano100Series.h.

## ◆ RTC_TLR_1MIN_Msk

#define RTC_TLR_1MIN_Msk (0xful << RTC_TLR_1MIN_Pos)

RTC_T::TLR: 1MIN Mask

Definition at line 8096 of file Nano100Series.h.

## ◆ RTC_TLR_1MIN_Pos

#define RTC_TLR_1MIN_Pos (8)

RTC_T::TLR: 1MIN Position

Definition at line 8095 of file Nano100Series.h.

## ◆ RTC_TLR_1SEC_Msk

#define RTC_TLR_1SEC_Msk (0xful << RTC_TLR_1SEC_Pos)

RTC_T::TLR: 1SEC Mask

Definition at line 8090 of file Nano100Series.h.

## ◆ RTC_TLR_1SEC_Pos

#define RTC_TLR_1SEC_Pos (0)

RTC_T::TLR: 1SEC Position

Definition at line 8089 of file Nano100Series.h.

## ◆ RTC_TSSR_24H_12H_Msk

#define RTC_TSSR_24H_12H_Msk (0x1ul << RTC_TSSR_24H_12H_Pos)

RTC_T::TSSR: 24hr_12hr Mask

Definition at line 8126 of file Nano100Series.h.

## ◆ RTC_TSSR_24H_12H_Pos

#define RTC_TSSR_24H_12H_Pos (0)

RTC_T::TSSR: 24hr_12hr Position

Definition at line 8125 of file Nano100Series.h.

## ◆ RTC_TTR_TTR_Msk

#define RTC_TTR_TTR_Msk (0x7ul << RTC_TTR_TTR_Pos)

RTC_T::TTR: TTR Mask

Definition at line 8189 of file Nano100Series.h.

## ◆ RTC_TTR_TTR_Pos

#define RTC_TTR_TTR_Pos (0)

RTC_T::TTR: TTR Position

Definition at line 8188 of file Nano100Series.h.

## ◆ RTC_TTR_TWKE_Msk

#define RTC_TTR_TWKE_Msk (0x1ul << RTC_TTR_TWKE_Pos)

RTC_T::TTR: TWKE Mask

Definition at line 8192 of file Nano100Series.h.

## ◆ RTC_TTR_TWKE_Pos

#define RTC_TTR_TWKE_Pos (3)

RTC_T::TTR: TWKE Position

Definition at line 8191 of file Nano100Series.h.

## ◆ SC_ALTCTL_ACT_EN_Msk

#define SC_ALTCTL_ACT_EN_Msk (0x1ul << SC_ALTCTL_ACT_EN_Pos)

SC_T::ALTCTL: ACT_EN Mask

Definition at line 8947 of file Nano100Series.h.

## ◆ SC_ALTCTL_ACT_EN_Pos

#define SC_ALTCTL_ACT_EN_Pos (3)

SC_T::ALTCTL: ACT_EN Position

Definition at line 8946 of file Nano100Series.h.

## ◆ SC_ALTCTL_DACT_EN_Msk

#define SC_ALTCTL_DACT_EN_Msk (0x1ul << SC_ALTCTL_DACT_EN_Pos)

SC_T::ALTCTL: DACT_EN Mask

Definition at line 8944 of file Nano100Series.h.

## ◆ SC_ALTCTL_DACT_EN_Pos

#define SC_ALTCTL_DACT_EN_Pos (2)

SC_T::ALTCTL: DACT_EN Position

Definition at line 8943 of file Nano100Series.h.

## ◆ SC_ALTCTL_INIT_SEL_Msk

#define SC_ALTCTL_INIT_SEL_Msk (0x3ul << SC_ALTCTL_INIT_SEL_Pos)

SC_T::ALTCTL: INIT_SEL Mask

Definition at line 8962 of file Nano100Series.h.

## ◆ SC_ALTCTL_INIT_SEL_Pos

#define SC_ALTCTL_INIT_SEL_Pos (8)

SC_T::ALTCTL: INIT_SEL Position

Definition at line 8961 of file Nano100Series.h.

## ◆ SC_ALTCTL_RX_BGT_EN_Msk

#define SC_ALTCTL_RX_BGT_EN_Msk (0x1ul << SC_ALTCTL_RX_BGT_EN_Pos)

SC_T::ALTCTL: RX_BGT_EN Mask

Definition at line 8965 of file Nano100Series.h.

## ◆ SC_ALTCTL_RX_BGT_EN_Pos

#define SC_ALTCTL_RX_BGT_EN_Pos (12)

SC_T::ALTCTL: RX_BGT_EN Position

Definition at line 8964 of file Nano100Series.h.

## ◆ SC_ALTCTL_RX_RST_Msk

#define SC_ALTCTL_RX_RST_Msk (0x1ul << SC_ALTCTL_RX_RST_Pos)

SC_T::ALTCTL: RX_RST Mask

Definition at line 8941 of file Nano100Series.h.

## ◆ SC_ALTCTL_RX_RST_Pos

#define SC_ALTCTL_RX_RST_Pos (1)

SC_T::ALTCTL: RX_RST Position

Definition at line 8940 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR0_ATV_Msk

#define SC_ALTCTL_TMR0_ATV_Msk (0x1ul << SC_ALTCTL_TMR0_ATV_Pos)

SC_T::ALTCTL: TMR0_ATV Mask

Definition at line 8968 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR0_ATV_Pos

#define SC_ALTCTL_TMR0_ATV_Pos (13)

SC_T::ALTCTL: TMR0_ATV Position

Definition at line 8967 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR0_SEN_Msk

#define SC_ALTCTL_TMR0_SEN_Msk (0x1ul << SC_ALTCTL_TMR0_SEN_Pos)

SC_T::ALTCTL: TMR0_SEN Mask

Definition at line 8953 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR0_SEN_Pos

#define SC_ALTCTL_TMR0_SEN_Pos (5)

SC_T::ALTCTL: TMR0_SEN Position

Definition at line 8952 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR1_ATV_Msk

#define SC_ALTCTL_TMR1_ATV_Msk (0x1ul << SC_ALTCTL_TMR1_ATV_Pos)

SC_T::ALTCTL: TMR1_ATV Mask

Definition at line 8971 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR1_ATV_Pos

#define SC_ALTCTL_TMR1_ATV_Pos (14)

SC_T::ALTCTL: TMR1_ATV Position

Definition at line 8970 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR1_SEN_Msk

#define SC_ALTCTL_TMR1_SEN_Msk (0x1ul << SC_ALTCTL_TMR1_SEN_Pos)

SC_T::ALTCTL: TMR1_SEN Mask

Definition at line 8956 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR1_SEN_Pos

#define SC_ALTCTL_TMR1_SEN_Pos (6)

SC_T::ALTCTL: TMR1_SEN Position

Definition at line 8955 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR2_ATV_Msk

#define SC_ALTCTL_TMR2_ATV_Msk (0x1ul << SC_ALTCTL_TMR2_ATV_Pos)

SC_T::ALTCTL: TMR2_ATV Mask

Definition at line 8974 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR2_ATV_Pos

#define SC_ALTCTL_TMR2_ATV_Pos (15)

SC_T::ALTCTL: TMR2_ATV Position

Definition at line 8973 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR2_SEN_Msk

#define SC_ALTCTL_TMR2_SEN_Msk (0x1ul << SC_ALTCTL_TMR2_SEN_Pos)

SC_T::ALTCTL: TMR2_SEN Mask

Definition at line 8959 of file Nano100Series.h.

## ◆ SC_ALTCTL_TMR2_SEN_Pos

#define SC_ALTCTL_TMR2_SEN_Pos (7)

SC_T::ALTCTL: TMR2_SEN Position

Definition at line 8958 of file Nano100Series.h.

## ◆ SC_ALTCTL_TX_RST_Msk

#define SC_ALTCTL_TX_RST_Msk (0x1ul << SC_ALTCTL_TX_RST_Pos)

SC_T::ALTCTL: TX_RST Mask

Definition at line 8938 of file Nano100Series.h.

## ◆ SC_ALTCTL_TX_RST_Pos

#define SC_ALTCTL_TX_RST_Pos (0)

SC_T::ALTCTL: TX_RST Position

Definition at line 8937 of file Nano100Series.h.

## ◆ SC_ALTCTL_WARST_EN_Msk

#define SC_ALTCTL_WARST_EN_Msk (0x1ul << SC_ALTCTL_WARST_EN_Pos)

SC_T::ALTCTL: WARST_EN Mask

Definition at line 8950 of file Nano100Series.h.

## ◆ SC_ALTCTL_WARST_EN_Pos

#define SC_ALTCTL_WARST_EN_Pos (4)

SC_T::ALTCTL: WARST_EN Position

Definition at line 8949 of file Nano100Series.h.

## ◆ SC_CTL_AUTO_CON_EN_Msk

#define SC_CTL_AUTO_CON_EN_Msk (0x1ul << SC_CTL_AUTO_CON_EN_Pos)

SC_T::CTL: AUTO_CON_EN Mask

Definition at line 8905 of file Nano100Series.h.

## ◆ SC_CTL_AUTO_CON_EN_Pos

#define SC_CTL_AUTO_CON_EN_Pos (3)

SC_T::CTL: AUTO_CON_EN Position

Definition at line 8904 of file Nano100Series.h.

## ◆ SC_CTL_BGT_Msk

#define SC_CTL_BGT_Msk (0x1ful << SC_CTL_BGT_Pos)

SC_T::CTL: BGT Mask

Definition at line 8914 of file Nano100Series.h.

## ◆ SC_CTL_BGT_Pos

#define SC_CTL_BGT_Pos (8)

SC_T::CTL: BGT Position

Definition at line 8913 of file Nano100Series.h.

## ◆ SC_CTL_CD_DEB_SEL_Msk

#define SC_CTL_CD_DEB_SEL_Msk (0x3ul << SC_CTL_CD_DEB_SEL_Pos)

SC_T::CTL: CD_DEB_SEL Mask

Definition at line 8935 of file Nano100Series.h.

## ◆ SC_CTL_CD_DEB_SEL_Pos

#define SC_CTL_CD_DEB_SEL_Pos (24)

SC_T::CTL: CD_DEB_SEL Position

Definition at line 8934 of file Nano100Series.h.

## ◆ SC_CTL_CON_SEL_Msk

#define SC_CTL_CON_SEL_Msk (0x3ul << SC_CTL_CON_SEL_Pos)

SC_T::CTL: CON_SEL Mask

Definition at line 8908 of file Nano100Series.h.

## ◆ SC_CTL_CON_SEL_Pos

#define SC_CTL_CON_SEL_Pos (4)

SC_T::CTL: CON_SEL Position

Definition at line 8907 of file Nano100Series.h.

## ◆ SC_CTL_DIS_RX_Msk

#define SC_CTL_DIS_RX_Msk (0x1ul << SC_CTL_DIS_RX_Pos)

SC_T::CTL: DIS_RX Mask

Definition at line 8899 of file Nano100Series.h.

## ◆ SC_CTL_DIS_RX_Pos

#define SC_CTL_DIS_RX_Pos (1)

SC_T::CTL: DIS_RX Position

Definition at line 8898 of file Nano100Series.h.

## ◆ SC_CTL_DIS_TX_Msk

#define SC_CTL_DIS_TX_Msk (0x1ul << SC_CTL_DIS_TX_Pos)

SC_T::CTL: DIS_TX Mask

Definition at line 8902 of file Nano100Series.h.

## ◆ SC_CTL_DIS_TX_Pos

#define SC_CTL_DIS_TX_Pos (2)

SC_T::CTL: DIS_TX Position

Definition at line 8901 of file Nano100Series.h.

## ◆ SC_CTL_RX_ERETRY_EN_Msk

#define SC_CTL_RX_ERETRY_EN_Msk (0x1ul << SC_CTL_RX_ERETRY_EN_Pos)

SC_T::CTL: RX_ERETRY_EN Mask

Definition at line 8926 of file Nano100Series.h.

## ◆ SC_CTL_RX_ERETRY_EN_Pos

#define SC_CTL_RX_ERETRY_EN_Pos (19)

SC_T::CTL: RX_ERETRY_EN Position

Definition at line 8925 of file Nano100Series.h.

## ◆ SC_CTL_RX_ERETRY_Msk

#define SC_CTL_RX_ERETRY_Msk (0x7ul << SC_CTL_RX_ERETRY_Pos)

SC_T::CTL: RX_ERETRY Mask

Definition at line 8923 of file Nano100Series.h.

## ◆ SC_CTL_RX_ERETRY_Pos

#define SC_CTL_RX_ERETRY_Pos (16)

SC_T::CTL: RX_ERETRY Position

Definition at line 8922 of file Nano100Series.h.

## ◆ SC_CTL_RX_FTRI_LEV_Msk

#define SC_CTL_RX_FTRI_LEV_Msk (0x3ul << SC_CTL_RX_FTRI_LEV_Pos)

SC_T::CTL: RX_FTRI_LEV Mask

Definition at line 8911 of file Nano100Series.h.

## ◆ SC_CTL_RX_FTRI_LEV_Pos

#define SC_CTL_RX_FTRI_LEV_Pos (6)

SC_T::CTL: RX_FTRI_LEV Position

Definition at line 8910 of file Nano100Series.h.

## ◆ SC_CTL_SC_CEN_Msk

#define SC_CTL_SC_CEN_Msk (0x1ul << SC_CTL_SC_CEN_Pos)

SC_T::CTL: SC_CEN Mask

Definition at line 8896 of file Nano100Series.h.

## ◆ SC_CTL_SC_CEN_Pos

#define SC_CTL_SC_CEN_Pos (0)

SC_T::CTL: SC_CEN Position

Definition at line 8895 of file Nano100Series.h.

## ◆ SC_CTL_SLEN_Msk

#define SC_CTL_SLEN_Msk (0x1ul << SC_CTL_SLEN_Pos)

SC_T::CTL: SLEN Mask

Definition at line 8920 of file Nano100Series.h.

## ◆ SC_CTL_SLEN_Pos

#define SC_CTL_SLEN_Pos (15)

SC_T::CTL: SLEN Position

Definition at line 8919 of file Nano100Series.h.

## ◆ SC_CTL_TMR_SEL_Msk

#define SC_CTL_TMR_SEL_Msk (0x3ul << SC_CTL_TMR_SEL_Pos)

SC_T::CTL: TMR_SEL Mask

Definition at line 8917 of file Nano100Series.h.

## ◆ SC_CTL_TMR_SEL_Pos

#define SC_CTL_TMR_SEL_Pos (13)

SC_T::CTL: TMR_SEL Position

Definition at line 8916 of file Nano100Series.h.

## ◆ SC_CTL_TX_ERETRY_EN_Msk

#define SC_CTL_TX_ERETRY_EN_Msk (0x1ul << SC_CTL_TX_ERETRY_EN_Pos)

SC_T::CTL: TX_ERETRY_EN Mask

Definition at line 8932 of file Nano100Series.h.

## ◆ SC_CTL_TX_ERETRY_EN_Pos

#define SC_CTL_TX_ERETRY_EN_Pos (23)

SC_T::CTL: TX_ERETRY_EN Position

Definition at line 8931 of file Nano100Series.h.

## ◆ SC_CTL_TX_ERETRY_Msk

#define SC_CTL_TX_ERETRY_Msk (0x7ul << SC_CTL_TX_ERETRY_Pos)

SC_T::CTL: TX_ERETRY Mask

Definition at line 8929 of file Nano100Series.h.

## ◆ SC_CTL_TX_ERETRY_Pos

#define SC_CTL_TX_ERETRY_Pos (20)

SC_T::CTL: TX_ERETRY Position

Definition at line 8928 of file Nano100Series.h.

## ◆ SC_DAT_DAT_Msk

#define SC_DAT_DAT_Msk (0xfful << SC_DAT_DAT_Pos)

SC_T::DAT: DAT Mask

Definition at line 8893 of file Nano100Series.h.

## ◆ SC_DAT_DAT_Pos

#define SC_DAT_DAT_Pos (0)

    @addtogroup SC_CONST SC Bit Field Definition
    Constant Definitions for SC Controller

SC_T::DAT: DAT Position

Definition at line 8892 of file Nano100Series.h.

## ◆ SC_EGTR_EGT_Msk

#define SC_EGTR_EGT_Msk (0xfful << SC_EGTR_EGT_Pos)

SC_T::EGTR: EGT Mask

Definition at line 8977 of file Nano100Series.h.

## ◆ SC_EGTR_EGT_Pos

#define SC_EGTR_EGT_Pos (0)

SC_T::EGTR: EGT Position

Definition at line 8976 of file Nano100Series.h.

## ◆ SC_ETUCR_COMPEN_EN_Msk

#define SC_ETUCR_COMPEN_EN_Msk (0x1ul << SC_ETUCR_COMPEN_EN_Pos)

SC_T::ETUCR: COMPEN_EN Mask

Definition at line 8986 of file Nano100Series.h.

## ◆ SC_ETUCR_COMPEN_EN_Pos

#define SC_ETUCR_COMPEN_EN_Pos (15)

SC_T::ETUCR: COMPEN_EN Position

Definition at line 8985 of file Nano100Series.h.

## ◆ SC_ETUCR_ETU_RDIV_Msk

#define SC_ETUCR_ETU_RDIV_Msk (0xffful << SC_ETUCR_ETU_RDIV_Pos)

SC_T::ETUCR: ETU_RDIV Mask

Definition at line 8983 of file Nano100Series.h.

## ◆ SC_ETUCR_ETU_RDIV_Pos

#define SC_ETUCR_ETU_RDIV_Pos (0)

SC_T::ETUCR: ETU_RDIV Position

Definition at line 8982 of file Nano100Series.h.

## ◆ SC_IER_ACON_ERR_IE_Msk

#define SC_IER_ACON_ERR_IE_Msk (0x1ul << SC_IER_ACON_ERR_IE_Pos)

SC_T::IER: ACON_ERR_IE Mask

Definition at line 9019 of file Nano100Series.h.

## ◆ SC_IER_ACON_ERR_IE_Pos

#define SC_IER_ACON_ERR_IE_Pos (10)

SC_T::IER: ACON_ERR_IE Position

Definition at line 9018 of file Nano100Series.h.

## ◆ SC_IER_BGT_IE_Msk

#define SC_IER_BGT_IE_Msk (0x1ul << SC_IER_BGT_IE_Pos)

SC_T::IER: BGT_IE Mask

Definition at line 9007 of file Nano100Series.h.

## ◆ SC_IER_BGT_IE_Pos

#define SC_IER_BGT_IE_Pos (6)

SC_T::IER: BGT_IE Position

Definition at line 9006 of file Nano100Series.h.

## ◆ SC_IER_CD_IE_Msk

#define SC_IER_CD_IE_Msk (0x1ul << SC_IER_CD_IE_Pos)

SC_T::IER: CD_IE Mask

Definition at line 9010 of file Nano100Series.h.

## ◆ SC_IER_CD_IE_Pos

#define SC_IER_CD_IE_Pos (7)

SC_T::IER: CD_IE Position

Definition at line 9009 of file Nano100Series.h.

## ◆ SC_IER_INIT_IE_Msk

#define SC_IER_INIT_IE_Msk (0x1ul << SC_IER_INIT_IE_Pos)

SC_T::IER: INIT_IE Mask

Definition at line 9013 of file Nano100Series.h.

## ◆ SC_IER_INIT_IE_Pos

#define SC_IER_INIT_IE_Pos (8)

SC_T::IER: INIT_IE Position

Definition at line 9012 of file Nano100Series.h.

## ◆ SC_IER_RDA_IE_Msk

#define SC_IER_RDA_IE_Msk (0x1ul << SC_IER_RDA_IE_Pos)

SC_T::IER: RDA_IE Mask

Definition at line 8989 of file Nano100Series.h.

## ◆ SC_IER_RDA_IE_Pos

#define SC_IER_RDA_IE_Pos (0)

SC_T::IER: RDA_IE Position

Definition at line 8988 of file Nano100Series.h.

## ◆ SC_IER_RTMR_IE_Msk

#define SC_IER_RTMR_IE_Msk (0x1ul << SC_IER_RTMR_IE_Pos)

SC_T::IER: RTMR_IE Mask

Definition at line 9016 of file Nano100Series.h.

## ◆ SC_IER_RTMR_IE_Pos

#define SC_IER_RTMR_IE_Pos (9)

SC_T::IER: RTMR_IE Position

Definition at line 9015 of file Nano100Series.h.

## ◆ SC_IER_TBE_IE_Msk

#define SC_IER_TBE_IE_Msk (0x1ul << SC_IER_TBE_IE_Pos)

SC_T::IER: TBE_IE Mask

Definition at line 8992 of file Nano100Series.h.

## ◆ SC_IER_TBE_IE_Pos

#define SC_IER_TBE_IE_Pos (1)

SC_T::IER: TBE_IE Position

Definition at line 8991 of file Nano100Series.h.

## ◆ SC_IER_TERR_IE_Msk

#define SC_IER_TERR_IE_Msk (0x1ul << SC_IER_TERR_IE_Pos)

SC_T::IER: TERR_IE Mask

Definition at line 8995 of file Nano100Series.h.

## ◆ SC_IER_TERR_IE_Pos

#define SC_IER_TERR_IE_Pos (2)

SC_T::IER: TERR_IE Position

Definition at line 8994 of file Nano100Series.h.

## ◆ SC_IER_TMR0_IE_Msk

#define SC_IER_TMR0_IE_Msk (0x1ul << SC_IER_TMR0_IE_Pos)

SC_T::IER: TMR0_IE Mask

Definition at line 8998 of file Nano100Series.h.

## ◆ SC_IER_TMR0_IE_Pos

#define SC_IER_TMR0_IE_Pos (3)

SC_T::IER: TMR0_IE Position

Definition at line 8997 of file Nano100Series.h.

## ◆ SC_IER_TMR1_IE_Msk

#define SC_IER_TMR1_IE_Msk (0x1ul << SC_IER_TMR1_IE_Pos)

SC_T::IER: TMR1_IE Mask

Definition at line 9001 of file Nano100Series.h.

## ◆ SC_IER_TMR1_IE_Pos

#define SC_IER_TMR1_IE_Pos (4)

SC_T::IER: TMR1_IE Position

Definition at line 9000 of file Nano100Series.h.

## ◆ SC_IER_TMR2_IE_Msk

#define SC_IER_TMR2_IE_Msk (0x1ul << SC_IER_TMR2_IE_Pos)

SC_T::IER: TMR2_IE Mask

Definition at line 9004 of file Nano100Series.h.

## ◆ SC_IER_TMR2_IE_Pos

#define SC_IER_TMR2_IE_Pos (5)

SC_T::IER: TMR2_IE Position

Definition at line 9003 of file Nano100Series.h.

## ◆ SC_ISR_ACON_ERR_IS_Msk

#define SC_ISR_ACON_ERR_IS_Msk (0x1ul << SC_ISR_ACON_ERR_IS_Pos)

SC_T::ISR: ACON_ERR_IS Mask

Definition at line 9052 of file Nano100Series.h.

## ◆ SC_ISR_ACON_ERR_IS_Pos

#define SC_ISR_ACON_ERR_IS_Pos (10)

SC_T::ISR: ACON_ERR_IS Position

Definition at line 9051 of file Nano100Series.h.

## ◆ SC_ISR_BGT_IS_Msk

#define SC_ISR_BGT_IS_Msk (0x1ul << SC_ISR_BGT_IS_Pos)

SC_T::ISR: BGT_IS Mask

Definition at line 9040 of file Nano100Series.h.

## ◆ SC_ISR_BGT_IS_Pos

#define SC_ISR_BGT_IS_Pos (6)

SC_T::ISR: BGT_IS Position

Definition at line 9039 of file Nano100Series.h.

## ◆ SC_ISR_CD_IS_Msk

#define SC_ISR_CD_IS_Msk (0x1ul << SC_ISR_CD_IS_Pos)

SC_T::ISR: CD_IS Mask

Definition at line 9043 of file Nano100Series.h.

## ◆ SC_ISR_CD_IS_Pos

#define SC_ISR_CD_IS_Pos (7)

SC_T::ISR: CD_IS Position

Definition at line 9042 of file Nano100Series.h.

## ◆ SC_ISR_INIT_IS_Msk

#define SC_ISR_INIT_IS_Msk (0x1ul << SC_ISR_INIT_IS_Pos)

SC_T::ISR: INIT_IS Mask

Definition at line 9046 of file Nano100Series.h.

## ◆ SC_ISR_INIT_IS_Pos

#define SC_ISR_INIT_IS_Pos (8)

SC_T::ISR: INIT_IS Position

Definition at line 9045 of file Nano100Series.h.

## ◆ SC_ISR_RDA_IS_Msk

#define SC_ISR_RDA_IS_Msk (0x1ul << SC_ISR_RDA_IS_Pos)

SC_T::ISR: RDA_IS Mask

Definition at line 9022 of file Nano100Series.h.

## ◆ SC_ISR_RDA_IS_Pos

#define SC_ISR_RDA_IS_Pos (0)

SC_T::ISR: RDA_IS Position

Definition at line 9021 of file Nano100Series.h.

## ◆ SC_ISR_RTMR_IS_Msk

#define SC_ISR_RTMR_IS_Msk (0x1ul << SC_ISR_RTMR_IS_Pos)

SC_T::ISR: RTMR_IS Mask

Definition at line 9049 of file Nano100Series.h.

## ◆ SC_ISR_RTMR_IS_Pos

#define SC_ISR_RTMR_IS_Pos (9)

SC_T::ISR: RTMR_IS Position

Definition at line 9048 of file Nano100Series.h.

## ◆ SC_ISR_TBE_IS_Msk

#define SC_ISR_TBE_IS_Msk (0x1ul << SC_ISR_TBE_IS_Pos)

SC_T::ISR: TBE_IS Mask

Definition at line 9025 of file Nano100Series.h.

## ◆ SC_ISR_TBE_IS_Pos

#define SC_ISR_TBE_IS_Pos (1)

SC_T::ISR: TBE_IS Position

Definition at line 9024 of file Nano100Series.h.

## ◆ SC_ISR_TERR_IS_Msk

#define SC_ISR_TERR_IS_Msk (0x1ul << SC_ISR_TERR_IS_Pos)

SC_T::ISR: TERR_IS Mask

Definition at line 9028 of file Nano100Series.h.

## ◆ SC_ISR_TERR_IS_Pos

#define SC_ISR_TERR_IS_Pos (2)

SC_T::ISR: TERR_IS Position

Definition at line 9027 of file Nano100Series.h.

## ◆ SC_ISR_TMR0_IS_Msk

#define SC_ISR_TMR0_IS_Msk (0x1ul << SC_ISR_TMR0_IS_Pos)

SC_T::ISR: TMR0_IS Mask

Definition at line 9031 of file Nano100Series.h.

## ◆ SC_ISR_TMR0_IS_Pos

#define SC_ISR_TMR0_IS_Pos (3)

SC_T::ISR: TMR0_IS Position

Definition at line 9030 of file Nano100Series.h.

## ◆ SC_ISR_TMR1_IS_Msk

#define SC_ISR_TMR1_IS_Msk (0x1ul << SC_ISR_TMR1_IS_Pos)

SC_T::ISR: TMR1_IS Mask

Definition at line 9034 of file Nano100Series.h.

## ◆ SC_ISR_TMR1_IS_Pos

#define SC_ISR_TMR1_IS_Pos (4)

SC_T::ISR: TMR1_IS Position

Definition at line 9033 of file Nano100Series.h.

## ◆ SC_ISR_TMR2_IS_Msk

#define SC_ISR_TMR2_IS_Msk (0x1ul << SC_ISR_TMR2_IS_Pos)

SC_T::ISR: TMR2_IS Mask

Definition at line 9037 of file Nano100Series.h.

## ◆ SC_ISR_TMR2_IS_Pos

#define SC_ISR_TMR2_IS_Pos (5)

SC_T::ISR: TMR2_IS Position

Definition at line 9036 of file Nano100Series.h.

## ◆ SC_PINCSR_ADAC_CD_EN_Msk

#define SC_PINCSR_ADAC_CD_EN_Msk (0x1ul << SC_PINCSR_ADAC_CD_EN_Pos)

SC_T::PINCSR: ADAC_CD_EN Mask

Definition at line 9124 of file Nano100Series.h.

## ◆ SC_PINCSR_ADAC_CD_EN_Pos

#define SC_PINCSR_ADAC_CD_EN_Pos (7)

SC_T::PINCSR: ADAC_CD_EN Position

Definition at line 9123 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_INS_F_Msk

#define SC_PINCSR_CD_INS_F_Msk (0x1ul << SC_PINCSR_CD_INS_F_Pos)

SC_T::PINCSR: CD_INS_F Mask

Definition at line 9115 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_INS_F_Pos

#define SC_PINCSR_CD_INS_F_Pos (3)

SC_T::PINCSR: CD_INS_F Position

Definition at line 9114 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_LEV_Msk

#define SC_PINCSR_CD_LEV_Msk (0x1ul << SC_PINCSR_CD_LEV_Pos)

SC_T::PINCSR: CD_LEV Mask

Definition at line 9133 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_LEV_Pos

#define SC_PINCSR_CD_LEV_Pos (10)

SC_T::PINCSR: CD_LEV Position

Definition at line 9132 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_PIN_ST_Msk

#define SC_PINCSR_CD_PIN_ST_Msk (0x1ul << SC_PINCSR_CD_PIN_ST_Pos)

SC_T::PINCSR: CD_PIN_ST Mask

Definition at line 9118 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_PIN_ST_Pos

#define SC_PINCSR_CD_PIN_ST_Pos (4)

SC_T::PINCSR: CD_PIN_ST Position

Definition at line 9117 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_REM_F_Msk

#define SC_PINCSR_CD_REM_F_Msk (0x1ul << SC_PINCSR_CD_REM_F_Pos)

SC_T::PINCSR: CD_REM_F Mask

Definition at line 9112 of file Nano100Series.h.

## ◆ SC_PINCSR_CD_REM_F_Pos

#define SC_PINCSR_CD_REM_F_Pos (2)

SC_T::PINCSR: CD_REM_F Position

Definition at line 9111 of file Nano100Series.h.

## ◆ SC_PINCSR_CLK_KEEP_Msk

#define SC_PINCSR_CLK_KEEP_Msk (0x1ul << SC_PINCSR_CLK_KEEP_Pos)

SC_T::PINCSR: CLK_KEEP Mask

Definition at line 9121 of file Nano100Series.h.

## ◆ SC_PINCSR_CLK_KEEP_Pos

#define SC_PINCSR_CLK_KEEP_Pos (6)

SC_T::PINCSR: CLK_KEEP Position

Definition at line 9120 of file Nano100Series.h.

## ◆ SC_PINCSR_POW_EN_Msk

#define SC_PINCSR_POW_EN_Msk (0x1ul << SC_PINCSR_POW_EN_Pos)

SC_T::PINCSR: POW_EN Mask

Definition at line 9106 of file Nano100Series.h.

## ◆ SC_PINCSR_POW_EN_Pos

#define SC_PINCSR_POW_EN_Pos (0)

SC_T::PINCSR: POW_EN Position

Definition at line 9105 of file Nano100Series.h.

## ◆ SC_PINCSR_POW_INV_Msk

#define SC_PINCSR_POW_INV_Msk (0x1ul << SC_PINCSR_POW_INV_Pos)

SC_T::PINCSR: POW_INV Mask

Definition at line 9136 of file Nano100Series.h.

## ◆ SC_PINCSR_POW_INV_Pos

#define SC_PINCSR_POW_INV_Pos (11)

SC_T::PINCSR: POW_INV Position

Definition at line 9135 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_DATA_I_ST_Msk

#define SC_PINCSR_SC_DATA_I_ST_Msk (0x1ul << SC_PINCSR_SC_DATA_I_ST_Pos)

SC_T::PINCSR: SC_DATA_I_ST Mask

Definition at line 9139 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_DATA_I_ST_Pos

#define SC_PINCSR_SC_DATA_I_ST_Pos (16)

SC_T::PINCSR: SC_DATA_I_ST Position

Definition at line 9138 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_DATA_O_Msk

#define SC_PINCSR_SC_DATA_O_Msk (0x1ul << SC_PINCSR_SC_DATA_O_Pos)

SC_T::PINCSR: SC_DATA_O Mask

Definition at line 9130 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_DATA_O_Pos

#define SC_PINCSR_SC_DATA_O_Pos (9)

SC_T::PINCSR: SC_DATA_O Position

Definition at line 9129 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_OEN_ST_Msk

#define SC_PINCSR_SC_OEN_ST_Msk (0x1ul << SC_PINCSR_SC_OEN_ST_Pos)

SC_T::PINCSR: SC_OEN_ST Mask

Definition at line 9127 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_OEN_ST_Pos

#define SC_PINCSR_SC_OEN_ST_Pos (8)

SC_T::PINCSR: SC_OEN_ST Position

Definition at line 9126 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_RST_Msk

#define SC_PINCSR_SC_RST_Msk (0x1ul << SC_PINCSR_SC_RST_Pos)

SC_T::PINCSR: SC_RST Mask

Definition at line 9109 of file Nano100Series.h.

## ◆ SC_PINCSR_SC_RST_Pos

#define SC_PINCSR_SC_RST_Pos (1)

SC_T::PINCSR: SC_RST Position

Definition at line 9108 of file Nano100Series.h.

## ◆ SC_RFTMR_RFTM_Msk

#define SC_RFTMR_RFTM_Msk (0x1fful << SC_RFTMR_RFTM_Pos)

SC_T::RFTMR: RFTM Mask

Definition at line 8980 of file Nano100Series.h.

## ◆ SC_RFTMR_RFTM_Pos

#define SC_RFTMR_RFTM_Pos (0)

SC_T::RFTMR: RFTM Position

Definition at line 8979 of file Nano100Series.h.

## ◆ SC_TDRA_TDR0_Msk

#define SC_TDRA_TDR0_Msk (0xfffffful << SC_TDRA_TDR0_Pos)

SC_T::TDRA: TDR0 Mask

Definition at line 9172 of file Nano100Series.h.

## ◆ SC_TDRA_TDR0_Pos

#define SC_TDRA_TDR0_Pos (0)

SC_T::TDRA: TDR0 Position

Definition at line 9171 of file Nano100Series.h.

## ◆ SC_TDRB_TDR1_Msk

#define SC_TDRB_TDR1_Msk (0xfful << SC_TDRB_TDR1_Pos)

SC_T::TDRB: TDR1 Mask

Definition at line 9175 of file Nano100Series.h.

## ◆ SC_TDRB_TDR1_Pos

#define SC_TDRB_TDR1_Pos (0)

SC_T::TDRB: TDR1 Position

Definition at line 9174 of file Nano100Series.h.

## ◆ SC_TDRB_TDR2_Msk

#define SC_TDRB_TDR2_Msk (0xfful << SC_TDRB_TDR2_Pos)

SC_T::TDRB: TDR2 Mask

Definition at line 9178 of file Nano100Series.h.

## ◆ SC_TDRB_TDR2_Pos

#define SC_TDRB_TDR2_Pos (8)

SC_T::TDRB: TDR2 Position

Definition at line 9177 of file Nano100Series.h.

## ◆ SC_TMR0_CNT_Msk

#define SC_TMR0_CNT_Msk (0xfffffful << SC_TMR0_CNT_Pos)

SC_T::TMR0: CNT Mask

Definition at line 9142 of file Nano100Series.h.

## ◆ SC_TMR0_CNT_Pos

#define SC_TMR0_CNT_Pos (0)

SC_T::TMR0: CNT Position

Definition at line 9141 of file Nano100Series.h.

## ◆ SC_TMR0_MODE_Msk

#define SC_TMR0_MODE_Msk (0xful << SC_TMR0_MODE_Pos)

SC_T::TMR0: MODE Mask

Definition at line 9145 of file Nano100Series.h.

## ◆ SC_TMR0_MODE_Pos

#define SC_TMR0_MODE_Pos (24)

SC_T::TMR0: MODE Position

Definition at line 9144 of file Nano100Series.h.

## ◆ SC_TMR1_CNT_Msk

#define SC_TMR1_CNT_Msk (0xfful << SC_TMR1_CNT_Pos)

SC_T::TMR1: CNT Mask

Definition at line 9148 of file Nano100Series.h.

## ◆ SC_TMR1_CNT_Pos

#define SC_TMR1_CNT_Pos (0)

SC_T::TMR1: CNT Position

Definition at line 9147 of file Nano100Series.h.

## ◆ SC_TMR1_MODE_Msk

#define SC_TMR1_MODE_Msk (0xful << SC_TMR1_MODE_Pos)

SC_T::TMR1: MODE Mask

Definition at line 9151 of file Nano100Series.h.

## ◆ SC_TMR1_MODE_Pos

#define SC_TMR1_MODE_Pos (24)

SC_T::TMR1: MODE Position

Definition at line 9150 of file Nano100Series.h.

## ◆ SC_TMR2_CNT_Msk

#define SC_TMR2_CNT_Msk (0xfful << SC_TMR2_CNT_Pos)

SC_T::TMR2: CNT Mask

Definition at line 9154 of file Nano100Series.h.

## ◆ SC_TMR2_CNT_Pos

#define SC_TMR2_CNT_Pos (0)

SC_T::TMR2: CNT Position

Definition at line 9153 of file Nano100Series.h.

## ◆ SC_TMR2_MODE_Msk

#define SC_TMR2_MODE_Msk (0xful << SC_TMR2_MODE_Pos)

SC_T::TMR2: MODE Mask

Definition at line 9157 of file Nano100Series.h.

## ◆ SC_TMR2_MODE_Pos

#define SC_TMR2_MODE_Pos (24)

SC_T::TMR2: MODE Position

Definition at line 9156 of file Nano100Series.h.

## ◆ SC_TRSR_RX_ATV_Msk

#define SC_TRSR_RX_ATV_Msk (0x1ul << SC_TRSR_RX_ATV_Pos)

SC_T::TRSR: RX_ATV Mask

Definition at line 9091 of file Nano100Series.h.

## ◆ SC_TRSR_RX_ATV_Pos

#define SC_TRSR_RX_ATV_Pos (23)

SC_T::TRSR: RX_ATV Position

Definition at line 9090 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EBR_F_Msk

#define SC_TRSR_RX_EBR_F_Msk (0x1ul << SC_TRSR_RX_EBR_F_Pos)

SC_T::TRSR: RX_EBR_F Mask

Definition at line 9070 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EBR_F_Pos

#define SC_TRSR_RX_EBR_F_Pos (6)

SC_T::TRSR: RX_EBR_F Position

Definition at line 9069 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EFR_F_Msk

#define SC_TRSR_RX_EFR_F_Msk (0x1ul << SC_TRSR_RX_EFR_F_Pos)

SC_T::TRSR: RX_EFR_F Mask

Definition at line 9067 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EFR_F_Pos

#define SC_TRSR_RX_EFR_F_Pos (5)

SC_T::TRSR: RX_EFR_F Position

Definition at line 9066 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EMPTY_F_Msk

#define SC_TRSR_RX_EMPTY_F_Msk (0x1ul << SC_TRSR_RX_EMPTY_F_Pos)

SC_T::TRSR: RX_EMPTY_F Mask

Definition at line 9058 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EMPTY_F_Pos

#define SC_TRSR_RX_EMPTY_F_Pos (1)

SC_T::TRSR: RX_EMPTY_F Position

Definition at line 9057 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EPA_F_Msk

#define SC_TRSR_RX_EPA_F_Msk (0x1ul << SC_TRSR_RX_EPA_F_Pos)

SC_T::TRSR: RX_EPA_F Mask

Definition at line 9064 of file Nano100Series.h.

## ◆ SC_TRSR_RX_EPA_F_Pos

#define SC_TRSR_RX_EPA_F_Pos (4)

SC_T::TRSR: RX_EPA_F Position

Definition at line 9063 of file Nano100Series.h.

## ◆ SC_TRSR_RX_FULL_F_Msk

#define SC_TRSR_RX_FULL_F_Msk (0x1ul << SC_TRSR_RX_FULL_F_Pos)

SC_T::TRSR: RX_FULL_F Mask

Definition at line 9061 of file Nano100Series.h.

## ◆ SC_TRSR_RX_FULL_F_Pos

#define SC_TRSR_RX_FULL_F_Pos (2)

SC_T::TRSR: RX_FULL_F Position

Definition at line 9060 of file Nano100Series.h.

## ◆ SC_TRSR_RX_OVER_ERETRY_Msk

#define SC_TRSR_RX_OVER_ERETRY_Msk (0x1ul << SC_TRSR_RX_OVER_ERETRY_Pos)

SC_T::TRSR: RX_OVER_ERETRY Mask

Definition at line 9088 of file Nano100Series.h.

## ◆ SC_TRSR_RX_OVER_ERETRY_Pos

#define SC_TRSR_RX_OVER_ERETRY_Pos (22)

SC_T::TRSR: RX_OVER_ERETRY Position

Definition at line 9087 of file Nano100Series.h.

## ◆ SC_TRSR_RX_OVER_F_Msk

#define SC_TRSR_RX_OVER_F_Msk (0x1ul << SC_TRSR_RX_OVER_F_Pos)

SC_T::TRSR: RX_OVER_F Mask

Definition at line 9055 of file Nano100Series.h.

## ◆ SC_TRSR_RX_OVER_F_Pos

#define SC_TRSR_RX_OVER_F_Pos (0)

SC_T::TRSR: RX_OVER_F Position

Definition at line 9054 of file Nano100Series.h.

## ◆ SC_TRSR_RX_POINT_F_Msk

#define SC_TRSR_RX_POINT_F_Msk (0x7ul << SC_TRSR_RX_POINT_F_Pos)

SC_T::TRSR: RX_POINT_F Mask

Definition at line 9082 of file Nano100Series.h.

## ◆ SC_TRSR_RX_POINT_F_Pos

#define SC_TRSR_RX_POINT_F_Pos (16)

SC_T::TRSR: RX_POINT_F Position

Definition at line 9081 of file Nano100Series.h.

## ◆ SC_TRSR_RX_REERR_Msk

#define SC_TRSR_RX_REERR_Msk (0x1ul << SC_TRSR_RX_REERR_Pos)

SC_T::TRSR: RX_REERR Mask

Definition at line 9085 of file Nano100Series.h.

## ◆ SC_TRSR_RX_REERR_Pos

#define SC_TRSR_RX_REERR_Pos (21)

SC_T::TRSR: RX_REERR Position

Definition at line 9084 of file Nano100Series.h.

## ◆ SC_TRSR_TX_ATV_Msk

#define SC_TRSR_TX_ATV_Msk (0x1ul << SC_TRSR_TX_ATV_Pos)

SC_T::TRSR: TX_ATV Mask

Definition at line 9103 of file Nano100Series.h.

## ◆ SC_TRSR_TX_ATV_Pos

#define SC_TRSR_TX_ATV_Pos (31)

SC_T::TRSR: TX_ATV Position

Definition at line 9102 of file Nano100Series.h.

## ◆ SC_TRSR_TX_EMPTY_F_Msk

#define SC_TRSR_TX_EMPTY_F_Msk (0x1ul << SC_TRSR_TX_EMPTY_F_Pos)

SC_T::TRSR: TX_EMPTY_F Mask

Definition at line 9076 of file Nano100Series.h.

## ◆ SC_TRSR_TX_EMPTY_F_Pos

#define SC_TRSR_TX_EMPTY_F_Pos (9)

SC_T::TRSR: TX_EMPTY_F Position

Definition at line 9075 of file Nano100Series.h.

## ◆ SC_TRSR_TX_FULL_F_Msk

#define SC_TRSR_TX_FULL_F_Msk (0x1ul << SC_TRSR_TX_FULL_F_Pos)

SC_T::TRSR: TX_FULL_F Mask

Definition at line 9079 of file Nano100Series.h.

## ◆ SC_TRSR_TX_FULL_F_Pos

#define SC_TRSR_TX_FULL_F_Pos (10)

SC_T::TRSR: TX_FULL_F Position

Definition at line 9078 of file Nano100Series.h.

## ◆ SC_TRSR_TX_OVER_ERETRY_Msk

#define SC_TRSR_TX_OVER_ERETRY_Msk (0x1ul << SC_TRSR_TX_OVER_ERETRY_Pos)

SC_T::TRSR: TX_OVER_ERETRY Mask

Definition at line 9100 of file Nano100Series.h.

## ◆ SC_TRSR_TX_OVER_ERETRY_Pos

#define SC_TRSR_TX_OVER_ERETRY_Pos (30)

SC_T::TRSR: TX_OVER_ERETRY Position

Definition at line 9099 of file Nano100Series.h.

## ◆ SC_TRSR_TX_OVER_F_Msk

#define SC_TRSR_TX_OVER_F_Msk (0x1ul << SC_TRSR_TX_OVER_F_Pos)

SC_T::TRSR: TX_OVER_F Mask

Definition at line 9073 of file Nano100Series.h.

## ◆ SC_TRSR_TX_OVER_F_Pos

#define SC_TRSR_TX_OVER_F_Pos (8)

SC_T::TRSR: TX_OVER_F Position

Definition at line 9072 of file Nano100Series.h.

## ◆ SC_TRSR_TX_POINT_F_Msk

#define SC_TRSR_TX_POINT_F_Msk (0x7ul << SC_TRSR_TX_POINT_F_Pos)

SC_T::TRSR: TX_POINT_F Mask

Definition at line 9094 of file Nano100Series.h.

## ◆ SC_TRSR_TX_POINT_F_Pos

#define SC_TRSR_TX_POINT_F_Pos (24)

SC_T::TRSR: TX_POINT_F Position

Definition at line 9093 of file Nano100Series.h.

## ◆ SC_TRSR_TX_REERR_Msk

#define SC_TRSR_TX_REERR_Msk (0x1ul << SC_TRSR_TX_REERR_Pos)

SC_T::TRSR: TX_REERR Mask

Definition at line 9097 of file Nano100Series.h.

## ◆ SC_TRSR_TX_REERR_Pos

#define SC_TRSR_TX_REERR_Pos (29)

SC_T::TRSR: TX_REERR Position

Definition at line 9096 of file Nano100Series.h.

## ◆ SC_UACTL_DATA_LEN_Msk

#define SC_UACTL_DATA_LEN_Msk (0x3ul << SC_UACTL_DATA_LEN_Pos)

SC_T::UACTL: DATA_LEN Mask

Definition at line 9163 of file Nano100Series.h.

## ◆ SC_UACTL_DATA_LEN_Pos

#define SC_UACTL_DATA_LEN_Pos (4)

SC_T::UACTL: DATA_LEN Position

Definition at line 9162 of file Nano100Series.h.

## ◆ SC_UACTL_OPE_Msk

#define SC_UACTL_OPE_Msk (0x1ul << SC_UACTL_OPE_Pos)

SC_T::UACTL: OPE Mask

Definition at line 9169 of file Nano100Series.h.

## ◆ SC_UACTL_OPE_Pos

#define SC_UACTL_OPE_Pos (7)

SC_T::UACTL: OPE Position

Definition at line 9168 of file Nano100Series.h.

## ◆ SC_UACTL_PBDIS_Msk

#define SC_UACTL_PBDIS_Msk (0x1ul << SC_UACTL_PBDIS_Pos)

SC_T::UACTL: PBDIS Mask

Definition at line 9166 of file Nano100Series.h.

## ◆ SC_UACTL_PBDIS_Pos

#define SC_UACTL_PBDIS_Pos (6)

SC_T::UACTL: PBDIS Position

Definition at line 9165 of file Nano100Series.h.

## ◆ SC_UACTL_UA_MODE_EN_Msk

#define SC_UACTL_UA_MODE_EN_Msk (0x1ul << SC_UACTL_UA_MODE_EN_Pos)

SC_T::UACTL: UA_MODE_EN Mask

Definition at line 9160 of file Nano100Series.h.

## ◆ SC_UACTL_UA_MODE_EN_Pos

#define SC_UACTL_UA_MODE_EN_Pos (0)

SC_T::UACTL: UA_MODE_EN Position

Definition at line 9159 of file Nano100Series.h.

## ◆ SPI_CLKDIV_DIVIDER1_Msk

#define SPI_CLKDIV_DIVIDER1_Msk (0xfful << SPI_CLKDIV_DIVIDER1_Pos)

SPI_T::CLKDIV: DIVIDER1 Mask

Definition at line 9658 of file Nano100Series.h.

## ◆ SPI_CLKDIV_DIVIDER1_Pos

#define SPI_CLKDIV_DIVIDER1_Pos (0)

SPI_T::CLKDIV: DIVIDER1 Position

Definition at line 9657 of file Nano100Series.h.

## ◆ SPI_CLKDIV_DIVIDER2_Msk

#define SPI_CLKDIV_DIVIDER2_Msk (0xfful << SPI_CLKDIV_DIVIDER2_Pos)

SPI_T::CLKDIV: DIVIDER2 Mask

Definition at line 9661 of file Nano100Series.h.

## ◆ SPI_CLKDIV_DIVIDER2_Pos

#define SPI_CLKDIV_DIVIDER2_Pos (16)

SPI_T::CLKDIV: DIVIDER2 Position

Definition at line 9660 of file Nano100Series.h.

## ◆ SPI_CTL_CLKP_Msk

#define SPI_CTL_CLKP_Msk (0x1ul << SPI_CTL_CLKP_Pos)

SPI_T::CTL: CLKP Mask

Definition at line 9586 of file Nano100Series.h.

## ◆ SPI_CTL_CLKP_Pos

#define SPI_CTL_CLKP_Pos (11)

SPI_T::CTL: CLKP Position

Definition at line 9585 of file Nano100Series.h.

## ◆ SPI_CTL_DUAL_IO_DIR_Msk

#define SPI_CTL_DUAL_IO_DIR_Msk (0x1ul << SPI_CTL_DUAL_IO_DIR_Pos)

SPI_T::CTL: DUAL_IO_DIR Mask

Definition at line 9610 of file Nano100Series.h.

## ◆ SPI_CTL_DUAL_IO_DIR_Pos

#define SPI_CTL_DUAL_IO_DIR_Pos (28)

SPI_T::CTL: DUAL_IO_DIR Position

Definition at line 9609 of file Nano100Series.h.

## ◆ SPI_CTL_DUAL_IO_EN_Msk

#define SPI_CTL_DUAL_IO_EN_Msk (0x1ul << SPI_CTL_DUAL_IO_EN_Pos)

SPI_T::CTL: DUAL_IO_EN Mask

Definition at line 9613 of file Nano100Series.h.

## ◆ SPI_CTL_DUAL_IO_EN_Pos

#define SPI_CTL_DUAL_IO_EN_Pos (29)

SPI_T::CTL: DUAL_IO_EN Position

Definition at line 9612 of file Nano100Series.h.

## ◆ SPI_CTL_FIFOM_Msk

#define SPI_CTL_FIFOM_Msk (0x1ul << SPI_CTL_FIFOM_Pos)

SPI_T::CTL: FIFOM Mask

Definition at line 9601 of file Nano100Series.h.

## ◆ SPI_CTL_FIFOM_Pos

#define SPI_CTL_FIFOM_Pos (21)

SPI_T::CTL: FIFOM Position

Definition at line 9600 of file Nano100Series.h.

## ◆ SPI_CTL_GO_BUSY_Msk

#define SPI_CTL_GO_BUSY_Msk (0x1ul << SPI_CTL_GO_BUSY_Pos)

SPI_T::CTL: GO_BUSY Mask

Definition at line 9571 of file Nano100Series.h.

## ◆ SPI_CTL_GO_BUSY_Pos

#define SPI_CTL_GO_BUSY_Pos (0)

    @addtogroup SPI_CONST SPI Bit Field Definition
    Constant Definitions for SPI Controller

SPI_T::CTL: GO_BUSY Position

Definition at line 9570 of file Nano100Series.h.

## ◆ SPI_CTL_INTEN_Msk

#define SPI_CTL_INTEN_Msk (0x1ul << SPI_CTL_INTEN_Pos)

SPI_T::CTL: INTEN Mask

Definition at line 9592 of file Nano100Series.h.

## ◆ SPI_CTL_INTEN_Pos

#define SPI_CTL_INTEN_Pos (17)

SPI_T::CTL: INTEN Position

Definition at line 9591 of file Nano100Series.h.

## ◆ SPI_CTL_LSB_Msk

#define SPI_CTL_LSB_Msk (0x1ul << SPI_CTL_LSB_Pos)

SPI_T::CTL: LSB Mask

Definition at line 9583 of file Nano100Series.h.

## ◆ SPI_CTL_LSB_Pos

#define SPI_CTL_LSB_Pos (10)

SPI_T::CTL: LSB Position

Definition at line 9582 of file Nano100Series.h.

## ◆ SPI_CTL_REORDER_Msk

#define SPI_CTL_REORDER_Msk (0x1ul << SPI_CTL_REORDER_Pos)

SPI_T::CTL: REORDER Mask

Definition at line 9598 of file Nano100Series.h.

## ◆ SPI_CTL_REORDER_Pos

#define SPI_CTL_REORDER_Pos (19)

SPI_T::CTL: REORDER Position

Definition at line 9597 of file Nano100Series.h.

## ◆ SPI_CTL_RX_NEG_Msk

#define SPI_CTL_RX_NEG_Msk (0x1ul << SPI_CTL_RX_NEG_Pos)

SPI_T::CTL: RX_NEG Mask

Definition at line 9574 of file Nano100Series.h.

## ◆ SPI_CTL_RX_NEG_Pos

#define SPI_CTL_RX_NEG_Pos (1)

SPI_T::CTL: RX_NEG Position

Definition at line 9573 of file Nano100Series.h.

## ◆ SPI_CTL_SLAVE_Msk

#define SPI_CTL_SLAVE_Msk (0x1ul << SPI_CTL_SLAVE_Pos)

SPI_T::CTL: SLAVE Mask

Definition at line 9595 of file Nano100Series.h.

## ◆ SPI_CTL_SLAVE_Pos

#define SPI_CTL_SLAVE_Pos (18)

SPI_T::CTL: SLAVE Position

Definition at line 9594 of file Nano100Series.h.

## ◆ SPI_CTL_SP_CYCLE_Msk

#define SPI_CTL_SP_CYCLE_Msk (0xful << SPI_CTL_SP_CYCLE_Pos)

SPI_T::CTL: SP_CYCLE Mask

Definition at line 9589 of file Nano100Series.h.

## ◆ SPI_CTL_SP_CYCLE_Pos

#define SPI_CTL_SP_CYCLE_Pos (12)

SPI_T::CTL: SP_CYCLE Position

Definition at line 9588 of file Nano100Series.h.

## ◆ SPI_CTL_TWOB_Msk

#define SPI_CTL_TWOB_Msk (0x1ul << SPI_CTL_TWOB_Pos)

SPI_T::CTL: TWOB Mask

Definition at line 9604 of file Nano100Series.h.

## ◆ SPI_CTL_TWOB_Pos

#define SPI_CTL_TWOB_Pos (22)

SPI_T::CTL: TWOB Position

Definition at line 9603 of file Nano100Series.h.

## ◆ SPI_CTL_TX_BIT_LEN_Msk

#define SPI_CTL_TX_BIT_LEN_Msk (0x1ful << SPI_CTL_TX_BIT_LEN_Pos)

SPI_T::CTL: TX_BIT_LEN Mask

Definition at line 9580 of file Nano100Series.h.

## ◆ SPI_CTL_TX_BIT_LEN_Pos

#define SPI_CTL_TX_BIT_LEN_Pos (3)

SPI_T::CTL: TX_BIT_LEN Position

Definition at line 9579 of file Nano100Series.h.

## ◆ SPI_CTL_TX_NEG_Msk

#define SPI_CTL_TX_NEG_Msk (0x1ul << SPI_CTL_TX_NEG_Pos)

SPI_T::CTL: TX_NEG Mask

Definition at line 9577 of file Nano100Series.h.

## ◆ SPI_CTL_TX_NEG_Pos

#define SPI_CTL_TX_NEG_Pos (2)

SPI_T::CTL: TX_NEG Position

Definition at line 9576 of file Nano100Series.h.

## ◆ SPI_CTL_VARCLK_EN_Msk

#define SPI_CTL_VARCLK_EN_Msk (0x1ul << SPI_CTL_VARCLK_EN_Pos)

SPI_T::CTL: VARCLK_EN Mask

Definition at line 9607 of file Nano100Series.h.

## ◆ SPI_CTL_VARCLK_EN_Pos

#define SPI_CTL_VARCLK_EN_Pos (23)

SPI_T::CTL: VARCLK_EN Position

Definition at line 9606 of file Nano100Series.h.

## ◆ SPI_CTL_WKEUP_EN_Msk

#define SPI_CTL_WKEUP_EN_Msk (0x1ul << SPI_CTL_WKEUP_EN_Pos)

SPI_T::CTL: WKEUP_EN Mask

Definition at line 9616 of file Nano100Series.h.

## ◆ SPI_CTL_WKEUP_EN_Pos

#define SPI_CTL_WKEUP_EN_Pos (31)

SPI_T::CTL: WKEUP_EN Position

Definition at line 9615 of file Nano100Series.h.

## ◆ SPI_DMA_PDMA_RST_Msk

#define SPI_DMA_PDMA_RST_Msk (0x1ul << SPI_DMA_PDMA_RST_Pos)

SPI_T::DMA: PDMA_RST Mask

Definition at line 9709 of file Nano100Series.h.

## ◆ SPI_DMA_PDMA_RST_Pos

#define SPI_DMA_PDMA_RST_Pos (2)

SPI_T::DMA: PDMA_RST Position

Definition at line 9708 of file Nano100Series.h.

## ◆ SPI_DMA_RX_DMA_EN_Msk

#define SPI_DMA_RX_DMA_EN_Msk (0x1ul << SPI_DMA_RX_DMA_EN_Pos)

SPI_T::DMA: RX_DMA_EN Mask

Definition at line 9706 of file Nano100Series.h.

## ◆ SPI_DMA_RX_DMA_EN_Pos

#define SPI_DMA_RX_DMA_EN_Pos (1)

SPI_T::DMA: RX_DMA_EN Position

Definition at line 9705 of file Nano100Series.h.

## ◆ SPI_DMA_TX_DMA_EN_Msk

#define SPI_DMA_TX_DMA_EN_Msk (0x1ul << SPI_DMA_TX_DMA_EN_Pos)

SPI_T::DMA: TX_DMA_EN Mask

Definition at line 9703 of file Nano100Series.h.

## ◆ SPI_DMA_TX_DMA_EN_Pos

#define SPI_DMA_TX_DMA_EN_Pos (0)

SPI_T::DMA: TX_DMA_EN Position

Definition at line 9702 of file Nano100Series.h.

## ◆ SPI_FFCTL_RX_CLR_Msk

#define SPI_FFCTL_RX_CLR_Msk (0x1ul << SPI_FFCTL_RX_CLR_Pos)

SPI_T::FFCTL: RX_CLR Mask

Definition at line 9712 of file Nano100Series.h.

## ◆ SPI_FFCTL_RX_CLR_Pos

#define SPI_FFCTL_RX_CLR_Pos (0)

SPI_T::FFCTL: RX_CLR Position

Definition at line 9711 of file Nano100Series.h.

## ◆ SPI_FFCTL_RX_INTEN_Msk

#define SPI_FFCTL_RX_INTEN_Msk (0x1ul << SPI_FFCTL_RX_INTEN_Pos)

SPI_T::FFCTL: RX_INTEN Mask

Definition at line 9718 of file Nano100Series.h.

## ◆ SPI_FFCTL_RX_INTEN_Pos

#define SPI_FFCTL_RX_INTEN_Pos (2)

SPI_T::FFCTL: RX_INTEN Position

Definition at line 9717 of file Nano100Series.h.

## ◆ SPI_FFCTL_RX_THRESHOLD_Msk

#define SPI_FFCTL_RX_THRESHOLD_Msk (0x7ul << SPI_FFCTL_RX_THRESHOLD_Pos)

SPI_T::FFCTL: RX_THRESHOLD Mask

Definition at line 9730 of file Nano100Series.h.

## ◆ SPI_FFCTL_RX_THRESHOLD_Pos

#define SPI_FFCTL_RX_THRESHOLD_Pos (24)

SPI_T::FFCTL: RX_THRESHOLD Position

Definition at line 9729 of file Nano100Series.h.

## ◆ SPI_FFCTL_RXOVR_INTEN_Msk

#define SPI_FFCTL_RXOVR_INTEN_Msk (0x1ul << SPI_FFCTL_RXOVR_INTEN_Pos)

SPI_T::FFCTL: RXOVR_INTEN Mask

Definition at line 9724 of file Nano100Series.h.

## ◆ SPI_FFCTL_RXOVR_INTEN_Pos

#define SPI_FFCTL_RXOVR_INTEN_Pos (4)

SPI_T::FFCTL: RXOVR_INTEN Position

Definition at line 9723 of file Nano100Series.h.

## ◆ SPI_FFCTL_TIMEOUT_EN_Msk

#define SPI_FFCTL_TIMEOUT_EN_Msk (0x1ul << SPI_FFCTL_TIMEOUT_EN_Pos)

SPI_T::FFCTL: TIMEOUT_EN Mask

Definition at line 9727 of file Nano100Series.h.

## ◆ SPI_FFCTL_TIMEOUT_EN_Pos

#define SPI_FFCTL_TIMEOUT_EN_Pos (7)

SPI_T::FFCTL: TIMEOUT_EN Position

Definition at line 9726 of file Nano100Series.h.

## ◆ SPI_FFCTL_TX_CLR_Msk

#define SPI_FFCTL_TX_CLR_Msk (0x1ul << SPI_FFCTL_TX_CLR_Pos)

SPI_T::FFCTL: TX_CLR Mask

Definition at line 9715 of file Nano100Series.h.

## ◆ SPI_FFCTL_TX_CLR_Pos

#define SPI_FFCTL_TX_CLR_Pos (1)

SPI_T::FFCTL: TX_CLR Position

Definition at line 9714 of file Nano100Series.h.

## ◆ SPI_FFCTL_TX_INTEN_Msk

#define SPI_FFCTL_TX_INTEN_Msk (0x1ul << SPI_FFCTL_TX_INTEN_Pos)

SPI_T::FFCTL: TX_INTEN Mask

Definition at line 9721 of file Nano100Series.h.

## ◆ SPI_FFCTL_TX_INTEN_Pos

#define SPI_FFCTL_TX_INTEN_Pos (3)

SPI_T::FFCTL: TX_INTEN Position

Definition at line 9720 of file Nano100Series.h.

## ◆ SPI_FFCTL_TX_THRESHOLD_Msk

#define SPI_FFCTL_TX_THRESHOLD_Msk (0x7ul << SPI_FFCTL_TX_THRESHOLD_Pos)

SPI_T::FFCTL: TX_THRESHOLD Mask

Definition at line 9733 of file Nano100Series.h.

## ◆ SPI_FFCTL_TX_THRESHOLD_Pos

#define SPI_FFCTL_TX_THRESHOLD_Pos (28)

SPI_T::FFCTL: TX_THRESHOLD Position

Definition at line 9732 of file Nano100Series.h.

## ◆ SPI_RX0_RDATA_Msk

#define SPI_RX0_RDATA_Msk (0xfffffffful << SPI_RX0_RDATA_Pos)

SPI_T::RX0: RDATA Mask

Definition at line 9688 of file Nano100Series.h.

## ◆ SPI_RX0_RDATA_Pos

#define SPI_RX0_RDATA_Pos (0)

SPI_T::RX0: RDATA Position

Definition at line 9687 of file Nano100Series.h.

## ◆ SPI_RX1_RDATA_Msk

#define SPI_RX1_RDATA_Msk (0xfffffffful << SPI_RX1_RDATA_Pos)

SPI_T::RX1: RDATA Mask

Definition at line 9691 of file Nano100Series.h.

## ◆ SPI_RX1_RDATA_Pos

#define SPI_RX1_RDATA_Pos (0)

SPI_T::RX1: RDATA Position

Definition at line 9690 of file Nano100Series.h.

## ◆ SPI_SSR_AUTOSS_Msk

#define SPI_SSR_AUTOSS_Msk (0x1ul << SPI_SSR_AUTOSS_Pos)

SPI_T::SSR: AUTOSS Mask

Definition at line 9670 of file Nano100Series.h.

## ◆ SPI_SSR_AUTOSS_Pos

#define SPI_SSR_AUTOSS_Pos (3)

SPI_T::SSR: AUTOSS Position

Definition at line 9669 of file Nano100Series.h.

## ◆ SPI_SSR_NOSLVSEL_Msk

#define SPI_SSR_NOSLVSEL_Msk (0x1ul << SPI_SSR_NOSLVSEL_Pos)

SPI_T::SSR: NOSLVSEL Mask

Definition at line 9676 of file Nano100Series.h.

## ◆ SPI_SSR_NOSLVSEL_Pos

#define SPI_SSR_NOSLVSEL_Pos (5)

SPI_T::SSR: NOSLVSEL Position

Definition at line 9675 of file Nano100Series.h.

## ◆ SPI_SSR_SLV_ABORT_Msk

#define SPI_SSR_SLV_ABORT_Msk (0x1ul << SPI_SSR_SLV_ABORT_Pos)

SPI_T::SSR: SLV_ABORT Mask

Definition at line 9679 of file Nano100Series.h.

## ◆ SPI_SSR_SLV_ABORT_Pos

#define SPI_SSR_SLV_ABORT_Pos (8)

SPI_T::SSR: SLV_ABORT Position

Definition at line 9678 of file Nano100Series.h.

## ◆ SPI_SSR_SS_INT_OPT_Msk

#define SPI_SSR_SS_INT_OPT_Msk (0x1ul << SPI_SSR_SS_INT_OPT_Pos)

SPI_T::SSR: SS_INT_OPT Mask

Definition at line 9685 of file Nano100Series.h.

## ◆ SPI_SSR_SS_INT_OPT_Pos

#define SPI_SSR_SS_INT_OPT_Pos (16)

SPI_T::SSR: SS_INT_OPT Position

Definition at line 9684 of file Nano100Series.h.

## ◆ SPI_SSR_SS_LTRIG_Msk

#define SPI_SSR_SS_LTRIG_Msk (0x1ul << SPI_SSR_SS_LTRIG_Pos)

SPI_T::SSR: SS_LTRIG Mask

Definition at line 9673 of file Nano100Series.h.

## ◆ SPI_SSR_SS_LTRIG_Pos

#define SPI_SSR_SS_LTRIG_Pos (4)

SPI_T::SSR: SS_LTRIG Position

Definition at line 9672 of file Nano100Series.h.

## ◆ SPI_SSR_SS_LVL_Msk

#define SPI_SSR_SS_LVL_Msk (0x1ul << SPI_SSR_SS_LVL_Pos)

SPI_T::SSR: SS_LVL Mask

Definition at line 9667 of file Nano100Series.h.

## ◆ SPI_SSR_SS_LVL_Pos

#define SPI_SSR_SS_LVL_Pos (2)

SPI_T::SSR: SS_LVL Position

Definition at line 9666 of file Nano100Series.h.

## ◆ SPI_SSR_SSR_Msk

#define SPI_SSR_SSR_Msk (0x3ul << SPI_SSR_SSR_Pos)

SPI_T::SSR: SSR Mask

Definition at line 9664 of file Nano100Series.h.

## ◆ SPI_SSR_SSR_Pos

#define SPI_SSR_SSR_Pos (0)

SPI_T::SSR: SSR Position

Definition at line 9663 of file Nano100Series.h.

## ◆ SPI_SSR_SSTA_INTEN_Msk

#define SPI_SSR_SSTA_INTEN_Msk (0x1ul << SPI_SSR_SSTA_INTEN_Pos)

SPI_T::SSR: SSTA_INTEN Mask

Definition at line 9682 of file Nano100Series.h.

## ◆ SPI_SSR_SSTA_INTEN_Pos

#define SPI_SSR_SSTA_INTEN_Pos (9)

SPI_T::SSR: SSTA_INTEN Position

Definition at line 9681 of file Nano100Series.h.

## ◆ SPI_STATUS_INTSTS_Msk

#define SPI_STATUS_INTSTS_Msk (0x1ul << SPI_STATUS_INTSTS_Pos)

SPI_T::STATUS: INTSTS Mask

Definition at line 9637 of file Nano100Series.h.

## ◆ SPI_STATUS_INTSTS_Pos

#define SPI_STATUS_INTSTS_Pos (7)

SPI_T::STATUS: INTSTS Position

Definition at line 9636 of file Nano100Series.h.

## ◆ SPI_STATUS_LTRIG_FLAG_Msk

#define SPI_STATUS_LTRIG_FLAG_Msk (0x1ul << SPI_STATUS_LTRIG_FLAG_Pos)

SPI_T::STATUS: LTRIG_FLAG Mask

Definition at line 9631 of file Nano100Series.h.

## ◆ SPI_STATUS_LTRIG_FLAG_Pos

#define SPI_STATUS_LTRIG_FLAG_Pos (4)

SPI_T::STATUS: LTRIG_FLAG Position

Definition at line 9630 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_EMPTY_Msk

#define SPI_STATUS_RX_EMPTY_Msk (0x1ul << SPI_STATUS_RX_EMPTY_Pos)

SPI_T::STATUS: RX_EMPTY Mask

Definition at line 9619 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_EMPTY_Pos

#define SPI_STATUS_RX_EMPTY_Pos (0)

SPI_T::STATUS: RX_EMPTY Position

Definition at line 9618 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_FIFO_CNT_Msk

#define SPI_STATUS_RX_FIFO_CNT_Msk (0xful << SPI_STATUS_RX_FIFO_CNT_Pos)

SPI_T::STATUS: RX_FIFO_CNT Mask

Definition at line 9652 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_FIFO_CNT_Pos

#define SPI_STATUS_RX_FIFO_CNT_Pos (16)

SPI_T::STATUS: RX_FIFO_CNT Position

Definition at line 9651 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_FULL_Msk

#define SPI_STATUS_RX_FULL_Msk (0x1ul << SPI_STATUS_RX_FULL_Pos)

SPI_T::STATUS: RX_FULL Mask

Definition at line 9622 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_FULL_Pos

#define SPI_STATUS_RX_FULL_Pos (1)

SPI_T::STATUS: RX_FULL Position

Definition at line 9621 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_OVER_RUN_Msk

#define SPI_STATUS_RX_OVER_RUN_Msk (0x1ul << SPI_STATUS_RX_OVER_RUN_Pos)

SPI_T::STATUS: RX_OVER_RUN Mask

Definition at line 9643 of file Nano100Series.h.

## ◆ SPI_STATUS_RX_OVER_RUN_Pos

#define SPI_STATUS_RX_OVER_RUN_Pos (9)

SPI_T::STATUS: RX_OVER_RUN Position

Definition at line 9642 of file Nano100Series.h.

## ◆ SPI_STATUS_RXINT_STS_Msk

#define SPI_STATUS_RXINT_STS_Msk (0x1ul << SPI_STATUS_RXINT_STS_Pos)

SPI_T::STATUS: RXINT_STS Mask

Definition at line 9640 of file Nano100Series.h.

## ◆ SPI_STATUS_RXINT_STS_Pos

#define SPI_STATUS_RXINT_STS_Pos (8)

SPI_T::STATUS: RXINT_STS Position

Definition at line 9639 of file Nano100Series.h.

## ◆ SPI_STATUS_SLV_START_INTSTS_Msk

#define SPI_STATUS_SLV_START_INTSTS_Msk (0x1ul << SPI_STATUS_SLV_START_INTSTS_Pos)

SPI_T::STATUS: SLV_START_INTSTS Mask

Definition at line 9634 of file Nano100Series.h.

## ◆ SPI_STATUS_SLV_START_INTSTS_Pos

#define SPI_STATUS_SLV_START_INTSTS_Pos (6)

SPI_T::STATUS: SLV_START_INTSTS Position

Definition at line 9633 of file Nano100Series.h.

## ◆ SPI_STATUS_TIME_OUT_STS_Msk

#define SPI_STATUS_TIME_OUT_STS_Msk (0x1ul << SPI_STATUS_TIME_OUT_STS_Pos)

SPI_T::STATUS: TIME_OUT_STS Mask

Definition at line 9649 of file Nano100Series.h.

## ◆ SPI_STATUS_TIME_OUT_STS_Pos

#define SPI_STATUS_TIME_OUT_STS_Pos (12)

SPI_T::STATUS: TIME_OUT_STS Position

Definition at line 9648 of file Nano100Series.h.

## ◆ SPI_STATUS_TX_EMPTY_Msk

#define SPI_STATUS_TX_EMPTY_Msk (0x1ul << SPI_STATUS_TX_EMPTY_Pos)

SPI_T::STATUS: TX_EMPTY Mask

Definition at line 9625 of file Nano100Series.h.

## ◆ SPI_STATUS_TX_EMPTY_Pos

#define SPI_STATUS_TX_EMPTY_Pos (2)

SPI_T::STATUS: TX_EMPTY Position

Definition at line 9624 of file Nano100Series.h.

## ◆ SPI_STATUS_TX_FIFO_CNT_Msk

#define SPI_STATUS_TX_FIFO_CNT_Msk (0xful << SPI_STATUS_TX_FIFO_CNT_Pos)

SPI_T::STATUS: TX_FIFO_CNT Mask

Definition at line 9655 of file Nano100Series.h.

## ◆ SPI_STATUS_TX_FIFO_CNT_Pos

#define SPI_STATUS_TX_FIFO_CNT_Pos (20)

SPI_T::STATUS: TX_FIFO_CNT Position

Definition at line 9654 of file Nano100Series.h.

## ◆ SPI_STATUS_TX_FULL_Msk

#define SPI_STATUS_TX_FULL_Msk (0x1ul << SPI_STATUS_TX_FULL_Pos)

SPI_T::STATUS: TX_FULL Mask

Definition at line 9628 of file Nano100Series.h.

## ◆ SPI_STATUS_TX_FULL_Pos

#define SPI_STATUS_TX_FULL_Pos (3)

SPI_T::STATUS: TX_FULL Position

Definition at line 9627 of file Nano100Series.h.

## ◆ SPI_STATUS_TXINT_STS_Msk

#define SPI_STATUS_TXINT_STS_Msk (0x1ul << SPI_STATUS_TXINT_STS_Pos)

SPI_T::STATUS: TXINT_STS Mask

Definition at line 9646 of file Nano100Series.h.

## ◆ SPI_STATUS_TXINT_STS_Pos

#define SPI_STATUS_TXINT_STS_Pos (10)

SPI_T::STATUS: TXINT_STS Position

Definition at line 9645 of file Nano100Series.h.

## ◆ SPI_TX0_TDATA_Msk

#define SPI_TX0_TDATA_Msk (0xfffffffful << SPI_TX0_TDATA_Pos)

SPI_T::TX0: TDATA Mask

Definition at line 9694 of file Nano100Series.h.

## ◆ SPI_TX0_TDATA_Pos

#define SPI_TX0_TDATA_Pos (0)

SPI_T::TX0: TDATA Position

Definition at line 9693 of file Nano100Series.h.

## ◆ SPI_TX1_TDATA_Msk

#define SPI_TX1_TDATA_Msk (0xfffffffful << SPI_TX1_TDATA_Pos)

SPI_T::TX1: TDATA Mask

Definition at line 9697 of file Nano100Series.h.

## ◆ SPI_TX1_TDATA_Pos

#define SPI_TX1_TDATA_Pos (0)

SPI_T::TX1: TDATA Position

Definition at line 9696 of file Nano100Series.h.

## ◆ SPI_VARCLK_VARCLK_Msk

#define SPI_VARCLK_VARCLK_Msk (0xfffffffful << SPI_VARCLK_VARCLK_Pos)

SPI_T::VARCLK: VARCLK Mask

Definition at line 9700 of file Nano100Series.h.

## ◆ SPI_VARCLK_VARCLK_Pos

#define SPI_VARCLK_VARCLK_Pos (0)

SPI_T::VARCLK: VARCLK Position

Definition at line 9699 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD17_EN_Msk

#define SYS_BODCTL_BOD17_EN_Msk (0x1ul << SYS_BODCTL_BOD17_EN_Pos)

SYS_T::BODCTL: BOD17_EN Mask

Definition at line 3314 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD17_EN_Pos

#define SYS_BODCTL_BOD17_EN_Pos (0)

SYS_T::BODCTL: BOD17_EN Position

Definition at line 3313 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD17_INT_EN_Msk

#define SYS_BODCTL_BOD17_INT_EN_Msk (0x1ul << SYS_BODCTL_BOD17_INT_EN_Pos)

SYS_T::BODCTL: BOD17_INT_EN Mask

Definition at line 3332 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD17_INT_EN_Pos

#define SYS_BODCTL_BOD17_INT_EN_Pos (8)

SYS_T::BODCTL: BOD17_INT_EN Position

Definition at line 3331 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD17_RST_EN_Msk

#define SYS_BODCTL_BOD17_RST_EN_Msk (0x1ul << SYS_BODCTL_BOD17_RST_EN_Pos)

SYS_T::BODCTL: BOD17_RST_EN Mask

Definition at line 3323 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD17_RST_EN_Pos

#define SYS_BODCTL_BOD17_RST_EN_Pos (4)

SYS_T::BODCTL: BOD17_RST_EN Position

Definition at line 3322 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD20_EN_Msk

#define SYS_BODCTL_BOD20_EN_Msk (0x1ul << SYS_BODCTL_BOD20_EN_Pos)

SYS_T::BODCTL: BOD20_EN Mask

Definition at line 3317 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD20_EN_Pos

#define SYS_BODCTL_BOD20_EN_Pos (1)

SYS_T::BODCTL: BOD20_EN Position

Definition at line 3316 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD20_INT_EN_Msk

#define SYS_BODCTL_BOD20_INT_EN_Msk (0x1ul << SYS_BODCTL_BOD20_INT_EN_Pos)

SYS_T::BODCTL: BOD20_INT_EN Mask

Definition at line 3335 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD20_INT_EN_Pos

#define SYS_BODCTL_BOD20_INT_EN_Pos (9)

SYS_T::BODCTL: BOD20_INT_EN Position

Definition at line 3334 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD20_RST_EN_Msk

#define SYS_BODCTL_BOD20_RST_EN_Msk (0x1ul << SYS_BODCTL_BOD20_RST_EN_Pos)

SYS_T::BODCTL: BOD20_RST_EN Mask

Definition at line 3326 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD20_RST_EN_Pos

#define SYS_BODCTL_BOD20_RST_EN_Pos (5)

SYS_T::BODCTL: BOD20_RST_EN Position

Definition at line 3325 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD25_EN_Msk

#define SYS_BODCTL_BOD25_EN_Msk (0x1ul << SYS_BODCTL_BOD25_EN_Pos)

SYS_T::BODCTL: BOD25_EN Mask

Definition at line 3320 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD25_EN_Pos

#define SYS_BODCTL_BOD25_EN_Pos (2)

SYS_T::BODCTL: BOD25_EN Position

Definition at line 3319 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD25_INT_EN_Msk

#define SYS_BODCTL_BOD25_INT_EN_Msk (0x1ul << SYS_BODCTL_BOD25_INT_EN_Pos)

SYS_T::BODCTL: BOD25_INT_EN Mask

Definition at line 3338 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD25_INT_EN_Pos

#define SYS_BODCTL_BOD25_INT_EN_Pos (10)

SYS_T::BODCTL: BOD25_INT_EN Position

Definition at line 3337 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD25_RST_EN_Msk

#define SYS_BODCTL_BOD25_RST_EN_Msk (0x1ul << SYS_BODCTL_BOD25_RST_EN_Pos)

SYS_T::BODCTL: BOD25_RST_EN Mask

Definition at line 3329 of file Nano100Series.h.

## ◆ SYS_BODCTL_BOD25_RST_EN_Pos

#define SYS_BODCTL_BOD25_RST_EN_Pos (6)

SYS_T::BODCTL: BOD25_RST_EN Position

Definition at line 3328 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD17_drop_Msk

#define SYS_BODSTS_BOD17_drop_Msk (0x1ul << SYS_BODSTS_BOD17_drop_Pos)

SYS_T::BODSTS: BOD17_drop Mask

Definition at line 3344 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD17_drop_Pos

#define SYS_BODSTS_BOD17_drop_Pos (1)

SYS_T::BODSTS: BOD17_drop Position

Definition at line 3343 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD17_rise_Msk

#define SYS_BODSTS_BOD17_rise_Msk (0x1ul << SYS_BODSTS_BOD17_rise_Pos)

SYS_T::BODSTS: BOD17_rise Mask

Definition at line 3353 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD17_rise_Pos

#define SYS_BODSTS_BOD17_rise_Pos (4)

SYS_T::BODSTS: BOD17_rise Position

Definition at line 3352 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD20_drop_Msk

#define SYS_BODSTS_BOD20_drop_Msk (0x1ul << SYS_BODSTS_BOD20_drop_Pos)

SYS_T::BODSTS: BOD20_drop Mask

Definition at line 3347 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD20_drop_Pos

#define SYS_BODSTS_BOD20_drop_Pos (2)

SYS_T::BODSTS: BOD20_drop Position

Definition at line 3346 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD20_rise_Msk

#define SYS_BODSTS_BOD20_rise_Msk (0x1ul << SYS_BODSTS_BOD20_rise_Pos)

SYS_T::BODSTS: BOD20_rise Mask

Definition at line 3356 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD20_rise_Pos

#define SYS_BODSTS_BOD20_rise_Pos (5)

SYS_T::BODSTS: BOD20_rise Position

Definition at line 3355 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD25_drop_Msk

#define SYS_BODSTS_BOD25_drop_Msk (0x1ul << SYS_BODSTS_BOD25_drop_Pos)

SYS_T::BODSTS: BOD25_drop Mask

Definition at line 3350 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD25_drop_Pos

#define SYS_BODSTS_BOD25_drop_Pos (3)

SYS_T::BODSTS: BOD25_drop Position

Definition at line 3349 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD25_rise_Msk

#define SYS_BODSTS_BOD25_rise_Msk (0x1ul << SYS_BODSTS_BOD25_rise_Pos)

SYS_T::BODSTS: BOD25_rise Mask

Definition at line 3359 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD25_rise_Pos

#define SYS_BODSTS_BOD25_rise_Pos (6)

SYS_T::BODSTS: BOD25_rise Position

Definition at line 3358 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD_INT_Msk

#define SYS_BODSTS_BOD_INT_Msk (0x1ul << SYS_BODSTS_BOD_INT_Pos)

SYS_T::BODSTS: BOD_INT Mask

Definition at line 3341 of file Nano100Series.h.

## ◆ SYS_BODSTS_BOD_INT_Pos

#define SYS_BODSTS_BOD_INT_Pos (0)

SYS_T::BODSTS: BOD_INT Position

Definition at line 3340 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_CHIP_RST_Msk

#define SYS_IPRST_CTL1_CHIP_RST_Msk (0x1ul << SYS_IPRST_CTL1_CHIP_RST_Pos)

SYS_T::IPRST_CTL1: CHIP_RST Mask

Definition at line 2972 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_CHIP_RST_Pos

#define SYS_IPRST_CTL1_CHIP_RST_Pos (0)

SYS_T::IPRST_CTL1: CHIP_RST Position

Definition at line 2971 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_CPU_RST_Msk

#define SYS_IPRST_CTL1_CPU_RST_Msk (0x1ul << SYS_IPRST_CTL1_CPU_RST_Pos)

SYS_T::IPRST_CTL1: CPU_RST Mask

Definition at line 2975 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_CPU_RST_Pos

#define SYS_IPRST_CTL1_CPU_RST_Pos (1)

SYS_T::IPRST_CTL1: CPU_RST Position

Definition at line 2974 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_DMA_RST_Msk

#define SYS_IPRST_CTL1_DMA_RST_Msk (0x1ul << SYS_IPRST_CTL1_DMA_RST_Pos)

SYS_T::IPRST_CTL1: DMA_RST Mask

Definition at line 2978 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_DMA_RST_Pos

#define SYS_IPRST_CTL1_DMA_RST_Pos (2)

SYS_T::IPRST_CTL1: DMA_RST Position

Definition at line 2977 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_EBI_RST_Msk

#define SYS_IPRST_CTL1_EBI_RST_Msk (0x1ul << SYS_IPRST_CTL1_EBI_RST_Pos)

SYS_T::IPRST_CTL1: EBI_RST Mask

Definition at line 2981 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL1_EBI_RST_Pos

#define SYS_IPRST_CTL1_EBI_RST_Pos (3)

SYS_T::IPRST_CTL1: EBI_RST Position

Definition at line 2980 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_ADC_RST_Msk

#define SYS_IPRST_CTL2_ADC_RST_Msk (0x1ul << SYS_IPRST_CTL2_ADC_RST_Pos)

SYS_T::IPRST_CTL2: ADC_RST Mask

Definition at line 3038 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_ADC_RST_Pos

#define SYS_IPRST_CTL2_ADC_RST_Pos (28)

SYS_T::IPRST_CTL2: ADC_RST Position

Definition at line 3037 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_DAC_RST_Msk

#define SYS_IPRST_CTL2_DAC_RST_Msk (0x1ul << SYS_IPRST_CTL2_DAC_RST_Pos)

SYS_T::IPRST_CTL2: DAC_RST Mask

Definition at line 3029 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_DAC_RST_Pos

#define SYS_IPRST_CTL2_DAC_RST_Pos (25)

SYS_T::IPRST_CTL2: DAC_RST Position

Definition at line 3028 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_GPIO_RST_Msk

#define SYS_IPRST_CTL2_GPIO_RST_Msk (0x1ul << SYS_IPRST_CTL2_GPIO_RST_Pos)

SYS_T::IPRST_CTL2: GPIO_RST Mask

Definition at line 2984 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_GPIO_RST_Pos

#define SYS_IPRST_CTL2_GPIO_RST_Pos (1)

SYS_T::IPRST_CTL2: GPIO_RST Position

Definition at line 2983 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_I2C0_RST_Msk

#define SYS_IPRST_CTL2_I2C0_RST_Msk (0x1ul << SYS_IPRST_CTL2_I2C0_RST_Pos)

SYS_T::IPRST_CTL2: I2C0_RST Mask

Definition at line 3002 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_I2C0_RST_Pos

#define SYS_IPRST_CTL2_I2C0_RST_Pos (8)

SYS_T::IPRST_CTL2: I2C0_RST Position

Definition at line 3001 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_I2C1_RST_Msk

#define SYS_IPRST_CTL2_I2C1_RST_Msk (0x1ul << SYS_IPRST_CTL2_I2C1_RST_Pos)

SYS_T::IPRST_CTL2: I2C1_RST Mask

Definition at line 3005 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_I2C1_RST_Pos

#define SYS_IPRST_CTL2_I2C1_RST_Pos (9)

SYS_T::IPRST_CTL2: I2C1_RST Position

Definition at line 3004 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_I2S_RST_Msk

#define SYS_IPRST_CTL2_I2S_RST_Msk (0x1ul << SYS_IPRST_CTL2_I2S_RST_Pos)

SYS_T::IPRST_CTL2: I2S_RST Mask

Definition at line 3041 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_I2S_RST_Pos

#define SYS_IPRST_CTL2_I2S_RST_Pos (29)

SYS_T::IPRST_CTL2: I2S_RST Position

Definition at line 3040 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_LCD_RST_Msk

#define SYS_IPRST_CTL2_LCD_RST_Msk (0x1ul << SYS_IPRST_CTL2_LCD_RST_Pos)

SYS_T::IPRST_CTL2: LCD_RST Mask

Definition at line 3032 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_LCD_RST_Pos

#define SYS_IPRST_CTL2_LCD_RST_Pos (26)

SYS_T::IPRST_CTL2: LCD_RST Position

Definition at line 3031 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_PWM0_RST_Msk

#define SYS_IPRST_CTL2_PWM0_RST_Msk (0x1ul << SYS_IPRST_CTL2_PWM0_RST_Pos)

SYS_T::IPRST_CTL2: PWM0_RST Mask

Definition at line 3023 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_PWM0_RST_Pos

#define SYS_IPRST_CTL2_PWM0_RST_Pos (20)

SYS_T::IPRST_CTL2: PWM0_RST Position

Definition at line 3022 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_PWM1_RST_Msk

#define SYS_IPRST_CTL2_PWM1_RST_Msk (0x1ul << SYS_IPRST_CTL2_PWM1_RST_Pos)

SYS_T::IPRST_CTL2: PWM1_RST Mask

Definition at line 3026 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_PWM1_RST_Pos

#define SYS_IPRST_CTL2_PWM1_RST_Pos (21)

SYS_T::IPRST_CTL2: PWM1_RST Position

Definition at line 3025 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SC0_RST_Msk

#define SYS_IPRST_CTL2_SC0_RST_Msk (0x1ul << SYS_IPRST_CTL2_SC0_RST_Pos)

SYS_T::IPRST_CTL2: SC0_RST Mask

Definition at line 3044 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SC0_RST_Pos

#define SYS_IPRST_CTL2_SC0_RST_Pos (30)

SYS_T::IPRST_CTL2: SC0_RST Position

Definition at line 3043 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SC1_RST_Msk

#define SYS_IPRST_CTL2_SC1_RST_Msk (0x1ul << SYS_IPRST_CTL2_SC1_RST_Pos)

SYS_T::IPRST_CTL2: SC1_RST Mask

Definition at line 3047 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SC1_RST_Pos

#define SYS_IPRST_CTL2_SC1_RST_Pos (31)

SYS_T::IPRST_CTL2: SC1_RST Position

Definition at line 3046 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SC2_RST_Msk

#define SYS_IPRST_CTL2_SC2_RST_Msk (0x1ul << SYS_IPRST_CTL2_SC2_RST_Pos)

SYS_T::IPRST_CTL2: SC2_RST Mask

Definition at line 2999 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SC2_RST_Pos

#define SYS_IPRST_CTL2_SC2_RST_Pos (7)

SYS_T::IPRST_CTL2: SC2_RST Position

Definition at line 2998 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SPI0_RST_Msk

#define SYS_IPRST_CTL2_SPI0_RST_Msk (0x1ul << SYS_IPRST_CTL2_SPI0_RST_Pos)

SYS_T::IPRST_CTL2: SPI0_RST Mask

Definition at line 3008 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SPI0_RST_Pos

#define SYS_IPRST_CTL2_SPI0_RST_Pos (12)

SYS_T::IPRST_CTL2: SPI0_RST Position

Definition at line 3007 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SPI1_RST_Msk

#define SYS_IPRST_CTL2_SPI1_RST_Msk (0x1ul << SYS_IPRST_CTL2_SPI1_RST_Pos)

SYS_T::IPRST_CTL2: SPI1_RST Mask

Definition at line 3011 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SPI1_RST_Pos

#define SYS_IPRST_CTL2_SPI1_RST_Pos (13)

SYS_T::IPRST_CTL2: SPI1_RST Position

Definition at line 3010 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SPI2_RST_Msk

#define SYS_IPRST_CTL2_SPI2_RST_Msk (0x1ul << SYS_IPRST_CTL2_SPI2_RST_Pos)

SYS_T::IPRST_CTL2: SPI2_RST Mask

Definition at line 3014 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_SPI2_RST_Pos

#define SYS_IPRST_CTL2_SPI2_RST_Pos (14)

SYS_T::IPRST_CTL2: SPI2_RST Position

Definition at line 3013 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR0_RST_Msk

#define SYS_IPRST_CTL2_TMR0_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR0_RST_Pos)

SYS_T::IPRST_CTL2: TMR0_RST Mask

Definition at line 2987 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR0_RST_Pos

#define SYS_IPRST_CTL2_TMR0_RST_Pos (2)

SYS_T::IPRST_CTL2: TMR0_RST Position

Definition at line 2986 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR1_RST_Msk

#define SYS_IPRST_CTL2_TMR1_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR1_RST_Pos)

SYS_T::IPRST_CTL2: TMR1_RST Mask

Definition at line 2990 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR1_RST_Pos

#define SYS_IPRST_CTL2_TMR1_RST_Pos (3)

SYS_T::IPRST_CTL2: TMR1_RST Position

Definition at line 2989 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR2_RST_Msk

#define SYS_IPRST_CTL2_TMR2_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR2_RST_Pos)

SYS_T::IPRST_CTL2: TMR2_RST Mask

Definition at line 2993 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR2_RST_Pos

#define SYS_IPRST_CTL2_TMR2_RST_Pos (4)

SYS_T::IPRST_CTL2: TMR2_RST Position

Definition at line 2992 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR3_RST_Msk

#define SYS_IPRST_CTL2_TMR3_RST_Msk (0x1ul << SYS_IPRST_CTL2_TMR3_RST_Pos)

SYS_T::IPRST_CTL2: TMR3_RST Mask

Definition at line 2996 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_TMR3_RST_Pos

#define SYS_IPRST_CTL2_TMR3_RST_Pos (5)

SYS_T::IPRST_CTL2: TMR3_RST Position

Definition at line 2995 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_UART0_RST_Msk

#define SYS_IPRST_CTL2_UART0_RST_Msk (0x1ul << SYS_IPRST_CTL2_UART0_RST_Pos)

SYS_T::IPRST_CTL2: UART0_RST Mask

Definition at line 3017 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_UART0_RST_Pos

#define SYS_IPRST_CTL2_UART0_RST_Pos (16)

SYS_T::IPRST_CTL2: UART0_RST Position

Definition at line 3016 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_UART1_RST_Msk

#define SYS_IPRST_CTL2_UART1_RST_Msk (0x1ul << SYS_IPRST_CTL2_UART1_RST_Pos)

SYS_T::IPRST_CTL2: UART1_RST Mask

Definition at line 3020 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_UART1_RST_Pos

#define SYS_IPRST_CTL2_UART1_RST_Pos (17)

SYS_T::IPRST_CTL2: UART1_RST Position

Definition at line 3019 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_USBD_RST_Msk

#define SYS_IPRST_CTL2_USBD_RST_Msk (0x1ul << SYS_IPRST_CTL2_USBD_RST_Pos)

SYS_T::IPRST_CTL2: USBD_RST Mask

Definition at line 3035 of file Nano100Series.h.

## ◆ SYS_IPRST_CTL2_USBD_RST_Pos

#define SYS_IPRST_CTL2_USBD_RST_Pos (27)

SYS_T::IPRST_CTL2: USBD_RST Position

Definition at line 3034 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_ERR_STOP_Msk

#define SYS_IRCTRIMCTL_ERR_STOP_Msk (0x1ul << SYS_IRCTRIMCTL_ERR_STOP_Pos)

SYS_T::IRCTRIMCTL: ERR_STOP Mask

Definition at line 3383 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_ERR_STOP_Pos

#define SYS_IRCTRIMCTL_ERR_STOP_Pos (8)

SYS_T::IRCTRIMCTL: ERR_STOP Position

Definition at line 3382 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_LOOP_Msk

#define SYS_IRCTRIMCTL_TRIM_LOOP_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

SYS_T::IRCTRIMCTL: TRIM_LOOP Mask

Definition at line 3377 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_LOOP_Pos

#define SYS_IRCTRIMCTL_TRIM_LOOP_Pos (4)

SYS_T::IRCTRIMCTL: TRIM_LOOP Position

Definition at line 3376 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Msk

#define SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos)

SYS_T::IRCTRIMCTL: TRIM_RETRY_CNT Mask

Definition at line 3380 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos

#define SYS_IRCTRIMCTL_TRIM_RETRY_CNT_Pos (6)

SYS_T::IRCTRIMCTL: TRIM_RETRY_CNT Position

Definition at line 3379 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_SEL_Msk

#define SYS_IRCTRIMCTL_TRIM_SEL_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_SEL_Pos)

SYS_T::IRCTRIMCTL: TRIM_SEL Mask

Definition at line 3374 of file Nano100Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_SEL_Pos

#define SYS_IRCTRIMCTL_TRIM_SEL_Pos (0)

SYS_T::IRCTRIMCTL: TRIM_SEL Position

Definition at line 3373 of file Nano100Series.h.

## ◆ SYS_IRCTRIMIEN_32K_ERR_IEN_Msk

#define SYS_IRCTRIMIEN_32K_ERR_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_32K_ERR_IEN_Pos)

SYS_T::IRCTRIMIEN: 32K_ERR_IEN Mask

Definition at line 3389 of file Nano100Series.h.

## ◆ SYS_IRCTRIMIEN_32K_ERR_IEN_Pos

#define SYS_IRCTRIMIEN_32K_ERR_IEN_Pos (2)

SYS_T::IRCTRIMIEN: 32K_ERR_IEN Position

Definition at line 3388 of file Nano100Series.h.

## ◆ SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk

#define SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos)

SYS_T::IRCTRIMIEN: TRIM_FAIL_IEN Mask

Definition at line 3386 of file Nano100Series.h.

## ◆ SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos

#define SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos (1)

SYS_T::IRCTRIMIEN: TRIM_FAIL_IEN Position

Definition at line 3385 of file Nano100Series.h.

## ◆ SYS_IRCTRIMINT_32K_ERR_INT_Msk

#define SYS_IRCTRIMINT_32K_ERR_INT_Msk (0x1ul << SYS_IRCTRIMINT_32K_ERR_INT_Pos)

SYS_T::IRCTRIMINT: 32K_ERR_INT Mask

Definition at line 3398 of file Nano100Series.h.

## ◆ SYS_IRCTRIMINT_32K_ERR_INT_Pos

#define SYS_IRCTRIMINT_32K_ERR_INT_Pos (2)

SYS_T::IRCTRIMINT: 32K_ERR_INT Position

Definition at line 3397 of file Nano100Series.h.

## ◆ SYS_IRCTRIMINT_FREQ_LOCK_Msk

#define SYS_IRCTRIMINT_FREQ_LOCK_Msk (0x1ul << SYS_IRCTRIMINT_FREQ_LOCK_Pos)

SYS_T::IRCTRIMINT: FREQ_LOCK Mask

Definition at line 3392 of file Nano100Series.h.

## ◆ SYS_IRCTRIMINT_FREQ_LOCK_Pos

#define SYS_IRCTRIMINT_FREQ_LOCK_Pos (0)

SYS_T::IRCTRIMINT: FREQ_LOCK Position

Definition at line 3391 of file Nano100Series.h.

## ◆ SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk

#define SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk (0x1ul << SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos)

SYS_T::IRCTRIMINT: TRIM_FAIL_INT Mask

Definition at line 3395 of file Nano100Series.h.

## ◆ SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos

#define SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos (1)

SYS_T::IRCTRIMINT: TRIM_FAIL_INT Position

Definition at line 3394 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_Msk

#define SYS_PA_H_MFP_PA10_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA10_MFP_Pos)

SYS_T::PA_H_MFP: PA10_MFP Mask

Definition at line 3083 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_Pos

#define SYS_PA_H_MFP_PA10_MFP_Pos (8)

SYS_T::PA_H_MFP: PA10_MFP Position

Definition at line 3082 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_Msk

#define SYS_PA_H_MFP_PA11_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA11_MFP_Pos)

SYS_T::PA_H_MFP: PA11_MFP Mask

Definition at line 3086 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_Pos

#define SYS_PA_H_MFP_PA11_MFP_Pos (12)

SYS_T::PA_H_MFP: PA11_MFP Position

Definition at line 3085 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_Msk

#define SYS_PA_H_MFP_PA12_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA12_MFP_Pos)

SYS_T::PA_H_MFP: PA12_MFP Mask

Definition at line 3089 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_Pos

#define SYS_PA_H_MFP_PA12_MFP_Pos (16)

SYS_T::PA_H_MFP: PA12_MFP Position

Definition at line 3088 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_Msk

#define SYS_PA_H_MFP_PA13_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA13_MFP_Pos)

SYS_T::PA_H_MFP: PA13_MFP Mask

Definition at line 3092 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_Pos

#define SYS_PA_H_MFP_PA13_MFP_Pos (20)

SYS_T::PA_H_MFP: PA13_MFP Position

Definition at line 3091 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_Msk

#define SYS_PA_H_MFP_PA14_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA14_MFP_Pos)

SYS_T::PA_H_MFP: PA14_MFP Mask

Definition at line 3095 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_Pos

#define SYS_PA_H_MFP_PA14_MFP_Pos (24)

SYS_T::PA_H_MFP: PA14_MFP Position

Definition at line 3094 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_Msk

#define SYS_PA_H_MFP_PA15_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA15_MFP_Pos)

SYS_T::PA_H_MFP: PA15_MFP Mask

Definition at line 3098 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_Pos

#define SYS_PA_H_MFP_PA15_MFP_Pos (28)

SYS_T::PA_H_MFP: PA15_MFP Position

Definition at line 3097 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_Msk

#define SYS_PA_H_MFP_PA8_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA8_MFP_Pos)

SYS_T::PA_H_MFP: PA8_MFP Mask

Definition at line 3077 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_Pos

#define SYS_PA_H_MFP_PA8_MFP_Pos (0)

SYS_T::PA_H_MFP: PA8_MFP Position

Definition at line 3076 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_Msk

#define SYS_PA_H_MFP_PA9_MFP_Msk (0x7ul << SYS_PA_H_MFP_PA9_MFP_Pos)

SYS_T::PA_H_MFP: PA9_MFP Mask

Definition at line 3080 of file Nano100Series.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_Pos

#define SYS_PA_H_MFP_PA9_MFP_Pos (4)

SYS_T::PA_H_MFP: PA9_MFP Position

Definition at line 3079 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_Msk

#define SYS_PA_L_MFP_PA0_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA0_MFP_Pos)

SYS_T::PA_L_MFP: PA0_MFP Mask

Definition at line 3053 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_Pos

#define SYS_PA_L_MFP_PA0_MFP_Pos (0)

SYS_T::PA_L_MFP: PA0_MFP Position

Definition at line 3052 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_Msk

#define SYS_PA_L_MFP_PA1_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA1_MFP_Pos)

SYS_T::PA_L_MFP: PA1_MFP Mask

Definition at line 3056 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_Pos

#define SYS_PA_L_MFP_PA1_MFP_Pos (4)

SYS_T::PA_L_MFP: PA1_MFP Position

Definition at line 3055 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_Msk

#define SYS_PA_L_MFP_PA2_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA2_MFP_Pos)

SYS_T::PA_L_MFP: PA2_MFP Mask

Definition at line 3059 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_Pos

#define SYS_PA_L_MFP_PA2_MFP_Pos (8)

SYS_T::PA_L_MFP: PA2_MFP Position

Definition at line 3058 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_Msk

#define SYS_PA_L_MFP_PA3_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA3_MFP_Pos)

SYS_T::PA_L_MFP: PA3_MFP Mask

Definition at line 3062 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_Pos

#define SYS_PA_L_MFP_PA3_MFP_Pos (12)

SYS_T::PA_L_MFP: PA3_MFP Position

Definition at line 3061 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_Msk

#define SYS_PA_L_MFP_PA4_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA4_MFP_Pos)

SYS_T::PA_L_MFP: PA4_MFP Mask

Definition at line 3065 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_Pos

#define SYS_PA_L_MFP_PA4_MFP_Pos (16)

SYS_T::PA_L_MFP: PA4_MFP Position

Definition at line 3064 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_Msk

#define SYS_PA_L_MFP_PA5_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA5_MFP_Pos)

SYS_T::PA_L_MFP: PA5_MFP Mask

Definition at line 3068 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_Pos

#define SYS_PA_L_MFP_PA5_MFP_Pos (20)

SYS_T::PA_L_MFP: PA5_MFP Position

Definition at line 3067 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_Msk

#define SYS_PA_L_MFP_PA6_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA6_MFP_Pos)

SYS_T::PA_L_MFP: PA6_MFP Mask

Definition at line 3071 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_Pos

#define SYS_PA_L_MFP_PA6_MFP_Pos (24)

SYS_T::PA_L_MFP: PA6_MFP Position

Definition at line 3070 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_Msk

#define SYS_PA_L_MFP_PA7_MFP_Msk (0x7ul << SYS_PA_L_MFP_PA7_MFP_Pos)

SYS_T::PA_L_MFP: PA7_MFP Mask

Definition at line 3074 of file Nano100Series.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_Pos

#define SYS_PA_L_MFP_PA7_MFP_Pos (28)

SYS_T::PA_L_MFP: PA7_MFP Position

Definition at line 3073 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_Msk

#define SYS_PB_H_MFP_PB10_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB10_MFP_Pos)

SYS_T::PB_H_MFP: PB10_MFP Mask

Definition at line 3131 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_Pos

#define SYS_PB_H_MFP_PB10_MFP_Pos (8)

SYS_T::PB_H_MFP: PB10_MFP Position

Definition at line 3130 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_Msk

#define SYS_PB_H_MFP_PB11_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB11_MFP_Pos)

SYS_T::PB_H_MFP: PB11_MFP Mask

Definition at line 3134 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_Pos

#define SYS_PB_H_MFP_PB11_MFP_Pos (12)

SYS_T::PB_H_MFP: PB11_MFP Position

Definition at line 3133 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_Msk

#define SYS_PB_H_MFP_PB12_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB12_MFP_Pos)

SYS_T::PB_H_MFP: PB12_MFP Mask

Definition at line 3137 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_Pos

#define SYS_PB_H_MFP_PB12_MFP_Pos (16)

SYS_T::PB_H_MFP: PB12_MFP Position

Definition at line 3136 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_Msk

#define SYS_PB_H_MFP_PB13_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB13_MFP_Pos)

SYS_T::PB_H_MFP: PB13_MFP Mask

Definition at line 3140 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_Pos

#define SYS_PB_H_MFP_PB13_MFP_Pos (20)

SYS_T::PB_H_MFP: PB13_MFP Position

Definition at line 3139 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_Msk

#define SYS_PB_H_MFP_PB14_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB14_MFP_Pos)

SYS_T::PB_H_MFP: PB14_MFP Mask

Definition at line 3143 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_Pos

#define SYS_PB_H_MFP_PB14_MFP_Pos (24)

SYS_T::PB_H_MFP: PB14_MFP Position

Definition at line 3142 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_Msk

#define SYS_PB_H_MFP_PB15_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB15_MFP_Pos)

SYS_T::PB_H_MFP: PB15_MFP Mask

Definition at line 3146 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_Pos

#define SYS_PB_H_MFP_PB15_MFP_Pos (28)

SYS_T::PB_H_MFP: PB15_MFP Position

Definition at line 3145 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_Msk

#define SYS_PB_H_MFP_PB8_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB8_MFP_Pos)

SYS_T::PB_H_MFP: PB8_MFP Mask

Definition at line 3125 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_Pos

#define SYS_PB_H_MFP_PB8_MFP_Pos (0)

SYS_T::PB_H_MFP: PB8_MFP Position

Definition at line 3124 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_Msk

#define SYS_PB_H_MFP_PB9_MFP_Msk (0x7ul << SYS_PB_H_MFP_PB9_MFP_Pos)

SYS_T::PB_H_MFP: PB9_MFP Mask

Definition at line 3128 of file Nano100Series.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_Pos

#define SYS_PB_H_MFP_PB9_MFP_Pos (4)

SYS_T::PB_H_MFP: PB9_MFP Position

Definition at line 3127 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_Msk

#define SYS_PB_L_MFP_PB0_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB0_MFP_Pos)

SYS_T::PB_L_MFP: PB0_MFP Mask

Definition at line 3101 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_Pos

#define SYS_PB_L_MFP_PB0_MFP_Pos (0)

SYS_T::PB_L_MFP: PB0_MFP Position

Definition at line 3100 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_Msk

#define SYS_PB_L_MFP_PB1_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB1_MFP_Pos)

SYS_T::PB_L_MFP: PB1_MFP Mask

Definition at line 3104 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_Pos

#define SYS_PB_L_MFP_PB1_MFP_Pos (4)

SYS_T::PB_L_MFP: PB1_MFP Position

Definition at line 3103 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_Msk

#define SYS_PB_L_MFP_PB2_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB2_MFP_Pos)

SYS_T::PB_L_MFP: PB2_MFP Mask

Definition at line 3107 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_Pos

#define SYS_PB_L_MFP_PB2_MFP_Pos (8)

SYS_T::PB_L_MFP: PB2_MFP Position

Definition at line 3106 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_Msk

#define SYS_PB_L_MFP_PB3_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB3_MFP_Pos)

SYS_T::PB_L_MFP: PB3_MFP Mask

Definition at line 3110 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_Pos

#define SYS_PB_L_MFP_PB3_MFP_Pos (12)

SYS_T::PB_L_MFP: PB3_MFP Position

Definition at line 3109 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_Msk

#define SYS_PB_L_MFP_PB4_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB4_MFP_Pos)

SYS_T::PB_L_MFP: PB4_MFP Mask

Definition at line 3113 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_Pos

#define SYS_PB_L_MFP_PB4_MFP_Pos (16)

SYS_T::PB_L_MFP: PB4_MFP Position

Definition at line 3112 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_Msk

#define SYS_PB_L_MFP_PB5_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB5_MFP_Pos)

SYS_T::PB_L_MFP: PB5_MFP Mask

Definition at line 3116 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_Pos

#define SYS_PB_L_MFP_PB5_MFP_Pos (20)

SYS_T::PB_L_MFP: PB5_MFP Position

Definition at line 3115 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_Msk

#define SYS_PB_L_MFP_PB6_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB6_MFP_Pos)

SYS_T::PB_L_MFP: PB6_MFP Mask

Definition at line 3119 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_Pos

#define SYS_PB_L_MFP_PB6_MFP_Pos (24)

SYS_T::PB_L_MFP: PB6_MFP Position

Definition at line 3118 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_Msk

#define SYS_PB_L_MFP_PB7_MFP_Msk (0x7ul << SYS_PB_L_MFP_PB7_MFP_Pos)

SYS_T::PB_L_MFP: PB7_MFP Mask

Definition at line 3122 of file Nano100Series.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_Pos

#define SYS_PB_L_MFP_PB7_MFP_Pos (28)

SYS_T::PB_L_MFP: PB7_MFP Position

Definition at line 3121 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_Msk

#define SYS_PC_H_MFP_PC10_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC10_MFP_Pos)

SYS_T::PC_H_MFP: PC10_MFP Mask

Definition at line 3179 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_Pos

#define SYS_PC_H_MFP_PC10_MFP_Pos (8)

SYS_T::PC_H_MFP: PC10_MFP Position

Definition at line 3178 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_Msk

#define SYS_PC_H_MFP_PC11_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC11_MFP_Pos)

SYS_T::PC_H_MFP: PC11_MFP Mask

Definition at line 3182 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_Pos

#define SYS_PC_H_MFP_PC11_MFP_Pos (12)

SYS_T::PC_H_MFP: PC11_MFP Position

Definition at line 3181 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_Msk

#define SYS_PC_H_MFP_PC12_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC12_MFP_Pos)

SYS_T::PC_H_MFP: PC12_MFP Mask

Definition at line 3185 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_Pos

#define SYS_PC_H_MFP_PC12_MFP_Pos (16)

SYS_T::PC_H_MFP: PC12_MFP Position

Definition at line 3184 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_Msk

#define SYS_PC_H_MFP_PC13_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC13_MFP_Pos)

SYS_T::PC_H_MFP: PC13_MFP Mask

Definition at line 3188 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_Pos

#define SYS_PC_H_MFP_PC13_MFP_Pos (20)

SYS_T::PC_H_MFP: PC13_MFP Position

Definition at line 3187 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_Msk

#define SYS_PC_H_MFP_PC14_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC14_MFP_Pos)

SYS_T::PC_H_MFP: PC14_MFP Mask

Definition at line 3191 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_Pos

#define SYS_PC_H_MFP_PC14_MFP_Pos (24)

SYS_T::PC_H_MFP: PC14_MFP Position

Definition at line 3190 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_Msk

#define SYS_PC_H_MFP_PC15_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC15_MFP_Pos)

SYS_T::PC_H_MFP: PC15_MFP Mask

Definition at line 3194 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_Pos

#define SYS_PC_H_MFP_PC15_MFP_Pos (28)

SYS_T::PC_H_MFP: PC15_MFP Position

Definition at line 3193 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_Msk

#define SYS_PC_H_MFP_PC8_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC8_MFP_Pos)

SYS_T::PC_H_MFP: PC8_MFP Mask

Definition at line 3173 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_Pos

#define SYS_PC_H_MFP_PC8_MFP_Pos (0)

SYS_T::PC_H_MFP: PC8_MFP Position

Definition at line 3172 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_Msk

#define SYS_PC_H_MFP_PC9_MFP_Msk (0x7ul << SYS_PC_H_MFP_PC9_MFP_Pos)

SYS_T::PC_H_MFP: PC9_MFP Mask

Definition at line 3176 of file Nano100Series.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_Pos

#define SYS_PC_H_MFP_PC9_MFP_Pos (4)

SYS_T::PC_H_MFP: PC9_MFP Position

Definition at line 3175 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_Msk

#define SYS_PC_L_MFP_PC0_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC0_MFP_Pos)

SYS_T::PC_L_MFP: PC0_MFP Mask

Definition at line 3149 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_Pos

#define SYS_PC_L_MFP_PC0_MFP_Pos (0)

SYS_T::PC_L_MFP: PC0_MFP Position

Definition at line 3148 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_Msk

#define SYS_PC_L_MFP_PC1_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC1_MFP_Pos)

SYS_T::PC_L_MFP: PC1_MFP Mask

Definition at line 3152 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_Pos

#define SYS_PC_L_MFP_PC1_MFP_Pos (4)

SYS_T::PC_L_MFP: PC1_MFP Position

Definition at line 3151 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_Msk

#define SYS_PC_L_MFP_PC2_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC2_MFP_Pos)

SYS_T::PC_L_MFP: PC2_MFP Mask

Definition at line 3155 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_Pos

#define SYS_PC_L_MFP_PC2_MFP_Pos (8)

SYS_T::PC_L_MFP: PC2_MFP Position

Definition at line 3154 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_Msk

#define SYS_PC_L_MFP_PC3_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC3_MFP_Pos)

SYS_T::PC_L_MFP: PC3_MFP Mask

Definition at line 3158 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_Pos

#define SYS_PC_L_MFP_PC3_MFP_Pos (12)

SYS_T::PC_L_MFP: PC3_MFP Position

Definition at line 3157 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_Msk

#define SYS_PC_L_MFP_PC4_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC4_MFP_Pos)

SYS_T::PC_L_MFP: PC4_MFP Mask

Definition at line 3161 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_Pos

#define SYS_PC_L_MFP_PC4_MFP_Pos (16)

SYS_T::PC_L_MFP: PC4_MFP Position

Definition at line 3160 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_Msk

#define SYS_PC_L_MFP_PC5_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC5_MFP_Pos)

SYS_T::PC_L_MFP: PC5_MFP Mask

Definition at line 3164 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_Pos

#define SYS_PC_L_MFP_PC5_MFP_Pos (20)

SYS_T::PC_L_MFP: PC5_MFP Position

Definition at line 3163 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_Msk

#define SYS_PC_L_MFP_PC6_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC6_MFP_Pos)

SYS_T::PC_L_MFP: PC6_MFP Mask

Definition at line 3167 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_Pos

#define SYS_PC_L_MFP_PC6_MFP_Pos (24)

SYS_T::PC_L_MFP: PC6_MFP Position

Definition at line 3166 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_Msk

#define SYS_PC_L_MFP_PC7_MFP_Msk (0x7ul << SYS_PC_L_MFP_PC7_MFP_Pos)

SYS_T::PC_L_MFP: PC7_MFP Mask

Definition at line 3170 of file Nano100Series.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_Pos

#define SYS_PC_L_MFP_PC7_MFP_Pos (28)

SYS_T::PC_L_MFP: PC7_MFP Position

Definition at line 3169 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_Msk

#define SYS_PD_H_MFP_PD10_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD10_MFP_Pos)

SYS_T::PD_H_MFP: PD10_MFP Mask

Definition at line 3227 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_Pos

#define SYS_PD_H_MFP_PD10_MFP_Pos (8)

SYS_T::PD_H_MFP: PD10_MFP Position

Definition at line 3226 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_Msk

#define SYS_PD_H_MFP_PD11_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD11_MFP_Pos)

SYS_T::PD_H_MFP: PD11_MFP Mask

Definition at line 3230 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_Pos

#define SYS_PD_H_MFP_PD11_MFP_Pos (12)

SYS_T::PD_H_MFP: PD11_MFP Position

Definition at line 3229 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_Msk

#define SYS_PD_H_MFP_PD12_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD12_MFP_Pos)

SYS_T::PD_H_MFP: PD12_MFP Mask

Definition at line 3233 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_Pos

#define SYS_PD_H_MFP_PD12_MFP_Pos (16)

SYS_T::PD_H_MFP: PD12_MFP Position

Definition at line 3232 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_Msk

#define SYS_PD_H_MFP_PD13_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD13_MFP_Pos)

SYS_T::PD_H_MFP: PD13_MFP Mask

Definition at line 3236 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_Pos

#define SYS_PD_H_MFP_PD13_MFP_Pos (20)

SYS_T::PD_H_MFP: PD13_MFP Position

Definition at line 3235 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD14_MFP_Msk

#define SYS_PD_H_MFP_PD14_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD14_MFP_Pos)

SYS_T::PD_H_MFP: PD14_MFP Mask

Definition at line 3239 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD14_MFP_Pos

#define SYS_PD_H_MFP_PD14_MFP_Pos (24)

SYS_T::PD_H_MFP: PD14_MFP Position

Definition at line 3238 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD15_MFP_Msk

#define SYS_PD_H_MFP_PD15_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD15_MFP_Pos)

SYS_T::PD_H_MFP: PD15_MFP Mask

Definition at line 3242 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD15_MFP_Pos

#define SYS_PD_H_MFP_PD15_MFP_Pos (28)

SYS_T::PD_H_MFP: PD15_MFP Position

Definition at line 3241 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_Msk

#define SYS_PD_H_MFP_PD8_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD8_MFP_Pos)

SYS_T::PD_H_MFP: PD8_MFP Mask

Definition at line 3221 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_Pos

#define SYS_PD_H_MFP_PD8_MFP_Pos (0)

SYS_T::PD_H_MFP: PD8_MFP Position

Definition at line 3220 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_Msk

#define SYS_PD_H_MFP_PD9_MFP_Msk (0x7ul << SYS_PD_H_MFP_PD9_MFP_Pos)

SYS_T::PD_H_MFP: PD9_MFP Mask

Definition at line 3224 of file Nano100Series.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_Pos

#define SYS_PD_H_MFP_PD9_MFP_Pos (4)

SYS_T::PD_H_MFP: PD9_MFP Position

Definition at line 3223 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_Msk

#define SYS_PD_L_MFP_PD0_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD0_MFP_Pos)

SYS_T::PD_L_MFP: PD0_MFP Mask

Definition at line 3197 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_Pos

#define SYS_PD_L_MFP_PD0_MFP_Pos (0)

SYS_T::PD_L_MFP: PD0_MFP Position

Definition at line 3196 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_Msk

#define SYS_PD_L_MFP_PD1_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD1_MFP_Pos)

SYS_T::PD_L_MFP: PD1_MFP Mask

Definition at line 3200 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_Pos

#define SYS_PD_L_MFP_PD1_MFP_Pos (4)

SYS_T::PD_L_MFP: PD1_MFP Position

Definition at line 3199 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_Msk

#define SYS_PD_L_MFP_PD2_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD2_MFP_Pos)

SYS_T::PD_L_MFP: PD2_MFP Mask

Definition at line 3203 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_Pos

#define SYS_PD_L_MFP_PD2_MFP_Pos (8)

SYS_T::PD_L_MFP: PD2_MFP Position

Definition at line 3202 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_Msk

#define SYS_PD_L_MFP_PD3_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD3_MFP_Pos)

SYS_T::PD_L_MFP: PD3_MFP Mask

Definition at line 3206 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_Pos

#define SYS_PD_L_MFP_PD3_MFP_Pos (12)

SYS_T::PD_L_MFP: PD3_MFP Position

Definition at line 3205 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_Msk

#define SYS_PD_L_MFP_PD4_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD4_MFP_Pos)

SYS_T::PD_L_MFP: PD4_MFP Mask

Definition at line 3209 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_Pos

#define SYS_PD_L_MFP_PD4_MFP_Pos (16)

SYS_T::PD_L_MFP: PD4_MFP Position

Definition at line 3208 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_Msk

#define SYS_PD_L_MFP_PD5_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD5_MFP_Pos)

SYS_T::PD_L_MFP: PD5_MFP Mask

Definition at line 3212 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_Pos

#define SYS_PD_L_MFP_PD5_MFP_Pos (20)

SYS_T::PD_L_MFP: PD5_MFP Position

Definition at line 3211 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_Msk

#define SYS_PD_L_MFP_PD6_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD6_MFP_Pos)

SYS_T::PD_L_MFP: PD6_MFP Mask

Definition at line 3215 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_Pos

#define SYS_PD_L_MFP_PD6_MFP_Pos (24)

SYS_T::PD_L_MFP: PD6_MFP Position

Definition at line 3214 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_Msk

#define SYS_PD_L_MFP_PD7_MFP_Msk (0x7ul << SYS_PD_L_MFP_PD7_MFP_Pos)

SYS_T::PD_L_MFP: PD7_MFP Mask

Definition at line 3218 of file Nano100Series.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_Pos

#define SYS_PD_L_MFP_PD7_MFP_Pos (28)

SYS_T::PD_L_MFP: PD7_MFP Position

Definition at line 3217 of file Nano100Series.h.

## ◆ SYS_PDID_PDID_Msk

#define SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)

SYS_T::PDID: PDID Mask

Definition at line 2951 of file Nano100Series.h.

## ◆ SYS_PDID_PDID_Pos

#define SYS_PDID_PDID_Pos (0)

    @addtogroup SYS_CONST SYS Bit Field Definition
    Constant Definitions for SYS Controller

SYS_T::PDID: PDID Position

Definition at line 2950 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE10_MFP_Msk

#define SYS_PE_H_MFP_PE10_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE10_MFP_Pos)

SYS_T::PE_H_MFP: PE10_MFP Mask

Definition at line 3275 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE10_MFP_Pos

#define SYS_PE_H_MFP_PE10_MFP_Pos (8)

SYS_T::PE_H_MFP: PE10_MFP Position

Definition at line 3274 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE11_MFP_Msk

#define SYS_PE_H_MFP_PE11_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE11_MFP_Pos)

SYS_T::PE_H_MFP: PE11_MFP Mask

Definition at line 3278 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE11_MFP_Pos

#define SYS_PE_H_MFP_PE11_MFP_Pos (12)

SYS_T::PE_H_MFP: PE11_MFP Position

Definition at line 3277 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE12_MFP_Msk

#define SYS_PE_H_MFP_PE12_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE12_MFP_Pos)

SYS_T::PE_H_MFP: PE12_MFP Mask

Definition at line 3281 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE12_MFP_Pos

#define SYS_PE_H_MFP_PE12_MFP_Pos (16)

SYS_T::PE_H_MFP: PE12_MFP Position

Definition at line 3280 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE13_MFP_Msk

#define SYS_PE_H_MFP_PE13_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE13_MFP_Pos)

SYS_T::PE_H_MFP: PE13_MFP Mask

Definition at line 3284 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE13_MFP_Pos

#define SYS_PE_H_MFP_PE13_MFP_Pos (20)

SYS_T::PE_H_MFP: PE13_MFP Position

Definition at line 3283 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE14_MFP_Msk

#define SYS_PE_H_MFP_PE14_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE14_MFP_Pos)

SYS_T::PE_H_MFP: PE14_MFP Mask

Definition at line 3287 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE14_MFP_Pos

#define SYS_PE_H_MFP_PE14_MFP_Pos (24)

SYS_T::PE_H_MFP: PE14_MFP Position

Definition at line 3286 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE15_MFP_Msk

#define SYS_PE_H_MFP_PE15_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE15_MFP_Pos)

SYS_T::PE_H_MFP: PE15_MFP Mask

Definition at line 3290 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE15_MFP_Pos

#define SYS_PE_H_MFP_PE15_MFP_Pos (28)

SYS_T::PE_H_MFP: PE15_MFP Position

Definition at line 3289 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_Msk

#define SYS_PE_H_MFP_PE8_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE8_MFP_Pos)

SYS_T::PE_H_MFP: PE8_MFP Mask

Definition at line 3269 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_Pos

#define SYS_PE_H_MFP_PE8_MFP_Pos (0)

SYS_T::PE_H_MFP: PE8_MFP Position

Definition at line 3268 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_Msk

#define SYS_PE_H_MFP_PE9_MFP_Msk (0x7ul << SYS_PE_H_MFP_PE9_MFP_Pos)

SYS_T::PE_H_MFP: PE9_MFP Mask

Definition at line 3272 of file Nano100Series.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_Pos

#define SYS_PE_H_MFP_PE9_MFP_Pos (4)

SYS_T::PE_H_MFP: PE9_MFP Position

Definition at line 3271 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_Msk

#define SYS_PE_L_MFP_PE0_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE0_MFP_Pos)

SYS_T::PE_L_MFP: PE0_MFP Mask

Definition at line 3245 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_Pos

#define SYS_PE_L_MFP_PE0_MFP_Pos (0)

SYS_T::PE_L_MFP: PE0_MFP Position

Definition at line 3244 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_Msk

#define SYS_PE_L_MFP_PE1_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE1_MFP_Pos)

SYS_T::PE_L_MFP: PE1_MFP Mask

Definition at line 3248 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_Pos

#define SYS_PE_L_MFP_PE1_MFP_Pos (4)

SYS_T::PE_L_MFP: PE1_MFP Position

Definition at line 3247 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE2_MFP_Msk

#define SYS_PE_L_MFP_PE2_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE2_MFP_Pos)

SYS_T::PE_L_MFP: PE2_MFP Mask

Definition at line 3251 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE2_MFP_Pos

#define SYS_PE_L_MFP_PE2_MFP_Pos (8)

SYS_T::PE_L_MFP: PE2_MFP Position

Definition at line 3250 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE3_MFP_Msk

#define SYS_PE_L_MFP_PE3_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE3_MFP_Pos)

SYS_T::PE_L_MFP: PE3_MFP Mask

Definition at line 3254 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE3_MFP_Pos

#define SYS_PE_L_MFP_PE3_MFP_Pos (12)

SYS_T::PE_L_MFP: PE3_MFP Position

Definition at line 3253 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE4_MFP_Msk

#define SYS_PE_L_MFP_PE4_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE4_MFP_Pos)

SYS_T::PE_L_MFP: PE4_MFP Mask

Definition at line 3257 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE4_MFP_Pos

#define SYS_PE_L_MFP_PE4_MFP_Pos (16)

SYS_T::PE_L_MFP: PE4_MFP Position

Definition at line 3256 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE5_MFP_Msk

#define SYS_PE_L_MFP_PE5_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE5_MFP_Pos)

SYS_T::PE_L_MFP: PE5_MFP Mask

Definition at line 3260 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE5_MFP_Pos

#define SYS_PE_L_MFP_PE5_MFP_Pos (20)

SYS_T::PE_L_MFP: PE5_MFP Position

Definition at line 3259 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE6_MFP_Msk

#define SYS_PE_L_MFP_PE6_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE6_MFP_Pos)

SYS_T::PE_L_MFP: PE6_MFP Mask

Definition at line 3263 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE6_MFP_Pos

#define SYS_PE_L_MFP_PE6_MFP_Pos (24)

SYS_T::PE_L_MFP: PE6_MFP Position

Definition at line 3262 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE7_MFP_Msk

#define SYS_PE_L_MFP_PE7_MFP_Msk (0x7ul << SYS_PE_L_MFP_PE7_MFP_Pos)

SYS_T::PE_L_MFP: PE7_MFP Mask

Definition at line 3266 of file Nano100Series.h.

## ◆ SYS_PE_L_MFP_PE7_MFP_Pos

#define SYS_PE_L_MFP_PE7_MFP_Pos (28)

SYS_T::PE_L_MFP: PE7_MFP Position

Definition at line 3265 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_Msk

#define SYS_PF_L_MFP_PF0_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF0_MFP_Pos)

SYS_T::PF_L_MFP: PF0_MFP Mask

Definition at line 3293 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_Pos

#define SYS_PF_L_MFP_PF0_MFP_Pos (0)

SYS_T::PF_L_MFP: PF0_MFP Position

Definition at line 3292 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_Msk

#define SYS_PF_L_MFP_PF1_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF1_MFP_Pos)

SYS_T::PF_L_MFP: PF1_MFP Mask

Definition at line 3296 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_Pos

#define SYS_PF_L_MFP_PF1_MFP_Pos (4)

SYS_T::PF_L_MFP: PF1_MFP Position

Definition at line 3295 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_Msk

#define SYS_PF_L_MFP_PF2_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF2_MFP_Pos)

SYS_T::PF_L_MFP: PF2_MFP Mask

Definition at line 3299 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_Pos

#define SYS_PF_L_MFP_PF2_MFP_Pos (8)

SYS_T::PF_L_MFP: PF2_MFP Position

Definition at line 3298 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_Msk

#define SYS_PF_L_MFP_PF3_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF3_MFP_Pos)

SYS_T::PF_L_MFP: PF3_MFP Mask

Definition at line 3302 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_Pos

#define SYS_PF_L_MFP_PF3_MFP_Pos (12)

SYS_T::PF_L_MFP: PF3_MFP Position

Definition at line 3301 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_Msk

#define SYS_PF_L_MFP_PF4_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF4_MFP_Pos)

SYS_T::PF_L_MFP: PF4_MFP Mask

Definition at line 3305 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_Pos

#define SYS_PF_L_MFP_PF4_MFP_Pos (16)

SYS_T::PF_L_MFP: PF4_MFP Position

Definition at line 3304 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_Msk

#define SYS_PF_L_MFP_PF5_MFP_Msk (0x7ul << SYS_PF_L_MFP_PF5_MFP_Pos)

SYS_T::PF_L_MFP: PF5_MFP Mask

Definition at line 3308 of file Nano100Series.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_Pos

#define SYS_PF_L_MFP_PF5_MFP_Pos (20)

SYS_T::PF_L_MFP: PF5_MFP Position

Definition at line 3307 of file Nano100Series.h.

## ◆ SYS_PORCTL_POR_DIS_CODE_Msk

#define SYS_PORCTL_POR_DIS_CODE_Msk (0xfffful << SYS_PORCTL_POR_DIS_CODE_Pos)

SYS_T::PORCTL: POR_DIS_CODE Mask

Definition at line 3311 of file Nano100Series.h.

## ◆ SYS_PORCTL_POR_DIS_CODE_Pos

#define SYS_PORCTL_POR_DIS_CODE_Pos (0)

SYS_T::PORCTL: POR_DIS_CODE Position

Definition at line 3310 of file Nano100Series.h.

## ◆ SYS_RegLockAddr_RegUnLock_Msk

#define SYS_RegLockAddr_RegUnLock_Msk (0x1ul << SYS_RegLockAddr_RegUnLock_Pos)

SYS_T::RegLockAddr: RegUnLock Mask

Definition at line 3401 of file Nano100Series.h.

## ◆ SYS_RegLockAddr_RegUnLock_Pos

#define SYS_RegLockAddr_RegUnLock_Pos (0)

SYS_T::RegLockAddr: RegUnLock Position

Definition at line 3400 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_BOD_Msk

#define SYS_RST_SRC_RSTS_BOD_Msk (0x1ul << SYS_RST_SRC_RSTS_BOD_Pos)

SYS_T::RST_SRC: RSTS_BOD Mask

Definition at line 2963 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_BOD_Pos

#define SYS_RST_SRC_RSTS_BOD_Pos (4)

SYS_T::RST_SRC: RSTS_BOD Position

Definition at line 2962 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_CPU_Msk

#define SYS_RST_SRC_RSTS_CPU_Msk (0x1ul << SYS_RST_SRC_RSTS_CPU_Pos)

SYS_T::RST_SRC: RSTS_CPU Mask

Definition at line 2969 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_CPU_Pos

#define SYS_RST_SRC_RSTS_CPU_Pos (7)

SYS_T::RST_SRC: RSTS_CPU Position

Definition at line 2968 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_PAD_Msk

#define SYS_RST_SRC_RSTS_PAD_Msk (0x1ul << SYS_RST_SRC_RSTS_PAD_Pos)

SYS_T::RST_SRC: RSTS_PAD Mask

Definition at line 2957 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_PAD_Pos

#define SYS_RST_SRC_RSTS_PAD_Pos (1)

SYS_T::RST_SRC: RSTS_PAD Position

Definition at line 2956 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_POR_Msk

#define SYS_RST_SRC_RSTS_POR_Msk (0x1ul << SYS_RST_SRC_RSTS_POR_Pos)

SYS_T::RST_SRC: RSTS_POR Mask

Definition at line 2954 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_POR_Pos

#define SYS_RST_SRC_RSTS_POR_Pos (0)

SYS_T::RST_SRC: RSTS_POR Position

Definition at line 2953 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_SYS_Msk

#define SYS_RST_SRC_RSTS_SYS_Msk (0x1ul << SYS_RST_SRC_RSTS_SYS_Pos)

SYS_T::RST_SRC: RSTS_SYS_T::Mask

Definition at line 2966 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_SYS_Pos

#define SYS_RST_SRC_RSTS_SYS_Pos (5)

SYS_T::RST_SRC: RSTS_SYS_T::Position

Definition at line 2965 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_WDT_Msk

#define SYS_RST_SRC_RSTS_WDT_Msk (0x1ul << SYS_RST_SRC_RSTS_WDT_Pos)

SYS_T::RST_SRC: RSTS_WDT Mask

Definition at line 2960 of file Nano100Series.h.

## ◆ SYS_RST_SRC_RSTS_WDT_Pos

#define SYS_RST_SRC_RSTS_WDT_Pos (2)

SYS_T::RST_SRC: RSTS_WDT Position

Definition at line 2959 of file Nano100Series.h.

## ◆ SYS_TEMPCTL_VTEMP_EN_Msk

#define SYS_TEMPCTL_VTEMP_EN_Msk (0x1ul << SYS_TEMPCTL_VTEMP_EN_Pos)

SYS_T::TEMPCTL: VTEMP_EN Mask

Definition at line 3050 of file Nano100Series.h.

## ◆ SYS_TEMPCTL_VTEMP_EN_Pos

#define SYS_TEMPCTL_VTEMP_EN_Pos (0)

SYS_T::TEMPCTL: VTEMP_EN Position

Definition at line 3049 of file Nano100Series.h.

## ◆ SYS_VREFCTL_BGP_EN_Msk

#define SYS_VREFCTL_BGP_EN_Msk (0x1ul << SYS_VREFCTL_BGP_EN_Pos)

SYS_T::VREFCTL: BGP_EN Mask

Definition at line 3362 of file Nano100Series.h.

## ◆ SYS_VREFCTL_BGP_EN_Pos

#define SYS_VREFCTL_BGP_EN_Pos (0)

SYS_T::VREFCTL: BGP_EN Position

Definition at line 3361 of file Nano100Series.h.

## ◆ SYS_VREFCTL_EXT_MODE_Msk

#define SYS_VREFCTL_EXT_MODE_Msk (0x1ul << SYS_VREFCTL_EXT_MODE_Pos)

SYS_T::VREFCTL: EXT_MODE Mask

Definition at line 3371 of file Nano100Series.h.

## ◆ SYS_VREFCTL_EXT_MODE_Pos

#define SYS_VREFCTL_EXT_MODE_Pos (3)

SYS_T::VREFCTL: EXT_MODE Position

Definition at line 3370 of file Nano100Series.h.

## ◆ SYS_VREFCTL_REG_EN_Msk

#define SYS_VREFCTL_REG_EN_Msk (0x1ul << SYS_VREFCTL_REG_EN_Pos)

SYS_T::VREFCTL: REG_EN Mask

Definition at line 3365 of file Nano100Series.h.

## ◆ SYS_VREFCTL_REG_EN_Pos

#define SYS_VREFCTL_REG_EN_Pos (1)

SYS_T::VREFCTL: REG_EN Position

Definition at line 3364 of file Nano100Series.h.

## ◆ SYS_VREFCTL_SEL25_Msk

#define SYS_VREFCTL_SEL25_Msk (0x1ul << SYS_VREFCTL_SEL25_Pos)

SYS_T::VREFCTL: SEL25 Mask

Definition at line 3368 of file Nano100Series.h.

## ◆ SYS_VREFCTL_SEL25_Pos

#define SYS_VREFCTL_SEL25_Pos (2)

SYS_T::VREFCTL: SEL25 Position

Definition at line 3367 of file Nano100Series.h.

## ◆ TIMER_CMPR_TMR_CMP_Msk

#define TIMER_CMPR_TMR_CMP_Msk (0xfffffful << TIMER_CMPR_TMR_CMP_Pos)

TIMER_T::CMPR: TMR_CMP Mask

Definition at line 10059 of file Nano100Series.h.

## ◆ TIMER_CMPR_TMR_CMP_Pos

#define TIMER_CMPR_TMR_CMP_Pos (0)

TIMER_T::CMPR: TMR_CMP Position

Definition at line 10058 of file Nano100Series.h.

## ◆ TIMER_CTL_ADC_TEEN_Msk

#define TIMER_CTL_ADC_TEEN_Msk (0x1ul << TIMER_CTL_ADC_TEEN_Pos)

TIMER_T::CTL: ADC_TEEN Mask

Definition at line 10017 of file Nano100Series.h.

## ◆ TIMER_CTL_ADC_TEEN_Pos

#define TIMER_CTL_ADC_TEEN_Pos (8)

TIMER_T::CTL: ADC_TEEN Position

Definition at line 10016 of file Nano100Series.h.

## ◆ TIMER_CTL_CAP_TRG_EN_Msk

#define TIMER_CTL_CAP_TRG_EN_Msk (0x1ul << TIMER_CTL_CAP_TRG_EN_Pos)

TIMER_T::CTL: CAP_TRG_EN Mask

Definition at line 10026 of file Nano100Series.h.

## ◆ TIMER_CTL_CAP_TRG_EN_Pos

#define TIMER_CTL_CAP_TRG_EN_Pos (11)

TIMER_T::CTL: CAP_TRG_EN Position

Definition at line 10025 of file Nano100Series.h.

## ◆ TIMER_CTL_DAC_TEEN_Msk

#define TIMER_CTL_DAC_TEEN_Msk (0x1ul << TIMER_CTL_DAC_TEEN_Pos)

TIMER_T::CTL: DAC_TEEN Mask

Definition at line 10020 of file Nano100Series.h.

## ◆ TIMER_CTL_DAC_TEEN_Pos

#define TIMER_CTL_DAC_TEEN_Pos (9)

TIMER_T::CTL: DAC_TEEN Position

Definition at line 10019 of file Nano100Series.h.

## ◆ TIMER_CTL_DBGACK_EN_Msk

#define TIMER_CTL_DBGACK_EN_Msk (0x1ul << TIMER_CTL_DBGACK_EN_Pos)

TIMER_T::CTL: DBGACK_EN Mask

Definition at line 10008 of file Nano100Series.h.

## ◆ TIMER_CTL_DBGACK_EN_Pos

#define TIMER_CTL_DBGACK_EN_Pos (3)

TIMER_T::CTL: DBGACK_EN Position

Definition at line 10007 of file Nano100Series.h.

## ◆ TIMER_CTL_EVENT_EDGE_Msk

#define TIMER_CTL_EVENT_EDGE_Msk (0x1ul << TIMER_CTL_EVENT_EDGE_Pos)

TIMER_T::CTL: EVENT_EDGE Mask

Definition at line 10032 of file Nano100Series.h.

## ◆ TIMER_CTL_EVENT_EDGE_Pos

#define TIMER_CTL_EVENT_EDGE_Pos (13)

TIMER_T::CTL: EVENT_EDGE Position

Definition at line 10031 of file Nano100Series.h.

## ◆ TIMER_CTL_EVENT_EN_Msk

#define TIMER_CTL_EVENT_EN_Msk (0x1ul << TIMER_CTL_EVENT_EN_Pos)

TIMER_T::CTL: EVENT_EN Mask

Definition at line 10029 of file Nano100Series.h.

## ◆ TIMER_CTL_EVENT_EN_Pos

#define TIMER_CTL_EVENT_EN_Pos (12)

TIMER_T::CTL: EVENT_EN Position

Definition at line 10028 of file Nano100Series.h.

## ◆ TIMER_CTL_EVNT_DEB_EN_Msk

#define TIMER_CTL_EVNT_DEB_EN_Msk (0x1ul << TIMER_CTL_EVNT_DEB_EN_Pos)

TIMER_T::CTL: EVNT_DEB_EN Mask

Definition at line 10035 of file Nano100Series.h.

## ◆ TIMER_CTL_EVNT_DEB_EN_Pos

#define TIMER_CTL_EVNT_DEB_EN_Pos (14)

TIMER_T::CTL: EVNT_DEB_EN Position

Definition at line 10034 of file Nano100Series.h.

## ◆ TIMER_CTL_INTR_TRG_EN_Msk

#define TIMER_CTL_INTR_TRG_EN_Msk (0x1ul << TIMER_CTL_INTR_TRG_EN_Pos)

TIMER_T::CTL: INTR_TRG_EN Mask

Definition at line 10053 of file Nano100Series.h.

## ◆ TIMER_CTL_INTR_TRG_EN_Pos

#define TIMER_CTL_INTR_TRG_EN_Pos (24)

TIMER_T::CTL: INTR_TRG_EN Position

Definition at line 10052 of file Nano100Series.h.

## ◆ TIMER_CTL_MODE_SEL_Msk

#define TIMER_CTL_MODE_SEL_Msk (0x3ul << TIMER_CTL_MODE_SEL_Pos)

TIMER_T::CTL: MODE_SEL Mask

Definition at line 10011 of file Nano100Series.h.

## ◆ TIMER_CTL_MODE_SEL_Pos

#define TIMER_CTL_MODE_SEL_Pos (4)

TIMER_T::CTL: MODE_SEL Position

Definition at line 10010 of file Nano100Series.h.

## ◆ TIMER_CTL_PDMA_TEEN_Msk

#define TIMER_CTL_PDMA_TEEN_Msk (0x1ul << TIMER_CTL_PDMA_TEEN_Pos)

TIMER_T::CTL: PDMA_TEEN Mask

Definition at line 10023 of file Nano100Series.h.

## ◆ TIMER_CTL_PDMA_TEEN_Pos

#define TIMER_CTL_PDMA_TEEN_Pos (10)

TIMER_T::CTL: PDMA_TEEN Position

Definition at line 10022 of file Nano100Series.h.

## ◆ TIMER_CTL_SW_RST_Msk

#define TIMER_CTL_SW_RST_Msk (0x1ul << TIMER_CTL_SW_RST_Pos)

TIMER_T::CTL: SW_RST Mask

Definition at line 10002 of file Nano100Series.h.

## ◆ TIMER_CTL_SW_RST_Pos

#define TIMER_CTL_SW_RST_Pos (1)

TIMER_T::CTL: SW_RST Position

Definition at line 10001 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_CNT_MODE_Msk

#define TIMER_CTL_TCAP_CNT_MODE_Msk (0x1ul << TIMER_CTL_TCAP_CNT_MODE_Pos)

TIMER_T::CTL: TCAP_CNT_MODE Mask

Definition at line 10047 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_CNT_MODE_Pos

#define TIMER_CTL_TCAP_CNT_MODE_Pos (20)

TIMER_T::CTL: TCAP_CNT_MODE Position

Definition at line 10046 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_DEB_EN_Msk

#define TIMER_CTL_TCAP_DEB_EN_Msk (0x1ul << TIMER_CTL_TCAP_DEB_EN_Pos)

TIMER_T::CTL: TCAP_DEB_EN Mask

Definition at line 10050 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_DEB_EN_Pos

#define TIMER_CTL_TCAP_DEB_EN_Pos (22)

TIMER_T::CTL: TCAP_DEB_EN Position

Definition at line 10049 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_EDGE_Msk

#define TIMER_CTL_TCAP_EDGE_Msk (0x3ul << TIMER_CTL_TCAP_EDGE_Pos)

TIMER_T::CTL: TCAP_EDGE Mask

Definition at line 10044 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_EDGE_Pos

#define TIMER_CTL_TCAP_EDGE_Pos (18)

TIMER_T::CTL: TCAP_EDGE Position

Definition at line 10043 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_EN_Msk

#define TIMER_CTL_TCAP_EN_Msk (0x1ul << TIMER_CTL_TCAP_EN_Pos)

TIMER_T::CTL: TCAP_EN Mask

Definition at line 10038 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_EN_Pos

#define TIMER_CTL_TCAP_EN_Pos (16)

TIMER_T::CTL: TCAP_EN Position

Definition at line 10037 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_MODE_Msk

#define TIMER_CTL_TCAP_MODE_Msk (0x1ul << TIMER_CTL_TCAP_MODE_Pos)

TIMER_T::CTL: TCAP_MODE Mask

Definition at line 10041 of file Nano100Series.h.

## ◆ TIMER_CTL_TCAP_MODE_Pos

#define TIMER_CTL_TCAP_MODE_Pos (17)

TIMER_T::CTL: TCAP_MODE Position

Definition at line 10040 of file Nano100Series.h.

## ◆ TIMER_CTL_TMR_ACT_Msk

#define TIMER_CTL_TMR_ACT_Msk (0x1ul << TIMER_CTL_TMR_ACT_Pos)

TIMER_T::CTL: TMR_ACT Mask

Definition at line 10014 of file Nano100Series.h.

## ◆ TIMER_CTL_TMR_ACT_Pos

#define TIMER_CTL_TMR_ACT_Pos (7)

TIMER_T::CTL: TMR_ACT Position

Definition at line 10013 of file Nano100Series.h.

## ◆ TIMER_CTL_TMR_EN_Msk

#define TIMER_CTL_TMR_EN_Msk (0x1ul << TIMER_CTL_TMR_EN_Pos)

TIMER_T::CTL: TMR_EN Mask

Definition at line 9999 of file Nano100Series.h.

## ◆ TIMER_CTL_TMR_EN_Pos

#define TIMER_CTL_TMR_EN_Pos (0)

    @addtogroup TMR_CONST TIMER Bit Field Definition
    Constant Definitions for TIMER Controller

TIMER_T::CTL: TMR_EN Position

Definition at line 9998 of file Nano100Series.h.

## ◆ TIMER_CTL_WAKE_EN_Msk

#define TIMER_CTL_WAKE_EN_Msk (0x1ul << TIMER_CTL_WAKE_EN_Pos)

TIMER_T::CTL: WAKE_EN Mask

Definition at line 10005 of file Nano100Series.h.

## ◆ TIMER_CTL_WAKE_EN_Pos

#define TIMER_CTL_WAKE_EN_Pos (2)

TIMER_T::CTL: WAKE_EN Position

Definition at line 10004 of file Nano100Series.h.

## ◆ TIMER_DR_TDR_Msk

#define TIMER_DR_TDR_Msk (0xfffffful << TIMER_DR_TDR_Pos)

TIMER_T::DR: TDR Mask

Definition at line 10080 of file Nano100Series.h.

## ◆ TIMER_DR_TDR_Pos

#define TIMER_DR_TDR_Pos (0)

TIMER_T::DR: TDR Position

Definition at line 10079 of file Nano100Series.h.

## ◆ TIMER_IER_TCAP_IE_Msk

#define TIMER_IER_TCAP_IE_Msk (0x1ul << TIMER_IER_TCAP_IE_Pos)

TIMER_T::IER: TCAP_IE Mask

Definition at line 10065 of file Nano100Series.h.

## ◆ TIMER_IER_TCAP_IE_Pos

#define TIMER_IER_TCAP_IE_Pos (1)

TIMER_T::IER: TCAP_IE Position

Definition at line 10064 of file Nano100Series.h.

## ◆ TIMER_IER_TMR_IE_Msk

#define TIMER_IER_TMR_IE_Msk (0x1ul << TIMER_IER_TMR_IE_Pos)

TIMER_T::IER: TMR_IE Mask

Definition at line 10062 of file Nano100Series.h.

## ◆ TIMER_IER_TMR_IE_Pos

#define TIMER_IER_TMR_IE_Pos (0)

TIMER_T::IER: TMR_IE Position

Definition at line 10061 of file Nano100Series.h.

## ◆ TIMER_ISR_NCAP_DET_STS_Msk

#define TIMER_ISR_NCAP_DET_STS_Msk (0x1ul << TIMER_ISR_NCAP_DET_STS_Pos)

TIMER_T::ISR: NCAP_DET_STS Mask

Definition at line 10077 of file Nano100Series.h.

## ◆ TIMER_ISR_NCAP_DET_STS_Pos

#define TIMER_ISR_NCAP_DET_STS_Pos (5)

TIMER_T::ISR: NCAP_DET_STS Position

Definition at line 10076 of file Nano100Series.h.

## ◆ TIMER_ISR_TCAP_IS_Msk

#define TIMER_ISR_TCAP_IS_Msk (0x1ul << TIMER_ISR_TCAP_IS_Pos)

TIMER_T::ISR: TCAP_IS Mask

Definition at line 10071 of file Nano100Series.h.

## ◆ TIMER_ISR_TCAP_IS_Pos

#define TIMER_ISR_TCAP_IS_Pos (1)

TIMER_T::ISR: TCAP_IS Position

Definition at line 10070 of file Nano100Series.h.

## ◆ TIMER_ISR_TMR_IS_Msk

#define TIMER_ISR_TMR_IS_Msk (0x1ul << TIMER_ISR_TMR_IS_Pos)

TIMER_T::ISR: TMR_IS Mask

Definition at line 10068 of file Nano100Series.h.

## ◆ TIMER_ISR_TMR_IS_Pos

#define TIMER_ISR_TMR_IS_Pos (0)

TIMER_T::ISR: TMR_IS Position

Definition at line 10067 of file Nano100Series.h.

## ◆ TIMER_ISR_TMR_WAKE_STS_Msk

#define TIMER_ISR_TMR_WAKE_STS_Msk (0x1ul << TIMER_ISR_TMR_WAKE_STS_Pos)

TIMER_T::ISR: TMR_WAKE_STS Mask

Definition at line 10074 of file Nano100Series.h.

## ◆ TIMER_ISR_TMR_WAKE_STS_Pos

#define TIMER_ISR_TMR_WAKE_STS_Pos (4)

TIMER_T::ISR: TMR_WAKE_STS Position

Definition at line 10073 of file Nano100Series.h.

## ◆ TIMER_PRECNT_PRESCALE_CNT_Msk

#define TIMER_PRECNT_PRESCALE_CNT_Msk (0xfful << TIMER_PRECNT_PRESCALE_CNT_Pos)

TIMER_T::PRECNT: PRESCALE_CNT Mask

Definition at line 10056 of file Nano100Series.h.

## ◆ TIMER_PRECNT_PRESCALE_CNT_Pos

#define TIMER_PRECNT_PRESCALE_CNT_Pos (0)

TIMER_T::PRECNT: PRESCALE_CNT Position

Definition at line 10055 of file Nano100Series.h.

## ◆ TIMER_TCAP_CAP_Msk

#define TIMER_TCAP_CAP_Msk (0xfffffful << TIMER_TCAP_CAP_Pos)

TIMER_T::TCAP: CAP Mask

Definition at line 10083 of file Nano100Series.h.

## ◆ TIMER_TCAP_CAP_Pos

#define TIMER_TCAP_CAP_Pos (0)

TIMER_T::TCAP: CAP Position

Definition at line 10082 of file Nano100Series.h.

## ◆ UART_ALT_CTL_ADDR_PID_MATCH_Msk

#define UART_ALT_CTL_ADDR_PID_MATCH_Msk (0xfful << UART_ALT_CTL_ADDR_PID_MATCH_Pos)

UART_T::ALT_CTL: ADDR_PID_MATCH Mask

Definition at line 10821 of file Nano100Series.h.

## ◆ UART_ALT_CTL_ADDR_PID_MATCH_Pos

#define UART_ALT_CTL_ADDR_PID_MATCH_Pos (24)

UART_T::ALT_CTL: ADDR_PID_MATCH Position

Definition at line 10820 of file Nano100Series.h.

## ◆ UART_ALT_CTL_Bit_ERR_EN_Msk

#define UART_ALT_CTL_Bit_ERR_EN_Msk (0x1ul << UART_ALT_CTL_Bit_ERR_EN_Pos)

UART_T::ALT_CTL: Bit_ERR_EN Mask

Definition at line 10806 of file Nano100Series.h.

## ◆ UART_ALT_CTL_Bit_ERR_EN_Pos

#define UART_ALT_CTL_Bit_ERR_EN_Pos (8)

UART_T::ALT_CTL: Bit_ERR_EN Position

Definition at line 10805 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_HEAD_SEL_Msk

#define UART_ALT_CTL_LIN_HEAD_SEL_Msk (0x3ul << UART_ALT_CTL_LIN_HEAD_SEL_Pos)

UART_T::ALT_CTL: LIN_HEAD_SEL Mask

Definition at line 10797 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_HEAD_SEL_Pos

#define UART_ALT_CTL_LIN_HEAD_SEL_Pos (4)

UART_T::ALT_CTL: LIN_HEAD_SEL Position

Definition at line 10796 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_RX_EN_Msk

#define UART_ALT_CTL_LIN_RX_EN_Msk (0x1ul << UART_ALT_CTL_LIN_RX_EN_Pos)

UART_T::ALT_CTL: LIN_RX_EN Mask

Definition at line 10800 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_RX_EN_Pos

#define UART_ALT_CTL_LIN_RX_EN_Pos (6)

UART_T::ALT_CTL: LIN_RX_EN Position

Definition at line 10799 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_TX_BCNT_Msk

#define UART_ALT_CTL_LIN_TX_BCNT_Msk (0x7ul << UART_ALT_CTL_LIN_TX_BCNT_Pos)

UART_T::ALT_CTL: LIN_TX_BCNT Mask

Definition at line 10794 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_TX_BCNT_Pos

#define UART_ALT_CTL_LIN_TX_BCNT_Pos (0)

UART_T::ALT_CTL: LIN_TX_BCNT Position

Definition at line 10793 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_TX_EN_Msk

#define UART_ALT_CTL_LIN_TX_EN_Msk (0x1ul << UART_ALT_CTL_LIN_TX_EN_Pos)

UART_T::ALT_CTL: LIN_TX_EN Mask

Definition at line 10803 of file Nano100Series.h.

## ◆ UART_ALT_CTL_LIN_TX_EN_Pos

#define UART_ALT_CTL_LIN_TX_EN_Pos (7)

UART_T::ALT_CTL: LIN_TX_EN Position

Definition at line 10802 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_AAD_Msk

#define UART_ALT_CTL_RS485_AAD_Msk (0x1ul << UART_ALT_CTL_RS485_AAD_Pos)

UART_T::ALT_CTL: RS485_AAD Mask

Definition at line 10812 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_AAD_Pos

#define UART_ALT_CTL_RS485_AAD_Pos (17)

UART_T::ALT_CTL: RS485_AAD Position

Definition at line 10811 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_ADD_EN_Msk

#define UART_ALT_CTL_RS485_ADD_EN_Msk (0x1ul << UART_ALT_CTL_RS485_ADD_EN_Pos)

UART_T::ALT_CTL: RS485_ADD_EN Mask

Definition at line 10818 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_ADD_EN_Pos

#define UART_ALT_CTL_RS485_ADD_EN_Pos (19)

UART_T::ALT_CTL: RS485_ADD_EN Position

Definition at line 10817 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_AUD_Msk

#define UART_ALT_CTL_RS485_AUD_Msk (0x1ul << UART_ALT_CTL_RS485_AUD_Pos)

UART_T::ALT_CTL: RS485_AUD Mask

Definition at line 10815 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_AUD_Pos

#define UART_ALT_CTL_RS485_AUD_Pos (18)

UART_T::ALT_CTL: RS485_AUD Position

Definition at line 10814 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_NMM_Msk

#define UART_ALT_CTL_RS485_NMM_Msk (0x1ul << UART_ALT_CTL_RS485_NMM_Pos)

UART_T::ALT_CTL: RS485_NMM Mask

Definition at line 10809 of file Nano100Series.h.

## ◆ UART_ALT_CTL_RS485_NMM_Pos

#define UART_ALT_CTL_RS485_NMM_Pos (16)

UART_T::ALT_CTL: RS485_NMM Position

Definition at line 10808 of file Nano100Series.h.

## ◆ UART_BAUD_BRD_Msk

#define UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)

UART_T::BAUD: BRD Mask

Definition at line 10779 of file Nano100Series.h.

## ◆ UART_BAUD_BRD_Pos

#define UART_BAUD_BRD_Pos (0)

UART_T::BAUD: BRD Position

Definition at line 10778 of file Nano100Series.h.

## ◆ UART_BAUD_DIV_16_EN_Msk

#define UART_BAUD_DIV_16_EN_Msk (0x1ul << UART_BAUD_DIV_16_EN_Pos)

UART_T::BAUD: DIV_16_EN Mask

Definition at line 10782 of file Nano100Series.h.

## ◆ UART_BAUD_DIV_16_EN_Pos

#define UART_BAUD_DIV_16_EN_Pos (31)

UART_T::BAUD: DIV_16_EN Position

Definition at line 10781 of file Nano100Series.h.

## ◆ UART_CTL_ABAUD_EN_Msk

#define UART_CTL_ABAUD_EN_Msk (0x1ul << UART_CTL_ABAUD_EN_Pos)

UART_T::CTL: ABAUD_EN Mask

Definition at line 10620 of file Nano100Series.h.

## ◆ UART_CTL_ABAUD_EN_Pos

#define UART_CTL_ABAUD_EN_Pos (12)

UART_T::CTL: ABAUD_EN Position

Definition at line 10619 of file Nano100Series.h.

## ◆ UART_CTL_AUTO_CTS_EN_Msk

#define UART_CTL_AUTO_CTS_EN_Msk (0x1ul << UART_CTL_AUTO_CTS_EN_Pos)

UART_T::CTL: AUTO_CTS_EN Mask

Definition at line 10605 of file Nano100Series.h.

## ◆ UART_CTL_AUTO_CTS_EN_Pos

#define UART_CTL_AUTO_CTS_EN_Pos (5)

UART_T::CTL: AUTO_CTS_EN Position

Definition at line 10604 of file Nano100Series.h.

## ◆ UART_CTL_AUTO_RTS_EN_Msk

#define UART_CTL_AUTO_RTS_EN_Msk (0x1ul << UART_CTL_AUTO_RTS_EN_Pos)

UART_T::CTL: AUTO_RTS_EN Mask

Definition at line 10602 of file Nano100Series.h.

## ◆ UART_CTL_AUTO_RTS_EN_Pos

#define UART_CTL_AUTO_RTS_EN_Pos (4)

UART_T::CTL: AUTO_RTS_EN Position

Definition at line 10601 of file Nano100Series.h.

## ◆ UART_CTL_DMA_RX_EN_Msk

#define UART_CTL_DMA_RX_EN_Msk (0x1ul << UART_CTL_DMA_RX_EN_Pos)

UART_T::CTL: DMA_RX_EN Mask

Definition at line 10608 of file Nano100Series.h.

## ◆ UART_CTL_DMA_RX_EN_Pos

#define UART_CTL_DMA_RX_EN_Pos (6)

UART_T::CTL: DMA_RX_EN Position

Definition at line 10607 of file Nano100Series.h.

## ◆ UART_CTL_DMA_TX_EN_Msk

#define UART_CTL_DMA_TX_EN_Msk (0x1ul << UART_CTL_DMA_TX_EN_Pos)

UART_T::CTL: DMA_TX_EN Mask

Definition at line 10611 of file Nano100Series.h.

## ◆ UART_CTL_DMA_TX_EN_Pos

#define UART_CTL_DMA_TX_EN_Pos (7)

UART_T::CTL: DMA_TX_EN Position

Definition at line 10610 of file Nano100Series.h.

## ◆ UART_CTL_RX_DIS_Msk

#define UART_CTL_RX_DIS_Msk (0x1ul << UART_CTL_RX_DIS_Pos)

UART_T::CTL: RX_DIS Mask

Definition at line 10596 of file Nano100Series.h.

## ◆ UART_CTL_RX_DIS_Pos

#define UART_CTL_RX_DIS_Pos (2)

UART_T::CTL: RX_DIS Position

Definition at line 10595 of file Nano100Series.h.

## ◆ UART_CTL_RX_RST_Msk

#define UART_CTL_RX_RST_Msk (0x1ul << UART_CTL_RX_RST_Pos)

UART_T::CTL: RX_RST Mask

Definition at line 10590 of file Nano100Series.h.

## ◆ UART_CTL_RX_RST_Pos

#define UART_CTL_RX_RST_Pos (0)

UART_T::CTL: RX_RST Position

Definition at line 10589 of file Nano100Series.h.

## ◆ UART_CTL_TX_DIS_Msk

#define UART_CTL_TX_DIS_Msk (0x1ul << UART_CTL_TX_DIS_Pos)

UART_T::CTL: TX_DIS Mask

Definition at line 10599 of file Nano100Series.h.

## ◆ UART_CTL_TX_DIS_Pos

#define UART_CTL_TX_DIS_Pos (3)

UART_T::CTL: TX_DIS Position

Definition at line 10598 of file Nano100Series.h.

## ◆ UART_CTL_TX_RST_Msk

#define UART_CTL_TX_RST_Msk (0x1ul << UART_CTL_TX_RST_Pos)

UART_T::CTL: TX_RST Mask

Definition at line 10593 of file Nano100Series.h.

## ◆ UART_CTL_TX_RST_Pos

#define UART_CTL_TX_RST_Pos (1)

UART_T::CTL: TX_RST Position

Definition at line 10592 of file Nano100Series.h.

## ◆ UART_CTL_WAKE_CTS_EN_Msk

#define UART_CTL_WAKE_CTS_EN_Msk (0x1ul << UART_CTL_WAKE_CTS_EN_Pos)

UART_T::CTL: WAKE_CTS_EN Mask

Definition at line 10614 of file Nano100Series.h.

## ◆ UART_CTL_WAKE_CTS_EN_Pos

#define UART_CTL_WAKE_CTS_EN_Pos (8)

UART_T::CTL: WAKE_CTS_EN Position

Definition at line 10613 of file Nano100Series.h.

## ◆ UART_CTL_WAKE_DATA_EN_Msk

#define UART_CTL_WAKE_DATA_EN_Msk (0x1ul << UART_CTL_WAKE_DATA_EN_Pos)

UART_T::CTL: WAKE_DATA_EN Mask

Definition at line 10617 of file Nano100Series.h.

## ◆ UART_CTL_WAKE_DATA_EN_Pos

#define UART_CTL_WAKE_DATA_EN_Pos (9)

UART_T::CTL: WAKE_DATA_EN Position

Definition at line 10616 of file Nano100Series.h.

## ◆ UART_DAT_DAT_Msk

#define UART_DAT_DAT_Msk (0xfful << UART_DAT_DAT_Pos)

UART_T::DAT: DAT Mask

Definition at line 10587 of file Nano100Series.h.

## ◆ UART_DAT_DAT_Pos

#define UART_DAT_DAT_Pos (0)

    @addtogroup UART_CONST UART Bit Field Definition
    Constant Definitions for UART Controller

UART_T::DAT: DAT Position

Definition at line 10586 of file Nano100Series.h.

## ◆ UART_FSR_BI_F_Msk

#define UART_FSR_BI_F_Msk (0x1ul << UART_FSR_BI_F_Pos)

UART_T::FSR: BI_F Mask

Definition at line 10737 of file Nano100Series.h.

## ◆ UART_FSR_BI_F_Pos

#define UART_FSR_BI_F_Pos (6)

UART_T::FSR: BI_F Position

Definition at line 10736 of file Nano100Series.h.

## ◆ UART_FSR_FE_F_Msk

#define UART_FSR_FE_F_Msk (0x1ul << UART_FSR_FE_F_Pos)

UART_T::FSR: FE_F Mask

Definition at line 10734 of file Nano100Series.h.

## ◆ UART_FSR_FE_F_Pos

#define UART_FSR_FE_F_Pos (5)

UART_T::FSR: FE_F Position

Definition at line 10733 of file Nano100Series.h.

## ◆ UART_FSR_PE_F_Msk

#define UART_FSR_PE_F_Msk (0x1ul << UART_FSR_PE_F_Pos)

UART_T::FSR: PE_F Mask

Definition at line 10731 of file Nano100Series.h.

## ◆ UART_FSR_PE_F_Pos

#define UART_FSR_PE_F_Pos (4)

UART_T::FSR: PE_F Position

Definition at line 10730 of file Nano100Series.h.

## ◆ UART_FSR_RX_EMPTY_F_Msk

#define UART_FSR_RX_EMPTY_F_Msk (0x1ul << UART_FSR_RX_EMPTY_F_Pos)

UART_T::FSR: RX_EMPTY_F Mask

Definition at line 10725 of file Nano100Series.h.

## ◆ UART_FSR_RX_EMPTY_F_Pos

#define UART_FSR_RX_EMPTY_F_Pos (1)

UART_T::FSR: RX_EMPTY_F Position

Definition at line 10724 of file Nano100Series.h.

## ◆ UART_FSR_RX_FULL_F_Msk

#define UART_FSR_RX_FULL_F_Msk (0x1ul << UART_FSR_RX_FULL_F_Pos)

UART_T::FSR: RX_FULL_F Mask

Definition at line 10728 of file Nano100Series.h.

## ◆ UART_FSR_RX_FULL_F_Pos

#define UART_FSR_RX_FULL_F_Pos (2)

UART_T::FSR: RX_FULL_F Position

Definition at line 10727 of file Nano100Series.h.

## ◆ UART_FSR_RX_OVER_F_Msk

#define UART_FSR_RX_OVER_F_Msk (0x1ul << UART_FSR_RX_OVER_F_Pos)

UART_T::FSR: RX_OVER_F Mask

Definition at line 10722 of file Nano100Series.h.

## ◆ UART_FSR_RX_OVER_F_Pos

#define UART_FSR_RX_OVER_F_Pos (0)

UART_T::FSR: RX_OVER_F Position

Definition at line 10721 of file Nano100Series.h.

## ◆ UART_FSR_RX_POINTER_F_Msk

#define UART_FSR_RX_POINTER_F_Msk (0x1ful << UART_FSR_RX_POINTER_F_Pos)

UART_T::FSR: RX_POINTER_F Mask

Definition at line 10752 of file Nano100Series.h.

## ◆ UART_FSR_RX_POINTER_F_Pos

#define UART_FSR_RX_POINTER_F_Pos (16)

UART_T::FSR: RX_POINTER_F Position

Definition at line 10751 of file Nano100Series.h.

## ◆ UART_FSR_TE_F_Msk

#define UART_FSR_TE_F_Msk (0x1ul << UART_FSR_TE_F_Pos)

UART_T::FSR: TE_F Mask

Definition at line 10749 of file Nano100Series.h.

## ◆ UART_FSR_TE_F_Pos

#define UART_FSR_TE_F_Pos (11)

UART_T::FSR: TE_F Position

Definition at line 10748 of file Nano100Series.h.

## ◆ UART_FSR_TX_EMPTY_F_Msk

#define UART_FSR_TX_EMPTY_F_Msk (0x1ul << UART_FSR_TX_EMPTY_F_Pos)

UART_T::FSR: TX_EMPTY_F Mask

Definition at line 10743 of file Nano100Series.h.

## ◆ UART_FSR_TX_EMPTY_F_Pos

#define UART_FSR_TX_EMPTY_F_Pos (9)

UART_T::FSR: TX_EMPTY_F Position

Definition at line 10742 of file Nano100Series.h.

## ◆ UART_FSR_TX_FULL_F_Msk

#define UART_FSR_TX_FULL_F_Msk (0x1ul << UART_FSR_TX_FULL_F_Pos)

UART_T::FSR: TX_FULL_F Mask

Definition at line 10746 of file Nano100Series.h.

## ◆ UART_FSR_TX_FULL_F_Pos

#define UART_FSR_TX_FULL_F_Pos (10)

UART_T::FSR: TX_FULL_F Position

Definition at line 10745 of file Nano100Series.h.

## ◆ UART_FSR_TX_OVER_F_Msk

#define UART_FSR_TX_OVER_F_Msk (0x1ul << UART_FSR_TX_OVER_F_Pos)

UART_T::FSR: TX_OVER_F Mask

Definition at line 10740 of file Nano100Series.h.

## ◆ UART_FSR_TX_OVER_F_Pos

#define UART_FSR_TX_OVER_F_Pos (8)

UART_T::FSR: TX_OVER_F Position

Definition at line 10739 of file Nano100Series.h.

## ◆ UART_FSR_TX_POINTER_F_Msk

#define UART_FSR_TX_POINTER_F_Msk (0x1ful << UART_FSR_TX_POINTER_F_Pos)

UART_T::FSR: TX_POINTER_F Mask

Definition at line 10755 of file Nano100Series.h.

## ◆ UART_FSR_TX_POINTER_F_Pos

#define UART_FSR_TX_POINTER_F_Pos (24)

UART_T::FSR: TX_POINTER_F Position

Definition at line 10754 of file Nano100Series.h.

## ◆ UART_FUN_SEL_FUN_SEL_Msk

#define UART_FUN_SEL_FUN_SEL_Msk (0x3ul << UART_FUN_SEL_FUN_SEL_Pos)

UART_T::FUN_SEL: FUN_SEL Mask

Definition at line 10824 of file Nano100Series.h.

## ◆ UART_FUN_SEL_FUN_SEL_Pos

#define UART_FUN_SEL_FUN_SEL_Pos (0)

UART_T::FUN_SEL: FUN_SEL Position

Definition at line 10823 of file Nano100Series.h.

## ◆ UART_IER_ABAUD_IE_Msk

#define UART_IER_ABAUD_IE_Msk (0x1ul << UART_IER_ABAUD_IE_Pos)

UART_T::IER: ABAUD_IE Mask

Definition at line 10668 of file Nano100Series.h.

## ◆ UART_IER_ABAUD_IE_Pos

#define UART_IER_ABAUD_IE_Pos (7)

UART_T::IER: ABAUD_IE Position

Definition at line 10667 of file Nano100Series.h.

## ◆ UART_IER_BUF_ERR_IE_Msk

#define UART_IER_BUF_ERR_IE_Msk (0x1ul << UART_IER_BUF_ERR_IE_Pos)

UART_T::IER: BUF_ERR_IE Mask

Definition at line 10662 of file Nano100Series.h.

## ◆ UART_IER_BUF_ERR_IE_Pos

#define UART_IER_BUF_ERR_IE_Pos (5)

UART_T::IER: BUF_ERR_IE Position

Definition at line 10661 of file Nano100Series.h.

## ◆ UART_IER_LIN_IE_Msk

#define UART_IER_LIN_IE_Msk (0x1ul << UART_IER_LIN_IE_Pos)

UART_T::IER: LIN_IE Mask

Definition at line 10671 of file Nano100Series.h.

## ◆ UART_IER_LIN_IE_Pos

#define UART_IER_LIN_IE_Pos (8)

UART_T::IER: LIN_IE Position

Definition at line 10670 of file Nano100Series.h.

## ◆ UART_IER_MODEM_IE_Msk

#define UART_IER_MODEM_IE_Msk (0x1ul << UART_IER_MODEM_IE_Pos)

UART_T::IER: MODEM_IE Mask

Definition at line 10656 of file Nano100Series.h.

## ◆ UART_IER_MODEM_IE_Pos

#define UART_IER_MODEM_IE_Pos (3)

UART_T::IER: MODEM_IE Position

Definition at line 10655 of file Nano100Series.h.

## ◆ UART_IER_RDA_IE_Msk

#define UART_IER_RDA_IE_Msk (0x1ul << UART_IER_RDA_IE_Pos)

UART_T::IER: RDA_IE Mask

Definition at line 10647 of file Nano100Series.h.

## ◆ UART_IER_RDA_IE_Pos

#define UART_IER_RDA_IE_Pos (0)

UART_T::IER: RDA_IE Position

Definition at line 10646 of file Nano100Series.h.

## ◆ UART_IER_RLS_IE_Msk

#define UART_IER_RLS_IE_Msk (0x1ul << UART_IER_RLS_IE_Pos)

UART_T::IER: RLS_IE Mask

Definition at line 10653 of file Nano100Series.h.

## ◆ UART_IER_RLS_IE_Pos

#define UART_IER_RLS_IE_Pos (2)

UART_T::IER: RLS_IE Position

Definition at line 10652 of file Nano100Series.h.

## ◆ UART_IER_RTO_IE_Msk

#define UART_IER_RTO_IE_Msk (0x1ul << UART_IER_RTO_IE_Pos)

UART_T::IER: RTO_IE Mask

Definition at line 10659 of file Nano100Series.h.

## ◆ UART_IER_RTO_IE_Pos

#define UART_IER_RTO_IE_Pos (4)

UART_T::IER: RTO_IE Position

Definition at line 10658 of file Nano100Series.h.

## ◆ UART_IER_THRE_IE_Msk

#define UART_IER_THRE_IE_Msk (0x1ul << UART_IER_THRE_IE_Pos)

UART_T::IER: THRE_IE Mask

Definition at line 10650 of file Nano100Series.h.

## ◆ UART_IER_THRE_IE_Pos

#define UART_IER_THRE_IE_Pos (1)

UART_T::IER: THRE_IE Position

Definition at line 10649 of file Nano100Series.h.

## ◆ UART_IER_WAKE_IE_Msk

#define UART_IER_WAKE_IE_Msk (0x1ul << UART_IER_WAKE_IE_Pos)

UART_T::IER: WAKE_IE Mask

Definition at line 10665 of file Nano100Series.h.

## ◆ UART_IER_WAKE_IE_Pos

#define UART_IER_WAKE_IE_Pos (6)

UART_T::IER: WAKE_IE Position

Definition at line 10664 of file Nano100Series.h.

## ◆ UART_IRCR_INV_RX_Msk

#define UART_IRCR_INV_RX_Msk (0x1ul << UART_IRCR_INV_RX_Pos)

UART_T::IRCR: INV_RX Mask

Definition at line 10791 of file Nano100Series.h.

## ◆ UART_IRCR_INV_RX_Pos

#define UART_IRCR_INV_RX_Pos (6)

UART_T::IRCR: INV_RX Position

Definition at line 10790 of file Nano100Series.h.

## ◆ UART_IRCR_INV_TX_Msk

#define UART_IRCR_INV_TX_Msk (0x1ul << UART_IRCR_INV_TX_Pos)

UART_T::IRCR: INV_TX Mask

Definition at line 10788 of file Nano100Series.h.

## ◆ UART_IRCR_INV_TX_Pos

#define UART_IRCR_INV_TX_Pos (5)

UART_T::IRCR: INV_TX Position

Definition at line 10787 of file Nano100Series.h.

## ◆ UART_IRCR_TX_SELECT_Msk

#define UART_IRCR_TX_SELECT_Msk (0x1ul << UART_IRCR_TX_SELECT_Pos)

UART_T::IRCR: TX_SELECT Mask

Definition at line 10785 of file Nano100Series.h.

## ◆ UART_IRCR_TX_SELECT_Pos

#define UART_IRCR_TX_SELECT_Pos (1)

UART_T::IRCR: TX_SELECT Position

Definition at line 10784 of file Nano100Series.h.

## ◆ UART_ISR_ABAUD_IS_Msk

#define UART_ISR_ABAUD_IS_Msk (0x1ul << UART_ISR_ABAUD_IS_Pos)

UART_T::ISR: ABAUD_IS Mask

Definition at line 10695 of file Nano100Series.h.

## ◆ UART_ISR_ABAUD_IS_Pos

#define UART_ISR_ABAUD_IS_Pos (7)

UART_T::ISR: ABAUD_IS Position

Definition at line 10694 of file Nano100Series.h.

## ◆ UART_ISR_BUF_ERR_IS_Msk

#define UART_ISR_BUF_ERR_IS_Msk (0x1ul << UART_ISR_BUF_ERR_IS_Pos)

UART_T::ISR: BUF_ERR_IS Mask

Definition at line 10689 of file Nano100Series.h.

## ◆ UART_ISR_BUF_ERR_IS_Pos

#define UART_ISR_BUF_ERR_IS_Pos (5)

UART_T::ISR: BUF_ERR_IS Position

Definition at line 10688 of file Nano100Series.h.

## ◆ UART_ISR_LIN_IS_Msk

#define UART_ISR_LIN_IS_Msk (0x1ul << UART_ISR_LIN_IS_Pos)

UART_T::ISR: LIN_IS Mask

Definition at line 10698 of file Nano100Series.h.

## ◆ UART_ISR_LIN_IS_Pos

#define UART_ISR_LIN_IS_Pos (8)

UART_T::ISR: LIN_IS Position

Definition at line 10697 of file Nano100Series.h.

## ◆ UART_ISR_MODEM_IS_Msk

#define UART_ISR_MODEM_IS_Msk (0x1ul << UART_ISR_MODEM_IS_Pos)

UART_T::ISR: MODEM_IS Mask

Definition at line 10683 of file Nano100Series.h.

## ◆ UART_ISR_MODEM_IS_Pos

#define UART_ISR_MODEM_IS_Pos (3)

UART_T::ISR: MODEM_IS Position

Definition at line 10682 of file Nano100Series.h.

## ◆ UART_ISR_RDA_IS_Msk

#define UART_ISR_RDA_IS_Msk (0x1ul << UART_ISR_RDA_IS_Pos)

UART_T::ISR: RDA_IS Mask

Definition at line 10674 of file Nano100Series.h.

## ◆ UART_ISR_RDA_IS_Pos

#define UART_ISR_RDA_IS_Pos (0)

UART_T::ISR: RDA_IS Position

Definition at line 10673 of file Nano100Series.h.

## ◆ UART_ISR_RLS_IS_Msk

#define UART_ISR_RLS_IS_Msk (0x1ul << UART_ISR_RLS_IS_Pos)

UART_T::ISR: RLS_IS Mask

Definition at line 10680 of file Nano100Series.h.

## ◆ UART_ISR_RLS_IS_Pos

#define UART_ISR_RLS_IS_Pos (2)

UART_T::ISR: RLS_IS Position

Definition at line 10679 of file Nano100Series.h.

## ◆ UART_ISR_RTO_IS_Msk

#define UART_ISR_RTO_IS_Msk (0x1ul << UART_ISR_RTO_IS_Pos)

UART_T::ISR: RTO_IS Mask

Definition at line 10686 of file Nano100Series.h.

## ◆ UART_ISR_RTO_IS_Pos

#define UART_ISR_RTO_IS_Pos (4)

UART_T::ISR: RTO_IS Position

Definition at line 10685 of file Nano100Series.h.

## ◆ UART_ISR_THRE_IS_Msk

#define UART_ISR_THRE_IS_Msk (0x1ul << UART_ISR_THRE_IS_Pos)

UART_T::ISR: THRE_IS Mask

Definition at line 10677 of file Nano100Series.h.

## ◆ UART_ISR_THRE_IS_Pos

#define UART_ISR_THRE_IS_Pos (1)

UART_T::ISR: THRE_IS Position

Definition at line 10676 of file Nano100Series.h.

## ◆ UART_ISR_WAKE_IS_Msk

#define UART_ISR_WAKE_IS_Msk (0x1ul << UART_ISR_WAKE_IS_Pos)

UART_T::ISR: WAKE_IS Mask

Definition at line 10692 of file Nano100Series.h.

## ◆ UART_ISR_WAKE_IS_Pos

#define UART_ISR_WAKE_IS_Pos (6)

UART_T::ISR: WAKE_IS Position

Definition at line 10691 of file Nano100Series.h.

## ◆ UART_MCSR_CTS_ST_Msk

#define UART_MCSR_CTS_ST_Msk (0x1ul << UART_MCSR_CTS_ST_Pos)

UART_T::MCSR: CTS_ST Mask

Definition at line 10767 of file Nano100Series.h.

## ◆ UART_MCSR_CTS_ST_Pos

#define UART_MCSR_CTS_ST_Pos (17)

UART_T::MCSR: CTS_ST Position

Definition at line 10766 of file Nano100Series.h.

## ◆ UART_MCSR_DCT_F_Msk

#define UART_MCSR_DCT_F_Msk (0x1ul << UART_MCSR_DCT_F_Pos)

UART_T::MCSR: DCT_F Mask

Definition at line 10770 of file Nano100Series.h.

## ◆ UART_MCSR_DCT_F_Pos

#define UART_MCSR_DCT_F_Pos (18)

UART_T::MCSR: DCT_F Position

Definition at line 10769 of file Nano100Series.h.

## ◆ UART_MCSR_LEV_CTS_Msk

#define UART_MCSR_LEV_CTS_Msk (0x1ul << UART_MCSR_LEV_CTS_Pos)

UART_T::MCSR: LEV_CTS Mask

Definition at line 10764 of file Nano100Series.h.

## ◆ UART_MCSR_LEV_CTS_Pos

#define UART_MCSR_LEV_CTS_Pos (16)

UART_T::MCSR: LEV_CTS Position

Definition at line 10763 of file Nano100Series.h.

## ◆ UART_MCSR_LEV_RTS_Msk

#define UART_MCSR_LEV_RTS_Msk (0x1ul << UART_MCSR_LEV_RTS_Pos)

UART_T::MCSR: LEV_RTS Mask

Definition at line 10758 of file Nano100Series.h.

## ◆ UART_MCSR_LEV_RTS_Pos

#define UART_MCSR_LEV_RTS_Pos (0)

UART_T::MCSR: LEV_RTS Position

Definition at line 10757 of file Nano100Series.h.

## ◆ UART_MCSR_RTS_ST_Msk

#define UART_MCSR_RTS_ST_Msk (0x1ul << UART_MCSR_RTS_ST_Pos)

UART_T::MCSR: RTS_ST Mask

Definition at line 10761 of file Nano100Series.h.

## ◆ UART_MCSR_RTS_ST_Pos

#define UART_MCSR_RTS_ST_Pos (1)

UART_T::MCSR: RTS_ST Position

Definition at line 10760 of file Nano100Series.h.

## ◆ UART_TLCTL_BCB_Msk

#define UART_TLCTL_BCB_Msk (0x1ul << UART_TLCTL_BCB_Pos)

UART_T::TLCTL: BCB Mask

Definition at line 10638 of file Nano100Series.h.

## ◆ UART_TLCTL_BCB_Pos

#define UART_TLCTL_BCB_Pos (6)

UART_T::TLCTL: BCB Position

Definition at line 10637 of file Nano100Series.h.

## ◆ UART_TLCTL_DATA_LEN_Msk

#define UART_TLCTL_DATA_LEN_Msk (0x3ul << UART_TLCTL_DATA_LEN_Pos)

UART_T::TLCTL: DATA_LEN Mask

Definition at line 10623 of file Nano100Series.h.

## ◆ UART_TLCTL_DATA_LEN_Pos

#define UART_TLCTL_DATA_LEN_Pos (0)

UART_T::TLCTL: DATA_LEN Position

Definition at line 10622 of file Nano100Series.h.

## ◆ UART_TLCTL_EPE_Msk

#define UART_TLCTL_EPE_Msk (0x1ul << UART_TLCTL_EPE_Pos)

UART_T::TLCTL: EPE Mask

Definition at line 10632 of file Nano100Series.h.

## ◆ UART_TLCTL_EPE_Pos

#define UART_TLCTL_EPE_Pos (4)

UART_T::TLCTL: EPE Position

Definition at line 10631 of file Nano100Series.h.

## ◆ UART_TLCTL_NSB_Msk

#define UART_TLCTL_NSB_Msk (0x1ul << UART_TLCTL_NSB_Pos)

UART_T::TLCTL: NSB Mask

Definition at line 10626 of file Nano100Series.h.

## ◆ UART_TLCTL_NSB_Pos

#define UART_TLCTL_NSB_Pos (2)

UART_T::TLCTL: NSB Position

Definition at line 10625 of file Nano100Series.h.

## ◆ UART_TLCTL_PBE_Msk

#define UART_TLCTL_PBE_Msk (0x1ul << UART_TLCTL_PBE_Pos)

UART_T::TLCTL: PBE Mask

Definition at line 10629 of file Nano100Series.h.

## ◆ UART_TLCTL_PBE_Pos

#define UART_TLCTL_PBE_Pos (3)

UART_T::TLCTL: PBE Position

Definition at line 10628 of file Nano100Series.h.

## ◆ UART_TLCTL_RFITL_Msk

#define UART_TLCTL_RFITL_Msk (0x3ul << UART_TLCTL_RFITL_Pos)

UART_T::TLCTL: RFITL Mask

Definition at line 10641 of file Nano100Series.h.

## ◆ UART_TLCTL_RFITL_Pos

#define UART_TLCTL_RFITL_Pos (8)

UART_T::TLCTL: RFITL Position

Definition at line 10640 of file Nano100Series.h.

## ◆ UART_TLCTL_RTS_TRI_LEV_Msk

#define UART_TLCTL_RTS_TRI_LEV_Msk (0x3ul << UART_TLCTL_RTS_TRI_LEV_Pos)

UART_T::TLCTL: RTS_TRI_LEV Mask

Definition at line 10644 of file Nano100Series.h.

## ◆ UART_TLCTL_RTS_TRI_LEV_Pos

#define UART_TLCTL_RTS_TRI_LEV_Pos (12)

UART_T::TLCTL: RTS_TRI_LEV Position

Definition at line 10643 of file Nano100Series.h.

## ◆ UART_TLCTL_SPE_Msk

#define UART_TLCTL_SPE_Msk (0x1ul << UART_TLCTL_SPE_Pos)

UART_T::TLCTL: SPE Mask

Definition at line 10635 of file Nano100Series.h.

## ◆ UART_TLCTL_SPE_Pos

#define UART_TLCTL_SPE_Pos (5)

UART_T::TLCTL: SPE Position

Definition at line 10634 of file Nano100Series.h.

## ◆ UART_TMCTL_DLY_Msk

#define UART_TMCTL_DLY_Msk (0xfful << UART_TMCTL_DLY_Pos)

UART_T::TMCTL: DLY Mask

Definition at line 10776 of file Nano100Series.h.

## ◆ UART_TMCTL_DLY_Pos

#define UART_TMCTL_DLY_Pos (16)

UART_T::TMCTL: DLY Position

Definition at line 10775 of file Nano100Series.h.

## ◆ UART_TMCTL_TOIC_Msk

#define UART_TMCTL_TOIC_Msk (0x1fful << UART_TMCTL_TOIC_Pos)

UART_T::TMCTL: TOIC Mask

Definition at line 10773 of file Nano100Series.h.

## ◆ UART_TMCTL_TOIC_Pos

#define UART_TMCTL_TOIC_Pos (0)

UART_T::TMCTL: TOIC Position

Definition at line 10772 of file Nano100Series.h.

## ◆ UART_TRSR_ABAUD_F_Msk

#define UART_TRSR_ABAUD_F_Msk (0x1ul << UART_TRSR_ABAUD_F_Pos)

UART_T::TRSR: ABAUD_F Mask

Definition at line 10704 of file Nano100Series.h.

## ◆ UART_TRSR_ABAUD_F_Pos

#define UART_TRSR_ABAUD_F_Pos (1)

UART_T::TRSR: ABAUD_F Position

Definition at line 10703 of file Nano100Series.h.

## ◆ UART_TRSR_ABAUD_TOUT_F_Msk

#define UART_TRSR_ABAUD_TOUT_F_Msk (0x1ul << UART_TRSR_ABAUD_TOUT_F_Pos)

UART_T::TRSR: ABAUD_TOUT_F Mask

Definition at line 10707 of file Nano100Series.h.

## ◆ UART_TRSR_ABAUD_TOUT_F_Pos

#define UART_TRSR_ABAUD_TOUT_F_Pos (2)

UART_T::TRSR: ABAUD_TOUT_F Position

Definition at line 10706 of file Nano100Series.h.

## ◆ UART_TRSR_BIT_ERR_F_Msk

#define UART_TRSR_BIT_ERR_F_Msk (0x1ul << UART_TRSR_BIT_ERR_F_Pos)

UART_T::TRSR: BIT_ERR_F Mask

Definition at line 10716 of file Nano100Series.h.

## ◆ UART_TRSR_BIT_ERR_F_Pos

#define UART_TRSR_BIT_ERR_F_Pos (5)

UART_T::TRSR: BIT_ERR_F Position

Definition at line 10715 of file Nano100Series.h.

## ◆ UART_TRSR_LIN_RX_F_Msk

#define UART_TRSR_LIN_RX_F_Msk (0x1ul << UART_TRSR_LIN_RX_F_Pos)

UART_T::TRSR: LIN_RX_F Mask

Definition at line 10713 of file Nano100Series.h.

## ◆ UART_TRSR_LIN_RX_F_Pos

#define UART_TRSR_LIN_RX_F_Pos (4)

UART_T::TRSR: LIN_RX_F Position

Definition at line 10712 of file Nano100Series.h.

## ◆ UART_TRSR_LIN_RX_SYNC_ERR_F_Msk

#define UART_TRSR_LIN_RX_SYNC_ERR_F_Msk (0x1ul << UART_TRSR_LIN_RX_SYNC_ERR_F_Pos)

UART_T::TRSR: LIN_RX_SYNC_ERR_F Mask

Definition at line 10719 of file Nano100Series.h.

## ◆ UART_TRSR_LIN_RX_SYNC_ERR_F_Pos

#define UART_TRSR_LIN_RX_SYNC_ERR_F_Pos (8)

UART_T::TRSR: LIN_RX_SYNC_ERR_F Position

Definition at line 10718 of file Nano100Series.h.

## ◆ UART_TRSR_LIN_TX_F_Msk

#define UART_TRSR_LIN_TX_F_Msk (0x1ul << UART_TRSR_LIN_TX_F_Pos)

UART_T::TRSR: LIN_TX_F Mask

Definition at line 10710 of file Nano100Series.h.

## ◆ UART_TRSR_LIN_TX_F_Pos

#define UART_TRSR_LIN_TX_F_Pos (3)

UART_T::TRSR: LIN_TX_F Position

Definition at line 10709 of file Nano100Series.h.

## ◆ UART_TRSR_RS485_ADDET_F_Msk

#define UART_TRSR_RS485_ADDET_F_Msk (0x1ul << UART_TRSR_RS485_ADDET_F_Pos)

UART_T::TRSR: RS485_ADDET_F Mask

Definition at line 10701 of file Nano100Series.h.

## ◆ UART_TRSR_RS485_ADDET_F_Pos

#define UART_TRSR_RS485_ADDET_F_Pos (0)

UART_T::TRSR: RS485_ADDET_F Position

Definition at line 10700 of file Nano100Series.h.

## ◆ USBD_BUFSEG_BUFSEG_Msk [1/2]

#define USBD_BUFSEG_BUFSEG_Msk (0x3ful << USBD_BUFSEG_BUFSEG_Pos)

USBD_T::BUFSEG: BUFSEG Mask

Definition at line 11283 of file Nano100Series.h.

## ◆ USBD_BUFSEG_BUFSEG_Msk [2/2]

#define USBD_BUFSEG_BUFSEG_Msk (0x3ful << USBD_BUFSEG_BUFSEG_Pos)

USBD_T::BUFSEG: BUFSEG Mask

Definition at line 11283 of file Nano100Series.h.

## ◆ USBD_BUFSEG_BUFSEG_Pos [1/2]

#define USBD_BUFSEG_BUFSEG_Pos (3)

USBD_T::BUFSEG: BUFSEG Position

Definition at line 11282 of file Nano100Series.h.

## ◆ USBD_BUFSEG_BUFSEG_Pos [2/2]

#define USBD_BUFSEG_BUFSEG_Pos (3)

USBD_T::BUFSEG: BUFSEG Position

Definition at line 11282 of file Nano100Series.h.

## ◆ USBD_BUSSTS_FLDET_Msk

#define USBD_BUSSTS_FLDET_Msk (0x1ul << USBD_BUSSTS_FLDET_Pos)

USBD_T::BUSSTS: FLDET Mask

Definition at line 11196 of file Nano100Series.h.

## ◆ USBD_BUSSTS_FLDET_Pos

#define USBD_BUSSTS_FLDET_Pos (4)

USBD_T::BUSSTS: FLDET Position

Definition at line 11195 of file Nano100Series.h.

## ◆ USBD_BUSSTS_RESUME_Msk

#define USBD_BUSSTS_RESUME_Msk (0x1ul << USBD_BUSSTS_RESUME_Pos)

USBD_T::BUSSTS: RESUME Mask

Definition at line 11190 of file Nano100Series.h.

## ◆ USBD_BUSSTS_RESUME_Pos

#define USBD_BUSSTS_RESUME_Pos (2)

USBD_T::BUSSTS: RESUME Position

Definition at line 11189 of file Nano100Series.h.

## ◆ USBD_BUSSTS_SUSPEND_Msk

#define USBD_BUSSTS_SUSPEND_Msk (0x1ul << USBD_BUSSTS_SUSPEND_Pos)

USBD_T::BUSSTS: SUSPEND Mask

Definition at line 11187 of file Nano100Series.h.

## ◆ USBD_BUSSTS_SUSPEND_Pos

#define USBD_BUSSTS_SUSPEND_Pos (1)

USBD_T::BUSSTS: SUSPEND Position

Definition at line 11186 of file Nano100Series.h.

## ◆ USBD_BUSSTS_TIMEOUT_Msk

#define USBD_BUSSTS_TIMEOUT_Msk (0x1ul << USBD_BUSSTS_TIMEOUT_Pos)

USBD_T::BUSSTS: TIMEOUT Mask

Definition at line 11193 of file Nano100Series.h.

## ◆ USBD_BUSSTS_TIMEOUT_Pos

#define USBD_BUSSTS_TIMEOUT_Pos (3)

USBD_T::BUSSTS: TIMEOUT Position

Definition at line 11192 of file Nano100Series.h.

## ◆ USBD_BUSSTS_USBRST_Msk

#define USBD_BUSSTS_USBRST_Msk (0x1ul << USBD_BUSSTS_USBRST_Pos)

USBD_T::BUSSTS: USBRST Mask

Definition at line 11184 of file Nano100Series.h.

## ◆ USBD_BUSSTS_USBRST_Pos

#define USBD_BUSSTS_USBRST_Pos (0)

USBD_T::BUSSTS: USBRST Position

Definition at line 11183 of file Nano100Series.h.

## ◆ USBD_CFG_CLRRDY_Msk

#define USBD_CFG_CLRRDY_Msk (0x1ul << USBD_CFG_CLRRDY_Pos)

USBD_T::CFG: CLRRDY Mask

Definition at line 11307 of file Nano100Series.h.

## ◆ USBD_CFG_CLRRDY_Pos

#define USBD_CFG_CLRRDY_Pos (15)

USBD_T::CFG: CLRRDY Position

Definition at line 11306 of file Nano100Series.h.

## ◆ USBD_CFG_CSTALL_Msk

#define USBD_CFG_CSTALL_Msk (0x1ul << USBD_CFG_CSTALL_Pos)

USBD_T::CFG: CSTALL Mask

Definition at line 11301 of file Nano100Series.h.

## ◆ USBD_CFG_CSTALL_Pos

#define USBD_CFG_CSTALL_Pos (8)

USBD_T::CFG: CSTALL Position

Definition at line 11300 of file Nano100Series.h.

## ◆ USBD_CFG_DSQ_SYNC_Msk

#define USBD_CFG_DSQ_SYNC_Msk (0x1ul << USBD_CFG_DSQ_SYNC_Pos)

USBD_T::CFG: DSQ_SYNC Mask

Definition at line 11298 of file Nano100Series.h.

## ◆ USBD_CFG_DSQ_SYNC_Pos

#define USBD_CFG_DSQ_SYNC_Pos (7)

USBD_T::CFG: DSQ_SYNC Position

Definition at line 11297 of file Nano100Series.h.

## ◆ USBD_CFG_EP_NUM_Msk

#define USBD_CFG_EP_NUM_Msk (0xful << USBD_CFG_EP_NUM_Pos)

USBD_T::CFG: EP_NUM Mask

Definition at line 11289 of file Nano100Series.h.

## ◆ USBD_CFG_EP_NUM_Pos

#define USBD_CFG_EP_NUM_Pos (0)

USBD_T::CFG: EP_NUM Position

Definition at line 11288 of file Nano100Series.h.

## ◆ USBD_CFG_EPMODE_Msk

#define USBD_CFG_EPMODE_Msk (0x3ul << USBD_CFG_EPMODE_Pos)

USBD_T::CFG: EPMODE Mask

Definition at line 11295 of file Nano100Series.h.

## ◆ USBD_CFG_EPMODE_Pos

#define USBD_CFG_EPMODE_Pos (5)

USBD_T::CFG: EPMODE Position

Definition at line 11294 of file Nano100Series.h.

## ◆ USBD_CFG_ISOCH_Msk

#define USBD_CFG_ISOCH_Msk (0x1ul << USBD_CFG_ISOCH_Pos)

USBD_T::CFG: ISOCH Mask

Definition at line 11292 of file Nano100Series.h.

## ◆ USBD_CFG_ISOCH_Pos

#define USBD_CFG_ISOCH_Pos (4)

USBD_T::CFG: ISOCH Position

Definition at line 11291 of file Nano100Series.h.

## ◆ USBD_CFG_SSTALL_Msk

#define USBD_CFG_SSTALL_Msk (0x1ul << USBD_CFG_SSTALL_Pos)

USBD_T::CFG: SSTALL Mask

Definition at line 11304 of file Nano100Series.h.

## ◆ USBD_CFG_SSTALL_Pos

#define USBD_CFG_SSTALL_Pos (9)

USBD_T::CFG: SSTALL Position

Definition at line 11303 of file Nano100Series.h.

## ◆ USBD_CTL_DPPU_EN_Msk

#define USBD_CTL_DPPU_EN_Msk (0x1ul << USBD_CTL_DPPU_EN_Pos)

USBD_T::CTL: DPPU_EN Mask

Definition at line 11172 of file Nano100Series.h.

## ◆ USBD_CTL_DPPU_EN_Pos

#define USBD_CTL_DPPU_EN_Pos (3)

USBD_T::CTL: DPPU_EN Position

Definition at line 11171 of file Nano100Series.h.

## ◆ USBD_CTL_DRVSE0_Msk

#define USBD_CTL_DRVSE0_Msk (0x1ul << USBD_CTL_DRVSE0_Pos)

USBD_T::CTL: DRVSE0 Mask

Definition at line 11175 of file Nano100Series.h.

## ◆ USBD_CTL_DRVSE0_Pos

#define USBD_CTL_DRVSE0_Pos (4)

USBD_T::CTL: DRVSE0 Position

Definition at line 11174 of file Nano100Series.h.

## ◆ USBD_CTL_PHY_EN_Msk

#define USBD_CTL_PHY_EN_Msk (0x1ul << USBD_CTL_PHY_EN_Pos)

USBD_T::CTL: PHY_EN Mask

Definition at line 11166 of file Nano100Series.h.

## ◆ USBD_CTL_PHY_EN_Pos

#define USBD_CTL_PHY_EN_Pos (1)

USBD_T::CTL: PHY_EN Position

Definition at line 11165 of file Nano100Series.h.

## ◆ USBD_CTL_PWRDB_Msk

#define USBD_CTL_PWRDB_Msk (0x1ul << USBD_CTL_PWRDB_Pos)

USBD_T::CTL: PWRDB Mask

Definition at line 11169 of file Nano100Series.h.

## ◆ USBD_CTL_PWRDB_Pos

#define USBD_CTL_PWRDB_Pos (2)

USBD_T::CTL: PWRDB Position

Definition at line 11168 of file Nano100Series.h.

## ◆ USBD_CTL_RWAKEUP_Msk

#define USBD_CTL_RWAKEUP_Msk (0x1ul << USBD_CTL_RWAKEUP_Pos)

USBD_T::CTL: RWAKEUP Mask

Definition at line 11178 of file Nano100Series.h.

## ◆ USBD_CTL_RWAKEUP_Pos

#define USBD_CTL_RWAKEUP_Pos (8)

USBD_T::CTL: RWAKEUP Position

Definition at line 11177 of file Nano100Series.h.

## ◆ USBD_CTL_USB_EN_Msk

#define USBD_CTL_USB_EN_Msk (0x1ul << USBD_CTL_USB_EN_Pos)

USBD_T::CTL: USB_EN Mask

Definition at line 11163 of file Nano100Series.h.

## ◆ USBD_CTL_USB_EN_Pos

#define USBD_CTL_USB_EN_Pos (0)

    @addtogroup USBD_CONST USBD Bit Field Definition
    Constant Definitions for USBD Controller

USBD_T::CTL: USB_EN Position

Definition at line 11162 of file Nano100Series.h.

## ◆ USBD_CTL_WAKEUP_EN_Msk

#define USBD_CTL_WAKEUP_EN_Msk (0x1ul << USBD_CTL_WAKEUP_EN_Pos)

USBD_T::CTL: WAKEUP_EN Mask

Definition at line 11181 of file Nano100Series.h.

## ◆ USBD_CTL_WAKEUP_EN_Pos

#define USBD_CTL_WAKEUP_EN_Pos (9)

USBD_T::CTL: WAKEUP_EN Position

Definition at line 11180 of file Nano100Series.h.

## ◆ USBD_EPSTS2_EPSTS6_Msk

#define USBD_EPSTS2_EPSTS6_Msk (0x7ul << USBD_EPSTS2_EPSTS6_Pos)

USBD_T::EPSTS2: EPSTS6 Mask

Definition at line 11277 of file Nano100Series.h.

## ◆ USBD_EPSTS2_EPSTS6_Pos

#define USBD_EPSTS2_EPSTS6_Pos (0)

USBD_T::EPSTS2: EPSTS6 Position

Definition at line 11276 of file Nano100Series.h.

## ◆ USBD_EPSTS2_EPSTS7_Msk

#define USBD_EPSTS2_EPSTS7_Msk (0x7ul << USBD_EPSTS2_EPSTS7_Pos)

USBD_T::EPSTS2: EPSTS7 Mask

Definition at line 11280 of file Nano100Series.h.

## ◆ USBD_EPSTS2_EPSTS7_Pos

#define USBD_EPSTS2_EPSTS7_Pos (4)

USBD_T::EPSTS2: EPSTS7 Position

Definition at line 11279 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS0_Msk

#define USBD_EPSTS_EPSTS0_Msk (0xful << USBD_EPSTS_EPSTS0_Pos)

USBD_T::EPSTS: EPSTS0 Mask

Definition at line 11256 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS0_Pos

#define USBD_EPSTS_EPSTS0_Pos (8)

USBD_T::EPSTS: EPSTS0 Position

Definition at line 11255 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS1_Msk

#define USBD_EPSTS_EPSTS1_Msk (0xful << USBD_EPSTS_EPSTS1_Pos)

USBD_T::EPSTS: EPSTS1 Mask

Definition at line 11259 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS1_Pos

#define USBD_EPSTS_EPSTS1_Pos (12)

USBD_T::EPSTS: EPSTS1 Position

Definition at line 11258 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS2_Msk

#define USBD_EPSTS_EPSTS2_Msk (0xful << USBD_EPSTS_EPSTS2_Pos)

USBD_T::EPSTS: EPSTS2 Mask

Definition at line 11262 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS2_Pos

#define USBD_EPSTS_EPSTS2_Pos (16)

USBD_T::EPSTS: EPSTS2 Position

Definition at line 11261 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS3_Msk

#define USBD_EPSTS_EPSTS3_Msk (0xful << USBD_EPSTS_EPSTS3_Pos)

USBD_T::EPSTS: EPSTS3 Mask

Definition at line 11265 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS3_Pos

#define USBD_EPSTS_EPSTS3_Pos (20)

USBD_T::EPSTS: EPSTS3 Position

Definition at line 11264 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS4_Msk

#define USBD_EPSTS_EPSTS4_Msk (0xful << USBD_EPSTS_EPSTS4_Pos)

USBD_T::EPSTS: EPSTS4 Mask

Definition at line 11268 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS4_Pos

#define USBD_EPSTS_EPSTS4_Pos (24)

USBD_T::EPSTS: EPSTS4 Position

Definition at line 11267 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS5_Msk

#define USBD_EPSTS_EPSTS5_Msk (0xful << USBD_EPSTS_EPSTS5_Pos)

USBD_T::EPSTS: EPSTS5 Mask

Definition at line 11271 of file Nano100Series.h.

## ◆ USBD_EPSTS_EPSTS5_Pos

#define USBD_EPSTS_EPSTS5_Pos (28)

USBD_T::EPSTS: EPSTS5 Position

Definition at line 11270 of file Nano100Series.h.

## ◆ USBD_EPSTS_OVERRUN_Msk

#define USBD_EPSTS_OVERRUN_Msk (0x1ul << USBD_EPSTS_OVERRUN_Pos)

USBD_T::EPSTS: OVERRUN Mask

Definition at line 11253 of file Nano100Series.h.

## ◆ USBD_EPSTS_OVERRUN_Pos

#define USBD_EPSTS_OVERRUN_Pos (7)

USBD_T::EPSTS: OVERRUN Position

Definition at line 11252 of file Nano100Series.h.

## ◆ USBD_FADDR_FADDR_Msk

#define USBD_FADDR_FADDR_Msk (0x7ful << USBD_FADDR_FADDR_Pos)

USBD_T::FADDR: FADDR Mask

Definition at line 11250 of file Nano100Series.h.

## ◆ USBD_FADDR_FADDR_Pos

#define USBD_FADDR_FADDR_Pos (0)

USBD_T::FADDR: FADDR Position

Definition at line 11249 of file Nano100Series.h.

## ◆ USBD_INTEN_BUSEVT_IE_Msk

#define USBD_INTEN_BUSEVT_IE_Msk (0x1ul << USBD_INTEN_BUSEVT_IE_Pos)

USBD_T::INTEN: BUSEVT_IE Mask

Definition at line 11199 of file Nano100Series.h.

## ◆ USBD_INTEN_BUSEVT_IE_Pos

#define USBD_INTEN_BUSEVT_IE_Pos (0)

USBD_T::INTEN: BUSEVT_IE Position

Definition at line 11198 of file Nano100Series.h.

## ◆ USBD_INTEN_FLDET_IE_Msk

#define USBD_INTEN_FLDET_IE_Msk (0x1ul << USBD_INTEN_FLDET_IE_Pos)

USBD_T::INTEN: FLDET_IE Mask

Definition at line 11205 of file Nano100Series.h.

## ◆ USBD_INTEN_FLDET_IE_Pos

#define USBD_INTEN_FLDET_IE_Pos (2)

USBD_T::INTEN: FLDET_IE Position

Definition at line 11204 of file Nano100Series.h.

## ◆ USBD_INTEN_USBEVT_IE_Msk

#define USBD_INTEN_USBEVT_IE_Msk (0x1ul << USBD_INTEN_USBEVT_IE_Pos)

USBD_T::INTEN: USBEVT_IE Mask

Definition at line 11202 of file Nano100Series.h.

## ◆ USBD_INTEN_USBEVT_IE_Pos

#define USBD_INTEN_USBEVT_IE_Pos (1)

USBD_T::INTEN: USBEVT_IE Position

Definition at line 11201 of file Nano100Series.h.

## ◆ USBD_INTEN_WAKEUP_IE_Msk

#define USBD_INTEN_WAKEUP_IE_Msk (0x1ul << USBD_INTEN_WAKEUP_IE_Pos)

USBD_T::INTEN: WAKEUP_IE Mask

Definition at line 11208 of file Nano100Series.h.

## ◆ USBD_INTEN_WAKEUP_IE_Pos

#define USBD_INTEN_WAKEUP_IE_Pos (3)

USBD_T::INTEN: WAKEUP_IE Position

Definition at line 11207 of file Nano100Series.h.

## ◆ USBD_INTSTS_BUS_STS_Msk

#define USBD_INTSTS_BUS_STS_Msk (0x1ul << USBD_INTSTS_BUS_STS_Pos)

USBD_T::INTSTS: BUS_STS Mask

Definition at line 11211 of file Nano100Series.h.

## ◆ USBD_INTSTS_BUS_STS_Pos

#define USBD_INTSTS_BUS_STS_Pos (0)

USBD_T::INTSTS: BUS_STS Position

Definition at line 11210 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT0_Msk

#define USBD_INTSTS_EPEVT0_Msk (0x1ul << USBD_INTSTS_EPEVT0_Pos)

USBD_T::INTSTS: EPEVT0 Mask

Definition at line 11223 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT0_Pos

#define USBD_INTSTS_EPEVT0_Pos (16)

USBD_T::INTSTS: EPEVT0 Position

Definition at line 11222 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT1_Msk

#define USBD_INTSTS_EPEVT1_Msk (0x1ul << USBD_INTSTS_EPEVT1_Pos)

USBD_T::INTSTS: EPEVT1 Mask

Definition at line 11226 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT1_Pos

#define USBD_INTSTS_EPEVT1_Pos (17)

USBD_T::INTSTS: EPEVT1 Position

Definition at line 11225 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT2_Msk

#define USBD_INTSTS_EPEVT2_Msk (0x1ul << USBD_INTSTS_EPEVT2_Pos)

USBD_T::INTSTS: EPEVT2 Mask

Definition at line 11229 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT2_Pos

#define USBD_INTSTS_EPEVT2_Pos (18)

USBD_T::INTSTS: EPEVT2 Position

Definition at line 11228 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT3_Msk

#define USBD_INTSTS_EPEVT3_Msk (0x1ul << USBD_INTSTS_EPEVT3_Pos)

USBD_T::INTSTS: EPEVT3 Mask

Definition at line 11232 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT3_Pos

#define USBD_INTSTS_EPEVT3_Pos (19)

USBD_T::INTSTS: EPEVT3 Position

Definition at line 11231 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT4_Msk

#define USBD_INTSTS_EPEVT4_Msk (0x1ul << USBD_INTSTS_EPEVT4_Pos)

USBD_T::INTSTS: EPEVT4 Mask

Definition at line 11235 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT4_Pos

#define USBD_INTSTS_EPEVT4_Pos (20)

USBD_T::INTSTS: EPEVT4 Position

Definition at line 11234 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT5_Msk

#define USBD_INTSTS_EPEVT5_Msk (0x1ul << USBD_INTSTS_EPEVT5_Pos)

USBD_T::INTSTS: EPEVT5 Mask

Definition at line 11238 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT5_Pos

#define USBD_INTSTS_EPEVT5_Pos (21)

USBD_T::INTSTS: EPEVT5 Position

Definition at line 11237 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT6_Msk

#define USBD_INTSTS_EPEVT6_Msk (0x1ul << USBD_INTSTS_EPEVT6_Pos)

USBD_T::INTSTS: EPEVT6 Mask

Definition at line 11241 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT6_Pos

#define USBD_INTSTS_EPEVT6_Pos (22)

USBD_T::INTSTS: EPEVT6 Position

Definition at line 11240 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT7_Msk

#define USBD_INTSTS_EPEVT7_Msk (0x1ul << USBD_INTSTS_EPEVT7_Pos)

USBD_T::INTSTS: EPEVT7 Mask

Definition at line 11244 of file Nano100Series.h.

## ◆ USBD_INTSTS_EPEVT7_Pos

#define USBD_INTSTS_EPEVT7_Pos (23)

USBD_T::INTSTS: EPEVT7 Position

Definition at line 11243 of file Nano100Series.h.

## ◆ USBD_INTSTS_FLD_STS_Msk

#define USBD_INTSTS_FLD_STS_Msk (0x1ul << USBD_INTSTS_FLD_STS_Pos)

USBD_T::INTSTS: FLD_STS Mask

Definition at line 11217 of file Nano100Series.h.

## ◆ USBD_INTSTS_FLD_STS_Pos

#define USBD_INTSTS_FLD_STS_Pos (2)

USBD_T::INTSTS: FLD_STS Position

Definition at line 11216 of file Nano100Series.h.

## ◆ USBD_INTSTS_SETUP_Msk

#define USBD_INTSTS_SETUP_Msk (0x1ul << USBD_INTSTS_SETUP_Pos)

USBD_T::INTSTS: SETUP Mask

Definition at line 11247 of file Nano100Series.h.

## ◆ USBD_INTSTS_SETUP_Pos

#define USBD_INTSTS_SETUP_Pos (31)

USBD_T::INTSTS: SETUP Position

Definition at line 11246 of file Nano100Series.h.

## ◆ USBD_INTSTS_USB_STS_Msk

#define USBD_INTSTS_USB_STS_Msk (0x1ul << USBD_INTSTS_USB_STS_Pos)

USBD_T::INTSTS: USB_STS Mask

Definition at line 11214 of file Nano100Series.h.

## ◆ USBD_INTSTS_USB_STS_Pos

#define USBD_INTSTS_USB_STS_Pos (1)

USBD_T::INTSTS: USB_STS Position

Definition at line 11213 of file Nano100Series.h.

## ◆ USBD_INTSTS_WKEUP_STS_Msk

#define USBD_INTSTS_WKEUP_STS_Msk (0x1ul << USBD_INTSTS_WKEUP_STS_Pos)

USBD_T::INTSTS: WKEUP_STS Mask

Definition at line 11220 of file Nano100Series.h.

## ◆ USBD_INTSTS_WKEUP_STS_Pos

#define USBD_INTSTS_WKEUP_STS_Pos (3)

USBD_T::INTSTS: WKEUP_STS Position

Definition at line 11219 of file Nano100Series.h.

## ◆ USBD_MXPLD_MXPLD_Msk

#define USBD_MXPLD_MXPLD_Msk (0x1fful << USBD_MXPLD_MXPLD_Pos)

USBD_T::MXPLD: MXPLD Mask

Definition at line 11286 of file Nano100Series.h.

## ◆ USBD_MXPLD_MXPLD_Pos

#define USBD_MXPLD_MXPLD_Pos (0)

USBD_T::MXPLD: MXPLD Position

Definition at line 11285 of file Nano100Series.h.

## ◆ USBD_PDMA_BYTEM_Msk

#define USBD_PDMA_BYTEM_Msk (0x1ul << USBD_PDMA_BYTEM_Pos)

USBD_T::PDMA: BYTEM Mask

Definition at line 11316 of file Nano100Series.h.

## ◆ USBD_PDMA_BYTEM_Pos

#define USBD_PDMA_BYTEM_Pos (2)

USBD_T::PDMA: BYTEM Position

Definition at line 11315 of file Nano100Series.h.

## ◆ USBD_PDMA_PDMA_RST_Msk

#define USBD_PDMA_PDMA_RST_Msk (0x1ul << USBD_PDMA_PDMA_RST_Pos)

USBD_T::PDMA: PDMA_RST Mask

Definition at line 11319 of file Nano100Series.h.

## ◆ USBD_PDMA_PDMA_RST_Pos

#define USBD_PDMA_PDMA_RST_Pos (3)

USBD_T::PDMA: PDMA_RST Position

Definition at line 11318 of file Nano100Series.h.

## ◆ USBD_PDMA_PDMA_RW_Msk

#define USBD_PDMA_PDMA_RW_Msk (0x1ul << USBD_PDMA_PDMA_RW_Pos)

USBD_T::PDMA: PDMA_RW Mask

Definition at line 11310 of file Nano100Series.h.

## ◆ USBD_PDMA_PDMA_RW_Pos

#define USBD_PDMA_PDMA_RW_Pos (0)

USBD_T::PDMA: PDMA_RW Position

Definition at line 11309 of file Nano100Series.h.

## ◆ USBD_PDMA_PDMA_TRG_Msk

#define USBD_PDMA_PDMA_TRG_Msk (0x1ul << USBD_PDMA_PDMA_TRG_Pos)

USBD_T::PDMA: PDMA_TRG Mask

Definition at line 11313 of file Nano100Series.h.

## ◆ USBD_PDMA_PDMA_TRG_Pos

#define USBD_PDMA_PDMA_TRG_Pos (1)

USBD_T::PDMA: PDMA_TRG Position

Definition at line 11312 of file Nano100Series.h.

## ◆ VDMA_BCR_VDMA_BCR_Msk

#define VDMA_BCR_VDMA_BCR_Msk (0xfffful << VDMA_BCR_VDMA_BCR_Pos)

VDMA_T::BCR: VDMA_BCR Mask

Definition at line 6540 of file Nano100Series.h.

## ◆ VDMA_BCR_VDMA_BCR_Pos

#define VDMA_BCR_VDMA_BCR_Pos (0)

VDMA_T::BCR: VDMA_BCR Position

Definition at line 6539 of file Nano100Series.h.

## ◆ VDMA_CBCR_VDMA_CBCR_Msk

#define VDMA_CBCR_VDMA_CBCR_Msk (0xfffful << VDMA_CBCR_VDMA_CBCR_Pos)

VDMA_T::CBCR: VDMA_CBCR Mask

Definition at line 6549 of file Nano100Series.h.

## ◆ VDMA_CBCR_VDMA_CBCR_Pos

#define VDMA_CBCR_VDMA_CBCR_Pos (0)

VDMA_T::CBCR: VDMA_CBCR Position

Definition at line 6548 of file Nano100Series.h.

## ◆ VDMA_CDAR_VDMA_CDAR_Msk

#define VDMA_CDAR_VDMA_CDAR_Msk (0xfffffffful << VDMA_CDAR_VDMA_CDAR_Pos)

VDMA_T::CDAR: VDMA_CDAR Mask

Definition at line 6546 of file Nano100Series.h.

## ◆ VDMA_CDAR_VDMA_CDAR_Pos

#define VDMA_CDAR_VDMA_CDAR_Pos (0)

VDMA_T::CDAR: VDMA_CDAR Position

Definition at line 6545 of file Nano100Series.h.

## ◆ VDMA_CSAR_VDMA_CSAR_Msk

#define VDMA_CSAR_VDMA_CSAR_Msk (0xfffffffful << VDMA_CSAR_VDMA_CSAR_Pos)

VDMA_T::CSAR: VDMA_CSAR Mask

Definition at line 6543 of file Nano100Series.h.

## ◆ VDMA_CSAR_VDMA_CSAR_Pos

#define VDMA_CSAR_VDMA_CSAR_Pos (0)

VDMA_T::CSAR: VDMA_CSAR Position

Definition at line 6542 of file Nano100Series.h.

## ◆ VDMA_CSR_DIR_SEL_Msk

#define VDMA_CSR_DIR_SEL_Msk (0x1ul << VDMA_CSR_DIR_SEL_Pos)

VDMA_T::CSR: DIR_SEL Mask

Definition at line 6528 of file Nano100Series.h.

## ◆ VDMA_CSR_DIR_SEL_Pos

#define VDMA_CSR_DIR_SEL_Pos (11)

VDMA_T::CSR: DIR_SEL Position

Definition at line 6527 of file Nano100Series.h.

## ◆ VDMA_CSR_STRIDE_EN_Msk

#define VDMA_CSR_STRIDE_EN_Msk (0x1ul << VDMA_CSR_STRIDE_EN_Pos)

VDMA_T::CSR: STRIDE_EN Mask

Definition at line 6525 of file Nano100Series.h.

## ◆ VDMA_CSR_STRIDE_EN_Pos

#define VDMA_CSR_STRIDE_EN_Pos (10)

VDMA_T::CSR: STRIDE_EN Position

Definition at line 6524 of file Nano100Series.h.

## ◆ VDMA_CSR_SW_RST_Msk

#define VDMA_CSR_SW_RST_Msk (0x1ul << VDMA_CSR_SW_RST_Pos)

VDMA_T::CSR: SW_RST Mask

Definition at line 6522 of file Nano100Series.h.

## ◆ VDMA_CSR_SW_RST_Pos

#define VDMA_CSR_SW_RST_Pos (1)

VDMA_T::CSR: SW_RST Position

Definition at line 6521 of file Nano100Series.h.

## ◆ VDMA_CSR_TRIG_EN_Msk

#define VDMA_CSR_TRIG_EN_Msk (0x1ul << VDMA_CSR_TRIG_EN_Pos)

VDMA_T::CSR: TRIG_EN Mask

Definition at line 6531 of file Nano100Series.h.

## ◆ VDMA_CSR_TRIG_EN_Pos

#define VDMA_CSR_TRIG_EN_Pos (23)

VDMA_T::CSR: TRIG_EN Position

Definition at line 6530 of file Nano100Series.h.

## ◆ VDMA_CSR_VDMACEN_Msk

#define VDMA_CSR_VDMACEN_Msk (0x1ul << VDMA_CSR_VDMACEN_Pos)

VDMA_T::CSR: VDMACEN Mask

Definition at line 6519 of file Nano100Series.h.

## ◆ VDMA_CSR_VDMACEN_Pos

#define VDMA_CSR_VDMACEN_Pos (0)

    @addtogroup VDMA_CONST VDMA Bit Field Definition
    Constant Definitions for VDMA Controller

VDMA_T::CSR: VDMACEN Position

Definition at line 6518 of file Nano100Series.h.

## ◆ VDMA_DAR_VDMA_DAR_Msk

#define VDMA_DAR_VDMA_DAR_Msk (0xfffffffful << VDMA_DAR_VDMA_DAR_Pos)

VDMA_T::DAR: VDMA_DAR Mask

Definition at line 6537 of file Nano100Series.h.

## ◆ VDMA_DAR_VDMA_DAR_Pos

#define VDMA_DAR_VDMA_DAR_Pos (0)

VDMA_T::DAR: VDMA_DAR Position

Definition at line 6536 of file Nano100Series.h.

## ◆ VDMA_DASOCR_DASTOBL_Msk

#define VDMA_DASOCR_DASTOBL_Msk (0xfffful << VDMA_DASOCR_DASTOBL_Pos)

VDMA_T::DASOCR: DASTOBL Mask

Definition at line 6570 of file Nano100Series.h.

## ◆ VDMA_DASOCR_DASTOBL_Pos

#define VDMA_DASOCR_DASTOBL_Pos (0)

VDMA_T::DASOCR: DASTOBL Position

Definition at line 6569 of file Nano100Series.h.

## ◆ VDMA_IER_TABORT_IE_Msk

#define VDMA_IER_TABORT_IE_Msk (0x1ul << VDMA_IER_TABORT_IE_Pos)

VDMA_T::IER: TABORT_IE Mask

Definition at line 6552 of file Nano100Series.h.

## ◆ VDMA_IER_TABORT_IE_Pos

#define VDMA_IER_TABORT_IE_Pos (0)

VDMA_T::IER: TABORT_IE Position

Definition at line 6551 of file Nano100Series.h.

## ◆ VDMA_IER_TD_IE_Msk

#define VDMA_IER_TD_IE_Msk (0x1ul << VDMA_IER_TD_IE_Pos)

VDMA_T::IER: TD_IE Mask

Definition at line 6555 of file Nano100Series.h.

## ◆ VDMA_IER_TD_IE_Pos

#define VDMA_IER_TD_IE_Pos (1)

VDMA_T::IER: TD_IE Position

Definition at line 6554 of file Nano100Series.h.

## ◆ VDMA_ISR_TABORT_IS_Msk

#define VDMA_ISR_TABORT_IS_Msk (0x1ul << VDMA_ISR_TABORT_IS_Pos)

VDMA_T::ISR: TABORT_IS Mask

Definition at line 6558 of file Nano100Series.h.

## ◆ VDMA_ISR_TABORT_IS_Pos

#define VDMA_ISR_TABORT_IS_Pos (0)

VDMA_T::ISR: TABORT_IS Position

Definition at line 6557 of file Nano100Series.h.

## ◆ VDMA_ISR_TD_IS_Msk

#define VDMA_ISR_TD_IS_Msk (0x1ul << VDMA_ISR_TD_IS_Pos)

VDMA_T::ISR: TD_IS Mask

Definition at line 6561 of file Nano100Series.h.

## ◆ VDMA_ISR_TD_IS_Pos

#define VDMA_ISR_TD_IS_Pos (1)

VDMA_T::ISR: TD_IS Position

Definition at line 6560 of file Nano100Series.h.

## ◆ VDMA_SAR_VDMA_SAR_Msk

#define VDMA_SAR_VDMA_SAR_Msk (0xfffffffful << VDMA_SAR_VDMA_SAR_Pos)

VDMA_T::SAR: VDMA_SAR Mask

Definition at line 6534 of file Nano100Series.h.

## ◆ VDMA_SAR_VDMA_SAR_Pos

#define VDMA_SAR_VDMA_SAR_Pos (0)

VDMA_T::SAR: VDMA_SAR Position

Definition at line 6533 of file Nano100Series.h.

## ◆ VDMA_SASOCR_SASTOBL_Msk

#define VDMA_SASOCR_SASTOBL_Msk (0xfffful << VDMA_SASOCR_SASTOBL_Pos)

VDMA_T::SASOCR: SASTOBL Mask

Definition at line 6564 of file Nano100Series.h.

## ◆ VDMA_SASOCR_SASTOBL_Pos

#define VDMA_SASOCR_SASTOBL_Pos (0)

VDMA_T::SASOCR: SASTOBL Position

Definition at line 6563 of file Nano100Series.h.

## ◆ VDMA_SASOCR_STBC_Msk

#define VDMA_SASOCR_STBC_Msk (0xfffful << VDMA_SASOCR_STBC_Pos)

VDMA_T::SASOCR: STBC Mask

Definition at line 6567 of file Nano100Series.h.

## ◆ VDMA_SASOCR_STBC_Pos

#define VDMA_SASOCR_STBC_Pos (16)

VDMA_T::SASOCR: STBC Position

Definition at line 6566 of file Nano100Series.h.

## ◆ WDT_CTL_WTE_Msk

#define WDT_CTL_WTE_Msk (0x1ul << WDT_CTL_WTE_Pos)

WDT_T::CTL: WTE Mask

Definition at line 11438 of file Nano100Series.h.

## ◆ WDT_CTL_WTE_Pos

#define WDT_CTL_WTE_Pos (3)

WDT_T::CTL: WTE Position

Definition at line 11437 of file Nano100Series.h.

## ◆ WDT_CTL_WTIS_Msk

#define WDT_CTL_WTIS_Msk (0x7ul << WDT_CTL_WTIS_Pos)

WDT_T::CTL: WTIS Mask

Definition at line 11441 of file Nano100Series.h.

## ◆ WDT_CTL_WTIS_Pos

#define WDT_CTL_WTIS_Pos (4)

WDT_T::CTL: WTIS Position

Definition at line 11440 of file Nano100Series.h.

## ◆ WDT_CTL_WTR_Msk

#define WDT_CTL_WTR_Msk (0x1ul << WDT_CTL_WTR_Pos)

WDT_T::CTL: WTR Mask

Definition at line 11429 of file Nano100Series.h.

## ◆ WDT_CTL_WTR_Pos

#define WDT_CTL_WTR_Pos (0)

    @addtogroup WDT_CONST WDT Bit Field Definition
    Constant Definitions for WDT Controller

WDT_T::CTL: WTR Position

Definition at line 11428 of file Nano100Series.h.

## ◆ WDT_CTL_WTRDSEL_Msk

#define WDT_CTL_WTRDSEL_Msk (0x3ul << WDT_CTL_WTRDSEL_Pos)

WDT_T::CTL: WTRDSEL Mask

Definition at line 11444 of file Nano100Series.h.

## ◆ WDT_CTL_WTRDSEL_Pos

#define WDT_CTL_WTRDSEL_Pos (8)

WDT_T::CTL: WTRDSEL Position

Definition at line 11443 of file Nano100Series.h.

## ◆ WDT_CTL_WTRE_Msk

#define WDT_CTL_WTRE_Msk (0x1ul << WDT_CTL_WTRE_Pos)

WDT_T::CTL: WTRE Mask

Definition at line 11432 of file Nano100Series.h.

## ◆ WDT_CTL_WTRE_Pos

#define WDT_CTL_WTRE_Pos (1)

WDT_T::CTL: WTRE Position

Definition at line 11431 of file Nano100Series.h.

## ◆ WDT_CTL_WTWKE_Msk

#define WDT_CTL_WTWKE_Msk (0x1ul << WDT_CTL_WTWKE_Pos)

WDT_T::CTL: WTWKE Mask

Definition at line 11435 of file Nano100Series.h.

## ◆ WDT_CTL_WTWKE_Pos

#define WDT_CTL_WTWKE_Pos (2)

WDT_T::CTL: WTWKE Position

Definition at line 11434 of file Nano100Series.h.

## ◆ WDT_IER_IE_Msk

#define WDT_IER_IE_Msk (0x1ul << WDT_IER_IE_Pos)

WDT_T::IER: IE Mask

Definition at line 11447 of file Nano100Series.h.

## ◆ WDT_IER_IE_Pos

#define WDT_IER_IE_Pos (0)

WDT_T::IER: IE Position

Definition at line 11446 of file Nano100Series.h.

## ◆ WDT_ISR_IS_Msk

#define WDT_ISR_IS_Msk (0x1ul << WDT_ISR_IS_Pos)

WDT_T::ISR: IS Mask

Definition at line 11450 of file Nano100Series.h.

## ◆ WDT_ISR_IS_Pos

#define WDT_ISR_IS_Pos (0)

WDT_T::ISR: IS Position

Definition at line 11449 of file Nano100Series.h.

## ◆ WDT_ISR_RST_IS_Msk

#define WDT_ISR_RST_IS_Msk (0x1ul << WDT_ISR_RST_IS_Pos)

WDT_T::ISR: RST_IS Mask

Definition at line 11453 of file Nano100Series.h.

## ◆ WDT_ISR_RST_IS_Pos

#define WDT_ISR_RST_IS_Pos (1)

WDT_T::ISR: RST_IS Position

Definition at line 11452 of file Nano100Series.h.

## ◆ WDT_ISR_WAKE_IS_Msk

#define WDT_ISR_WAKE_IS_Msk (0x1ul << WDT_ISR_WAKE_IS_Pos)

WDT_T::ISR: WAKE_IS Mask

Definition at line 11456 of file Nano100Series.h.

## ◆ WDT_ISR_WAKE_IS_Pos

#define WDT_ISR_WAKE_IS_Pos (2)

WDT_T::ISR: WAKE_IS Position

Definition at line 11455 of file Nano100Series.h.

## ◆ WWDT_CR_DBGEN_Msk

#define WWDT_CR_DBGEN_Msk (0x1ul << WWDT_CR_DBGEN_Pos)

WWDT_T::CR: DBGEN Mask

Definition at line 11572 of file Nano100Series.h.

## ◆ WWDT_CR_DBGEN_Pos

#define WWDT_CR_DBGEN_Pos (31)

WWDT_T::CR: DBGEN Position

Definition at line 11571 of file Nano100Series.h.

## ◆ WWDT_CR_PERIODSEL_Msk

#define WWDT_CR_PERIODSEL_Msk (0xful << WWDT_CR_PERIODSEL_Pos)

WWDT_T::CR: PERIODSEL Mask

Definition at line 11566 of file Nano100Series.h.

## ◆ WWDT_CR_PERIODSEL_Pos

#define WWDT_CR_PERIODSEL_Pos (8)

WWDT_T::CR: PERIODSEL Position

Definition at line 11565 of file Nano100Series.h.

## ◆ WWDT_CR_WINCMP_Msk

#define WWDT_CR_WINCMP_Msk (0x3ful << WWDT_CR_WINCMP_Pos)

WWDT_T::CR: WINCMP Mask

Definition at line 11569 of file Nano100Series.h.

## ◆ WWDT_CR_WINCMP_Pos

#define WWDT_CR_WINCMP_Pos (16)

WWDT_T::CR: WINCMP Position

Definition at line 11568 of file Nano100Series.h.

## ◆ WWDT_CR_WWDTEN_Msk

#define WWDT_CR_WWDTEN_Msk (0x1ul << WWDT_CR_WWDTEN_Pos)

WWDT_T::CR: WWDTEN Mask

Definition at line 11563 of file Nano100Series.h.

## ◆ WWDT_CR_WWDTEN_Pos

#define WWDT_CR_WWDTEN_Pos (0)

WWDT_T::CR: WWDTEN Position

Definition at line 11562 of file Nano100Series.h.

## ◆ WWDT_IER_WWDTIE_Msk

#define WWDT_IER_WWDTIE_Msk (0x1ul << WWDT_IER_WWDTIE_Pos)

WWDT_T::IER: WWDTIE Mask

Definition at line 11575 of file Nano100Series.h.

## ◆ WWDT_IER_WWDTIE_Pos

#define WWDT_IER_WWDTIE_Pos (0)

WWDT_T::IER: WWDTIE Position

Definition at line 11574 of file Nano100Series.h.

## ◆ WWDT_RLD_WWDTRLD_Msk

#define WWDT_RLD_WWDTRLD_Msk (0xfffffffful << WWDT_RLD_RLD_Pos)

WWDT_T::RLD: RLD Mask

Definition at line 11560 of file Nano100Series.h.

## ◆ WWDT_RLD_WWDTRLD_Pos

#define WWDT_RLD_WWDTRLD_Pos (0)

    @addtogroup WWDT_CONST WWDT Bit Field Definition
    Constant Definitions for WWDT Controller

WWDT_T::RLD: RLD Position

Definition at line 11559 of file Nano100Series.h.

## ◆ WWDT_STS_IF_Msk

#define WWDT_STS_IF_Msk (0x1ul << WWDT_STS_IF_Pos)

WWDT_T::STS: IF Mask

Definition at line 11578 of file Nano100Series.h.

## ◆ WWDT_STS_IF_Pos

#define WWDT_STS_IF_Pos (0)

WWDT_T::STS: IF Position

Definition at line 11577 of file Nano100Series.h.

## ◆ WWDT_STS_RF_Msk

#define WWDT_STS_RF_Msk (0x1ul << WWDT_STS_RF_Pos)

WWDT_T::STS: RF Mask

Definition at line 11581 of file Nano100Series.h.

## ◆ WWDT_STS_RF_Pos

#define WWDT_STS_RF_Pos (1)

WWDT_T::STS: RF Position

Definition at line 11580 of file Nano100Series.h.

## ◆ WWDT_VAL_WWDTVAL_Msk

#define WWDT_VAL_WWDTVAL_Msk (0x3ful << WWDT_VAL_WWDTVAL_Pos)

WWDT_T::VAL: WWDTVAL Mask

Definition at line 11584 of file Nano100Series.h.

## ◆ WWDT_VAL_WWDTVAL_Pos

#define WWDT_VAL_WWDTVAL_Pos (0)

WWDT_T::VAL: WWDTVAL Position

Definition at line 11583 of file Nano100Series.h.