| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
SPI_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | STATUS
__IO uint32_t | CLKDIV
__IO uint32_t | SSR
__I uint32_t | RX0
__I uint32_t | RX1
uint32_t | RESERVE0 [2]
__O uint32_t | TX0
__O uint32_t | TX1
uint32_t | RESERVE1 [3]
__IO uint32_t | VARCLK
__IO uint32_t | DMA
__IO uint32_t | FFCTL
uint32_t | RESERVE2 [4]

## Detailed Description

    @addtogroup SPI Serial Peripheral Interface Controller(SPI)
    Memory Mapped Structure for SPI Controller

Definition at line 8460 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h