| Nano102_112 Series BSP V3.03.002 The Board Support Package for Nano102_112 Series

sys.h
Go to the documentation of this file.
1 /**************************************************************************/
12 #ifndef __SYS_H__
13 #define __SYS_H__
14
15 #ifdef __cplusplus
16 extern "C"
17 {
18 #endif
19
32 /*---------------------------------------------------------------------------------------------------------*/
33 /* Module Reset Control Resister constant definitions. */
34 /*---------------------------------------------------------------------------------------------------------*/
35 #define CPU_RST ((0x0<<24) | SYS_IPRST_CTL1_CPU_RST_Pos )
36 #define CHIP_RST ((0x0<<24) | SYS_IPRST_CTL1_CHIP_RST_Pos )
37 #define DMA_RST ((0x0<<24) | SYS_IPRST_CTL1_DMA_RST_Pos )
38 #define SC1_RST ((0x4<<24) | SYS_IPRST_CTL2_SC1_RST_Pos )
39 #define SC0_RST ((0x4<<24) | SYS_IPRST_CTL2_SC0_RST_Pos )
40 #define ADC_RST ((0x4<<24) | SYS_IPRST_CTL2_ADC_RST_Pos )
41 #define LCD_RST ((0x4<<24) | SYS_IPRST_CTL2_LCD_RST_Pos )
42 #define ACMP01_RST ((0x4<<24) | SYS_IPRST_CTL2_ACMP01_RST_Pos )
43 #define PWM0_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM0_RST_Pos )
44 #define UART1_RST ((0x4<<24) | SYS_IPRST_CTL2_UART1_RST_Pos )
45 #define UART0_RST ((0x4<<24) | SYS_IPRST_CTL2_UART0_RST_Pos )
46 #define SPI1_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI1_RST_Pos )
47 #define SPI0_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI0_RST_Pos )
48 #define I2C1_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C1_RST_Pos )
49 #define I2C0_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C0_RST_Pos )
50 #define TMR3_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR3_RST_Pos )
51 #define TMR2_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR2_RST_Pos )
52 #define TMR1_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR1_RST_Pos )
53 #define TMR0_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR0_RST_Pos )
54 #define GPIO_RST ((0x4<<24) | SYS_IPRST_CTL2_GPIO_RST_Pos )
56 /*---------------------------------------------------------------------------------------------------------*/
57 /* Multi-Function constant definitions. */
58 /*---------------------------------------------------------------------------------------------------------*/
59
60 /********************* Bit definition of VREFCTL register **********************/
61 #define SYS_VREFCTL_BGP_EN ((uint32_t)0x00000001)
62 #define SYS_VREFCTL_REG_EN ((uint32_t)0x00000002)
63 #define SYS_VREFCTL_SEL25 ((uint32_t)0x00000008)
64 #define SYS_VREFCTL_SEL18 ((uint32_t)0x00000004)
65 #define SYS_VREFCTL_SEL15 ((uint32_t)0x00000000)
66 #define SYS_VREFCTL_EXTMODE ((uint32_t)0x00000010)
69 /********************* Bit definition of LDOCTL register **********************/
70 #define SYS_LDOCTL_LDO_PD ((uint32_t)0x00000001)
71 #define SYS_LDOCTL_LDO_LEVEL16 ((uint32_t)0x00000004)
72 #define SYS_LDOCTL_LDO_LEVEL18 ((uint32_t)0x00000008)
75 /********************* Bit definition of IRCTRIMCTL register **********************/
76 #define SYS_IRCTRIMCTL_TRIM_11_0592M ((uint32_t)0x00000001)
77 #define SYS_IRCTRIMCTL_TRIM_12M ((uint32_t)0x00000002)
78 #define SYS_IRCTRIMCTL_TRIM_16M ((uint32_t)0x00000003)
80 #define SYS_IRCTRIMCTL_LOOP_4CLK ((uint32_t)0x00000000)
81 #define SYS_IRCTRIMCTL_LOOP_8CLK ((uint32_t)0x00000010)
82 #define SYS_IRCTRIMCTL_LOOP_16CLK ((uint32_t)0x00000020)
83 #define SYS_IRCTRIMCTL_LOOP_32CLK ((uint32_t)0x00000030)
85 #define SYS_IRCTRIMCTL_RETRY_64 ((uint32_t)0x00000000)
86 #define SYS_IRCTRIMCTL_RETRY_128 ((uint32_t)0x00000040)
87 #define SYS_IRCTRIMCTL_RETRY_256 ((uint32_t)0x00000080)
88 #define SYS_IRCTRIMCTL_RETRY_512 ((uint32_t)0x000000C0)
90 #define SYS_IRCTRIMCTL_CLKERR_STOP ((uint32_t)0x00000100)
92 /********************* Bit definition of IRCTRIMIEN register **********************/
93 #define SYS_IRCTRIMIEN_DISABLE ((uint32_t)0x00000000)
94 #define SYS_IRCTRIMIEN_FAIL_EN ((uint32_t)0x00000002)
95 #define SYS_IRCTRIMIEN_32KERR_EN ((uint32_t)0x00000004)
97 /********************* Bit definition of IRCTRIMINT register **********************/
98 #define SYS_IRCTRIMINT_FREQLOCK ((uint32_t)0x00000001)
99 #define SYS_IRCTRIMINT_FAIL_INT ((uint32_t)0x00000002)
100 #define SYS_IRCTRIMINT_32KERR_INT ((uint32_t)0x00000004)
102 /********************* Bit definition of PA_L_MFP register **********************/
103 #define SYS_PA_L_MFP_PA7_MFP_GPA7 (0UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
104 #define SYS_PA_L_MFP_PA7_MFP_ADC_CH7 (2UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
105 #define SYS_PA_L_MFP_PA7_MFP_SC1_CD (4UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
108 #define SYS_PA_L_MFP_PA6_MFP_GPA6 (0UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
109 #define SYS_PA_L_MFP_PA6_MFP_ADC_CH6 (2UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
110 #define SYS_PA_L_MFP_PA6_MFP_ACMP0_O (3UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
111 #define SYS_PA_L_MFP_PA6_MFP_SC0_RST (4UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
112 #define SYS_PA_L_MFP_PA6_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
115 #define SYS_PA_L_MFP_PA5_MFP_GPA5 (0UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
116 #define SYS_PA_L_MFP_PA5_MFP_ADC_CH5 (2UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
117 #define SYS_PA_L_MFP_PA5_MFP_ACMP0_N (3UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
118 #define SYS_PA_L_MFP_PA5_MFP_SC0_PWR (4UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
119 #define SYS_PA_L_MFP_PA5_MFP_I2C1_SDA (5UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
120 #define SYS_PA_L_MFP_PA5_MFP_SPI1_SS0 (6UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
121 #define SYS_PA_L_MFP_PA5_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
123 #define SYS_PA_L_MFP_PA4_MFP_GPA4 (0UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
124 #define SYS_PA_L_MFP_PA4_MFP_ADC_CH4 (2UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
125 #define SYS_PA_L_MFP_PA4_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
126 #define SYS_PA_L_MFP_PA4_MFP_SC0_CD (4UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
127 #define SYS_PA_L_MFP_PA4_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
129 #define SYS_PA_L_MFP_PA3_MFP_GPA3 (0UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
130 #define SYS_PA_L_MFP_PA3_MFP_EINT1 (1UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
131 #define SYS_PA_L_MFP_PA3_MFP_ADC_CH3 (2UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
132 #define SYS_PA_L_MFP_PA3_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
133 #define SYS_PA_L_MFP_PA3_MFP_SC0_DAT (4UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
134 #define SYS_PA_L_MFP_PA3_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
136 #define SYS_PA_L_MFP_PA2_MFP_GPA2 (0UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
137 #define SYS_PA_L_MFP_PA2_MFP_EINT0 (1UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
138 #define SYS_PA_L_MFP_PA2_MFP_ADC_CH2 (2UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
139 #define SYS_PA_L_MFP_PA2_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
140 #define SYS_PA_L_MFP_PA2_MFP_SC0_CLK (4UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
141 #define SYS_PA_L_MFP_PA2_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
143 #define SYS_PA_L_MFP_PA1_MFP_GPA1 (0UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
144 #define SYS_PA_L_MFP_PA1_MFP_ADC_CH1 (2UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
145 #define SYS_PA_L_MFP_PA1_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
146 #define SYS_PA_L_MFP_PA1_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
148 #define SYS_PA_L_MFP_PA0_MFP_GPA0 (0UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
149 #define SYS_PA_L_MFP_PA0_MFP_ADC_CH0 (2UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
151 /********************* Bit definition of PA_H_MFP register **********************/
152 #define SYS_PA_H_MFP_PA15_MFP_GPA15 (0UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
153 #define SYS_PA_H_MFP_PA15_MFP_TMR3_CAP (2UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
154 #define SYS_PA_H_MFP_PA15_MFP_ACMP1_O (3UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
155 #define SYS_PA_H_MFP_PA15_MFP_I2C1_SDA (5UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
156 #define SYS_PA_H_MFP_PA15_MFP_SPI1_SS0 (6UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
157 #define SYS_PA_H_MFP_PA15_MFP_LCD_S16 (8UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
158 #define SYS_PA_H_MFP_PA15_MFP_LCD_S30 (8UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
160 #define SYS_PA_H_MFP_PA14_MFP_GPA14 (0UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
161 #define SYS_PA_H_MFP_PA14_MFP_I2C1_SCL (5UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
162 #define SYS_PA_H_MFP_PA14_MFP_SPI1_SCLK (6UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
163 #define SYS_PA_H_MFP_PA14_MFP_LCD_S17 (8UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
164 #define SYS_PA_H_MFP_PA14_MFP_LCD_S31 (8UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
165 #define SYS_PA_H_MFP_PA14_MFP_ACMP0_C (9UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
167 #define SYS_PA_H_MFP_PA13_MFP_GPA13 (0UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
168 #define SYS_PA_H_MFP_PA13_MFP_ACMP1_N (3UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
169 #define SYS_PA_H_MFP_PA13_MFP_I2C0_SDA (5UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
170 #define SYS_PA_H_MFP_PA13_MFP_SPI1_MISO0 (6UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
171 #define SYS_PA_H_MFP_PA13_MFP_UART0_RX (7UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
172 #define SYS_PA_H_MFP_PA13_MFP_LCD_S18 (8UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
174 #define SYS_PA_H_MFP_PA12_MFP_GPA12 (0UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
175 #define SYS_PA_H_MFP_PA12_MFP_ACMP1_P (3UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
176 #define SYS_PA_H_MFP_PA12_MFP_I2C0_SCL (5UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
177 #define SYS_PA_H_MFP_PA12_MFP_SPI1_MOSI0 (6UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
178 #define SYS_PA_H_MFP_PA12_MFP_UART0_TX (7UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
179 #define SYS_PA_H_MFP_PA12_MFP_LCD_S19 (8UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
181 #define SYS_PA_H_MFP_PA11_MFP_GPA11 (0UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
182 #define SYS_PA_H_MFP_PA11_MFP_ADC_EXT (2UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
183 #define SYS_PA_H_MFP_PA11_MFP_SC0_DAT (4UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
185 #define SYS_PA_H_MFP_PA10_MFP_GPA10 (0UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
186 #define SYS_PA_H_MFP_PA10_MFP_SC0_CLK (4UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
188 #define SYS_PA_H_MFP_PA9_MFP_GPA9 (0UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
189 #define SYS_PA_H_MFP_PA9_MFP_SC0_RST (4UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
191 #define SYS_PA_H_MFP_PA8_MFP_GPA8 (0UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
192 #define SYS_PA_H_MFP_PA8_MFP_SC0_PWR (4UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
194 /********************* Bit definition of PB_L_MFP register **********************/
195 #define SYS_PB_L_MFP_PB7_MFP_GPB7 (0UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
196 #define SYS_PB_L_MFP_PB7_MFP_SC0_CD (4UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
197 #define SYS_PB_L_MFP_PB7_MFP_UART1_CTS (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
198 #define SYS_PB_L_MFP_PB7_MFP_LCD_S33 (8UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
200 #define SYS_PB_L_MFP_PB6_MFP_GPB6 (0UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
201 #define SYS_PB_L_MFP_PB6_MFP_CKO0 (1UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
202 #define SYS_PB_L_MFP_PB6_MFP_SPI1_SS1 (6UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
203 #define SYS_PB_L_MFP_PB6_MFP_UART1_TX (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
204 #define SYS_PB_L_MFP_PB6_MFP_LCD_S25 (8UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
205 #define SYS_PB_L_MFP_PB6_MFP_LCD_S34 (8UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
207 #define SYS_PB_L_MFP_PB5_MFP_GPB5 (0UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
208 #define SYS_PB_L_MFP_PB5_MFP_SPI1_MOSI1 (6UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
209 #define SYS_PB_L_MFP_PB5_MFP_UART1_RX (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
210 #define SYS_PB_L_MFP_PB5_MFP_LCD_S35 (8UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
212 #define SYS_PB_L_MFP_PB4_MFP_GPB4 (0UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
213 #define SYS_PB_L_MFP_PB4_MFP_SPI1_MISO1 (6UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
214 #define SYS_PB_L_MFP_PB4_MFP_UART1_RTS (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
216 #define SYS_PB_L_MFP_PB3_MFP_GPB3 (0UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
217 #define SYS_PB_L_MFP_PB3_MFP_TMR2_CNT (2UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
218 #define SYS_PB_L_MFP_PB3_MFP_I2C0_SDA (5UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
219 #define SYS_PB_L_MFP_PB3_MFP_SPI1_MISO1 (6UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
220 #define SYS_PB_L_MFP_PB3_MFP_UART0_CTS (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
221 #define SYS_PB_L_MFP_PB3_MFP_LCD_S26 (8UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
222 #define SYS_PB_L_MFP_PB3_MFP_TMR2_OUT (0xAUL<<SYS_PB_L_MFP_PB3_MFP_Pos)
224 #define SYS_PB_L_MFP_PB2_MFP_GPB2 (0UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
225 #define SYS_PB_L_MFP_PB2_MFP_TMR3_CNT (2UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
226 #define SYS_PB_L_MFP_PB2_MFP_I2C0_SCL (5UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
227 #define SYS_PB_L_MFP_PB2_MFP_SPI1_MOSI1 (6UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
228 #define SYS_PB_L_MFP_PB2_MFP_UART0_RTS (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
229 #define SYS_PB_L_MFP_PB2_MFP_LCD_S27 (8UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
230 #define SYS_PB_L_MFP_PB2_MFP_TMR3_OUT (0xAUL<<SYS_PB_L_MFP_PB2_MFP_Pos)
232 #define SYS_PB_L_MFP_PB1_MFP_GPB1 (0UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
233 #define SYS_PB_L_MFP_PB1_MFP_EINT1 (1UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
234 #define SYS_PB_L_MFP_PB1_MFP_TMR2_CAP (2UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
235 #define SYS_PB_L_MFP_PB1_MFP_UART0_RX (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
236 #define SYS_PB_L_MFP_PB1_MFP_LCD_S28 (8UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
238 #define SYS_PB_L_MFP_PB0_MFP_GPB0 (0UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
239 #define SYS_PB_L_MFP_PB0_MFP_CKO1 (1UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
240 #define SYS_PB_L_MFP_PB0_MFP_UART0_TX (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
241 #define SYS_PB_L_MFP_PB0_MFP_LCD_S29 (8UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
243 /********************* Bit definition of PB_H_MFP register **********************/
244 #define SYS_PB_H_MFP_PB15_MFP_GPB15 (0UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
245 #define SYS_PB_H_MFP_PB15_MFP_SPI0_SS0 (6UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
246 #define SYS_PB_H_MFP_PB15_MFP_UART0_CTS (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
247 #define SYS_PB_H_MFP_PB15_MFP_LCD_S12 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
248 #define SYS_PB_H_MFP_PB15_MFP_LCD_S19 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
249 #define SYS_PB_H_MFP_PB15_MFP_LCD_S23 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
251 #define SYS_PB_H_MFP_PB14_MFP_GPB14 (0UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
252 #define SYS_PB_H_MFP_PB14_MFP_SPI0_SCLK (6UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
253 #define SYS_PB_H_MFP_PB14_MFP_UART0_TX (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
254 #define SYS_PB_H_MFP_PB14_MFP_LCD_S13 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
255 #define SYS_PB_H_MFP_PB14_MFP_LCD_S20 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
256 #define SYS_PB_H_MFP_PB14_MFP_LCD_S24 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
258 #define SYS_PB_H_MFP_PB13_MFP_GPB13 (0UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
259 #define SYS_PB_H_MFP_PB13_MFP_SPI0_MISO0 (6UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
260 #define SYS_PB_H_MFP_PB13_MFP_UART0_RX (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
261 #define SYS_PB_H_MFP_PB13_MFP_LCD_S14 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
262 #define SYS_PB_H_MFP_PB13_MFP_LCD_S21 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
263 #define SYS_PB_H_MFP_PB13_MFP_LCD_S25 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
265 #define SYS_PB_H_MFP_PB12_MFP_GPB12 (0UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
266 #define SYS_PB_H_MFP_PB12_MFP_CKO0 (1UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
267 #define SYS_PB_H_MFP_PB12_MFP_TMR0_CNT (2UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
268 #define SYS_PB_H_MFP_PB12_MFP_SPI0_MOSI0 (6UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
269 #define SYS_PB_H_MFP_PB12_MFP_UART0_RTS (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
270 #define SYS_PB_H_MFP_PB12_MFP_LCD_S15 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
271 #define SYS_PB_H_MFP_PB12_MFP_LCD_S22 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
272 #define SYS_PB_H_MFP_PB12_MFP_LCD_S26 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
273 #define SYS_PB_H_MFP_PB12_MFP_TMR0_OUT (0xAUL<<SYS_PB_H_MFP_PB12_MFP_Pos)
275 #define SYS_PB_H_MFP_PB11_MFP_GPB11 (0UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
276 #define SYS_PB_H_MFP_PB11_MFP_TMR1_CNT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
277 #define SYS_PB_H_MFP_PB11_MFP_SPI0_MISO1 (6UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
278 #define SYS_PB_H_MFP_PB11_MFP_UART1_RTS (7UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
279 #define SYS_PB_H_MFP_PB11_MFP_LCD_S23 (8UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
280 #define SYS_PB_H_MFP_PB11_MFP_LCD_S27 (8UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
281 #define SYS_PB_H_MFP_PB11_MFP_TMR1_OUT (0xAUL<<SYS_PB_H_MFP_PB11_MFP_Pos)
283 #define SYS_PB_H_MFP_PB10_MFP_GPB10 (0UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
284 #define SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI1 (6UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
285 #define SYS_PB_H_MFP_PB10_MFP_UART1_RX (7UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
286 #define SYS_PB_H_MFP_PB10_MFP_LCD_S24 (8UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
287 #define SYS_PB_H_MFP_PB10_MFP_LCD_S28 (8UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
289 #define SYS_PB_H_MFP_PB9_MFP_GPB9 (0UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
290 #define SYS_PB_H_MFP_PB9_MFP_PWM0_CH1 (3UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
291 #define SYS_PB_H_MFP_PB9_MFP_LCD_S31 (8UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
293 #define SYS_PB_H_MFP_PB8_MFP_GPB8 (0UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
294 #define SYS_PB_H_MFP_PB8_MFP_EINT1 (1UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
295 #define SYS_PB_H_MFP_PB8_MFP_TMR0_CNT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
296 #define SYS_PB_H_MFP_PB8_MFP_PWM0_CH0 (3UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
297 #define SYS_PB_H_MFP_PB8_MFP_SNOOPER (4UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
298 #define SYS_PB_H_MFP_PB8_MFP_LCD_S32 (8UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
299 #define SYS_PB_H_MFP_PB8_MFP_TMR0_OUT (0xAUL<<SYS_PB_H_MFP_PB8_MFP_Pos)
301 /********************* Bit definition of PC_L_MFP register **********************/
302 #define SYS_PC_L_MFP_PC7_MFP_GPC7 (0UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
303 #define SYS_PC_L_MFP_PC7_MFP_SC0_PWR (4UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
304 #define SYS_PC_L_MFP_PC7_MFP_UART1_RX (7UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
305 #define SYS_PC_L_MFP_PC7_MFP_LCD_S4 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
306 #define SYS_PC_L_MFP_PC7_MFP_LCD_S11 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
307 #define SYS_PC_L_MFP_PC7_MFP_LCD_S15 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
309 #define SYS_PC_L_MFP_PC6_MFP_GPC6 (0UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
310 #define SYS_PC_L_MFP_PC6_MFP_SC0_DAT (4UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
311 #define SYS_PC_L_MFP_PC6_MFP_UART1_RTS (7UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
312 #define SYS_PC_L_MFP_PC6_MFP_LCD_S5 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
313 #define SYS_PC_L_MFP_PC6_MFP_LCD_S12 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
314 #define SYS_PC_L_MFP_PC6_MFP_LCD_S16 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
316 #define SYS_PC_L_MFP_PC5_MFP_GPC5 (0UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
317 #define SYS_PC_L_MFP_PC5_MFP_SC0_CD (4UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
318 #define SYS_PC_L_MFP_PC5_MFP_LCD_S6 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
319 #define SYS_PC_L_MFP_PC5_MFP_LCD_S13 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
320 #define SYS_PC_L_MFP_PC5_MFP_LCD_S17 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
322 #define SYS_PC_L_MFP_PC4_MFP_GPC4 (0UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
323 #define SYS_PC_L_MFP_PC4_MFP_EINT0 (1UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
324 #define SYS_PC_L_MFP_PC4_MFP_SC0_CLK (4UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
325 #define SYS_PC_L_MFP_PC4_MFP_UART1_CTS (7UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
326 #define SYS_PC_L_MFP_PC4_MFP_LCD_S7 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
327 #define SYS_PC_L_MFP_PC4_MFP_LCD_S14 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
328 #define SYS_PC_L_MFP_PC4_MFP_LCD_S18 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
330 #define SYS_PC_L_MFP_PC3_MFP_GPC3 (0UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
331 #define SYS_PC_L_MFP_PC3_MFP_PWM0_CH3 (3UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
332 #define SYS_PC_L_MFP_PC3_MFP_I2C1_SDA (5UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
333 #define SYS_PC_L_MFP_PC3_MFP_LCD_S8 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
334 #define SYS_PC_L_MFP_PC3_MFP_LCD_S15 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
335 #define SYS_PC_L_MFP_PC3_MFP_LCD_S19 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
337 #define SYS_PC_L_MFP_PC2_MFP_GPC2 (0UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
338 #define SYS_PC_L_MFP_PC2_MFP_PWM0_CH2 (3UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
339 #define SYS_PC_L_MFP_PC2_MFP_I2C1_SCL (5UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
340 #define SYS_PC_L_MFP_PC2_MFP_LCD_S9 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
341 #define SYS_PC_L_MFP_PC2_MFP_LCD_S16 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
342 #define SYS_PC_L_MFP_PC2_MFP_LCD_S20 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
344 #define SYS_PC_L_MFP_PC1_MFP_GPC1 (0UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
345 #define SYS_PC_L_MFP_PC1_MFP_PWM0_CH1 (3UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
346 #define SYS_PC_L_MFP_PC1_MFP_I2C0_SDA (5UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
347 #define SYS_PC_L_MFP_PC1_MFP_LCD_S10 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
348 #define SYS_PC_L_MFP_PC1_MFP_LCD_S17 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
349 #define SYS_PC_L_MFP_PC1_MFP_LCD_S21 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
351 #define SYS_PC_L_MFP_PC0_MFP_GPC0 (0UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
352 #define SYS_PC_L_MFP_PC0_MFP_PWM0_CH0 (3UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
353 #define SYS_PC_L_MFP_PC0_MFP_I2C0_SCL (5UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
354 #define SYS_PC_L_MFP_PC0_MFP_SPI0_SS1 (6UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
355 #define SYS_PC_L_MFP_PC0_MFP_LCD_S11 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
356 #define SYS_PC_L_MFP_PC0_MFP_LCD_S18 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
357 #define SYS_PC_L_MFP_PC0_MFP_LCD_S22 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
359 /********************* Bit definition of PC_H_MFP register **********************/
360 #define SYS_PC_H_MFP_PC15_MFP_GPC15 (0UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
361 #define SYS_PC_H_MFP_PC15_MFP_SC1_PWR (4UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
362 #define SYS_PC_H_MFP_PC15_MFP_LCD_S0 (8UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
363 #define SYS_PC_H_MFP_PC15_MFP_LCD_S7 (8UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
365 #define SYS_PC_H_MFP_PC14_MFP_GPC14 (0UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
366 #define SYS_PC_H_MFP_PC14_MFP_SC1_CD (4UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
367 #define SYS_PC_H_MFP_PC14_MFP_LCD_S1 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
368 #define SYS_PC_H_MFP_PC14_MFP_LCD_S8 (8UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
370 #define SYS_PC_H_MFP_PC13_MFP_GPC13 (0UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
371 #define SYS_PC_H_MFP_PC13_MFP_SC1_DAT (4UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
372 #define SYS_PC_H_MFP_PC13_MFP_LCD_S9 (8UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
374 #define SYS_PC_H_MFP_PC12_MFP_GPC12 (0UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
375 #define SYS_PC_H_MFP_PC12_MFP_SC1_CLK (4UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
376 #define SYS_PC_H_MFP_PC12_MFP_LCD_S10 (8UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
378 #define SYS_PC_H_MFP_PC11_MFP_GPC11 (0UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
379 #define SYS_PC_H_MFP_PC11_MFP_SC1_PWR (4UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
380 #define SYS_PC_H_MFP_PC11_MFP_I2C1_SDA (5UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
381 #define SYS_PC_H_MFP_PC11_MFP_LCD_S11 (8UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
383 #define SYS_PC_H_MFP_PC10_MFP_GPC10 (0UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
384 #define SYS_PC_H_MFP_PC10_MFP_SC1_CD (4UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
385 #define SYS_PC_H_MFP_PC10_MFP_I2C1_SCL (5UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
386 #define SYS_PC_H_MFP_PC10_MFP_LCD_S12 (8UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
388 #define SYS_PC_H_MFP_PC9_MFP_GPC9 (0UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
389 #define SYS_PC_H_MFP_PC9_MFP_LCD_S2 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
390 #define SYS_PC_H_MFP_PC9_MFP_LCD_S9 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
391 #define SYS_PC_H_MFP_PC9_MFP_LCD_S13 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
393 #define SYS_PC_H_MFP_PC8_MFP_GPC8 (0UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
394 #define SYS_PC_H_MFP_PC8_MFP_SC0_RST (4UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
395 #define SYS_PC_H_MFP_PC8_MFP_UART1_TX (7UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
396 #define SYS_PC_H_MFP_PC8_MFP_LCD_S3 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
397 #define SYS_PC_H_MFP_PC8_MFP_LCD_S10 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
398 #define SYS_PC_H_MFP_PC8_MFP_LCD_S14 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
400 /********************* Bit definition of PD_L_MFP register **********************/
401 #define SYS_PD_L_MFP_PD7_MFP_GPD7 (0UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
402 #define SYS_PD_L_MFP_PD7_MFP_SC1_CLK (4UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
403 #define SYS_PD_L_MFP_PD7_MFP_LCD_COM3 (8UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
405 #define SYS_PD_L_MFP_PD6_MFP_GPD6 (0UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
406 #define SYS_PD_L_MFP_PD6_MFP_LCD_S0 (8UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
407 #define SYS_PD_L_MFP_PD6_MFP_LCD_COM4 (8UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
409 #define SYS_PD_L_MFP_PD5_MFP_GPD5 (0UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
410 #define SYS_PD_L_MFP_PD5_MFP_LCD_S1 (8UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
411 #define SYS_PD_L_MFP_PD5_MFP_LCD_COM5 (8UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
413 #define SYS_PD_L_MFP_PD4_MFP_GPD4 (0UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
414 #define SYS_PD_L_MFP_PD4_MFP_SC1_RST (4UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
415 #define SYS_PD_L_MFP_PD4_MFP_LCD_S2 (8UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
417 #define SYS_PD_L_MFP_PD3_MFP_GPD3 (0UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
418 #define SYS_PD_L_MFP_PD3_MFP_LCD_S3 (8UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
420 #define SYS_PD_L_MFP_PD2_MFP_GPD2 (0UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
421 #define SYS_PD_L_MFP_PD2_MFP_LCD_S4 (8UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
423 #define SYS_PD_L_MFP_PD1_MFP_GPD1 (0UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
424 #define SYS_PD_L_MFP_PD1_MFP_LCD_S5 (8UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
426 #define SYS_PD_L_MFP_PD0_MFP_GPD0 (0UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
427 #define SYS_PD_L_MFP_PD0_MFP_LCD_S6 (8UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
429 /********************* Bit definition of PD_H_MFP register **********************/
430 #define SYS_PD_H_MFP_PD15_MFP_GPD15 (0UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
431 #define SYS_PD_H_MFP_PD15_MFP_LCD_V3 (8UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
433 #define SYS_PD_H_MFP_PD14_MFP_GPD14 (0UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
434 #define SYS_PD_H_MFP_PD14_MFP_LCD_V2 (8UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
436 #define SYS_PD_H_MFP_PD13_MFP_GPD13 (0UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
437 #define SYS_PD_H_MFP_PD13_MFP_EINT1 (1UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
438 #define SYS_PD_H_MFP_PD13_MFP_LCD_V1 (8UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
440 #define SYS_PD_H_MFP_PD12_MFP_GPD12 (0UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
441 #define SYS_PD_H_MFP_PD12_MFP_CKO0 (1UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
442 #define SYS_PD_H_MFP_PD12_MFP_TMR1_CNT (2UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
443 #define SYS_PD_H_MFP_PD12_MFP_PWM0_CH0 (3UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
444 #define SYS_PD_H_MFP_PD12_MFP_LCD_DH1 (8UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
445 #define SYS_PD_H_MFP_PD12_MFP_CLK_Hz (9UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
446 #define SYS_PD_H_MFP_PD12_MFP_TMR1_OUT (0xAUL<<SYS_PD_H_MFP_PD12_MFP_Pos)
448 #define SYS_PD_H_MFP_PD11_MFP_GPD11 (0UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
449 #define SYS_PD_H_MFP_PD11_MFP_TMR0_CAP (2UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
450 #define SYS_PD_H_MFP_PD11_MFP_PWM0_CH1 (3UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
451 #define SYS_PD_H_MFP_PD11_MFP_LCD_DH2 (8UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
453 #define SYS_PD_H_MFP_PD10_MFP_GPD10 (0UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
454 #define SYS_PD_H_MFP_PD10_MFP_TMR1_CAP (2UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
455 #define SYS_PD_H_MFP_PD10_MFP_PWM0_CH2 (3UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
456 #define SYS_PD_H_MFP_PD10_MFP_LCD_COM0 (8UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
458 #define SYS_PD_H_MFP_PD9_MFP_GPD9 (0UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
459 #define SYS_PD_H_MFP_PD9_MFP_PWM0_CH3 (3UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
460 #define SYS_PD_H_MFP_PD9_MFP_SC1_RST (4UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
461 #define SYS_PD_H_MFP_PD9_MFP_LCD_COM1 (8UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
463 #define SYS_PD_H_MFP_PD8_MFP_GPD8 (0UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
464 #define SYS_PD_H_MFP_PD8_MFP_SC1_DAT (4UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
465 #define SYS_PD_H_MFP_PD8_MFP_LCD_COM2 (8UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
467 /********************* Bit definition of PE_L_MFP register **********************/
468 #define SYS_PE_L_MFP_PE7_MFP_GPE7 (0UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
469 #define SYS_PE_L_MFP_PE7_MFP_SC1_DAT (4UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
471 #define SYS_PE_L_MFP_PE6_MFP_GPE6 (0UL<<SYS_PE_L_MFP_PE6_MFP_Pos)
472 #define SYS_PE_L_MFP_PE6_MFP_SC1_CLK (4UL<<SYS_PE_L_MFP_PE6_MFP_Pos)
474 #define SYS_PE_L_MFP_PE5_MFP_GPE5 (0UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
475 #define SYS_PE_L_MFP_PE5_MFP_SC1_PWR (4UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
477 #define SYS_PE_L_MFP_PE4_MFP_GPE4 (0UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
478 #define SYS_PE_L_MFP_PE4_MFP_SC1_RST (4UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
480 #define SYS_PE_L_MFP_PE3_MFP_GPE3 (0UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
481 #define SYS_PE_L_MFP_PE3_MFP_SPI0_SS0 (6UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
483 #define SYS_PE_L_MFP_PE2_MFP_GPE2 (0UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
484 #define SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK (6UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
486 #define SYS_PE_L_MFP_PE1_MFP_GPE1 (0UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
487 #define SYS_PE_L_MFP_PE1_MFP_SPI0_MISO0 (6UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
489 #define SYS_PE_L_MFP_PE0_MFP_GPE0 (0UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
490 #define SYS_PE_L_MFP_PE0_MFP_SPI0_MOSI0 (6UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
492 /********************* Bit definition of PE_H_MFP register **********************/
493 #define SYS_PE_H_MFP_PE9_MFP_GPE9 (0UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
494 #define SYS_PE_H_MFP_PE9_MFP_PWM0_CH3 (3UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
495 #define SYS_PE_H_MFP_PE9_MFP_LCD_S29 (8UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
497 #define SYS_PE_H_MFP_PE8_MFP_GPE8 (0UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
498 #define SYS_PE_H_MFP_PE8_MFP_PWM0_CH2 (3UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
499 #define SYS_PE_H_MFP_PE8_MFP_LCD_S30 (8UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
501 /********************* Bit definition of PF_L_MFP register **********************/
502 #define SYS_PF_L_MFP_PF5_MFP_GPF5 (0UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
503 #define SYS_PF_L_MFP_PF5_MFP_TMR0_CAP (2UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
504 #define SYS_PF_L_MFP_PF5_MFP_PWM0_CH3 (3UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
505 #define SYS_PF_L_MFP_PF5_MFP_ACMP_C (9UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
506 #define SYS_PF_L_MFP_PF5_MFP_ICE_DAT (0xFUL<<SYS_PF_L_MFP_PF5_MFP_Pos)
508 #define SYS_PF_L_MFP_PF4_MFP_GPF4 (0UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
509 #define SYS_PF_L_MFP_PF4_MFP_CKO1 (1UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
510 #define SYS_PF_L_MFP_PF4_MFP_TMR1_CAP (2UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
511 #define SYS_PF_L_MFP_PF4_MFP_PWM0_CH2 (3UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
512 #define SYS_PF_L_MFP_PF4_MFP_CLK_Hz (9UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
513 #define SYS_PF_L_MFP_PF4_MFP_ICE_CLK (0xFUL<<SYS_PF_L_MFP_PF4_MFP_Pos)
515 #define SYS_PF_L_MFP_PF3_MFP_GPF3 (0UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
516 #define SYS_PF_L_MFP_PF3_MFP_EINT0 (1UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
517 #define SYS_PF_L_MFP_PF3_MFP_TMR2_CAP (2UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
518 #define SYS_PF_L_MFP_PF3_MFP_UART1_TX (7UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
519 #define SYS_PF_L_MFP_PF3_MFP_XT1_OUT (0xFUL<<SYS_PF_L_MFP_PF3_MFP_Pos)
521 #define SYS_PF_L_MFP_PF2_MFP_GPF2 (0UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
522 #define SYS_PF_L_MFP_PF2_MFP_EINT1 (1UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
523 #define SYS_PF_L_MFP_PF2_MFP_TMR3_CAP (2UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
524 #define SYS_PF_L_MFP_PF2_MFP_UART1_RX (7UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
525 #define SYS_PF_L_MFP_PF2_MFP_XT1_IN (0xFUL<<SYS_PF_L_MFP_PF2_MFP_Pos)
527 #define SYS_PF_L_MFP_PF1_MFP_GPF1 (0UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
528 #define SYS_PF_L_MFP_PF1_MFP_TMR2_CNT (2UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
529 #define SYS_PF_L_MFP_PF1_MFP_X32_OUT (0xFUL<<SYS_PF_L_MFP_PF1_MFP_Pos)
530 #define SYS_PF_L_MFP_PF1_MFP_TMR2_OUT (0xAUL<<SYS_PF_L_MFP_PF1_MFP_Pos)
532 #define SYS_PF_L_MFP_PF0_MFP_GPF0 (0UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
533 #define SYS_PF_L_MFP_PF0_MFP_TMR3_CNT (2UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
534 #define SYS_PF_L_MFP_PF0_MFP_X32_IN (0xFUL<<SYS_PF_L_MFP_PF0_MFP_Pos)
535 #define SYS_PF_L_MFP_PF0_MFP_TMR3_OUT (0xAUL<<SYS_PF_L_MFP_PF0_MFP_Pos)
538 #define MFP_LCD_TYPEA() { \
539 SYS->PB_L_MFP = (SYS->PB_L_MFP &~(0xFFF00000)) | (0x88800000); /* seg 35 ~ 33 */\
540 SYS->PB_H_MFP = 0x88888888; /* seg 32 ~ 31, 28 ~ 23 */\
541 SYS->PC_L_MFP = 0x88888888; /* seg 22 ~ 15 */\
542 SYS->PC_H_MFP = 0x88888888; /* seg 14 ~ 7 */\
543 SYS->PD_L_MFP = 0x88888888; /* seg 6 ~ 0, COM3 */\
544 SYS->PD_H_MFP = 0x88888888; /* COM2 ~ 0, DH2 ~ 1, V3 ~1 */\
545 SYS->PE_H_MFP = (SYS->PE_H_MFP &~(0x000000FF)) | (0x00000088); /* seg 30, 29 */\
546 PB->OFFD |= 0xFFE00000;\
547 PC->OFFD |= 0xFFFF0000;\
548 PD->OFFD |= 0xFFFF0000;\
549 PE->OFFD |= 0x03000000;\
550 }
551 /* end of group NANO1X2_SYS_EXPORTED_CONSTANTS */
553
563 #define SYS_CLEAR_BOD_INT_FLAG() (SYS->BODSTS |= SYS_BODSTS_BOD_INT_Msk)
564
571 #define SYS_DISABLE_BOD25() (SYS->BODCTL &= ~SYS_BODCTL_BOD25_EN_Msk)
572
579 #define SYS_ENABLE_BOD25() (SYS->BODCTL |= SYS_BODCTL_BOD25_EN_Msk)
580
587 #define SYS_DISABLE_BOD20() (SYS->BODCTL &= ~SYS_BODCTL_BOD20_EN_Msk)
588
595 #define SYS_ENABLE_BOD20() (SYS->BODCTL |= SYS_BODCTL_BOD20_EN_Msk)
596
603 #define SYS_DISABLE_BOD17() (SYS->BODCTL &= ~SYS_BODCTL_BOD17_EN_Msk)
604
611 #define SYS_ENABLE_BOD17() (SYS->BODCTL |= SYS_BODCTL_BOD17_EN_Msk)
612
620 #define SYS_GET_BOD_INT_FLAG() (SYS->BODSTS & SYS_BODSTS_BOD_INT_Msk)
621
630 #define SYS_GET_BOD25_OUTPUT() (SYS->BODSTS & SYS_BODSTS_BOD25_drop_Msk)
631
640 #define SYS_GET_BOD20_OUTPUT() (SYS->BODSTS & SYS_BODSTS_BOD20_drop_Msk)
641
650 #define SYS_GET_BOD17_OUTPUT() (SYS->BODSTS & SYS_BODSTS_BOD17_drop_Msk)
651
658 #define SYS_DISABLE_BOD25_RST() (SYS->BODCTL &= ~SYS_BODCTL_BOD25_RST_EN_Msk)
659
666 #define SYS_ENABLE_BOD25_RST() (SYS->BODCTL |= SYS_BODCTL_BOD25_RST_EN_Msk)
667
674 #define SYS_DISABLE_BOD20_RST() (SYS->BODCTL &= ~SYS_BODCTL_BOD20_RST_EN_Msk)
675
682 #define SYS_ENABLE_BOD20_RST() (SYS->BODCTL |= SYS_BODCTL_BOD20_RST_EN_Msk)
683
690 #define SYS_DISABLE_BOD17_RST() (SYS->BODCTL &= ~SYS_BODCTL_BOD17_RST_EN_Msk)
691
698 #define SYS_ENABLE_BOD17_RST() (SYS->BODCTL |= SYS_BODCTL_BOD17_RST_EN_Msk)
699
707 #define SYS_IS_BOD_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_BOD_Msk)
708
709
717 #define SYS_IS_CPU_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_CPU_Msk)
718
726 #define SYS_IS_POR_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_POR_Msk)
727
735 #define SYS_IS_RSTPIN_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_PAD_Msk)
736
744 #define SYS_IS_SYSTEM_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_SYS_Msk)
745
746
754 #define SYS_IS_WDT_RST() (SYS->RST_SRC & SYS_RST_SRC_RSTS_WDT_Msk)
755
762 #define SYS_DISABLE_POR() (SYS->PORCTL = 0x5AA5)
763
770 #define SYS_ENABLE_POR() (SYS->PORCTL = 0)
771
772
785 #define SYS_CLEAR_RST_SOURCE(u32RstSrc) (SYS->RST_SRC |= u32RstSrc )
786
794 __STATIC_INLINE void SYS_UnlockReg(void)
795 {
796 while(SYS->RegLockAddr != SYS_RegLockAddr_RegUnLock_Msk) {
797 SYS->RegLockAddr = 0x59;
798 SYS->RegLockAddr = 0x16;
799 SYS->RegLockAddr = 0x88;
800 }
801 }
802
810 __STATIC_INLINE void SYS_LockReg(void)
811 {
812 SYS->RegLockAddr = 0;
813 }
814
823 #define SYS_GET_IRCTRIM_INT_FLAG() (SYS->IRCTRIMINT)
824
833 #define SYS_CLEAR_IRCTRIM_INT_FLAG(u32IRCTrimFlg) (SYS->IRCTRIMINT = u32IRCTrimFlg )
834
835 void SYS_ClearResetSrc(uint32_t u32Src);
836 uint32_t SYS_GetBODStatus(void);
837 uint32_t SYS_GetResetSrc(void);
838 uint32_t SYS_IsRegLocked(void);
839 void SYS_LockReg(void);
840 void SYS_UnlockReg(void);
841 uint32_t SYS_ReadPDID(void);
842 void SYS_ResetChip(void);
843 void SYS_ResetCPU(void);
844 void SYS_ResetModule(uint32_t u32ModuleIndex);
845 void SYS_EnableBOD(int32_t i32Mode, uint32_t u32BODLevel);
846 void SYS_DisableBOD(void);
847 void SYS_EnableIRCTrim(uint32_t u32TrimSel,uint32_t u32TrimEnInt);
848 void SYS_DisableIRCTrim(void); /* end of group NANO1X2_SYS_EXPORTED_FUNCTIONS */
850 /* end of group NANO1X2_SYS_Driver */
852 /* end of group NANO1X2_Device_Driver */
854
855 #ifdef __cplusplus
856 }
857 #endif
858
859 #endif //__SYS_H__
860
861 /*** (C) COPYRIGHT 2014 Nuvoton Technology Corp. ***/
862
863
SYS_ResetCPU
void SYS_ResetCPU(void)
This function reset CPU.
Definition: sys.c:95
SYS_EnableBOD
void SYS_EnableBOD(int32_t i32Mode, uint32_t u32BODLevel)
This function configure BOD function. Configure BOD reset or interrupt mode and set Brown-out voltage...
Definition: sys.c:146
SYS_EnableIRCTrim
void SYS_EnableIRCTrim(uint32_t u32TrimSel, uint32_t u32TrimEnInt)
This function enable HIRC trim function.
Definition: sys.c:173
SYS_DisableIRCTrim
void SYS_DisableIRCTrim(void)
This function disable HIRC trim function.
Definition: sys.c:184
SYS_DisableBOD
void SYS_DisableBOD(void)
This function disable BOD function.
Definition: sys.c:156
SYS_ResetModule
void SYS_ResetModule(uint32_t u32ModuleIndex)
This function reset selected modules.
Definition: sys.c:125
SYS_GetResetSrc
uint32_t SYS_GetResetSrc(void)
This function get the system reset source register value.
Definition: sys.c:54
SYS_RegLockAddr_RegUnLock_Msk
#define SYS_RegLockAddr_RegUnLock_Msk
Definition: Nano1X2Series.h:4062
SYS_LockReg
__STATIC_INLINE void SYS_LockReg(void)
Enable register write-protection function.
Definition: sys.h:810
SYS_ClearResetSrc
void SYS_ClearResetSrc(uint32_t u32Src)
This function clear the selected system reset source.
Definition: sys.c:32
SYS_ReadPDID
uint32_t SYS_ReadPDID(void)
This function get product ID.
Definition: sys.c:75
SYS_GetBODStatus
uint32_t SYS_GetBODStatus(void)
This function get Brown-out detector output status.
Definition: sys.c:44
SYS_UnlockReg
__STATIC_INLINE void SYS_UnlockReg(void)
Disable register write-protection function.
Definition: sys.h:794
SYS
#define SYS
Pointer to SYS register structure.
Definition: Nano1X2Series.h:10650
SYS_IsRegLocked
uint32_t SYS_IsRegLocked(void)
This function check register write-protection bit setting.
Definition: sys.c:65
SYS_ResetChip
void SYS_ResetChip(void)
This function reset chip.
Definition: sys.c:85