CMSIS-RTOS RTX: Configuration of CMSIS-RTOS RTX

| CMSIS-RTOS RTX Version 4.80 CMSIS-RTOS RTX: Real-Time Operating System for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Configuration of CMSIS-RTOS RTX

The file RTX_Conf_CM.c is used to define the configuration parameters of CMSIS-RTOS RTX. This file must be part of every project that is using the CMSIS-RTOS RTX kernel.

The configuration file uses Configuration Wizard Annotations. Depending on the development tool that is used, this might lead to a more user friendly graphical representation of the settings. The following is a screenshot of the same configuration file using µVision's Configuration Wizard view:

RTX_Conf_CM.c in Configuration Wizard View

The configuration options are explained on these pages:

- Thread Configuration
- RTX Kernel Tick Timer Configuration
- System Configuration

Other configuration options not covered by the Configuration Wizard are explained here:

- Configuration for Low-Power Modes
- SVC Functions