| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
LCD_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | DISPCTL
__IO uint32_t | MEM_0
__IO uint32_t | MEM_1
__IO uint32_t | MEM_2
__IO uint32_t | MEM_3
__IO uint32_t | MEM_4
__IO uint32_t | MEM_5
__IO uint32_t | MEM_6
__IO uint32_t | MEM_7
__IO uint32_t | MEM_8
uint32_t | RESERVE0 [1]
__IO uint32_t | FCR
__IO uint32_t | FCSTS

## Detailed Description

    @addtogroup LCD LCD Controller(LCD)
    Memory Mapped Structure for LCD Controller

Definition at line 5241 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h