| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
PWM_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
__IO uint32_t | PRES
__IO uint32_t | CLKSEL
__IO uint32_t | CTL
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | OE
uint32_t | RESERVE0 [1]
__IO uint32_t | DUTY0
__I uint32_t | DATA0
uint32_t | RESERVE1 [1]
__IO uint32_t | DUTY1
__I uint32_t | DATA1
uint32_t | RESERVE2 [1]
__IO uint32_t | DUTY2
__I uint32_t | DATA2
uint32_t | RESERVE3 [1]
__IO uint32_t | DUTY3
__I uint32_t | DATA3
uint32_t | RESERVE4 [3]
__IO uint32_t | CAPCTL
__IO uint32_t | CAPINTEN
__IO uint32_t | CAPINTSTS
__I uint32_t | CRL0
__I uint32_t | CFL0
__I uint32_t | CRL1
__I uint32_t | CFL1
__I uint32_t | CRL2
__I uint32_t | CFL2
__I uint32_t | CRL3
__I uint32_t | CFL3
__I uint32_t | PDMACH0
__I uint32_t | PDMACH2
__IO uint32_t | ADTRGEN
__IO uint32_t | ADTRGSTS

## Detailed Description

    @addtogroup PWM Pulse Width Modulation Controller(PWM)
    Memory Mapped Structure for PWM Controller

Definition at line 5734 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h