| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
I2C_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
__IO uint32_t | CON
__IO uint32_t | INTSTS
__I uint32_t | STATUS
__IO uint32_t | DIV
__IO uint32_t | TOUT
__IO uint32_t | DATA
__IO uint32_t | SADDR0
__IO uint32_t | SADDR1
uint32_t | RESERVE0 [2]
__IO uint32_t | SAMASK0
__IO uint32_t | SAMASK1
uint32_t | RESERVE1 [4]
__IO uint32_t | CON2
__IO uint32_t | STATUS2

## Detailed Description

    @addtogroup I2C Inter-IC Bus Controller(I2C)
    Memory Mapped Structure for I2C Controller

Definition at line 4890 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h