CMSIS-DAP: DAP_ResetTarget

| CMSIS-DAP Version 1.1.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_ResetTarget
General Commands

Reset Target with Device specific sequence. More...

Reset Target with Device specific sequence.

The DAP_ResetTarget Command requests a target reset with a device specific command sequence. This command calls the user configurable function RESET_TARGET.

DAP_ResetTarget Command:

BYTE |
> 0x0A |
******|

DAP_ResetTarget Response:

BYTE | BYTE | BYTE |
< 0x0A | Status | Execute |
******|********|*********|

- Execute: indicates whether a device specific reset sequence was executed.
  - no device specific reset sequence is implemented.
  - 1 = a device specific reset sequence is implemented.
- Status: Response Status