| Nano102_112 Series BSP V3.03.002 The Board Support Package for Nano102_112 Series

Functions
acmp.c File Reference

Nano 102/112 series Analog Comparator(ACMP) driver source file. More...

`#include "Nano1X2Series.h"`

Go to the source code of this file.

## Functions
void | ACMP_Open (ACMP_T *Acmp, uint32_t u32ChNum, uint32_t u32NegSrc, uint32_t u32HysteresisEn)
| This function open and configure comparator parameters. More...
void | ACMP_Close (ACMP_T *Acmp, uint32_t u32ChNum)
| This function close comparator. More...
void | ACMP_SetSigmaDeltaConv (uint32_t u32TimerNum, uint32_t u32TriggerPolarity, uint32_t u32PosPin, uint32_t u32ChargePin)
| This function configure ACMP to sigma-delta mode. More...
void | ACMP_SetSlopeConv (uint32_t u32TimerNum, uint32_t u32TriggerPolarity, uint32_t u32PosPin, uint32_t u32ChargePin)
| This function configure ACMP to slope mode. More...

## Detailed Description

Nano 102/112 series Analog Comparator(ACMP) driver source file.

Version
  V1.00

Revision
  20

Date
  15/06/16 11:09a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013~2014 Nuvoton Technology Corp. All rights reserved.

Definition in file acmp.c.