| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
SC_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
union {
__I uint32_t SC_T::RBR
__O uint32_t SC_T::THR
}; |
__IO uint32_t | CTL
__IO uint32_t | ALTCTL
__IO uint32_t | EGTR
__IO uint32_t | RFTMR
__IO uint32_t | ETUCR
__IO uint32_t | IER
__IO uint32_t | ISR
__IO uint32_t | TRSR
__IO uint32_t | PINCSR
__IO uint32_t | TMR0
__IO uint32_t | TMR1
__IO uint32_t | TMR2
__IO uint32_t | UACTL
__I uint32_t | TDRA
__I uint32_t | TDRB

## Detailed Description

    @addtogroup SC Smart Card Host Interface Controller(SC)
    Memory Mapped Structure for SC Controller

Definition at line 7543 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h