| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
UART_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
union {
__I uint32_t UART_T::RBR
__O uint32_t UART_T::THR
}; |
__IO uint32_t | CTL
__IO uint32_t | TLCTL
__IO uint32_t | IER
__IO uint32_t | ISR
__IO uint32_t | TRSR
__IO uint32_t | FSR
__IO uint32_t | MCSR
__IO uint32_t | TMCTL
__IO uint32_t | BAUD
uint32_t | RESERVE0 [2]
__IO uint32_t | IRCR
__IO uint32_t | ALT_CTL
__IO uint32_t | FUN_SEL
__IO uint32_t | BR_COMP

## Detailed Description

    @addtogroup UART Universal Asynchronous Receiver/Transmitter Controller(UART)
    Memory Mapped Structure for UART Controller

Definition at line 9479 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h