| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
CLK_T Struct Reference
NANO102/112 Definitions

`#include <Nano1X2Series.h>`

## Data Fields
__IO uint32_t | PWRCTL
__IO uint32_t | AHBCLK
__IO uint32_t | APBCLK
__I uint32_t | CLKSTATUS
__IO uint32_t | CLKSEL0
__IO uint32_t | CLKSEL1
__IO uint32_t | CLKSEL2
__IO uint32_t | CLKDIV0
__IO uint32_t | CLKDIV1
__IO uint32_t | PLLCTL
__IO uint32_t | FRQDIV0
uint32_t | RESERVE0 [1]
__IO uint32_t | WK_INTSTS
__IO uint32_t | APB_DIV
__IO uint32_t | FRQDIV1
__IO uint32_t | SP_DET
__I uint32_t | SP_STS

## Detailed Description

    @addtogroup CLK System Clock Controller(CLK)
    Memory Mapped Structure for CLK Controller

Definition at line 903 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h