| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

Data Fields
RTC_T Struct Reference

`#include <Nano1X2Series.h>`

## Data Fields
__IO uint32_t | INIR
__O uint32_t | AER
__IO uint32_t | FCR
__IO uint32_t | TLR
__IO uint32_t | CLR
__IO uint32_t | TSSR
__IO uint32_t | DWR
__IO uint32_t | TAR
__IO uint32_t | CAR
__I uint32_t | LIR
__IO uint32_t | RIER
__IO uint32_t | RIIR
__IO uint32_t | TTR
uint32_t | RESERVE0 [2]
__IO uint32_t | SPRCTL
__IO uint32_t | SPR [20]

## Detailed Description

    @addtogroup RTC Real Time Clock Controller(RTC)
    Memory Mapped Structure for RTC Controller

Definition at line 7071 of file Nano1X2Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Nano1X2Series/Include/Nano1X2Series.h