| NANO102/112 BSP V3.04.000 The Board Support Package for Nano102/112 Series

lcd.h
Go to the documentation of this file.
1/**************************************************************************/
12#ifndef __LCD_H__
13#define __LCD_H__
14
15#ifdef __cplusplus
16 extern "C"
17{
18#endif
19
20#include <stdint.h>
21//#include <stdbool.h>
22
23
38/*---------------------------------------------------------------------------------------------------------*/
39/* Macro, type and constant definitions */
40/*---------------------------------------------------------------------------------------------------------*/
41
43
44#define LCD_FREQ_DIV32 ((uint32_t) 0x00000000)
45#define LCD_FREQ_DIV64 ((uint32_t) 0x00000010)
46#define LCD_FREQ_DIV96 ((uint32_t) 0x00000020)
47#define LCD_FREQ_DIV128 ((uint32_t) 0x00000030)
48#define LCD_FREQ_DIV192 ((uint32_t) 0x00000040)
49#define LCD_FREQ_DIV256 ((uint32_t) 0x00000050)
50#define LCD_FREQ_DIV384 ((uint32_t) 0x00000060)
51#define LCD_FREQ_DIV512 ((uint32_t) 0x00000070)
53#define LCD_MUX_STATIC ((uint32_t) 0x00000000)
54#define LCD_MUX_ONE_SECOND ((uint32_t) 0x00000002)
55#define LCD_MUX_ONE_THIRD ((uint32_t) 0x00000004)
56#define LCD_MUX_ONE_FOURTH ((uint32_t) 0x00000006)
57#define LCD_MUX_ONE_FIFTH ((uint32_t) 0x00000008)
58#define LCD_MUX_ONE_SIXTH ((uint32_t) 0x0000000A)
60#define LCD_BIAS_STATIC ((uint32_t) 0x00000000)
61#define LCD_BIAS_HALF ((uint32_t) 0x00000002)
62#define LCD_BIAS_THIRD ((uint32_t) 0x00000004)
64#define LCD_CPUMP_DIV1 ((uint32_t) 0x00000000)
65#define LCD_CPUMP_DIV2 ((uint32_t) 0x00000800)
66#define LCD_CPUMP_DIV4 ((uint32_t) 0x00001000)
67#define LCD_CPUMP_DIV8 ((uint32_t) 0x00001800)
68#define LCD_CPUMP_DIV16 ((uint32_t) 0x00002000)
69#define LCD_CPUMP_DIV32 ((uint32_t) 0x00002800)
70#define LCD_CPUMP_DIV64 ((uint32_t) 0x00003000)
71#define LCD_CPUMP_DIV128 ((uint32_t) 0x00003800)
73#define LCD_CPVOl_2_7V ((uint32_t) 0x00000000)
74#define LCD_CPVOl_2_8V ((uint32_t) 0x00000100)
75#define LCD_CPVOl_2_9V ((uint32_t) 0x00000200)
76#define LCD_CPVOl_3V ((uint32_t) 0x00000300)
77#define LCD_CPVOl_3_1V ((uint32_t) 0x00000400)
78#define LCD_CPVOl_3_2V ((uint32_t) 0x00000500)
79#define LCD_CPVOl_3_3V ((uint32_t) 0x00000600)
80#define LCD_CPVOl_3_4V ((uint32_t) 0x00000700)
82#define LCD_FCPRESC_DIV1 ((uint32_t) 0x00000000)
83#define LCD_FCPRESC_DIV2 ((uint32_t) 0x00000004)
84#define LCD_FCPRESC_DIV4 ((uint32_t) 0x00000008)
85#define LCD_FCPRESC_DIV8 ((uint32_t) 0x0000000C)
87#define LCD_FRAMECOUNT_INT ((uint32_t) 0x00000001)
88#define LCD_POWERDOWN_INT ((uint32_t) 0x00000002)
89#define LCD_ALL_INT ((uint32_t) 0x00000003) /* end of group NANO1X2_LCD_EXPORTED_CONSTANTS */
92
93
97 typedef enum {
98 LCD_C_TYPE = 0,
99 LCD_EXTERNAL_R_TYPE = 1,
100 LCD_INTERNAL_R_TYPE = 2,
101 LCD_EXTERNAL_C_TYPE = 3
102} LCD_PanelType;
103 /* end of group NANO1X2_LCD_EXPORTED_STRUCTS */
105
106
118#define LCD_GET_PD_INT_FLAG() ((LCD->FCSTS & LCD_FCSTS_PDSTS_Msk) >> LCD_FCSTS_PDSTS_Pos)
119
127#define LCD_CLR_PD_INT_FLAG() (LCD->FCSTS = LCD_FCSTS_PDSTS_Msk)
128
136#define LCD_GET_FRAME_CNT_INT_FLAG() ((LCD->FCSTS & LCD_FCSTS_FCSTS_Msk) >> LCD_FCSTS_FCSTS_Pos)
137
145#define LCD_CLR_FRAME_CNT_INT_FLAG() (LCD->FCSTS = LCD_FCSTS_FCSTS_Msk)
146
154#define LCD_ENABLE_PD_DISPLAY() (LCD->CTL |= LCD_CTL_PDDISP_EN_Msk)
155
163#define LCD_DISABLE_PD_DISPLAY() (LCD->CTL &= ~LCD_CTL_PDDISP_EN_Msk)
164
165uint32_t LCD_EnableFrameCounter(uint32_t u32Count);
166 void LCD_DisableFrameCounter(void);
167uint32_t LCD_EnableBlink(uint32_t u32ms);
168 void LCD_DisableBlink(void);
169 void LCD_EnableInt(uint32_t IntSrc);
170 void LCD_DisableInt(uint32_t IntSrc);
171uint32_t LCD_Open(uint32_t u32DrivingType, uint32_t u32ComNum, uint32_t u32BiasLevel, uint32_t u32FramerateDiv, uint32_t u32DrivingVol);
172 void LCD_SetPixel(uint32_t u32Com, uint32_t u32Seg, uint32_t u32OnFlag);
173 void LCD_SetAllPixels(uint32_t u32OnOff);
174 void LCD_Close(void);
175
184 static __INLINE void LCD_EnableDisplay(void)
185{
186 /* Enable LCD */
187 LCD->CTL |= LCD_CTL_EN_Msk;
188}
189
198 static __INLINE void LCD_DisableDisplay(void)
199{
200 /* Enable LCD */
201 LCD->CTL &= ~LCD_CTL_EN_Msk;
202}
203
204
205 /* end of group NANO1X2_LCD_EXPORTED_FUNCTIONS */
207
208 /* end of group NANO1X2_LCD_Driver */
210 /* end of group NANO1X2_Device_Driver */
212
213
214#ifdef __cplusplus
215}
216#endif
217
218#endif /* __LCD_H__ */
219
220
221
222/*** (C) COPYRIGHT 2014 Nuvoton Technology Corp. ***/
223
224
LCD_CTL_EN_Msk
#define LCD_CTL_EN_Msk
Definition: Nano1X2Series.h:5557
LCD_SetPixel
void LCD_SetPixel(uint32_t u32Com, uint32_t u32Seg, uint32_t u32OnFlag)
Enables a segment on the LCD display.
Definition: lcd.c:62
LCD_SetAllPixels
void LCD_SetAllPixels(uint32_t u32OnOff)
LCD Enable/Disable all segments.
Definition: lcd.c:166
LCD_Open
uint32_t LCD_Open(uint32_t u32DrivingType, uint32_t u32ComNum, uint32_t u32BiasLevel, uint32_t u32FramerateDiv, uint32_t u32DrivingVol)
LCD Initialization routine.
Definition: lcd.c:287
LCD_EnableDisplay
static __INLINE void LCD_EnableDisplay(void)
Enable LCD controller.
Definition: lcd.h:184
LCD_EnableInt
void LCD_EnableInt(uint32_t IntSrc)
This function is used to enable LCD interrupt.
Definition: lcd.c:444
LCD_EnableBlink
uint32_t LCD_EnableBlink(uint32_t u32ms)
Enable Blink function in LCD controller.
Definition: lcd.c:376
LCD_Close
void LCD_Close(void)
The function is used to disable LCD controller.
Definition: lcd.c:362
LCD_DisableInt
void LCD_DisableInt(uint32_t IntSrc)
This function is used to disable LCD specified interrupt.
Definition: lcd.c:466
LCD_DisableFrameCounter
void LCD_DisableFrameCounter(void)
Disable frame count function.
Definition: lcd.c:264
LCD_DisableBlink
void LCD_DisableBlink(void)
Disable Blink function in LCD controller.
Definition: lcd.c:423
LCD_EnableFrameCounter
uint32_t LCD_EnableFrameCounter(uint32_t u32Count)
Set Frame Count and Enable frame count.
Definition: lcd.c:210
LCD_DisableDisplay
static __INLINE void LCD_DisableDisplay(void)
Disable LCD controller.
Definition: lcd.h:198
LCD_PanelType
LCD_PanelType
Definition: lcd.h:97
LCD_EXTERNAL_C_TYPE
@ LCD_EXTERNAL_C_TYPE
Definition: lcd.h:101
LCD_INTERNAL_R_TYPE
@ LCD_INTERNAL_R_TYPE
Definition: lcd.h:100
LCD_C_TYPE
@ LCD_C_TYPE
Definition: lcd.h:98
LCD_EXTERNAL_R_TYPE
@ LCD_EXTERNAL_R_TYPE
Definition: lcd.h:99
LCD
#define LCD
Pointer to LCD register structure.
Definition: Nano1X2Series.h:10644