| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions | Variables
scuart.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | SCUART_CHAR_LEN_5
#define | SCUART_CHAR_LEN_6
#define | SCUART_CHAR_LEN_7
#define | SCUART_CHAR_LEN_8
#define | SCUART_PARITY_NONE
#define | SCUART_PARITY_ODD
#define | SCUART_PARITY_EVEN
#define | SCUART_STOP_BIT_1
#define | SCUART_STOP_BIT_2
#define | SCUART_TIMEOUT_ERR
#define | SCUART_WRITE(sc, u8Data)
| Write Data to Tx data register. More...
#define | SCUART_GET_TX_EMPTY(sc)
| Get TX FIFO empty flag status from register. More...
#define | SCUART_GET_TX_FULL(sc)
| Get TX FIFO full flag status from register. More...
#define | SCUART_WAIT_TX_EMPTY(sc)
| Wait specified smartcard port transmission complete. More...
#define | SCUART_IS_TX_FULL(sc)
| Check specified smartcard port transmit FIFO is full or not. More...
#define | SCUART_IS_TX_EMPTY(sc)
| Check specified smartcard port transmission is over. More...
#define | SCUART_READ(sc)
| Read Rx data register. More...
#define | SCUART_GET_RX_EMPTY(sc)
| Get RX FIFO empty flag status from register. More...
#define | SCUART_GET_RX_FULL(sc)
| Get RX FIFO full flag status from register. More...
#define | SCUART_IS_RX_READY(sc)
| Check if receive data number in FIFO reach FIFO trigger level or not. More...
#define | SCUART_IS_RX_FULL(sc)
| Check specified smartcard port receive FIFO is full or not. More...
#define | SCUART_ENABLE_INT(sc, u32Mask)
| Enable specified interrupts. More...
#define | SCUART_DISABLE_INT(sc, u32Mask)
| Disable specified interrupts. More...
#define | SCUART_GET_INT_FLAG(sc, u32Type)
| Get specified interrupt flag/status. More...
#define | SCUART_CLR_INT_FLAG(sc, u32Type)
| Clear specified interrupt flag/status. More...
#define | SCUART_GET_ERR_FLAG(sc)
| Get receive error flag/status. More...
#define | SCUART_CLR_ERR_FLAG(sc, u32Mask)
| Clear specified receive error flag/status. More...

## Functions
void | SCUART_Close (SC_T *sc)
| The function is used to disable smartcard interface UART mode. More...
uint32_t | SCUART_Open (SC_T *sc, uint32_t u32baudrate)
| This function use to enable smartcard module UART mode and set baudrate. More...
uint32_t | SCUART_Read (SC_T *sc, uint8_t *pu8RxBuf, uint32_t u32ReadBytes)
| The function is used to read Rx data from RX FIFO. More...
uint32_t | SCUART_SetLineConfig (SC_T *sc, uint32_t u32Baudrate, uint32_t u32DataWidth, uint32_t u32Parity, uint32_t u32StopBits)
| This function use to config smartcard UART mode line setting. More...
void | SCUART_SetTimeoutCnt (SC_T *sc, uint32_t u32TOC)
| This function use to set receive timeout count. More...
uint32_t | SCUART_Write (SC_T *sc, uint8_t *pu8TxBuf, uint32_t u32WriteBytes)
| This function is to write data into transmit FIFO to send data out. More...

## Variables
int32_t | g_SCUART_i32ErrCode