| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
OTG_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | PHYCTL
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__I uint32_t | STATUS

## Detailed Description

    @addtogroup OTG USB On-The-Go Controller(OTG)
    Memory Mapped Structure for OTG Controller

Definition at line 17746 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h