| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Functions
rtc.c File Reference

NUC472/NUC442 RTC driver source file. More...

`#include <stdio.h>`
`#include "NUC472_442.h"`
Include dependency graph for rtc.c:

Go to the source code of this file.

## Functions
void | RTC_32KCalibration (int32_t i32FrequencyX100)
| Set Frequency Compensation Data. More...
void | RTC_Open (S_RTC_TIME_DATA_T *sPt)
| This function is used to: More...
void | RTC_GetDateAndTime (S_RTC_TIME_DATA_T *sPt)
| Read current date/time from RTC setting. More...
void | RTC_GetAlarmDateAndTime (S_RTC_TIME_DATA_T *sPt)
| Read alarm date/time from RTC setting. More...
void | RTC_SetDateAndTime (S_RTC_TIME_DATA_T *sPt)
| This function is used to update date/time to RTC. More...
void | RTC_SetAlarmDateAndTime (S_RTC_TIME_DATA_T *sPt)
| This function is used to set alarm date/time to RTC. More...
void | RTC_SetDate (uint32_t u32Year, uint32_t u32Month, uint32_t u32Day, uint32_t u32DayOfWeek)
| This function is used to update date to RTC. More...
void | RTC_SetTime (uint32_t u32Hour, uint32_t u32Minute, uint32_t u32Second, uint32_t u32TimeMode, uint32_t u32AmPm)
| This function is used to update time to RTC. More...
void | RTC_SetAlarmDate (uint32_t u32Year, uint32_t u32Month, uint32_t u32Day)
| This function is used to set alarm date to RTC. More...
void | RTC_SetAlarmTime (uint32_t u32Hour, uint32_t u32Minute, uint32_t u32Second, uint32_t u32TimeMode, uint32_t u32AmPm)
| This function is used to set alarm date to RTC. More...
int32_t | RTC_EnableSpareAccess (void)
| The spare registers access enable. More...
void | RTC_EnableTamperDetection (uint32_t u32PinNumber, uint32_t u32PinCondition, uint32_t u32IntFlag, uint32_t u32ClearFlag, uint32_t u32DestroyEn)
| This function is used to: More...
void | RTC_DisableTamperDetection (uint32_t u32PinNumber)
| This function is used to disable tamper detection function. More...
uint32_t | RTC_GetDayOfWeek (void)
| This function is used to get day of week. More...
void | RTC_SetTickPeriod (uint32_t u32TickSelection)
| The function is used to set time tick period for periodic time tick Interrupt. More...
void | RTC_EnableInt (uint32_t u32IntFlagMask)
| The function is used to enable specified interrupt. More...
void | RTC_DisableInt (uint32_t u32IntFlagMask)
| The function is used to disable specified interrupt. More...
void | RTC_Close (void)
| Disable RTC clock. More...

## Detailed Description

NUC472/NUC442 RTC driver source file.

Version
  V1.00

Revision
  18

Date
  15/11/26 10:43a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file rtc.c.