| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
USBD_T Struct Reference

`#include <NUC472_442.h>`

Collaboration diagram for USBD_T:
[legend]

## Data Fields
__I uint32_t | GINTSTS
__IO uint32_t | GINTEN
__IO uint32_t | BUSINTSTS
__IO uint32_t | BUSINTEN
__IO uint32_t | OPER
__I uint32_t | FRAMECNT
__IO uint32_t | FADDR
__IO uint32_t | TEST
union {
__IO uint32_t USBD_T::CEPDAT
__IO uint8_t USBD_T::CEPDAT_BYTE
}; |
| Define Control-Endpoint Data Register 32-bit or 8-bit access. More...
__IO uint32_t | CEPCTL
__IO uint32_t | CEPINTEN
__IO uint32_t | CEPINTSTS
__IO uint32_t | CEPTXCNT
__I uint32_t | CEPRXCNT
__I uint32_t | CEPDATCNT
__I uint32_t | SETUP1_0
__I uint32_t | SETUP3_2
__I uint32_t | SETUP5_4
__I uint32_t | SETUP7_6
__IO uint32_t | CEPBUFSTART
__IO uint32_t | CEPBUFEND
__IO uint32_t | DMACTL
__IO uint32_t | DMACNT
USBD_EP_T | EP [12]
__IO uint32_t | DMAADDR
__IO uint32_t | PHYCTL

## Detailed Description

Definition at line 27258 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h