| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions
sys.h File Reference

NUC472/NUC442 SYS Header File. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | PDMA_RST
#define | EBI_RST
#define | USBH_RST
#define | EMAC_RST
#define | SDH_RST
#define | CRC_RST
#define | CAP_RST
#define | CRYPTO_RST
#define | GPIO_RST
#define | TMR0_RST
#define | TMR1_RST
#define | TMR2_RST
#define | TMR3_RST
#define | ACMP_RST
#define | I2C0_RST
#define | I2C1_RST
#define | I2C2_RST
#define | I2C3_RST
#define | SPI0_RST
#define | SPI1_RST
#define | SPI2_RST
#define | SPI3_RST
#define | UART0_RST
#define | UART1_RST
#define | UART2_RST
#define | UART3_RST
#define | UART4_RST
#define | UART5_RST
#define | CAN0_RST
#define | CAN1_RST
#define | OTG_RST
#define | USBD_RST
#define | ADC_RST
#define | I2S0_RST
#define | I2S1_RST
#define | PS2_RST
#define | SC0_RST
#define | SC1_RST
#define | SC2_RST
#define | SC3_RST
#define | SC4_RST
#define | SC5_RST
#define | I2C4_RST
#define | PWM0_RST
#define | PWM1_RST
#define | QEI0_RST
#define | QEI1_RST
#define | SYS_BODCTL_BODVL_2_2V
#define | SYS_BODCTL_BODVL_2_7V
#define | SYS_BODCTL_BODVL_3_8V
#define | SYS_BODCTL_BODVL_4_5V
#define | SYS_BODCTL_BODRSTEN
#define | SYS_BODCTL_BODINTEN
#define | SYS_BODCTL_BODLPM
#define | SYS_BODCTL_BODOUT
#define | SYS_BODCTL_LVREN
#define | SYS_VREFCTL_VREF_2_65V
#define | SYS_VREFCTL_VREF_2_048V
#define | SYS_VREFCTL_VREF_3_072V
#define | SYS_VREFCTL_VREF_4_096V
#define | SYS_VREFCTL_VREF_AVDD
#define | SYS_VREFCTL_ADCMODESEL_EADC
#define | SYS_VREFCTL_ADCMODESEL_ADC
#define | SYS_VREFCTL_PWMSYNCMODE_EN
#define | SYS_USBPHY_USBROLE_OTG_V33_EN
#define | SYS_USBPHY_USBROLE_STD_USBD
#define | SYS_USBPHY_USBROLE_STD_USBH
#define | SYS_USBPHY_USBROLE_ID_DEPH
#define | SYS_USBPHY_USBROLE_ON_THE_GO
#define | SYS_GPA_MFPL_PA0MFP_GPIO
#define | SYS_GPA_MFPL_PA0MFP_TAMPER0
#define | SYS_GPA_MFPL_PA0MFP_SC0_CD
#define | SYS_GPA_MFPL_PA0MFP_CAN1_RXD
#define | SYS_GPA_MFPL_PA0MFP_INT0
#define | SYS_GPA_MFPL_PA1MFP_GPIO
#define | SYS_GPA_MFPL_PA1MFP_TAMPER1
#define | SYS_GPA_MFPL_PA1MFP_SC5_CD
#define | SYS_GPA_MFPL_PA1MFP_CAN1_TXD
#define | SYS_GPA_MFPL_PA1MFP_EBI_A22
#define | SYS_GPA_MFPL_PA2MFP_GPIO
#define | SYS_GPA_MFPL_PA2MFP_SC2_DAT
#define | SYS_GPA_MFPL_PA2MFP_SPI3_MISO0
#define | SYS_GPA_MFPL_PA2MFP_I2S0_MCLK
#define | SYS_GPA_MFPL_PA2MFP_BRAKE11
#define | SYS_GPA_MFPL_PA2MFP_CAP_SFIELD
#define | SYS_GPA_MFPL_PA2MFP_EBI_A12
#define | SYS_GPA_MFPL_PA3MFP_GPIO
#define | SYS_GPA_MFPL_PA3MFP_SC2_CLK
#define | SYS_GPA_MFPL_PA3MFP_SPI3_MOSI0
#define | SYS_GPA_MFPL_PA3MFP_I2S0_DO
#define | SYS_GPA_MFPL_PA3MFP_BRAKE10
#define | SYS_GPA_MFPL_PA3MFP_EBI_A13
#define | SYS_GPA_MFPL_PA4MFP_GPIO
#define | SYS_GPA_MFPL_PA4MFP_SC2_PWR
#define | SYS_GPA_MFPL_PA4MFP_SPI3_CLK
#define | SYS_GPA_MFPL_PA4MFP_I2S0_DI
#define | SYS_GPA_MFPL_PA4MFP_QEI1_Z
#define | SYS_GPA_MFPL_PA4MFP_EBI_A14
#define | SYS_GPA_MFPL_PA4MFP_ECAP1_IC2
#define | SYS_GPA_MFPL_PA5MFP_GPIO
#define | SYS_GPA_MFPL_PA5MFP_SC2_RST
#define | SYS_GPA_MFPL_PA5MFP_SPI3_SS0
#define | SYS_GPA_MFPL_PA5MFP_I2S0_BCLK
#define | SYS_GPA_MFPL_PA5MFP_PWM0_CH0
#define | SYS_GPA_MFPL_PA5MFP_PWM0_0
#define | SYS_GPA_MFPL_PA5MFP_QEI1_B
#define | SYS_GPA_MFPL_PA5MFP_EBI_A15
#define | SYS_GPA_MFPL_PA5MFP_ECAP1_IC1
#define | SYS_GPA_MFPL_PA6MFP_GPIO
#define | SYS_GPA_MFPL_PA6MFP_SC2_CD
#define | SYS_GPA_MFPL_PA6MFP_I2S0_LRCK
#define | SYS_GPA_MFPL_PA6MFP_PWM0_CH1
#define | SYS_GPA_MFPL_PA6MFP_PWM0_1
#define | SYS_GPA_MFPL_PA6MFP_QEI1_A
#define | SYS_GPA_MFPL_PA6MFP_CAN1_TXD
#define | SYS_GPA_MFPL_PA6MFP_EBI_A16
#define | SYS_GPA_MFPL_PA6MFP_ECAP1_IC0
#define | SYS_GPA_MFPL_PA7MFP_GPIO
#define | SYS_GPA_MFPL_PA7MFP_SC0_CLK
#define | SYS_GPA_MFPL_PA7MFP_SPI3_SS0
#define | SYS_GPA_MFPL_PA7MFP_PWM1_CH3
#define | SYS_GPA_MFPL_PA7MFP_PWM1_3
#define | SYS_GPA_MFPL_PA7MFP_EPWM0_CH5
#define | SYS_GPA_MFPL_PA7MFP_EPWM0_5
#define | SYS_GPA_MFPL_PA7MFP_EBI_A17
#define | SYS_GPA_MFPH_PA8MFP_GPIO
#define | SYS_GPA_MFPH_PA8MFP_SC0_RST
#define | SYS_GPA_MFPH_PA8MFP_SPI3_CLK
#define | SYS_GPA_MFPH_PA8MFP_PWM1_CH2
#define | SYS_GPA_MFPH_PA8MFP_PWM1_2
#define | SYS_GPA_MFPH_PA8MFP_EPWM0_CH4
#define | SYS_GPA_MFPH_PA8MFP_EPWM0_4
#define | SYS_GPA_MFPH_PA8MFP_EBI_A18
#define | SYS_GPA_MFPH_PA9MFP_GPIO
#define | SYS_GPA_MFPH_PA9MFP_SC0_PWR
#define | SYS_GPA_MFPH_PA9MFP_SPI3_MISO0
#define | SYS_GPA_MFPH_PA9MFP_PWM1_CH1
#define | SYS_GPA_MFPH_PA9MFP_PWM1_1
#define | SYS_GPA_MFPH_PA9MFP_EPWM0_CH3
#define | SYS_GPA_MFPH_PA9MFP_EPWM0_3
#define | SYS_GPA_MFPH_PA9MFP_EBI_A19
#define | SYS_GPA_MFPH_PA10MFP_GPIO
#define | SYS_GPA_MFPH_PA10MFP_SC0_DAT
#define | SYS_GPA_MFPH_PA10MFP_SPI3_MOSI0
#define | SYS_GPA_MFPH_PA10MFP_PWM1_CH0
#define | SYS_GPA_MFPH_PA10MFP_PWM1_0
#define | SYS_GPA_MFPH_PA10MFP_EPWM0_CH2
#define | SYS_GPA_MFPH_PA10MFP_EPWM0_2
#define | SYS_GPA_MFPH_PA10MFP_EBI_A20
#define | SYS_GPA_MFPH_PA11MFP_GPIO
#define | SYS_GPA_MFPH_PA11MFP_UART0_RTS
#define | SYS_GPA_MFPH_PA11MFP_SPI3_MISO1
#define | SYS_GPA_MFPH_PA11MFP_PWM0_CH5
#define | SYS_GPA_MFPH_PA11MFP_PWM0_5
#define | SYS_GPA_MFPH_PA11MFP_EPWM0_CH1
#define | SYS_GPA_MFPH_PA11MFP_EPWM0_1
#define | SYS_GPA_MFPH_PA11MFP_EBI_AD0
#define | SYS_GPA_MFPH_PA12MFP_GPIO
#define | SYS_GPA_MFPH_PA12MFP_UART0_CTS
#define | SYS_GPA_MFPH_PA12MFP_SPI3_MOSI1
#define | SYS_GPA_MFPH_PA12MFP_PWM0_CH4
#define | SYS_GPA_MFPH_PA12MFP_PWM0_4
#define | SYS_GPA_MFPH_PA12MFP_EPWM0_CH0
#define | SYS_GPA_MFPH_PA12MFP_EPWM0_0
#define | SYS_GPA_MFPH_PA12MFP_EBI_AD1
#define | SYS_GPA_MFPH_PA13MFP_GPIO
#define | SYS_GPA_MFPH_PA13MFP_UART0_RXD
#define | SYS_GPA_MFPH_PA13MFP_SC3_DAT
#define | SYS_GPA_MFPH_PA13MFP_PWM1_CH4
#define | SYS_GPA_MFPH_PA13MFP_PWM1_4
#define | SYS_GPA_MFPH_PA13MFP_EBI_AD2
#define | SYS_GPA_MFPH_PA14MFP_GPIO
#define | SYS_GPA_MFPH_PA14MFP_UART0_TXD
#define | SYS_GPA_MFPH_PA14MFP_SC3_CLK
#define | SYS_GPA_MFPH_PA14MFP_PWM1_CH5
#define | SYS_GPA_MFPH_PA14MFP_PWM1_5
#define | SYS_GPA_MFPH_PA14MFP_EBI_AD3
#define | SYS_GPA_MFPH_PA15MFP_GPIO
#define | SYS_GPA_MFPH_PA15MFP_SC3_PWR
#define | SYS_GPA_MFPH_PA15MFP_UART2_RTS
#define | SYS_GPA_MFPH_PA15MFP_I2C0_SCL
#define | SYS_GPA_MFPH_PA15MFP_EBI_A21
#define | SYS_GPB_MFPL_PB0MFP_GPIO
#define | SYS_GPB_MFPL_PB0MFP_USB0_OTG5V_ST
#define | SYS_GPB_MFPL_PB0MFP_I2C4_SCL
#define | SYS_GPB_MFPL_PB0MFP_INT1
#define | SYS_GPB_MFPL_PB1MFP_GPIO
#define | SYS_GPB_MFPL_PB1MFP_USB0_OTG5V_EN
#define | SYS_GPB_MFPL_PB1MFP_I2C4_SDA
#define | SYS_GPB_MFPL_PB1MFP_TM1_CNT_OUT
#define | SYS_GPB_MFPL_PB2MFP_GPIO
#define | SYS_GPB_MFPL_PB2MFP_UART1_RXD
#define | SYS_GPB_MFPL_PB2MFP_SPI2_SS0
#define | SYS_GPB_MFPL_PB2MFP_USB1_D_N
#define | SYS_GPB_MFPL_PB2MFP_EBI_AD4
#define | SYS_GPB_MFPL_PB3MFP_GPIO
#define | SYS_GPB_MFPL_PB3MFP_UART1_TXD
#define | SYS_GPB_MFPL_PB3MFP_SPI2_CLK
#define | SYS_GPB_MFPL_PB3MFP_USB1_D_P
#define | SYS_GPB_MFPL_PB3MFP_EBI_AD5
#define | SYS_GPB_MFPL_PB4MFP_GPIO
#define | SYS_GPB_MFPL_PB4MFP_UART1_RTS
#define | SYS_GPB_MFPL_PB4MFP_SPI2_MISO0
#define | SYS_GPB_MFPL_PB4MFP_UART4_RXD
#define | SYS_GPB_MFPL_PB4MFP_TM0_CNT_OUT
#define | SYS_GPB_MFPL_PB4MFP_EBI_AD6
#define | SYS_GPB_MFPL_PB5MFP_GPIO
#define | SYS_GPB_MFPL_PB5MFP_UART1_CTS
#define | SYS_GPB_MFPL_PB5MFP_SPI2_MOSI0
#define | SYS_GPB_MFPL_PB5MFP_UART4_TXD
#define | SYS_GPB_MFPL_PB5MFP_EBI_AD7
#define | SYS_GPB_MFPL_PB6MFP_GPIO
#define | SYS_GPB_MFPL_PB6MFP_I2C2_SCL
#define | SYS_GPB_MFPL_PB6MFP_BRAKE01
#define | SYS_GPB_MFPL_PB6MFP_UART4_RTS
#define | SYS_GPB_MFPL_PB6MFP_PWM1_CH4
#define | SYS_GPB_MFPL_PB6MFP_PWM1_4
#define | SYS_GPB_MFPL_PB6MFP_EPWM1_CH0
#define | SYS_GPB_MFPL_PB6MFP_EPWM1_0
#define | SYS_GPB_MFPL_PB6MFP_EBI_AD8
#define | SYS_GPB_MFPL_PB7MFP_GPIO
#define | SYS_GPB_MFPL_PB7MFP_I2C2_SDA
#define | SYS_GPB_MFPL_PB7MFP_BRAKE00
#define | SYS_GPB_MFPL_PB7MFP_UART4_CTS
#define | SYS_GPB_MFPL_PB7MFP_PWM1_CH5
#define | SYS_GPB_MFPL_PB7MFP_PWM1_5
#define | SYS_GPB_MFPL_PB7MFP_EPWM1_CH1
#define | SYS_GPB_MFPL_PB7MFP_EPWM1_1
#define | SYS_GPB_MFPL_PB7MFP_ETM_TRACE_DATA3
#define | SYS_GPB_MFPL_PB7MFP_EBI_AD9
#define | SYS_GPB_MFPH_PB8MFP_GPIO
#define | SYS_GPB_MFPH_PB8MFP_UART5_CTS
#define | SYS_GPB_MFPH_PB8MFP_EPWM1_CH2
#define | SYS_GPB_MFPH_PB8MFP_EPWM1_2
#define | SYS_GPB_MFPH_PB8MFP_ETM_TRACE_DATA2
#define | SYS_GPB_MFPH_PB8MFP_EBI_AD10
#define | SYS_GPB_MFPH_PB9MFP_GPIO
#define | SYS_GPB_MFPH_PB9MFP_UART5_RTS
#define | SYS_GPB_MFPH_PB9MFP_EPWM1_CH3
#define | SYS_GPB_MFPH_PB9MFP_EPWM1_3
#define | SYS_GPB_MFPH_PB9MFP_ETM_TRACE_DATA1
#define | SYS_GPB_MFPH_PB9MFP_EBI_AD11
#define | SYS_GPB_MFPH_PB10MFP_GPIO
#define | SYS_GPB_MFPH_PB10MFP_UART5_TXD
#define | SYS_GPB_MFPH_PB10MFP_EPWM1_CH4
#define | SYS_GPB_MFPH_PB10MFP_EPWM1_4
#define | SYS_GPB_MFPH_PB10MFP_ETM_TRACE_DATA0
#define | SYS_GPB_MFPH_PB10MFP_EBI_AD12
#define | SYS_GPB_MFPH_PB11MFP_GPIO
#define | SYS_GPB_MFPH_PB11MFP_UART5_RXD
#define | SYS_GPB_MFPH_PB11MFP_EPWM1_CH5
#define | SYS_GPB_MFPH_PB11MFP_EPWM1_5
#define | SYS_GPB_MFPH_PB11MFP_ETM_TRACE_CLK
#define | SYS_GPB_MFPH_PB11MFP_EBI_AD13
#define | SYS_GPB_MFPH_PB12MFP_GPIO
#define | SYS_GPB_MFPH_PB12MFP_UART4_RTS
#define | SYS_GPB_MFPH_PB12MFP_SPI2_MISO1
#define | SYS_GPB_MFPH_PB12MFP_CAN0_RXD
#define | SYS_GPB_MFPH_PB12MFP_EMAC_MII_MDC
#define | SYS_GPB_MFPH_PB12MFP_EBI_AD14
#define | SYS_GPB_MFPH_PB13MFP_GPIO
#define | SYS_GPB_MFPH_PB13MFP_UART4_CTS
#define | SYS_GPB_MFPH_PB13MFP_SPI2_MOSI1
#define | SYS_GPB_MFPH_PB13MFP_CAN0_TXD
#define | SYS_GPB_MFPH_PB13MFP_EMAC_MII_MDIO
#define | SYS_GPB_MFPH_PB13MFP_EBI_AD15
#define | SYS_GPB_MFPH_PB14MFP_GPIO
#define | SYS_GPB_MFPH_PB14MFP_I2S1_MCLK
#define | SYS_GPB_MFPH_PB14MFP_SC1_RST
#define | SYS_GPB_MFPH_PB14MFP_BRAKE01
#define | SYS_GPB_MFPH_PB14MFP_EMAC_MII_MDC
#define | SYS_GPB_MFPH_PB15MFP_GPIO
#define | SYS_GPB_MFPH_PB15MFP_I2S1_DO
#define | SYS_GPB_MFPH_PB15MFP_SC1_DAT
#define | SYS_GPB_MFPH_PB15MFP_BRAKE00
#define | SYS_GPB_MFPH_PB15MFP_EMAC_MII_MDIO
#define | SYS_GPC_MFPL_PC0MFP_GPIO
#define | SYS_GPC_MFPL_PC0MFP_I2S1_DI
#define | SYS_GPC_MFPL_PC0MFP_SC1_DAT
#define | SYS_GPC_MFPL_PC0MFP_UART4_RXD
#define | SYS_GPC_MFPL_PC0MFP_EMAC_REFCLK
#define | SYS_GPC_MFPL_PC0MFP_EBI_MCLK
#define | SYS_GPC_MFPL_PC0MFP_INT2
#define | SYS_GPC_MFPL_PC1MFP_GPIO
#define | SYS_GPC_MFPL_PC1MFP_I2S1_BCLK
#define | SYS_GPC_MFPL_PC1MFP_SC1_CLK
#define | SYS_GPC_MFPL_PC1MFP_UART4_TXD
#define | SYS_GPC_MFPL_PC1MFP_TM3_CNT_OUT
#define | SYS_GPC_MFPL_PC1MFP_EMAC_MII_RXERR
#define | SYS_GPC_MFPL_PC1MFP_EBI_AD13
#define | SYS_GPC_MFPL_PC2MFP_GPIO
#define | SYS_GPC_MFPL_PC2MFP_I2S1_LRCK
#define | SYS_GPC_MFPL_PC2MFP_SC1_PWR
#define | SYS_GPC_MFPL_PC2MFP_UART4_RTS
#define | SYS_GPC_MFPL_PC2MFP_SPI0_SS0
#define | SYS_GPC_MFPL_PC2MFP_EMAC_MII_RXDV
#define | SYS_GPC_MFPL_PC2MFP_EBI_AD12
#define | SYS_GPC_MFPL_PC3MFP_GPIO
#define | SYS_GPC_MFPL_PC3MFP_I2S1_MCLK
#define | SYS_GPC_MFPL_PC3MFP_SC1_CD
#define | SYS_GPC_MFPL_PC3MFP_UART4_CTS
#define | SYS_GPC_MFPL_PC3MFP_SPI0_MISO1
#define | SYS_GPC_MFPL_PC3MFP_QEI0_Z
#define | SYS_GPC_MFPL_PC3MFP_EMAC_MII_RXD1
#define | SYS_GPC_MFPL_PC3MFP_EBI_AD11
#define | SYS_GPC_MFPL_PC3MFP_ECAP0_IC2
#define | SYS_GPC_MFPL_PC4MFP_GPIO
#define | SYS_GPC_MFPL_PC4MFP_I2S1_DO
#define | SYS_GPC_MFPL_PC4MFP_SC1_RST
#define | SYS_GPC_MFPL_PC4MFP_SPI0_MOSI1
#define | SYS_GPC_MFPL_PC4MFP_QEI0_B
#define | SYS_GPC_MFPL_PC4MFP_EMAC_MII_RXD0
#define | SYS_GPC_MFPL_PC4MFP_EBI_AD10
#define | SYS_GPC_MFPL_PC4MFP_ECAP0_IC1
#define | SYS_GPC_MFPL_PC5MFP_GPIO
#define | SYS_GPC_MFPL_PC5MFP_CLK_O
#define | SYS_GPC_MFPL_PC5MFP_CLKO
#define | SYS_GPC_MFPL_PC5MFP_QEI0_A
#define | SYS_GPC_MFPL_PC5MFP_EMAC_MII_RXCLK
#define | SYS_GPC_MFPL_PC5MFP_EBI_MCLK
#define | SYS_GPC_MFPL_PC5MFP_ECAP0_IC0
#define | SYS_GPC_MFPL_PC6MFP_GPIO
#define | SYS_GPC_MFPL_PC6MFP_TM2_EXT
#define | SYS_GPC_MFPL_PC6MFP_SPI0_MISO0
#define | SYS_GPC_MFPL_PC6MFP_TM2_CNT_OUT
#define | SYS_GPC_MFPL_PC6MFP_EMAC_MII_TXD0
#define | SYS_GPC_MFPL_PC6MFP_EBI_AD9
#define | SYS_GPC_MFPL_PC7MFP_GPIO
#define | SYS_GPC_MFPL_PC7MFP_TM1_EXT
#define | SYS_GPC_MFPL_PC7MFP_SPI0_MOSI0
#define | SYS_GPC_MFPL_PC7MFP_EMAC_MII_TXD1
#define | SYS_GPC_MFPL_PC7MFP_EBI_AD8
#define | SYS_GPC_MFPH_PC8MFP_GPIO
#define | SYS_GPC_MFPH_PC8MFP_TM0_EXT
#define | SYS_GPC_MFPH_PC8MFP_SPI0_CLK
#define | SYS_GPC_MFPH_PC8MFP_EMAC_MII_TXEN
#define | SYS_GPC_MFPH_PC9MFP_GPIO
#define | SYS_GPC_MFPH_PC9MFP_STADC
#define | SYS_GPC_MFPH_PC9MFP_UART2_CTS
#define | SYS_GPC_MFPH_PC9MFP_SC3_RST
#define | SYS_GPC_MFPH_PC9MFP_I2C0_SDA
#define | SYS_GPC_MFPH_PC9MFP_CAP_DATA1
#define | SYS_GPC_MFPH_PC9MFP_I2C3_SCL
#define | SYS_GPC_MFPH_PC9MFP_EBI_A22
#define | SYS_GPC_MFPH_PC9MFP_SD1_DAT0
#define | SYS_GPC_MFPH_PC9MFP_EBI_A6
#define | SYS_GPC_MFPH_PC10MFP_GPIO
#define | SYS_GPC_MFPH_PC10MFP_SC3_CD
#define | SYS_GPC_MFPH_PC10MFP_UART2_RXD
#define | SYS_GPC_MFPH_PC10MFP_PWM0_CH2
#define | SYS_GPC_MFPH_PC10MFP_PWM0_2
#define | SYS_GPC_MFPH_PC10MFP_EBI_A23
#define | SYS_GPC_MFPH_PC10MFP_EBI_AD2
#define | SYS_GPC_MFPH_PC11MFP_GPIO
#define | SYS_GPC_MFPH_PC11MFP_UART2_TXD
#define | SYS_GPC_MFPH_PC11MFP_PWM0_CH3
#define | SYS_GPC_MFPH_PC11MFP_PWM0_3
#define | SYS_GPC_MFPH_PC11MFP_EBI_A24
#define | SYS_GPC_MFPH_PC11MFP_EBI_AD3
#define | SYS_GPC_MFPH_PC12MFP_GPIO
#define | SYS_GPC_MFPH_PC12MFP_SPI1_SS0
#define | SYS_GPC_MFPH_PC12MFP_SC4_CD
#define | SYS_GPC_MFPH_PC12MFP_SD1_CDn
#define | SYS_GPC_MFPH_PC12MFP_CAP_DATA7
#define | SYS_GPC_MFPH_PC12MFP_ETM_TRACE_DATA3
#define | SYS_GPC_MFPH_PC12MFP_EBI_A0
#define | SYS_GPC_MFPH_PC13MFP_GPIO
#define | SYS_GPC_MFPH_PC13MFP_SPI1_MOSI1
#define | SYS_GPC_MFPH_PC13MFP_SC4_RST
#define | SYS_GPC_MFPH_PC13MFP_SD1_CMD
#define | SYS_GPC_MFPH_PC13MFP_CAP_DATA6
#define | SYS_GPC_MFPH_PC13MFP_ETM_TRACE_DATA2
#define | SYS_GPC_MFPH_PC13MFP_EBI_A1
#define | SYS_GPC_MFPH_PC14MFP_GPIO
#define | SYS_GPC_MFPH_PC14MFP_SPI1_MISO1
#define | SYS_GPC_MFPH_PC14MFP_SC4_PWR
#define | SYS_GPC_MFPH_PC14MFP_TM3_EXT
#define | SYS_GPC_MFPH_PC14MFP_SD1_CLK
#define | SYS_GPC_MFPH_PC14MFP_CAP_DATA5
#define | SYS_GPC_MFPH_PC14MFP_ETM_TRACE_DATA1
#define | SYS_GPC_MFPH_PC14MFP_EBI_A2
#define | SYS_GPC_MFPH_PC15MFP_GPIO
#define | SYS_GPC_MFPH_PC15MFP_SPI1_MOSI0
#define | SYS_GPC_MFPH_PC15MFP_SC4_DAT
#define | SYS_GPC_MFPH_PC15MFP_SD1_DAT3
#define | SYS_GPC_MFPH_PC15MFP_CAP_DATA4
#define | SYS_GPC_MFPH_PC15MFP_ETM_TRACE_DATA0
#define | SYS_GPC_MFPH_PC15MFP_EBI_A3
#define | SYS_GPD_MFPL_PD0MFP_GPIO
#define | SYS_GPD_MFPL_PD0MFP_SPI1_MISO0
#define | SYS_GPD_MFPL_PD0MFP_SC4_CLK
#define | SYS_GPD_MFPL_PD0MFP_SD1_DAT2
#define | SYS_GPD_MFPL_PD0MFP_CAP_DATA3
#define | SYS_GPD_MFPL_PD0MFP_ETM_TRACE_CLK
#define | SYS_GPD_MFPL_PD0MFP_EBI_A4
#define | SYS_GPD_MFPL_PD0MFP_INT3
#define | SYS_GPD_MFPL_PD1MFP_GPIO
#define | SYS_GPD_MFPL_PD1MFP_SPI1_CLK
#define | SYS_GPD_MFPL_PD1MFP_TM0_CNT_OUT
#define | SYS_GPD_MFPL_PD1MFP_SD1_DAT1
#define | SYS_GPD_MFPL_PD1MFP_CAP_DATA2
#define | SYS_GPD_MFPL_PD1MFP_EBI_A5
#define | SYS_GPD_MFPL_PD2MFP_GPIO
#define | SYS_GPD_MFPL_PD2MFP_STADC
#define | SYS_GPD_MFPL_PD2MFP_I2C3_SCL
#define | SYS_GPD_MFPL_PD2MFP_SD1_DAT0
#define | SYS_GPD_MFPL_PD2MFP_CAP_DATA1
#define | SYS_GPD_MFPL_PD2MFP_EBI_A6
#define | SYS_GPD_MFPL_PD3MFP_GPIO
#define | SYS_GPD_MFPL_PD3MFP_SC5_CLK
#define | SYS_GPD_MFPL_PD3MFP_I2C3_SDA
#define | SYS_GPD_MFPL_PD3MFP_ACMP2_O
#define | SYS_GPD_MFPL_PD3MFP_SD0_CDn
#define | SYS_GPD_MFPL_PD3MFP_CAP_DATA0
#define | SYS_GPD_MFPL_PD3MFP_JTAG_TDO
#define | SYS_GPD_MFPL_PD3MFP_EBI_A7
#define | SYS_GPD_MFPL_PD4MFP_GPIO
#define | SYS_GPD_MFPL_PD4MFP_SC5_CD
#define | SYS_GPD_MFPL_PD4MFP_UART3_RXD
#define | SYS_GPD_MFPL_PD4MFP_ACMP1_O
#define | SYS_GPD_MFPL_PD4MFP_CAP_SCLK
#define | SYS_GPD_MFPL_PD4MFP_JTAG_TDI
#define | SYS_GPD_MFPL_PD4MFP_EBI_A8
#define | SYS_GPD_MFPL_PD5MFP_GPIO
#define | SYS_GPD_MFPL_PD5MFP_SC5_RST
#define | SYS_GPD_MFPL_PD5MFP_UART3_TXD
#define | SYS_GPD_MFPL_PD5MFP_CAP_VSYNC
#define | SYS_GPD_MFPL_PD5MFP_JTAG_nTRST
#define | SYS_GPD_MFPL_PD5MFP_EBI_A9
#define | SYS_GPD_MFPL_PD6MFP_GPIO
#define | SYS_GPD_MFPL_PD6MFP_SC5_PWR
#define | SYS_GPD_MFPL_PD6MFP_UART3_RTS
#define | SYS_GPD_MFPL_PD6MFP_SD0_CMD
#define | SYS_GPD_MFPL_PD6MFP_CAP_HSYNC
#define | SYS_GPD_MFPL_PD6MFP_EBI_A10
#define | SYS_GPD_MFPL_PD7MFP_GPIO
#define | SYS_GPD_MFPL_PD7MFP_SC5_DAT
#define | SYS_GPD_MFPL_PD7MFP_UART3_CTS
#define | SYS_GPD_MFPL_PD7MFP_SD0_CLK
#define | SYS_GPD_MFPL_PD7MFP_CAP_PIXCLK
#define | SYS_GPD_MFPL_PD7MFP_EBI_A11
#define | SYS_GPD_MFPH_PD8MFP_GPIO
#define | SYS_GPD_MFPH_PD8MFP_SPI3_MISO1
#define | SYS_GPD_MFPH_PD8MFP_I2C0_SCL
#define | SYS_GPD_MFPH_PD9MFP_GPIO
#define | SYS_GPD_MFPH_PD9MFP_SPI3_MOSI1
#define | SYS_GPD_MFPH_PD9MFP_I2C0_SDA
#define | SYS_GPD_MFPH_PD10MFP_GPIO
#define | SYS_GPD_MFPH_PD10MFP_SC3_DAT
#define | SYS_GPD_MFPH_PD10MFP_I2C4_SCL
#define | SYS_GPD_MFPH_PD11MFP_GPIO
#define | SYS_GPD_MFPH_PD11MFP_SC3_RST
#define | SYS_GPD_MFPH_PD11MFP_TM3_CNT_OUT
#define | SYS_GPD_MFPH_PD12MFP_GPIO
#define | SYS_GPD_MFPH_PD12MFP_SC3_CLK
#define | SYS_GPD_MFPH_PD12MFP_I2C4_SDA
#define | SYS_GPD_MFPH_PD13MFP_GPIO
#define | SYS_GPD_MFPH_PD13MFP_SPI1_SS0
#define | SYS_GPD_MFPH_PD13MFP_UART5_CTS
#define | SYS_GPD_MFPH_PD13MFP_ECAP0_IC2
#define | SYS_GPD_MFPH_PD14MFP_GPIO
#define | SYS_GPD_MFPH_PD14MFP_SPI1_CLK
#define | SYS_GPD_MFPH_PD14MFP_UART5_RTS
#define | SYS_GPD_MFPH_PD14MFP_ECAP0_IC1
#define | SYS_GPD_MFPH_PD15MFP_GPIO
#define | SYS_GPD_MFPH_PD15MFP_SPI1_MISO0
#define | SYS_GPD_MFPH_PD15MFP_UART5_TXD
#define | SYS_GPD_MFPH_PD15MFP_ECAP0_IC0
#define | SYS_GPE_MFPL_PE0MFP_GPIO
#define | SYS_GPE_MFPL_PE0MFP_ADC0_0
#define | SYS_GPE_MFPL_PE0MFP_INT4
#define | SYS_GPE_MFPL_PE1MFP_GPIO
#define | SYS_GPE_MFPL_PE1MFP_ADC0_1
#define | SYS_GPE_MFPL_PE1MFP_TM2_CNT_OUT
#define | SYS_GPE_MFPL_PE2MFP_GPIO
#define | SYS_GPE_MFPL_PE2MFP_ADC0_2
#define | SYS_GPE_MFPL_PE2MFP_ACMP0_O
#define | SYS_GPE_MFPL_PE2MFP_SPI0_MISO0
#define | SYS_GPE_MFPL_PE3MFP_GPIO
#define | SYS_GPE_MFPL_PE3MFP_ADC0_3
#define | SYS_GPE_MFPL_PE3MFP_ACMP0_P3
#define | SYS_GPE_MFPL_PE3MFP_SPI0_MOSI0
#define | SYS_GPE_MFPL_PE4MFP_GPIO
#define | SYS_GPE_MFPL_PE4MFP_ADC0_4
#define | SYS_GPE_MFPL_PE4MFP_ACMP0_P2
#define | SYS_GPE_MFPL_PE4MFP_SPI0_SS0
#define | SYS_GPE_MFPL_PE5MFP_GPIO
#define | SYS_GPE_MFPL_PE5MFP_ADC0_5
#define | SYS_GPE_MFPL_PE5MFP_ACMP0_P1
#define | SYS_GPE_MFPL_PE5MFP_SPI0_CLK
#define | SYS_GPE_MFPL_PE5MFP_SD0_CDn
#define | SYS_GPE_MFPL_PE6MFP_GPIO
#define | SYS_GPE_MFPL_PE6MFP_ADC0_6
#define | SYS_GPE_MFPL_PE6MFP_ACMP0_P0
#define | SYS_GPE_MFPL_PE6MFP_SPI0_MISO0
#define | SYS_GPE_MFPL_PE6MFP_SD0_CMD
#define | SYS_GPE_MFPL_PE6MFP_EBI_nWR
#define | SYS_GPE_MFPL_PE7MFP_GPIO
#define | SYS_GPE_MFPL_PE7MFP_ADC0_7
#define | SYS_GPE_MFPL_PE7MFP_ACMP0_N
#define | SYS_GPE_MFPL_PE7MFP_SPI0_MOSI0
#define | SYS_GPE_MFPL_PE7MFP_SD0_CLK
#define | SYS_GPE_MFPL_PE7MFP_EBI_nRD
#define | SYS_GPE_MFPH_PE8MFP_GPIO
#define | SYS_GPE_MFPH_PE8MFP_ADC0_8
#define | SYS_GPE_MFPH_PE8MFP_ADC1_0
#define | SYS_GPE_MFPH_PE8MFP_ACMP1_N
#define | SYS_GPE_MFPH_PE8MFP_TM1_CNT_OUT
#define | SYS_GPE_MFPH_PE8MFP_SD0_DAT3
#define | SYS_GPE_MFPH_PE8MFP_EBI_ALE
#define | SYS_GPE_MFPH_PE9MFP_GPIO
#define | SYS_GPE_MFPH_PE9MFP_ADC0_9
#define | SYS_GPE_MFPH_PE9MFP_ADC1_1
#define | SYS_GPE_MFPH_PE9MFP_ACMP1_P0
#define | SYS_GPE_MFPH_PE9MFP_SD0_DAT2
#define | SYS_GPE_MFPH_PE9MFP_EBI_nWRH
#define | SYS_GPE_MFPH_PE10MFP_GPIO
#define | SYS_GPE_MFPH_PE10MFP_ADC0_10
#define | SYS_GPE_MFPH_PE10MFP_ADC1_2
#define | SYS_GPE_MFPH_PE10MFP_ACMP1_P1
#define | SYS_GPE_MFPH_PE10MFP_SPI0_MISO1
#define | SYS_GPE_MFPH_PE10MFP_SD0_DAT1
#define | SYS_GPE_MFPH_PE10MFP_EBI_nWRL
#define | SYS_GPE_MFPH_PE11MFP_GPIO
#define | SYS_GPE_MFPH_PE11MFP_ADC0_11
#define | SYS_GPE_MFPH_PE11MFP_ADC1_3
#define | SYS_GPE_MFPH_PE11MFP_ACMP1_P2
#define | SYS_GPE_MFPH_PE11MFP_SPI0_MOSI1
#define | SYS_GPE_MFPH_PE11MFP_SD0_DAT0
#define | SYS_GPE_MFPH_PE11MFP_ACMP2_P3
#define | SYS_GPE_MFPH_PE11MFP_EBI_nCS0
#define | SYS_GPE_MFPH_PE12MFP_GPIO
#define | SYS_GPE_MFPH_PE12MFP_ADC1_4
#define | SYS_GPE_MFPH_PE12MFP_ACMP1_P3
#define | SYS_GPE_MFPH_PE12MFP_ACMP2_P2
#define | SYS_GPE_MFPH_PE12MFP_EBI_nCS1
#define | SYS_GPE_MFPH_PE13MFP_GPIO
#define | SYS_GPE_MFPH_PE13MFP_ADC1_5
#define | SYS_GPE_MFPH_PE13MFP_ACMP2_P1
#define | SYS_GPE_MFPH_PE13MFP_EBI_nCS2
#define | SYS_GPE_MFPH_PE14MFP_GPIO
#define | SYS_GPE_MFPH_PE14MFP_ADC1_6
#define | SYS_GPE_MFPH_PE14MFP_ACMP2_P0
#define | SYS_GPE_MFPH_PE14MFP_EBI_nCS3
#define | SYS_GPE_MFPH_PE15MFP_GPIO
#define | SYS_GPE_MFPH_PE15MFP_ADC1_7
#define | SYS_GPE_MFPH_PE15MFP_ACMP2_N
#define | SYS_GPF_MFPL_PF0MFP_GPIO
#define | SYS_GPF_MFPL_PF0MFP_SPI1_MOSI0
#define | SYS_GPF_MFPL_PF0MFP_UART5_RXD
#define | SYS_GPF_MFPL_PF0MFP_INT5
#define | SYS_GPF_MFPL_PF1MFP_GPIO
#define | SYS_GPF_MFPL_PF1MFP_SPI2_MOSI1
#define | SYS_GPF_MFPL_PF2MFP_GPIO
#define | SYS_GPF_MFPL_PF2MFP_SPI3_SS0
#define | SYS_GPF_MFPL_PF2MFP_SD0_DAT3
#define | SYS_GPF_MFPL_PF2MFP_EMAC_MII_RXD3
#define | SYS_GPF_MFPL_PF3MFP_GPIO
#define | SYS_GPF_MFPL_PF3MFP_SPI3_CLK
#define | SYS_GPF_MFPL_PF3MFP_SD0_DAT2
#define | SYS_GPF_MFPL_PF3MFP_EMAC_MII_RXD2
#define | SYS_GPF_MFPL_PF4MFP_GPIO
#define | SYS_GPF_MFPL_PF4MFP_SPI3_MISO0
#define | SYS_GPF_MFPL_PF4MFP_SD0_DAT1
#define | SYS_GPF_MFPL_PF4MFP_EMAC_MII_COL0
#define | SYS_GPF_MFPL_PF5MFP_GPIO
#define | SYS_GPF_MFPL_PF5MFP_SPI3_MOSI0
#define | SYS_GPF_MFPL_PF5MFP_SD0_DAT0
#define | SYS_GPF_MFPL_PF5MFP_EMAC_MII_CRS
#define | SYS_GPF_MFPL_PF6MFP_GPIO
#define | SYS_GPF_MFPL_PF6MFP_UART2_RXD
#define | SYS_GPF_MFPL_PF6MFP_SD0_CDn
#define | SYS_GPF_MFPL_PF6MFP_EMAC_MII_TXCLK
#define | SYS_GPF_MFPL_PF7MFP_GPIO
#define | SYS_GPF_MFPL_PF7MFP_UART2_TXD
#define | SYS_GPF_MFPL_PF7MFP_SD0_CMD
#define | SYS_GPF_MFPL_PF7MFP_EMAC_MII_TXD3
#define | SYS_GPF_MFPH_PF8MFP_GPIO
#define | SYS_GPF_MFPH_PF8MFP_UART2_RTS
#define | SYS_GPF_MFPH_PF8MFP_SD0_CLK
#define | SYS_GPF_MFPH_PF8MFP_EMAC_MII_TXD2
#define | SYS_GPF_MFPH_PF9MFP_GPIO
#define | SYS_GPF_MFPH_PF9MFP_OPA0_IN_P
#define | SYS_GPF_MFPH_PF9MFP_OPA0_P
#define | SYS_GPF_MFPH_PF9MFP_PWM0_CH0
#define | SYS_GPF_MFPH_PF9MFP_PWM0_0
#define | SYS_GPF_MFPH_PF10MFP_GPIO
#define | SYS_GPF_MFPH_PF10MFP_OPA0_IN_N
#define | SYS_GPF_MFPH_PF10MFP_OPA0_N
#define | SYS_GPF_MFPH_PF10MFP_PWM0_CH1
#define | SYS_GPF_MFPH_PF10MFP_PWM0_1
#define | SYS_GPF_MFPH_PF11MFP_GPIO
#define | SYS_GPF_MFPH_PF11MFP_OPA0_O
#define | SYS_GPF_MFPH_PF11MFP_UART1_RTS
#define | SYS_GPF_MFPH_PF12MFP_GPIO
#define | SYS_GPF_MFPH_PF12MFP_OPA1_IN_P
#define | SYS_GPF_MFPH_PF12MFP_OPA1_P
#define | SYS_GPF_MFPH_PF12MFP_UART1_CTS
#define | SYS_GPF_MFPH_PF13MFP_GPIO
#define | SYS_GPF_MFPH_PF13MFP_OPA1_IN_N
#define | SYS_GPF_MFPH_PF13MFP_OPA1_N
#define | SYS_GPF_MFPH_PF13MFP_UART1_TXD
#define | SYS_GPF_MFPH_PF14MFP_GPIO
#define | SYS_GPF_MFPH_PF14MFP_OPA1_O
#define | SYS_GPF_MFPH_PF14MFP_UART1_RXD
#define | SYS_GPF_MFPH_PF15MFP_GPIO
#define | SYS_GPF_MFPH_PF15MFP_UART0_RTS
#define | SYS_GPG_MFPL_PG0MFP_GPIO
#define | SYS_GPG_MFPL_PG0MFP_UART0_CTS
#define | SYS_GPG_MFPL_PG0MFP_INT6
#define | SYS_GPG_MFPL_PG1MFP_GPIO
#define | SYS_GPG_MFPL_PG1MFP_UART0_RXD
#define | SYS_GPG_MFPL_PG2MFP_GPIO
#define | SYS_GPG_MFPL_PG2MFP_UART0_TXD
#define | SYS_GPG_MFPL_PG3MFP_GPIO
#define | SYS_GPG_MFPL_PG3MFP_PS2_CLK
#define | SYS_GPG_MFPL_PG3MFP_I2S1_DO
#define | SYS_GPG_MFPL_PG3MFP_SC1_RST
#define | SYS_GPG_MFPL_PG4MFP_GPIO
#define | SYS_GPG_MFPL_PG4MFP_PS2_DAT
#define | SYS_GPG_MFPL_PG4MFP_I2S1_DI
#define | SYS_GPG_MFPL_PG4MFP_SC1_PWR
#define | SYS_GPG_MFPL_PG5MFP_GPIO
#define | SYS_GPG_MFPL_PG5MFP_I2S1_BCLK
#define | SYS_GPG_MFPL_PG5MFP_SC1_DAT
#define | SYS_GPG_MFPL_PG6MFP_GPIO
#define | SYS_GPG_MFPL_PG6MFP_I2S1_LRCK
#define | SYS_GPG_MFPL_PG6MFP_SC1_CLK
#define | SYS_GPG_MFPL_PG7MFP_GPIO
#define | SYS_GPG_MFPL_PG7MFP_SPI2_MISO0
#define | SYS_GPG_MFPL_PG7MFP_I2S1_MCLK
#define | SYS_GPG_MFPL_PG7MFP_SC1_CD
#define | SYS_GPG_MFPL_PG7MFP_SC3_RST
#define | SYS_GPG_MFPH_PG8MFP_GPIO
#define | SYS_GPG_MFPH_PG8MFP_SPI2_MOSI0
#define | SYS_GPG_MFPH_PG8MFP_I2S1_DO
#define | SYS_GPG_MFPH_PG8MFP_UART4_RTS
#define | SYS_GPG_MFPH_PG8MFP_SC3_DAT
#define | SYS_GPG_MFPH_PG9MFP_GPIO
#define | SYS_GPG_MFPH_PG9MFP_SPI2_CLK
#define | SYS_GPG_MFPH_PG9MFP_I2S1_DI
#define | SYS_GPG_MFPH_PG9MFP_UART4_CTS
#define | SYS_GPG_MFPH_PG9MFP_SC3_CLK
#define | SYS_GPG_MFPH_PG10MFP_GPIO
#define | SYS_GPG_MFPH_PG10MFP_ICE_CLK
#define | SYS_GPG_MFPH_PG10MFP_JTAG_TCLK
#define | SYS_GPG_MFPH_PG11MFP_GPIO
#define | SYS_GPG_MFPH_PG11MFP_ICE_DAT
#define | SYS_GPG_MFPH_PG11MFP_JTAG_TMS
#define | SYS_GPG_MFPH_PG12MFP_GPIO
#define | SYS_GPG_MFPH_PG12MFP_XT1_OUT
#define | SYS_GPG_MFPH_PG13MFP_GPIO
#define | SYS_GPG_MFPH_PG13MFP_XT1_IN
#define | SYS_GPG_MFPH_PG14MFP_GPIO
#define | SYS_GPG_MFPH_PG14MFP_X32K_OUT
#define | SYS_GPG_MFPH_PG14MFP_I2C1_SDA
#define | SYS_GPG_MFPH_PG15MFP_GPIO
#define | SYS_GPG_MFPH_PG15MFP_X32K_IN
#define | SYS_GPG_MFPH_PG15MFP_I2C1_SCL
#define | SYS_GPH_MFPL_PH0MFP_GPIO
#define | SYS_GPH_MFPL_PH0MFP_I2C1_SCL
#define | SYS_GPH_MFPL_PH0MFP_UART4_RXD
#define | SYS_GPH_MFPL_PH0MFP_CAN1_RXD
#define | SYS_GPH_MFPL_PH0MFP_INT7
#define | SYS_GPH_MFPL_PH1MFP_GPIO
#define | SYS_GPH_MFPL_PH1MFP_UART4_TXD
#define | SYS_GPH_MFPL_PH1MFP_I2C1_SDA
#define | SYS_GPH_MFPL_PH1MFP_CAN1_TXD
#define | SYS_GPH_MFPL_PH2MFP_GPIO
#define | SYS_GPH_MFPL_PH2MFP_UART2_CTS
#define | SYS_GPH_MFPL_PH3MFP_GPIO
#define | SYS_GPH_MFPL_PH3MFP_I2C3_SCL
#define | SYS_GPH_MFPL_PH4MFP_GPIO
#define | SYS_GPH_MFPL_PH4MFP_I2C3_SDA
#define | SYS_GPH_MFPL_PH5MFP_GPIO
#define | SYS_GPH_MFPL_PH5MFP_SPI2_SS0
#define | SYS_GPH_MFPL_PH6MFP_GPIO
#define | SYS_GPH_MFPL_PH6MFP_SPI2_CLK
#define | SYS_GPH_MFPL_PH7MFP_GPIO
#define | SYS_GPH_MFPL_PH7MFP_SPI2_MISO0
#define | SYS_GPH_MFPH_PH8MFP_GPIO
#define | SYS_GPH_MFPH_PH8MFP_SPI2_MOSI0
#define | SYS_GPH_MFPH_PH9MFP_GPIO
#define | SYS_GPH_MFPH_PH9MFP_SPI2_MISO1
#define | SYS_GPH_MFPH_PH10MFP_GPIO
#define | SYS_GPH_MFPH_PH10MFP_SPI2_MOSI1
#define | SYS_GPH_MFPH_PH11MFP_GPIO
#define | SYS_GPH_MFPH_PH11MFP_UART3_RXD
#define | SYS_GPH_MFPH_PH12MFP_GPIO
#define | SYS_GPH_MFPH_PH12MFP_UART3_TXD
#define | SYS_GPH_MFPH_PH13MFP_GPIO
#define | SYS_GPH_MFPH_PH13MFP_UART3_RTS
#define | SYS_GPH_MFPH_PH14MFP_GPIO
#define | SYS_GPH_MFPH_PH14MFP_UART3_CTS
#define | SYS_GPH_MFPH_PH15MFP_GPIO
#define | SYS_GPH_MFPH_PH15MFP_SC5_CLK
#define | SYS_GPI_MFPL_PI0MFP_GPIO
#define | SYS_GPI_MFPL_PI0MFP_SC5_RST
#define | SYS_GPI_MFPL_PI1MFP_GPIO
#define | SYS_GPI_MFPL_PI1MFP_SC5_PWR
#define | SYS_GPI_MFPL_PI2MFP_GPIO
#define | SYS_GPI_MFPL_PI2MFP_SC5_DAT
#define | SYS_GPI_MFPL_PI3MFP_GPIO
#define | SYS_GPI_MFPL_PI3MFP_SPI3_SS0
#define | SYS_GPI_MFPL_PI4MFP_GPIO
#define | SYS_GPI_MFPL_PI4MFP_SPI3_CLK
#define | SYS_GPI_MFPL_PI5MFP_GPIO
#define | SYS_GPI_MFPL_PI5MFP_SPI3_MISO0
#define | SYS_GPI_MFPL_PI6MFP_GPIO
#define | SYS_GPI_MFPL_PI6MFP_SPI3_MOSI0
#define | SYS_GPI_MFPL_PI7MFP_GPIO
#define | SYS_GPI_MFPL_PI7MFP_I2C2_SCL
#define | SYS_GPI_MFPL_PI7MFP_SPI3_MISO1
#define | SYS_GPI_MFPH_PI8MFP_GPIO
#define | SYS_GPI_MFPH_PI8MFP_I2C2_SDA
#define | SYS_GPI_MFPH_PI8MFP_SPI3_MOSI1
#define | SYS_GPI_MFPH_PI9MFP_GPIO
#define | SYS_GPI_MFPH_PI9MFP_I2C4_SCL
#define | SYS_GPI_MFPH_PI10MFP_GPIO
#define | SYS_GPI_MFPH_PI11MFP_GPIO
#define | SYS_GPI_MFPH_PI11MFP_SPI2_SS0
#define | SYS_GPI_MFPH_PI11MFP_I2S1_BCLK
#define | SYS_GPI_MFPH_PI11MFP_I2C4_SCL
#define | SYS_GPI_MFPH_PI11MFP_SC3_PWR
#define | SYS_GPI_MFPH_PI12MFP_GPIO
#define | SYS_GPI_MFPH_PI12MFP_SPI2_MISO1
#define | SYS_GPI_MFPH_PI12MFP_I2S1_LRCK
#define | SYS_GPI_MFPH_PI12MFP_I2C4_SDA
#define | SYS_GPI_MFPH_PI12MFP_SC3_CD
#define | SYS_GPI_MFPH_PI13MFP_GPIO
#define | SYS_GPI_MFPH_PI14MFP_GPIO
#define | SYS_GPI_MFPH_PI15MFP_GPIO
#define | SYS_CLEAR_BOD_INT_FLAG() (SYS->BODCTL |= SYS_BODCTL_BODINTF_Msk)
| Clear Brown-out detector interrupt flag. More...
#define | SYS_CLEAR_BOD_LPM() (SYS->BODCTL &= ~SYS_BODCTL_BODLPM_Msk)
| Set Brown-out detector function to normal mode. More...
#define | SYS_DISABLE_BOD() (SYS->BODCTL &= ~SYS_BODCTL_BODEN_Msk)
| Disable Brown-out detector function. More...
#define | SYS_ENABLE_BOD() (SYS->BODCTL |= SYS_BODCTL_BODEN_Msk)
| Enable Brown-out detector function. More...
#define | SYS_GET_BOD_INT_FLAG() (SYS->BODCTL & SYS_BODCTL_BODINTF_Msk)
| Get Brown-out detector interrupt flag. More...
#define | SYS_GET_BOD_OUTPUT() (SYS->BODCTL & SYS_BODCTL_BODOUT_Msk)
| Get Brown-out detector status. More...
#define | SYS_DISABLE_BOD_RST() (SYS->BODCTL &= ~SYS_BODCTL_BODRSTEN_Msk)
| Disable Brown-out detector interrupt function. More...
#define | SYS_ENABLE_BOD_RST() (SYS->BODCTL |= SYS_BODCTL_BODRSTEN_Msk)
| Enable Brown-out detector reset function. More...
#define | SYS_SET_BOD_LPM() (SYS->BODCTL |= SYS_BODCTL_BODLPM_Msk)
| Set Brown-out detector function low power mode. More...
#define | SYS_SET_BOD_LEVEL(u32Level) (SYS->BODCTL = (SYS->BODCTL & ~SYS_BODCTL_BODVL_Msk) | u32Level)
| Set Brown-out detector voltage level. More...
#define | SYS_IS_BOD_RST() (SYS->RSTSTS & SYS_RSTSTS_BODRF_Msk)
| Get reset source is from Brown-out detector reset. More...
#define | SYS_IS_CPU_RST() (SYS->RSTSTS & SYS_RSTSTS_CPURF_Msk)
| Get reset source is from CPU reset. More...
#define | SYS_IS_LVR_RST() (SYS->RSTSTS & SYS_RSTSTS_LVRF_Msk)
| Get reset source is from LVR Reset. More...
#define | SYS_IS_POR_RST() (SYS->RSTSTS & SYS_RSTSTS_PORF_Msk)
| Get reset source is from Power-on Reset. More...
#define | SYS_IS_RSTPIN_RST() (SYS->RSTSTS & SYS_RSTSTS_PINRF_Msk)
| Get reset source is from reset pin reset. More...
#define | SYS_IS_SYSTEM_RST() (SYS->RSTSTS & SYS_RSTSTS_SYSRF_Msk)
| Get reset source is from system reset. More...
#define | SYS_IS_WDT_RST() (SYS->RSTSTS & SYS_RSTSTS_WDTRF_Msk)
| Get reset source is from window watch dog reset. More...
#define | SYS_DISABLE_LVR() (SYS->BODCTL &= ~SYS_BODCTL_LVREN_Msk)
| Disable Low-Voltage-Reset function. More...
#define | SYS_ENABLE_LVR() (SYS->BODCTL |= SYS_BODCTL_LVREN_Msk)
| Enable Low-Voltage-Reset function. More...
#define | SYS_DISABLE_POR() (SYS->PORCTL = 0x5AA5)
| Disable Power-on Reset function. More...
#define | SYS_ENABLE_POR() (SYS->PORCTL = 0)
| Enable Power-on Reset function. More...
#define | SYS_CLEAR_RST_SOURCE(u32RstSrc) (SYS->RSTSTS = u32RstSrc )
| Clear reset source flag. More...

## Functions
void | SYS_ClearResetSrc (uint32_t u32RstSrc)
| This function clear the selected system reset source. More...
uint32_t | SYS_GetBODStatus ()
| This function get Brown-out detector output status. More...
uint32_t | SYS_GetResetSrc (void)
| This function get the system reset source register value. More...
uint32_t | SYS_IsRegLocked (void)
| This function check register write-protection bit setting. More...
void | SYS_LockReg (void)
| This function enable register write-protection function. More...
void | SYS_UnlockReg (void)
| This function disable register write-protection function. More...
uint32_t | SYS_ReadPDID (void)
| This function get product ID. More...
void | SYS_ResetChip (void)
| This function reset chip. More...
void | SYS_ResetCPU (void)
| This function reset CPU. More...
void | SYS_ResetModule (uint32_t u32ModuleIndex)
| This function reset selected modules. More...
void | SYS_EnableBOD (int32_t i32Mode, uint32_t u32BODLevel)
| This function configure BOD function. Configure BOD reset or interrupt mode and set Brown-out voltage level. Enable Brown-out function. More...
void | SYS_DisableBOD (void)
| This function disable BOD function. More...

## Detailed Description

NUC472/NUC442 SYS Header File.

Version
  V1.0 $Revision 1 $

Date
  15/10/21 1:35p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file sys.h.