| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
PWM_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CLKPSC
__IO uint32_t | CLKDIV
__IO uint32_t | CTL
__IO uint32_t | CNTEN
__IO uint32_t | PERIOD [6]
__IO uint32_t | CMPDAT [6]
__I uint32_t | CNT [6]
__IO uint32_t | MSKEN
__IO uint32_t | MSK
__IO uint32_t | DTCTL
__IO uint32_t | TRGADCTL
__IO uint32_t | TRGADCSTS
__IO uint32_t | BRKCTL
__IO uint32_t | INTCTL
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | POEN
__IO uint32_t | CAPCTL
__IO uint32_t | CAPINEN
__I uint32_t | CAPSTS
__I uint32_t | RCAPDAT0
__I uint32_t | FCAPDAT0
__I uint32_t | RCAPDAT1
__I uint32_t | FCAPDAT1
__I uint32_t | RCAPDAT2
__I uint32_t | FCAPDAT2
__I uint32_t | RCAPDAT3
__I uint32_t | FCAPDAT3
__I uint32_t | RCAPDAT4
__I uint32_t | FCAPDAT4
__I uint32_t | RCAPDAT5
__I uint32_t | FCAPDAT5
__I uint32_t | SBS [6]

## Detailed Description

    @addtogroup PWM Pulse Width Modulation Controller(PWM)
    Memory Mapped Structure for PWM Controller

Definition at line 19042 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h