| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
SCLIB_CARD_INFO_T Struct Reference
NUC472/NUC442 Library » Smartcard Library » Smartcard Library Exported Constants » Smartcard Library Exported Structs

A structure holds smartcard information. More...

`#include <sclib.h>`

## Data Fields
uint32_t | T
| Protocol, ether SCLIB_PROTOCOL_T0 or SCLIB_PROTOCOL_T1. More...
uint32_t | ATR_Len
| ATR length, between SCLIB_MAX_ATR_LEN and SCLIB_MIN_ATR_LEN. More...
uint8_t | ATR_Buf [SCLIB_MAX_ATR_LEN]
| Buffer holds ATR answered by smartcard. More...

## Detailed Description

A structure holds smartcard information.

Definition at line 97 of file sclib.h.

The documentation for this struct was generated from the following file:

- SmartcardLib/Include/sclib.h