| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
ECAP_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CNT
__IO uint32_t | HOLD0
__IO uint32_t | HOLD1
__IO uint32_t | HOLD2
__IO uint32_t | CNTCMP
__IO uint32_t | CTL0
__IO uint32_t | CTL1
__IO uint32_t | STATUS

## Detailed Description

    @addtogroup ECAP Enhanced Input Capture Timer(ECAP)
    Memory Mapped Structure for ECAP Controller

Definition at line 2422 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h